<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<!--This file is created by the TCatPlcCtrl automatically. Manually changes will be overwritten!-->
<PlcProjectInfo xmlns:p="http://www.beckhoff.com/2002/01/TcPlcProjectDesc">
	<ProjectInfo>
		<Path>C:\Focke\M741\74116931.pro</Path>
		<IsLibrary>false</IsLibrary>
		<ChangeDate>2021-10-28T21:29:12</ChangeDate>
		<Library>
			<Name>FC800.lib</Name>
			<Path>C:\TWINCAT\PLC\LIB\FC800.lib</Path>
		</Library>
		<Library>
			<Name>STANDARD.LIB</Name>
			<Path>C:\TWINCAT\PLC\LIB\STANDARD.LIB</Path>
			<ChangeDate>1998-06-05T19:03:02</ChangeDate>
		</Library>
		<Library>
			<Name>PlcSystem.lib</Name>
			<Path>C:\TWINCAT\PLC\LIB\PlcSystem.lib</Path>
			<ChangeDate>2001-07-19T19:03:02</ChangeDate>
		</Library>
	</ProjectInfo>
	<RoutingInfo>
		<AdsInfo>
			<NetId>150.150.98.3.1.1</NetId>
			<Port>811</Port>
			<TargetName>
				<![CDATA[Target: Local (150.150.98.3.1.1), Run Time: 2]]>
			</TargetName>
		</AdsInfo>
	</RoutingInfo>
	<CompilerInfo>
		<CpuFamily>x86</CpuFamily>
		<CompilerVersion>2.9.10.0</CompilerVersion>
		<Alignment>Byte</Alignment>
		<PackSize>1</PackSize>
		<TwinCATVersion>2.10.0</TwinCATVersion>
		<TCatPlcCtrlVersion>2.10.1016</TCatPlcCtrlVersion>
	</CompilerInfo>
	<TargetInfo>
		<CpuFamily>x86</CpuFamily>
		<DataAreaInfo>
			<DataSize>1048576</DataSize>
			<RetainSize>32768</RetainSize>
			<MAreaSize>32768</MAreaSize>
			<InputSize>16384</InputSize>
			<OutputSize>16384</OutputSize>
			<MaxNumOfPOUs>2048</MaxNumOfPOUs>
		</DataAreaInfo>
	</TargetInfo>
	<TaskInfos>
		<TaskInfo>
			<Name>TASK1</Name>
			<Priority>0</Priority>
			<CycleTime>2</CycleTime>
			<CycleTimeUs>2000</CycleTimeUs>
			<Calls>
				<ProgramCall>_CPU1</ProgramCall>
			</Calls>
		</TaskInfo>
		<TaskInfo>
			<Name>TASK2</Name>
			<Priority>1</Priority>
			<CycleTime>20</CycleTime>
			<CycleTimeUs>20000</CycleTimeUs>
			<Calls>
				<ProgramCall>_CPU2</ProgramCall>
			</Calls>
		</TaskInfo>
		<TaskInfo>
			<Name>TASK3</Name>
			<Priority>2</Priority>
			<CycleTime>100</CycleTime>
			<CycleTimeUs>100000</CycleTimeUs>
			<Calls>
				<ProgramCall>_INTERVAL</ProgramCall>
			</Calls>
		</TaskInfo>
	</TaskInfos>
	<DirectoryInfos>
		<DirectoryInfo>
			<Type>LibraryDir</Type>
			<Path>C:\TWINCAT\PLC\LIB\</Path>
		</DirectoryInfo>
		<DirectoryInfo>
			<Type>CompileDir</Type>
			<Path>C:\TWINCAT\PLC\</Path>
		</DirectoryInfo>
	</DirectoryInfos>
	<DataTypes>
		<DataType>
			<Name Decoration="102F59AF" Crc32="0820300822" LastChange="2018-05-25T18:55:28">SFC_RESERVOIR</Name>
			<BitSize>376</BitSize>
			<SubItem>
				<Name>TRANS</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name>TRANS_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name>TRANS_3</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name>TRANS_4</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name>PACKET_SENSOR_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name>PACKET_SENSOR_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name>EXIT_STOP_SENSOR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name>INIT</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_INIT</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name>CLOSE_EXIT_STOP_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>72</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_CLOSE_EXIT_STOP_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<SubItem>
				<Name>CLOSE_INFEED_STOP_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>88</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_CLOSE_INFEED_STOP_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name>ROTATION_POSITION_FILLING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_ROTATION_POSITION_FILLING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>112</BitOffs>
			</SubItem>
			<SubItem>
				<Name>PACKET_GUIDE_UPPER_BELT_RAISING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>120</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_PACKET_GUIDE_UPPER_BELT_RAISING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>128</BitOffs>
			</SubItem>
			<SubItem>
				<Name>PACKET_GUIDE_UPPER_BELT_LOWERING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_PACKET_GUIDE_UPPER_BELT_LOWERING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>144</BitOffs>
			</SubItem>
			<SubItem>
				<Name>OPEN_INFEED_STOP_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>152</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_OPEN_INFEED_STOP_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>160</BitOffs>
			</SubItem>
			<SubItem>
				<Name>END_FILLING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>168</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_END_FILLING_1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>176</BitOffs>
			</SubItem>
			<SubItem>
				<Name>CLOSE_INFEED_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>184</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_CLOSE_INFEED_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>192</BitOffs>
			</SubItem>
			<SubItem>
				<Name>CLOSE_EXIT_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>200</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_CLOSE_EXIT_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>208</BitOffs>
			</SubItem>
			<SubItem>
				<Name>ROTATION_POSITION_CLEARING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>216</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_ROTATION_POSITION_CLEARING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>224</BitOffs>
			</SubItem>
			<SubItem>
				<Name>PACKET_GUIDE_UPPER_BELT_RAISING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>232</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_PACKET_GUIDE_UPPER_BELT_RAISING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>240</BitOffs>
			</SubItem>
			<SubItem>
				<Name>PACKET_GUIDE_UPPER_BELT_LOWERING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>248</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_PACKET_GUIDE_UPPER_BELT_LOWERING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>256</BitOffs>
			</SubItem>
			<SubItem>
				<Name>OPEN_EXIT_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>264</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_OPEN_EXIT_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>272</BitOffs>
			</SubItem>
			<SubItem>
				<Name>OPEN_INFEED_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>280</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_OPEN_INFEED_STOP_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>288</BitOffs>
			</SubItem>
			<SubItem>
				<Name>END_CLEARING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>296</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_END_CLEARING_2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>304</BitOffs>
			</SubItem>
			<SubItem>
				<Name>FINAL_POSITION_FILLING_3</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>312</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_FINAL_POSITION_FILLING_3</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>320</BitOffs>
			</SubItem>
			<SubItem>
				<Name>FINAL_POSITION_CLEARING_4</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_FINAL_POSITION_CLEARING_4</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>336</BitOffs>
			</SubItem>
			<SubItem>
				<Name>END_FINAL_POSITION_CLEARING_4</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name>_END_FINAL_POSITION_CLEARING_4</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>352</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input">SFCPause</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>360</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input">SFCInit</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>368</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>326</CodeIndex>
				<InitIndex>327</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001024D">ARRAY [0..255] OF WORD</Name>
			<Type>WORD</Type>
			<BitSize>4096</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>256</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="20017954">ARRAY [1..4] OF SYSTEMTASKINFOTYPE</Name>
			<Type Decoration="100863C1">SYSTEMTASKINFOTYPE</Type>
			<BitSize>1056</BitSize>
			<ArrayInfo>
				<LBound>1</LBound>
				<Elements>4</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001034D">ARRAY [0..511] OF WORD</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Kurven 						/ 	cams]]>
			</Comment>
			<BitSize>8192</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>512</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="1003051C" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">R_TRIG</Name>
			<BitSize>24</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">M</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CLK</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Signal to detect]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Edge detected]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>217</CodeIndex>
				<InitIndex>218</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10060D24" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">TOF</Name>
			<BitSize>120</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">M</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[internal variable]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">StartTime</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[internal variable]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">IN</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[starts timer with falling edge, resets timer with rising edge]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">PT</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[time to pass, before Q is set]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[is FALSE, PT seconds after IN had a falling edge]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">ET</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[elapsed time]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>88</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>227</CodeIndex>
				<InitIndex>228</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10060D24" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">TON</Name>
			<BitSize>120</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">M</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[internal variable]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">StartTime</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[internal variable]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">IN</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[starts timer with rising edge, resets timer with falling edge]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">PT</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[time to pass, before Q is set]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[is TRUE, PT seconds after IN had a rising edge]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">ET</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[elapsed time]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>88</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>229</CodeIndex>
				<InitIndex>230</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="1003051C" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">F_TRIG</Name>
			<BitSize>24</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">M</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CLK</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Signal to detect]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Edge detected]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>210</CodeIndex>
				<InitIndex>211</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="1010B9A5" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">FILEOPEN</Name>
			<BitSize>2520</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">OPEN_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<Comment>
					<![CDATA[ams net id]]>
				</Comment>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">FPATHNAME</Name>
				<Type Decoration="40000101">STRING(256)</Type>
				<Comment>
					<![CDATA[max filename length = 256]]>
				</Comment>
				<BitSize>2056</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">OPENMODE</Name>
				<Type>DWORD</Type>
				<Comment>
					<![CDATA[create (for write - default), open for write, open for read]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>2384</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">OPEN</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[open control input]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>2416</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>2424</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>2456</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>2464</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>2472</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">HFILE</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>2504</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>270</CodeIndex>
				<InitIndex>271</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100E6FAC" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">FILECLOSE</Name>
			<BitSize>432</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLOSE_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<Comment>
					<![CDATA[ams net id]]>
				</Comment>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">HFILE</Name>
				<Type>UINT</Type>
				<Comment>
					<![CDATA[file handle obtained through 'open']]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLOSE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[close control input]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>352</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>384</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>392</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>400</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>268</CodeIndex>
				<InitIndex>269</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10117973" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">FILEREAD</Name>
			<BitSize>528</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READ_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<Comment>
					<![CDATA[ams net id]]>
				</Comment>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">HFILE</Name>
				<Type>UINT</Type>
				<Comment>
					<![CDATA[file handle]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUFADDR</Name>
				<Type>DWORD</Type>
				<Comment>
					<![CDATA[buffer address for read]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">COUNT</Name>
				<Type>UDINT</Type>
				<Comment>
					<![CDATA[count of bytes for read]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READ</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[read/write control input]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>416</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>448</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>456</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>464</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">COUNT_R</Name>
				<Type>UDINT</Type>
				<Comment>
					<![CDATA[count of bytes actually read]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>496</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>272</CodeIndex>
				<InitIndex>273</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10117A8C" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">FILEWRITE</Name>
			<BitSize>528</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITE_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<Comment>
					<![CDATA[ams net id]]>
				</Comment>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">HFILE</Name>
				<Type>UINT</Type>
				<Comment>
					<![CDATA[file handle]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUFADDR</Name>
				<Type>DWORD</Type>
				<Comment>
					<![CDATA[buffer address for write]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">COUNT</Name>
				<Type>UDINT</Type>
				<Comment>
					<![CDATA[count of bytes for write]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[write control input]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>416</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>448</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>456</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>464</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">COUNT_W</Name>
				<Type>UDINT</Type>
				<Comment>
					<![CDATA[count of bytes actually written]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>496</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>276</CodeIndex>
				<InitIndex>277</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100306C8" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RS</Name>
			<BitSize>24</BitSize>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">SET</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RESET1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>221</CodeIndex>
				<InitIndex>222</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100306C6" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">SR</Name>
			<BitSize>24</BitSize>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">SET1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RESET</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>225</CodeIndex>
				<InitIndex>226</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10050B9B" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">TP</Name>
			<BitSize>112</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">StartTime</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[internal variable]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">IN</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Trigger for Start of the Signal]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">PT</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[The length of the High-Signal in 10ms]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[The pulse]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>72</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">ET</Name>
				<Type>TIME</Type>
				<Comment>
					<![CDATA[The current phase of the High-Signal]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>231</CodeIndex>
				<InitIndex>232</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10060AFD" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CTD</Name>
			<BitSize>64</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">M</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Variable for CD Edge Detection]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Count Down on rising edge]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LOAD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Load Start Value]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">PV</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[Start Value]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Counter reached 0]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CV</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[Current Counter Value]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>203</CodeIndex>
				<InitIndex>204</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10060B75" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CTU</Name>
			<BitSize>64</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">M</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Variable for CU Edge Detection]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CU</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Count Up]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RESET</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Reset Counter to 0]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">PV</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[Counter Limit]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">Q</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Counter reached the Limit]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CV</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[Current Counter Value]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>205</CodeIndex>
				<InitIndex>206</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100A13D0" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CTUD</Name>
			<BitSize>96</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">MU</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Variable for CU Edge Detection]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">MD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Variable for CD Edge Detection]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CU</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Count Up]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Count Down]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RESET</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Reset Counter to Null]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LOAD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Load Start Value]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">PV</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[Start Value / Counter Limit]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">QU</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Counter reached Limit]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">QD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[Counter reached Null]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>72</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CV</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[Current Counter Value]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>207</CodeIndex>
				<InitIndex>208</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100409DC" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">SEMA</Name>
			<BitSize>32</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">X</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CLAIM</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RELEASE</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>223</CodeIndex>
				<InitIndex>224</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="1010B86F" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSRDDEVINFO</Name>
			<BitSize>624</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RDINFO_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RDINFO</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>352</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>384</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>392</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>400</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DEVNAME</Name>
				<Type Decoration="40000014">STRING(19)</Type>
				<BitSize>160</BitSize>
				<BitOffs>432</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DEVVER</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>592</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>236</CodeIndex>
				<InitIndex>237</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10107803" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSRDSTATE</Name>
			<BitSize>464</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RDSTATE_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RDSTATE</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>352</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>384</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>392</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>400</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSSTATE</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>432</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DEVSTATE</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>448</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>238</CodeIndex>
				<InitIndex>239</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10158AAA" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSRDWRT</Name>
			<BitSize>656</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRTRD_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PDESTADDR_I</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>168</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>360</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITELEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>440</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READLEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>472</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SRCADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>504</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DESTADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>536</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRTRD</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>568</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>576</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>608</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>616</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>624</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>240</CodeIndex>
				<InitIndex>241</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10168E90" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSRDWRTEX</Name>
			<BitSize>688</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRTRD_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PDESTADDR_I</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>168</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>360</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITELEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>440</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READLEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>472</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SRCADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>504</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DESTADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>536</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRTRD</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>568</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>576</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>608</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>616</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>624</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">COUNT_R</Name>
				<Type>UDINT</Type>
				<Comment>
					<![CDATA[count of bytes actually read]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>656</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>242</CodeIndex>
				<InitIndex>243</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100B6644" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSRDWRTIND</Name>
			<BitSize>424</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEAR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEAR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">VALID</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>216</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">INVOKEID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>232</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>264</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>296</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RDLENGTH</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRTLENGTH</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>360</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DATAADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>392</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>244</CodeIndex>
				<InitIndex>245</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10085BA4" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSRDWRTRES</Name>
			<BitSize>352</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESPOND_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>200</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">INVOKEID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>216</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESULT</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>248</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>280</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DATAADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>312</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESPOND</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>246</CodeIndex>
				<InitIndex>247</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10127C36" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSREAD</Name>
			<BitSize>560</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READ_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DESTADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>440</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READ</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>472</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>480</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>512</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>520</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>528</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>248</CodeIndex>
				<InitIndex>249</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10137FF5" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSREADEX</Name>
			<BitSize>592</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READ_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DESTADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>440</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">READ</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>472</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>480</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>512</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>520</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>528</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">COUNT_R</Name>
				<Type>UDINT</Type>
				<Comment>
					<![CDATA[count of bytes actually read]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>560</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>250</CodeIndex>
				<InitIndex>251</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10095D93" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSREADIND</Name>
			<BitSize>360</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEAR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEAR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">VALID</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>216</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">INVOKEID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>232</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>264</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>296</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LENGTH</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>252</CodeIndex>
				<InitIndex>253</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10085BA4" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSREADRES</Name>
			<BitSize>352</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESPOND_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>200</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">INVOKEID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>216</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESULT</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>248</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>280</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DATAADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>312</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESPOND</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>254</CodeIndex>
				<InitIndex>255</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10127CAC" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSWRITE</Name>
			<BitSize>560</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITE_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SRCADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>440</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITE</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>472</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>480</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>512</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>520</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>528</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>256</CodeIndex>
				<InitIndex>257</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100A6162" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSWRITEIND</Name>
			<BitSize>392</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEAR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEAR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">VALID</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>216</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">INVOKEID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>232</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXGRP</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>264</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">IDXOFFS</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>296</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LENGTH</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DATAADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>360</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>258</CodeIndex>
				<InitIndex>259</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10065567" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSWRITERES</Name>
			<BitSize>288</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESPOND_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>200</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">INVOKEID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>216</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESULT</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>248</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">RESPOND</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>280</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>260</CodeIndex>
				<InitIndex>261</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10127D1A" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSWRTCTL</Name>
			<BitSize>528</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITE_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PORT</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSSTATE</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DEVSTATE</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>360</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LEN</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SRCADDR</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITE</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>440</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>448</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>480</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>488</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>496</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>262</CodeIndex>
				<InitIndex>263</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001024B">ARRAY [0..249] OF UINT</Name>
			<Type>UINT</Type>
			<BitSize>4000</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>250</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="10063C57" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">DRAND</Name>
			<BitSize>4136</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">FirstCall_i</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">HoldRand_i</Name>
				<Type>DINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">R250_Buffer_i</Name>
				<Type Decoration="2001024B">ARRAY [0..249] OF UINT</Type>
				<BitSize>4000</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">R250_Index</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>4040</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">Seed</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>4056</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">Num</Name>
				<Type>LREAL</Type>
				<BitSize>64</BitSize>
				<BitOffs>4072</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>266</CodeIndex>
				<InitIndex>267</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100F7316" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">FILESEEK</Name>
			<BitSize>464</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">STAMP_I</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ACCESSCNT_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">WRITE_SAV_I</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TICKSTART_I</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">NETID</Name>
				<Type Decoration="40000018">STRING(23)</Type>
				<Comment>
					<![CDATA[ams net id]]>
				</Comment>
				<BitSize>192</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">HFILE</Name>
				<Type>UINT</Type>
				<Comment>
					<![CDATA[file handle]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SEEKPOS</Name>
				<Type>UDINT</Type>
				<Comment>
					<![CDATA[byte number for seek set]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SEEK</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[seek control input]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>376</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">TMOUT</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>384</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">BUSY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>416</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>424</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ERRID</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>432</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>274</CodeIndex>
				<InitIndex>275</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10010527" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">GETCPUACCOUNT</Name>
			<BitSize>32</BitSize>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">cpuAccountDW</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>279</CodeIndex>
				<InitIndex>280</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="1002092B" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">GETCPUCOUNTER</Name>
			<BitSize>64</BitSize>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">cpuCntLoDW</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">cpuCntHiDW</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>281</CodeIndex>
				<InitIndex>282</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100102BD" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">GETCURTASKINDEX</Name>
			<BitSize>8</BitSize>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">index</Name>
				<Type>BYTE</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>283</CodeIndex>
				<InitIndex>284</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100207EF" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">GETSYSTEMTIME</Name>
			<BitSize>64</BitSize>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">timeLoDW</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">timeHiDW</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>285</CodeIndex>
				<InitIndex>286</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10066081" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SYSTEMINFOTYPE</Name>
			<BitSize>320</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">runTimeNo</Name>
				<Type>BYTE</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">projectName</Name>
				<Type Decoration="40000021">STRING(32)</Type>
				<BitSize>264</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">numberOfTasks</Name>
				<Type>BYTE</Type>
				<BitSize>8</BitSize>
				<BitOffs>272</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">onlineChangeCount</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>280</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">bootDataFlags</Name>
				<Type>BYTE</Type>
				<BitSize>8</BitSize>
				<BitOffs>296</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">systemStateFlags</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>304</BitOffs>
			</SubItem>
		</DataType>
		<DataType>
			<Name Decoration="100863C1" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SYSTEMTASKINFOTYPE</Name>
			<BitSize>264</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">active</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">taskName</Name>
				<Type Decoration="40000011">STRING(16)</Type>
				<BitSize>136</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">firstCycle</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>144</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">cycleTimeExceeded</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>152</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">cycleTime</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>160</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">lastExecTime</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>192</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">priority</Name>
				<Type>BYTE</Type>
				<BitSize>8</BitSize>
				<BitOffs>224</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">cycleCount</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>232</BitOffs>
			</SubItem>
		</DataType>
		<DataType>
			<Name Decoration="2001034D" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB512</Name>
			<Type Decoration="2001034D">ARRAY [0..511] OF WORD</Type>
			<BitSize>8192</BitSize>
		</DataType>
		<DataType>
			<Name Decoration="2001024D" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DATABLOCK</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<BitSize>4096</BitSize>
		</DataType>
		<DataType>
			<Name Decoration="2001054D">ARRAY [0..1023] OF WORD</Name>
			<Type>WORD</Type>
			<BitSize>16384</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>1024</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001054D" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB1024</Name>
			<Type Decoration="2001054D">ARRAY [0..1023] OF WORD</Type>
			<BitSize>16384</BitSize>
		</DataType>
		<DataType>
			<Name Decoration="2001024E">ARRAY [0..256] OF WORD</Name>
			<Type>WORD</Type>
			<BitSize>4112</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>257</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="1025E07C" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB_FILE_DB256</Name>
			<BitSize>13624</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D: Anzahl Bytes im Datenblock
								GB: 	Number of bytes in block	
								E: 	Número de bytes en bloque						
								F:	nombre de bytes dans le bloc]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">REQUEST_LOAD</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">REQUEST_SAVE</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VERIFY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TIMEOUT</Name>
				<Type Decoration="10060D24">TON</Type>
				<BitSize>120</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TMAX</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>160</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">STEP_LOAD</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>192</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">STEP_SAVE</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>208</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">T_DELAY</Name>
				<Type Decoration="10060D24">TON</Type>
				<BitSize>120</BitSize>
				<BitOffs>224</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RT_LOAD</Name>
				<Type Decoration="1003051C">R_TRIG</Type>
				<BitSize>24</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RT_SAVE</Name>
				<Type Decoration="1003051C">R_TRIG</Type>
				<BitSize>24</BitSize>
				<BitOffs>368</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">HANDLE</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>392</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_OPEN</Name>
				<Type Decoration="1010B9A5">FILEOPEN</Type>
				<BitSize>2520</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_CLOSE</Name>
				<Type Decoration="100E6FAC">FILECLOSE</Type>
				<BitSize>432</BitSize>
				<BitOffs>2928</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_READ</Name>
				<Type Decoration="10117973">FILEREAD</Type>
				<BitSize>528</BitSize>
				<BitOffs>3360</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_WRITE</Name>
				<Type Decoration="10117A8C">FILEWRITE</Type>
				<BitSize>528</BitSize>
				<BitOffs>3888</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">READ_BUFFER</Name>
				<Type Decoration="2001024E">ARRAY [0..256] OF WORD</Type>
				<BitSize>4112</BitSize>
				<BitOffs>4416</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">WRITE_BUFFER</Name>
				<Type Decoration="2001024E">ARRAY [0..256] OF WORD</Type>
				<BitSize>4112</BitSize>
				<BitOffs>8528</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">INDEX</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>12640</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TRY</Name>
				<Type>BYTE</Type>
				<BitSize>8</BitSize>
				<BitOffs>12656</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SUMM</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>12664</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SIZE</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>12680</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">R_BASE</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>12696</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">W_BASE</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>12728</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT_W</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>12760</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT_R</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>12792</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VERIFY_ERROR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>12824</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SUMM1</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>12832</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">FILENAME</Name>
				<Type Decoration="40000051">STRING(80)</Type>
				<Comment>
					<![CDATA[D: Kompletter Filename	
								GB: 	Filename(including path)	
								E: 	Nombre completo de fichero
								F: 	Nom complet de fichier]]>
				</Comment>
				<BitSize>648</BitSize>
				<BitOffs>12864</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SAVE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: 0--> 1 löst Schreiben aus / GB:  0 -->1 to write data		
								E: 0--> 1activa escritura		/ F: 0 -> 1 active écriture]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>13512</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOAD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: 0 --> 1 löst Laden aus	/ GB: 0 -->1 to read data		
								E: 0 --> 1 activa lectura		/ F: 0 --> 1 active lecture]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>13520</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BUSY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Transfer in Aktion			/ GB: file access in progress	
								E: Acceso a ficheros en progreso/F: accès au fichier en action]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>13528</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Störung bei Aktion			/ GB: Fault on read / write		
								E:  Fallo en lectura/escritura		/ F: erreur de lecture / d'écriture]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>13536</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SAVE_READY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Schreibvorgang erfolgreich	/ GB: Write data o.k.			
								E:  Escribir datos o.k.			/ F: écriture	données ok]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>13544</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOAD_READY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Lesevorgang erfolgreich	/ GB: read data o.k.			
								 Lectura o.k.					/ F: lecture données ok]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>13552</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">EXTERNAL_SAVE</Name>
				<Type Pointer="1">WORD</Type>
				<Comment>
					<![CDATA[D: =1 löst Speichern aus , wird anschließend auf 0 gesetzt
								GB:  =1 starts a save request, value is set to 0 when ok.		
								E:  	=1 activa la demanda grabar y luego es puesto a 0 si o.k.	
								F:	=1 déclenche  demande de mémorisation, valeur mise  à 0 
									si ok]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>13560</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB_256</Name>
				<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
				<Comment>
					<![CDATA[DB]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>13592</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>63</CodeIndex>
				<InitIndex>64</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001034E">ARRAY [0..512] OF WORD</Name>
			<Type>WORD</Type>
			<BitSize>8208</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>513</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="1025E22A" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB_FILE_DB512</Name>
			<BitSize>21816</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D: Anzahl Bytes im Datenblock
								GB: 	Number of bytes in block	
								E: 	Número de bytes en bloque						
								F:	nombre de bytes dans le bloc]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">REQUEST_LOAD</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">REQUEST_SAVE</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VERIFY</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TIMEOUT</Name>
				<Type Decoration="10060D24">TON</Type>
				<BitSize>120</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TMAX</Name>
				<Type>TIME</Type>
				<BitSize>32</BitSize>
				<BitOffs>160</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">STEP_LOAD</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>192</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">STEP_SAVE</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>208</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">T_DELAY</Name>
				<Type Decoration="10060D24">TON</Type>
				<BitSize>120</BitSize>
				<BitOffs>224</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RT_LOAD</Name>
				<Type Decoration="1003051C">R_TRIG</Type>
				<BitSize>24</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RT_SAVE</Name>
				<Type Decoration="1003051C">R_TRIG</Type>
				<BitSize>24</BitSize>
				<BitOffs>368</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">HANDLE</Name>
				<Type>UINT</Type>
				<BitSize>16</BitSize>
				<BitOffs>392</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_OPEN</Name>
				<Type Decoration="1010B9A5">FILEOPEN</Type>
				<BitSize>2520</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_CLOSE</Name>
				<Type Decoration="100E6FAC">FILECLOSE</Type>
				<BitSize>432</BitSize>
				<BitOffs>2928</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_READ</Name>
				<Type Decoration="10117973">FILEREAD</Type>
				<BitSize>528</BitSize>
				<BitOffs>3360</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_WRITE</Name>
				<Type Decoration="10117A8C">FILEWRITE</Type>
				<BitSize>528</BitSize>
				<BitOffs>3888</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">READ_BUFFER</Name>
				<Type Decoration="2001034E">ARRAY [0..512] OF WORD</Type>
				<BitSize>8208</BitSize>
				<BitOffs>4416</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">WRITE_BUFFER</Name>
				<Type Decoration="2001034E">ARRAY [0..512] OF WORD</Type>
				<BitSize>8208</BitSize>
				<BitOffs>12624</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">INDEX</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>20832</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TRY</Name>
				<Type>BYTE</Type>
				<BitSize>8</BitSize>
				<BitOffs>20848</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SUMM</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>20856</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SIZE</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>20872</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">R_BASE</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>20888</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">W_BASE</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>20920</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT_W</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>20952</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT_R</Name>
				<Type>UDINT</Type>
				<BitSize>32</BitSize>
				<BitOffs>20984</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VERIFY_ERROR</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>21016</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SUMM1</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>21024</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">FILENAME</Name>
				<Type Decoration="40000051">STRING(80)</Type>
				<Comment>
					<![CDATA[D: Kompletter Filename	
								GB: 	Filename(including path)	
								E: 	Nombre completo de fichero
								F: 	Nom complet de fichier]]>
				</Comment>
				<BitSize>648</BitSize>
				<BitOffs>21056</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SAVE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: 0--> 1 löst Schreiben aus / GB:  0 -->1 to write data		
								E: 0--> 1activa escritura		/ F: 0 -> 1 active écriture]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>21704</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOAD</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: 0 --> 1 löst Laden aus	/ GB: 0 -->1 to read data		
								E: 0 --> 1 activa lectura		/ F: 0 --> 1 active lecture]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>21712</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BUSY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Transfer in Aktion			/ GB: file access in progress	
								E: Acceso a ficheros en progreso/F: accès au fichier en action]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>21720</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Störung bei Aktion			/ GB: Fault on read / write		
								E:  Fallo en lectura/escritura		/ F: erreur de lecture / d'écriture]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>21728</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SAVE_READY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Schreibvorgang erfolgreich	/ GB: Write data o.k.			
								E:  Escribir datos o.k.			/ F: écriture	données ok]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>21736</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOAD_READY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Lesevorgang erfolgreich	/ GB: read data o.k.			
								 Lectura o.k.					/ F: lecture données ok]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>21744</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">EXTERNAL_SAVE</Name>
				<Type Pointer="1">WORD</Type>
				<Comment>
					<![CDATA[D: =1 löst Speichern aus , wird anschließend auf 0 gesetzt
								GB:  =1 starts a save request, value is set to 0 when ok.		
								E:  	=1 activa la demanda grabar y luego es puesto a 0 si o.k.	
								F:	=1 déclenche  demande de mémorisation, valeur mise  à 0 
									si ok]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>21752</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB_512</Name>
				<Type Decoration="2001034D" Pointer="1">ARRAY [0..511] OF WORD</Type>
				<Comment>
					<![CDATA[DB]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>21784</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>65</CodeIndex>
				<InitIndex>66</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001018D">ARRAY [0..63] OF WORD</Name>
			<Type>WORD</Type>
			<BitSize>1024</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>64</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001018D" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB64</Name>
			<Type Decoration="2001018D">ARRAY [0..63] OF WORD</Type>
			<BitSize>1024</BitSize>
		</DataType>
		<DataType>
			<Name Decoration="100D2C0E" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB_PRESSURE_FAULT</Name>
			<BitSize>152</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VALUE</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">IN</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Analog-Eingangswert
								GB:	Analog input]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LIMIT_HIGH</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Obergrenze Druck / Vakuum
								GB:	Upper limit pressure / vacuum]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LIMIT_LOW</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Untergrenze Druck / Vakuum
								GB:	Lower limit pressure / vacuum]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">EN_PRESSURE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Fehlerauswertung Druckluft ein
								GB:	Enable pressure fault detection]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">EN_VACUUM</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Fehlerauswertung Vakuum ein
								GB:	Enable vacuum fault detection]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>72</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MODE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: TRUE = Vakuum FALSE = Druck
								GB:	True = vacuum, FALSE = pressure]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Fehler ist aufgetreten
								GB:	Fault detected]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>88</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VAL</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D: Wert für Anzeige
								GB:	Diaplay value]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MAX_VALUE</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D: Obergrenze für Visualisierung
								GB:	Upper limit visualisation]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>112</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR_HIGH</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Überdruck
								GB:	Pressure too high]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>128</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR_LOW</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Unterdruck
								GB:	Pressure too low]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR_SENSOR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Sensor
								GB:	Sensor fault]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>144</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>86</CodeIndex>
				<InitIndex>87</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="2001015D">ARRAY [0..15] OF WORD</Name>
			<Type>WORD</Type>
			<BitSize>256</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>16</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="101A7D13" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB191_ERRORS</Name>
			<BitSize>592</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">NP</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MASK_END</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>8</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MASK</Name>
				<Type Decoration="2001015D">ARRAY [0..15] OF WORD</Type>
				<BitSize>256</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">P_ALT</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Pointer alter Störspeicher NR+9
								GB: 	Pointer previous fault buffer NR +9			
  								E: 	Indicador memoria anterior de fallo NR+9	
								F:	Pointeur de mémoire antérieure d'erreur  NR+9]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>280</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">P_STOER</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Pointer alter Störspeicher NR+29 			
								GB: 	Pointer previous fault buffer NR +29			
								E:  	Indicador memoria anterior de fallo NR+29	
								F:	Pointeur de mémoire antérieure d'erreur NR+29]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>296</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">P_ERSTW</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Pointer Erstwertfehler NR +49 				
								GB:  Pointer leading error NR +49				
								E:  	Indicador fallo primer valor NR +49		
								F:	Pointeur d'erreur de valeur primaire NR +49]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>312</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">STOER_SP</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Störspeicher aktuell / GB: actual faults			
								   E: Fallos reales / F: mémoire d'erreur actuelle]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>328</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">M_ERSTWERT</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Hilfsmerker "Störung vorhanden" 
								GB: 	Aauxiliary flag "error exists"
								E: 	Marca auxiliar "avería presente" 
								F:	mémento aux. "erreur existante"]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>344</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERSTWERT</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Erstwertfehler DW 66	
								GB: 	Firstup fault 		
								 E: 	Fallo primer valor DW 66
								 F: 	Erreur de valeur primaire DW 66]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>352</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">FLANKEN</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D:  Steigende Flanken Fehler				
								GB: 	Rising edges errors			
								E:  	Fallo flanco positivo 
								F:	Erreur flanc positiv]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>368</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SHOW</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>384</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BITPOS</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>400</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MASKE</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>416</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_WORD</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: 16 Störbits / GB: 16 error flags
						           E: 16 bits de fallo / F: 16 bits de panne]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>432</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">M_END</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Maske für Endstellung mit Ware					
							 	1 = Endstellung 0 = Stop							
							    GB: Mask "programmed stop" run with material		
								 1 = stop position 0 = stop							
							    E:  Máscara "parada programada activa",	
							 	 funcionamiento normal con producto		
								 1 = parada programada 0 = parada 
							    F:	Masque pour la position finale, fonctionnement 
								normal avec marchandise 
								1 = position finale 0 = arrêt]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>448</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">M_EMPTY</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Maske für Endstellung Fahren ohne Ware
								 1 = Endstellung 0 = STOP					
							 GB: Mask "programmed stop ", run without product 	
								 1 = programmed stop 0 = stop				
							  E:  Máscara "parada programada", funcionamiento sin producto 
								 1 = parada programada 0 = parada 	
							  F:	Masque "arrêt programmé", fonctionnement sans marchandise
								 1 = position finale 0 = arrêt]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>464</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">M_INCHING</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: Maske für Unterdrückung Einrichten			
								1 = Störung ausgeblendet	0 = Störung scharf	
							  GB:  Mask to override errors in inching mode		
								1 = error deactivated 	0 = error active		
							  E:  Máscara para suprimir averías en modo de ajuste	
								1 = avería deactivada 0 = avería activada		
							  F:	Masque pour surinscrire les erreurs en mode "à coups" 
								1 = erreur désactivée 0 = erreur activée]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>480</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">NR</Name>
				<Type>BYTE</Type>
				<Comment>
					<![CDATA[D: Nummer des Blocks 1..16 / GB: Number of block	1..16
							   E:  Número de bloque 1..16 / F: Numéro de bloc 1..16]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>496</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">INCHING</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Einrichtbetrieb aktiv / GB: Inching mode active
							    E: Modo de ajuste activo /	F: Mode "à coups" actif]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>504</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RESET</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Störung zurücksetzen / GB: Clear errors 
							    E: Resetear avería / F: Remise à zéro d'erreur]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>512</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BETR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Betriebsart wechseln / GB: Change operation mode 
							    E: Cambiar modo de operación 
							    F: Changer mode de fonctionnement]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>520</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">EMPTY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Fahren ohne Ware aktiv
							  GB: Run without material
							    E: Funcionamiento sin producto 
							    F:Fonctionnement sans marchandise]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>528</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SWAP_BYTE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: high- und lowbyte tauschen
							  GB: Swap high- and low byte 
							    E: Conmutar byte alto y bajo 
							    F:	échanger byte du haut avec byte du bas]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>536</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">STOP</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:    	Maschine Schnellstop
							GB: 	Process FAST stop of machine
							E:   	Parada inmediata de máquina	
							F:   	Arrêt rapide de la machine]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>544</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ENDPOS</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: 	Maschine Anhalten In Endstellung
							GB:  Programmed stop of machine (end position)	
							E: 	Parar máquina en parada programada (posición inicial)
							F:	Arrêter la machine en position finale]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>552</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB</Name>
				<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
				<Comment>
					<![CDATA[D: Puffer mit Störungen
								  GB: Buffer for error flags		
								     E: Búfer con fallos 
								     F: Mémoire  tampon pour erreurs]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>560</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>139</CodeIndex>
				<InitIndex>140</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="200142EB">ARRAY [0..10] OF STRING(80)</Name>
			<Type Decoration="40000051">STRING(80)</Type>
			<BitSize>7128</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>11</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="200142EB" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB_STRING</Name>
			<Type Decoration="200142EB">ARRAY [0..10] OF STRING(80)</Type>
			<BitSize>7128</BitSize>
		</DataType>
		<DataType>
			<Name Decoration="20010732">ARRAY [0..1439] OF DWORD</Name>
			<Type>DWORD</Type>
			<BitSize>46080</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>1440</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="10148508" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB31_HD12CAM</Name>
			<BitSize>46408</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">FIELD</Name>
				<Type Decoration="20010732">ARRAY [0..1439] OF DWORD</Type>
				<BitSize>46080</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">POINT</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>46080</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">INDEX</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>46096</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>46112</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MASK</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>46128</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNT_CAM</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>46160</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RT_RE_INIT</Name>
				<Type Decoration="1003051C">R_TRIG</Type>
				<BitSize>24</BitSize>
				<BitOffs>46176</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">START</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>46200</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">END</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>46216</BitOffs>
			</SubItem>
			<SubItem>
				<Name Constant="1" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MAX_SIZE</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>46232</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">POSITION</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Maschinenposition (0..1439)	
							GB:	Angular machine position  
							E:	Posición angular de máquina	
							F:	Position angulaire de machine (0..1439)]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>46248</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">START_INDEX</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Index für Startwert Kurve 1
							GB:	Index of first cam data	 		
							E:	 Índice de valor de arranque leva 1					
							F:	Index de valeur de démarrage came 1
								  Visipro = 21		Visi2000 = 10,90,170,(250)]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>46264</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MAX_POS</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Größter zulässiger Wert 
							GB:	Highest legal value (eg. 359) 
							E:	Mayor valor legal (p.ej. 359)			
							F	Valeur admissible la plus grande]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>46280</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MAX_CAM</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	0..32 Anzahl aktive Kurven 
							GB:	0..32 number of cams 	
							E:	0 .. 32 número de levas activas	
							F:	0..32  nombre de cames actives]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>46296</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">INIT</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:Daten initialisieren	
							GB:	Re-init data			
							E:	Inicializar datos			
							F:	Initialiser données]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>46312</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SUPRESS</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Alle 1°-Kurven unterdrücken
							GB: 	Suppress all 1°-cams		
							E:	Suprimir todas las levas de 1°	
							F:	supprimer toutes les cames d'1 °]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>46320</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">CAM32</Name>
				<Type>DWORD</Type>
				<Comment>
					<![CDATA[D:32 Kurven  			/ GB: 32 cams			
								E:	32 levas				/ F: 32 cames]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>46328</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Unzulässige Daten	/ GB: Illegal data		
								E:	Datos ilegales		/ F: données illégales]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>46360</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">READY</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Interne Tabelle bereit / GB:	Internal data is ready	
								E:	Tabla interna está lista	/ F: tableau interne est prêt]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>46368</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DATA</Name>
				<Type Decoration="2001034D" Pointer="1">ARRAY [0..511] OF WORD</Type>
				<Comment>
					<![CDATA[D:	Array mit Kurvendaten
							GB:	Array including cam data 	
							E:	Conjunto con datos de leva	
							F:	Array avec données de cames]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>46376</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>160</CodeIndex>
				<InitIndex>161</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="101663EC" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB34_CAMCONTROL2</Name>
			<BitSize>488</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">USED1_32</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">USED33_64</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">AKTIV1_32</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">AKTIV33_64</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR_INT</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>128</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TAKT_ALT</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">T_MAX</Name>
				<Type Decoration="10060D24">TON</Type>
				<BitSize>120</BitSize>
				<BitOffs>144</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">EDGE</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>264</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ANGLE_OLD</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>272</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DELTA</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>288</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">CYCLE</Name>
				<Type>DWORD</Type>
				<BitSize>32</BitSize>
				<BitOffs>304</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">CAM1_32</Name>
				<Type>DWORD</Type>
				<Comment>
					<![CDATA[D:	Erster Satz von 32 Kurven für Überwachung
								GB:	First set of 32 CAM's to be controlled			
								E:	Primer juego de 32 levas a vigilar 		
								F:	Premier jeu de 32 cames pour surveillance]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>336</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">CAM33_64</Name>
				<Type>DWORD</Type>
				<Comment>
					<![CDATA[D:	Zweiter Satz von 32 Kurven
								GB:	Second set of 32 CAM's to be controlled		
								E:	Segundo juego de 32 levas a vigilar		
								F:	Second jeu de 32 cames pour surveillance]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>368</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RESET</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Löscht Fehlermeldung
								GB:	Clears error flag							
								E:	Borra marca de fallo					
								F:	Efface mémento d'erreurs]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>400</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">CLOCK</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Maschinentakt, Auswertung bei steigender Flanke
								GB:	Machine clock (detection on rising edge)	
								E:	Reloj de máquina, detección de flanco positivo	
								F:	Cycle de machine, évaluation lors de flancs positifs]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>408</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RUN</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Maschine läuft ( N > 0 )
								GB:	Machine is running (N > 0 )	
								E:	Máquina está en funcionamiento ( N > 0) 	
								F:	Machine est en fonctionnement]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>416</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ANGLE</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Maschinenstellung[°]	
								GB:	Actual machine position [ ° ]
								E:	Posición actual de máquina		
								F:	Position actuelle de la machine [ ° ]]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>424</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ANGLE_MAX</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Max. Schrittweite zwischen zwei Aufrufen			
								GB:	Maximum step between two cycles[ ° ]			
								E:	Paso máximo entre dos ciclos	
								F:	Largeur max. d'étape entre deux cycles[°]]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>440</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Meldesignale bei Kurvenfehler					
								GB:	Error-Signal when CAM is missing				
								E:	Señal de fallo en caso de fallo de leva	
								F:	Signal d'erreur en cas d'erreur de came]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>456</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR_A</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[GB: Diagnostic --> angular step too big]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>464</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR_B</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[GB: Diagnostic --> cam trigger timeout]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>472</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR_C</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[GB: Diagnostic --> cam fault]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>480</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>162</CodeIndex>
				<InitIndex>163</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="100B1FB5" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB39_PARITY2</Name>
			<BitSize>192</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RATE</Name>
				<Type>REAL</Type>
				<Comment>
					<![CDATA[GB: Error-Rate (0..1)						
								E: Tasa de fallo (0..1)					
								F: Taux d'erreurs  (0..1)]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">FILTER</Name>
				<Type>REAL</Type>
				<BitSize>32</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VALUE</Name>
				<Type>WORD</Type>
				<BitSize>16</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BIT</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MAXIMUM</Name>
				<Type>REAL</Type>
				<BitSize>32</BitSize>
				<BitOffs>88</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">GRAY</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Winkelposition Maschine 					
								GB:	Actual shaft position in degree				
								E:	Posición angular del eje					
								F:	Position angulaire de l'arbre]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>120</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RESET</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[RESET]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">PARITY_FLAG</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Parity-Bit Absolutwertgeber
								GB	Parity flag of absolute encoder						
								E:	Bit de paridad de encoder absoluto				
								F:	Entraînement principal activé et 
									valeur de consigne > 0]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>144</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SPEED</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Aktuelle Maschinengeschwindigkeit
								GB:	Actual machine speed							
								E:	Velocidad real de máquina						
								F:	Vitesse actuelle de la machine]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>152</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SPEEDLIMIT</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D:	Maximalgeschwindigkeit für Auswertung 		
								GB:	Maximum speed for parity detection			
								E:	Max. velocidad de detección de paridad	
								F:	Vitesse max. de détection de parité]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>168</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ERROR</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D:	Geberfehler		/ GB:	Error detected 
								E: 	Fallo detectado	/ F: Erreur de codeur]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>184</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>164</CodeIndex>
				<InitIndex>165</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="10093330" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB75_DBCOPY</Name>
			<BitSize>168</BitSize>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">POINT_QUELLE</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">POINT_ZIEL</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">COUNTDOWN</Name>
				<Type>INT</Type>
				<BitSize>16</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">QUELLE_START</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D: Anfang des Quellbereichs
									GB:	Start index source data to be transferred		
									E: 	Principio de datos fuente a transferir 	
									F:	Départ du domaine de source]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ZIEL_START</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D: Anfang des Zielbereichs	
									GB:  Start index target data		
									E:  	Principio de datos de objeto 
									F:	Départ du domaine de but]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">ANZAHL</Name>
				<Type>INT</Type>
				<Comment>
					<![CDATA[D: Anzahl Datenworte		
									GB:  Number of elements	
									E:  	Número de dato elemental 	
									F:	Nombre de mots de données]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SWAP_BYTE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: High- und LowByte tauschen
									GB: 	Swap high and low byte	
									E:  	Intercambiar byte alto y bajo 	
									F:	Echanger byte haut et byte bas]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB_QUELLE</Name>
				<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
				<Comment>
					<![CDATA[D: Quell-Datenbaustein
									GB:  Source data block			
									E:  	 Datos fuente 		
									F:	Bloc de données de source]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="InOut" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DB_ZIEL</Name>
				<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
				<Comment>
					<![CDATA[D: Ziel-Datenbaustein
									GB: Target data				
									E: 	Datos objeto 		
									F:	Bloc de données de but]]>
				</Comment>
				<BitSize>32</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>183</CodeIndex>
				<InitIndex>184</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="200301C4">ARRAY [0..1, 1..20, 0..99] OF WORD</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[Datenfeld für Datenaustausch]]>
			</Comment>
			<BitSize>64000</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>2</Elements>
			</ArrayInfo>
			<ArrayInfo>
				<LBound>1</LBound>
				<Elements>20</Elements>
			</ArrayInfo>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>100</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="101222B0" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">WORD_BIT</Name>
			<BitSize>152</BitSize>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">WORT</Name>
				<Type>WORD</Type>
				<Comment>
					<![CDATA[D: 	16 Bits mit Daten	/ GB: 16 bits of data]]>
				</Comment>
				<BitSize>16</BitSize>
				<BitOffs>0</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SWAP_BYTE</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: 	High- und Lowbyte tauschen
								GB:	Swap high- and Lowbyte]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>16</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B0</Name>
				<Type>BOOL</Type>
				<Comment>
					<![CDATA[D: Niederwertigstes Bit / GB: least significant bit]]>
				</Comment>
				<BitSize>8</BitSize>
				<BitOffs>24</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B1</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>32</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B2</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>40</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B3</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>48</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B4</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>56</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B5</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>64</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B6</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>72</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B7</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>80</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B8</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>88</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B9</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>96</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B10</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>104</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B11</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>112</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B12</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>120</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B13</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>128</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B14</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>136</BitOffs>
			</SubItem>
			<SubItem>
				<Name FbParameter="Output" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B15</Name>
				<Type>BOOL</Type>
				<BitSize>8</BitSize>
				<BitOffs>144</BitOffs>
			</SubItem>
			<FbInfo>
				<CodeIndex>199</CodeIndex>
				<InitIndex>200</InitIndex>
			</FbInfo>
		</DataType>
		<DataType>
			<Name Decoration="20010154">ARRAY [0..15] OF BYTE</Name>
			<Type>BYTE</Type>
			<BitSize>128</BitSize>
			<ArrayInfo>
				<LBound>0</LBound>
				<Elements>16</Elements>
			</ArrayInfo>
		</DataType>
		<DataType>
			<Name Decoration="20010154" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">DP_BLOCK</Name>
			<Type Decoration="20010154">ARRAY [0..15] OF BYTE</Type>
			<BitSize>128</BitSize>
		</DataType>
	</DataTypes>
	<Functions>
		<Function>
			<Name Decoration="1003CF58" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CONCAT</Name>
			<FunInfo>
				<CodeIndex>202</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">CONCAT</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR1</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR2</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10048DE1" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">DELETE</Name>
			<FunInfo>
				<CodeIndex>209</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">DELETE</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LEN</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">POS</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10038BEA" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">FIND</Name>
			<FunInfo>
				<CodeIndex>212</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">FIND</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR1</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR2</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="1004D151" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">INSERT</Name>
			<FunInfo>
				<CodeIndex>213</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">INSERT</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR1</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR2</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">POS</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10038BD5" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LEFT</Name>
			<FunInfo>
				<CodeIndex>214</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LEFT</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">SIZE</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10024688" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LEN</Name>
			<FunInfo>
				<CodeIndex>215</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LEN</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10048D08" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">MID</Name>
			<FunInfo>
				<CodeIndex>216</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">MID</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">LEN</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">POS</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="1005D217" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">REPLACE</Name>
			<FunInfo>
				<CodeIndex>219</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">REPLACE</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR1</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR2</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">L</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">P</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10038C28" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RIGHT</Name>
			<FunInfo>
				<CodeIndex>220</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">RIGHT</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">STR</Name>
					<Type Decoration="40000100">STRING(255)</Type>
					<BitSize>2048</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\STANDARD.LIB">SIZE</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100452BA" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSLOGDINT</Name>
			<FunInfo>
				<CodeIndex>233</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSLOGDINT</Name>
					<Type>DINT</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">msgCtrlMask</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">msgFmtStr</Name>
					<Type Decoration="400000FF">STRING(254)</Type>
					<BitSize>2040</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">dintArg</Name>
					<Type>DINT</Type>
					<BitSize>32</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="1004537F" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSLOGLREAL</Name>
			<FunInfo>
				<CodeIndex>234</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSLOGLREAL</Name>
					<Type>DINT</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">msgCtrlMask</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">msgFmtStr</Name>
					<Type Decoration="400000FF">STRING(254)</Type>
					<BitSize>2040</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">lrealArg</Name>
					<Type>LREAL</Type>
					<BitSize>64</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100493FB" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSLOGSTR</Name>
			<FunInfo>
				<CodeIndex>235</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ADSLOGSTR</Name>
					<Type>DINT</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">msgCtrlMask</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">msgFmtStr</Name>
					<Type Decoration="400000FF">STRING(254)</Type>
					<BitSize>2040</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">strArg</Name>
					<Type Decoration="40000051">STRING(80)</Type>
					<BitSize>648</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10030A7D" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEARBIT32</Name>
			<FunInfo>
				<CodeIndex>264</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CLEARBIT32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">bitNo</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10040D41" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CSETBIT32</Name>
			<FunInfo>
				<CodeIndex>265</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">CSETBIT32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">bitNo</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">bitVal</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[value to which the bit should be set]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="1003099A" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">GETBIT32</Name>
			<FunInfo>
				<CodeIndex>278</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">GETBIT32</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">bitNo</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10040D1E" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LPTSIGNAL</Name>
			<FunInfo>
				<CodeIndex>287</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">LPTSIGNAL</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PortAddr</Name>
					<Type>UINT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">PinNo</Name>
					<Type>UINT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">OnOff</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100307F2" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ROL32</Name>
			<FunInfo>
				<CodeIndex>288</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ROL32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">n</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100307F8" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ROR32</Name>
			<FunInfo>
				<CodeIndex>289</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">ROR32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">n</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10030A02" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SETBIT32</Name>
			<FunInfo>
				<CodeIndex>290</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SETBIT32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">bitNo</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100307EC" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SHL32</Name>
			<FunInfo>
				<CodeIndex>291</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SHL32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">n</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100307F2" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SHR32</Name>
			<FunInfo>
				<CodeIndex>292</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">SHR32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">inVal32</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\PlcSystem.lib">n</Name>
					<Type>SINT</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100308D8" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BITCOUNTER</Name>
			<FunInfo>
				<CodeIndex>19</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BITCOUNTER</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BUFFER</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">IN</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10122401" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_BIT_WORD</Name>
			<FunInfo>
				<CodeIndex>20</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_BIT_WORD</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B0</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[D: Erstes Bit / GB: first bit / E: Primer bit / F: Premier bit]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B1</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B2</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B3</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B4</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B5</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B6</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B7</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B8</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B9</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B10</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B11</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B12</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B13</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B14</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">B15</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[D: Letztes Bit / GB: Last Bit / E: Último bit  /F: Dernier bit]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SWAP_BYTE</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10053453" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_GET_BIT</Name>
			<FunInfo>
				<CodeIndex>21</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_GET_BIT</Name>
					<Type>BOOL</Type>
					<BitSize>8</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name Constant="1" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MASKE</Name>
					<Type Decoration="2001015D">ARRAY [0..15] OF WORD</Type>
					<BitSize>256</BitSize>
				</FunParameter>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">Index7001</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VALUE</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D: Datenwert, aus dem das Bit extrahiert werden soll	
						GB:  Value to extract one "logical" bit				
						E: 	Valor de lo cual se extrae un bit "lógico"			
						F:	Valeur de données de laquelle le bit doit être extrait]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">POS</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D: Bitposition des gesuchten Bits [0..15]			
						GB:  Bit position of the requested bit [0..15]			
						E: 	Posición del bit [0...15] que se busca			
						F:	Position de bit du bit recherché [0..15]]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10030866" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_MASK16</Name>
			<FunInfo>
				<CodeIndex>22</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">F_MASK16</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">BIT</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[D:	Bit zum Aktivieren des Wertes	
							GB: 	Bit to enable transmission of the value		
							E:	Bit para activar el valor	
							F:	Bit pour activer la valeur]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VALUE</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D:	Wert, der bei gesetztem Bit ausgegeben wird	
							GB: 	Result value when BIT = TRUE				  
							E:	Valor de resultado si bit es activo			
							F:	Valeur de résultat quand BIT = TRUE]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10073A4A" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MANIPULATE_BIT</Name>
			<FunInfo>
				<CodeIndex>39</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MANIPULATE_BIT</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MASKE</Name>
					<Type Decoration="2001015D">ARRAY [0..15] OF WORD</Type>
					<BitSize>256</BitSize>
				</FunParameter>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">Index7001</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">VALUE</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D: 	Zu modifizierender Wert	
							GB: 	VALUE to be modified
							E:  	VALUE a modificar		
							F:	VALUE à modifier]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">NR</Name>
					<Type>BYTE</Type>
					<Comment>
						<![CDATA[D:	0 ... 15  Bitnummer 
							GB: 	0 ...15 bit offset		
							E: 	0 ... 15 desplazamiento
							F:	Numéro de bit 0 ... 15]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SET</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[D: Bit setzen / GB: set bit / E: Colocar bit/ F: Fixer un bit]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">CLEAR</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[D: Bit löschen / GB: Clear bit / E: Borrar bit/ F: Effacer un bit]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10083D1E" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB_GRAY</Name>
			<FunInfo>
				<CodeIndex>71</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB_GRAY</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">PRESET</Name>
					<Type Decoration="2001015D">ARRAY [0..15] OF WORD</Type>
					<BitSize>256</BitSize>
				</FunParameter>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">MASK</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">RESULT</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">Index7001</Name>
					<Type>INT</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">GRAY</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D:	Graycode max. 16 Bit				
								GB:	Graycode (max. size 16 bit)
								E:	Código de Gray max. 16 bit		
								F:	Code de Gray max. 16 bits]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">WIDTH</Name>
					<Type>BYTE</Type>
					<Comment>
						<![CDATA[D:	Codebreite Graycode
								GB:	Number of BITS  in Gray code (size)
								E:	Número de bits en código de Gray	
								F:	Nombre de bits en code de Gray]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">OFFSET</Name>
					<Type>INT</Type>
					<Comment>
						<![CDATA[D:	Offset "0°" Graycode	
								GB:	Offset " 0° " in Gray code 
								E:	Desplazamiento "0" en código de Gray	
								F:	Déplacement "0" en code de Gray]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10061780" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FUN_KL5001_SSI</Name>
			<FunInfo>
				<CodeIndex>192</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FUN_KL5001_SSI</Name>
					<Type>REAL</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">Inkrements</Name>
					<Type>DINT</Type>
					<BitSize>32</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">PCDH</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D:	High-Wort SSI-Geber
							GB:	High-word of SSI encoder 
							E: 	Palabra significativa del encoder SSI 
							F: 	Mot de poids fort  du codeur SSI]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">PCDL</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D: 	Low-Wort SSI-Geber
							GB:	Low-word of SSI encoder 
							E:	Palabra menos significativa del encoder SSI 
							F: 	Mot de poids faible du codeur SSI]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">FORWARD</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[D: 	Zählrichtung
							GB:	Counter direction 
							E: 	Dirección de conteo 
							F: 	Direction de comptage]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">PLUS_MINUS_180</Name>
					<Type>BOOL</Type>
					<Comment>
						<![CDATA[D:	Wertebereich -180.0...180.0, statt 0...360.0 Grad
							GB:	Position range from -180.0 to 180.0 instead of from 0 to 360.0 
								degrees
                                                          	E: 	Gama de valores de -180.0 a 180.0 en vez de 0 a 360.0 grados                                              
                                                                	F: 	Gamme de valeurs de -180.0 à 180.0 au lieu de 0 à 360.0 degrés]]>
					</Comment>
					<BitSize>8</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="1002046D" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SWAP</Name>
			<FunInfo>
				<CodeIndex>194</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">SWAP</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">IN</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10030E38" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TWO_WORD_TO_DINT</Name>
			<FunInfo>
				<CodeIndex>195</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TWO_WORD_TO_DINT</Name>
					<Type>DINT</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">HIGH_WORD</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOW_WORD</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10030E2E" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TWO_WORD_TO_DWORD</Name>
			<FunInfo>
				<CodeIndex>196</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TWO_WORD_TO_DWORD</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">HIGHWORD</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D:	Höherwertiges Datenwort / GB: significant word		
							 E: Dato elemental significativo / F: Mot significatif]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOWWORD</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D: Niederwertiges Datenwort/ GB: less significant word	
							E:  Dato elemental significativo / F: Mot moins significatif]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="10030EBC" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TWO_WORD_TO_LREAL</Name>
			<FunInfo>
				<CodeIndex>197</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">TWO_WORD_TO_LREAL</Name>
					<Type>LREAL</Type>
					<BitSize>64</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">HIGH_WORD</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOW_WORD</Name>
					<Type>WORD</Type>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
		<Function>
			<Name Decoration="100309B1" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">UMW</Name>
			<FunInfo>
				<CodeIndex>198</CodeIndex>
				<ReturnValue>
					<Name IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">UMW</Name>
					<Type>DWORD</Type>
					<BitSize>32</BitSize>
				</ReturnValue>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">HIGHWORD</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D:	Höherwertiges Datenwort / GB: significant word
							 E: Dato elemental significativo / F: Mot significatif]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
				<FunParameter>
					<Name FunParameter="Input" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">LOWWORD</Name>
					<Type>WORD</Type>
					<Comment>
						<![CDATA[D: Niederwertiges Datenwort/ GB: less significant word	
							E:  Dato elemental significativo / F: Mot moins significatif]]>
					</Comment>
					<BitSize>16</BitSize>
				</FunParameter>
			</FunInfo>
		</Function>
	</Functions>
	<Programs>
		<Program>
			<Name Decoration="10023BAF" Crc32="0522514425" LastChange="2018-05-25T18:55:28">_CPU1</Name>
			<PrgInfo>
				<CodeIndex>298</CodeIndex>
				<Symbol>
					<Name>_CPU1.RT_RESTART</Name>
				</Symbol>
				<Symbol>
					<Name>_CPU1.TOF_RESTART</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10021C71" Crc32="3039402578" LastChange="2018-05-25T18:55:28">_CPU2</Name>
			<PrgInfo>
				<CodeIndex>299</CodeIndex>
				<Symbol>
					<Name>_CPU2.RT_CLOCK</Name>
				</Symbol>
				<Symbol>
					<Name>_CPU2.TOGGLE</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100356BB" Crc32="1855075688" LastChange="2018-05-25T18:55:28">CPU1_PB083_MOTORS</Name>
			<PrgInfo>
				<CodeIndex>303</CodeIndex>
				<Symbol>
					<Name>CPU1_PB083_MOTORS.RT_AUTO1</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB083_MOTORS.TOF_BELTMOTOR</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB083_MOTORS.RS_DISCH_POS</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1007ABF5" Crc32="3073253346" LastChange="2018-05-25T18:55:28">CPU1_PB084_REFEED_MODE</Name>
			<PrgInfo>
				<CodeIndex>304</CodeIndex>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE.RS_FEED_POSSIBLE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE.RS_ROT_FOR_REFEED</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE.DRUM_ROT_FOR_REFEED</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE.RS_ROT_DISCH</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE.CTUD_STOP_DRUM</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE.COUNTER_STOP_DRUM</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE.TP_RESET_GUARD</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1013BD03" Crc32="3689699139" LastChange="2018-05-25T18:55:28">CPU1_PB084_REFEED_MODE_2</Name>
			<PrgInfo>
				<CodeIndex>305</CodeIndex>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RT_PACKETS_FEEDING_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RT_FEEDING_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RS_FEEDING_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.FEEDING_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RS_FEEDING_ENABLE_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.FEEDING_ENABLE_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RS_FEEDING_ACTIVE_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RS_AF_ROT_FOR_REFEED_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.AF_DRUM_ROT_FOR_REFEED_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RS_ROT_FOR_REFEED_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RT_STOP_DRUM_FILL_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.CTUD_STOP_DRUM_FILL_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.COUNTER_STOP_DRUM_FILL_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RT_ROT_DISCH_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.TON_FEEDING</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.FT_FEEDING_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.RS_ROT_DISCH_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.CTUD_STOP_DRUM_CLEAR_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB084_REFEED_MODE_2.COUNTER_STOP_DRUM_CLEAR_2</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100FC235" Crc32="2267935633" LastChange="2018-05-25T18:55:28">CPU1_PB085_VALVE_CONTROL</Name>
			<PrgInfo>
				<CodeIndex>306</CodeIndex>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.RS_FIRST_LAYER_DISCH</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.FIRST_LAYER_DISCH</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.SR_PREP_STOP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.PREP_STOP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.TON_PREP_STOP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.TON_PREP_STOP_2ND_LAYER</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.RS_STOP_DISCHARGE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.TON_WAIT</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.RESERVOIR</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.TON_CLEAR</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.SR_UPPER_BELT_INTERLOCK</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.TON_UPPER_BELT</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.RS_UPPER_BELT</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.UPPER_BELT_LIFTED</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB085_VALVE_CONTROL.TOF_UPPER_BELT</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1029F202" Crc32="0807623527" LastChange="2019-07-16T20:02:25">CPU1_PB087_VARIABLE_LEVEL</Name>
			<PrgInfo>
				<CodeIndex>307</CodeIndex>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.RT_PACKETS_FEEDING</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.RT_FEEDING</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TON_FEEDING</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.RS_VARIABLE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.RT_INC</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.INC_COUNTER</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.RT_DEC</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.DEC_COUNTER</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.CTUD_FILL_LEVEL</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SETPOINT_1</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SETPOINT_2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SETPOINT_3</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SETPOINT_4</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SETPOINT_5</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SETPOINT_6</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_0</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_0</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_LT_SETP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_LE_SETP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_SETP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_GE_SETP_HYST</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_LE_N1</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_N2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_MAX</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SR_CLEARING_ENABLE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TOF_PACK_IN_RESERVOIR</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SR_FILLING_POSSIBLE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TON_BACK_UP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TON_BACK_UP_DISCHARGE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SR_PREPARE_CLEAR</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SR_ENABLE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TOF_ENABLE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TON_START_CLEAR</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TON_LEVEL_0</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.DELAY_LEVEL_0</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SR_CLEARING_POSSIBLE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.SR_NO_SYNCHRON</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.TON_SYNCHRON</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.RS_CELLO_STOP</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.CTUD_STOP_PACKER</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB087_VARIABLE_LEVEL.COUNTER_STOP_PACKER</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10048845" Crc32="4239830451" LastChange="2018-05-25T18:55:28">CPU1_PB088_ERRORS</Name>
			<PrgInfo>
				<CodeIndex>308</CodeIndex>
				<Symbol>
					<Name>CPU1_PB088_ERRORS.TON_BACK_UP_INFEED</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB088_ERRORS.SR_BACK_UP_INFEED</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB088_ERRORS.TON_BACK_UP_DISCHARGE</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB088_ERRORS.TON_DISCHARGE_BLOCK</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100E2844" Crc32="3585575273" LastChange="2018-05-25T18:55:28">FX087_FILL_LEVEL</Name>
			<PrgInfo>
				<CodeIndex>309</CodeIndex>
				<Symbol>
					<Name PrgParameter="Input">FX087_FILL_LEVEL.SETPOINT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">FX087_FILL_LEVEL.COUNTER</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">FX087_FILL_LEVEL.FACTOR</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">FX087_FILL_LEVEL.N1</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">FX087_FILL_LEVEL.N2</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">FX087_FILL_LEVEL.N3</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">FX087_FILL_LEVEL.HYSTERESIS</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">FX087_FILL_LEVEL.VALUE1</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">FX087_FILL_LEVEL.VALUE2</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">FX087_FILL_LEVEL.VALUE3</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">FX087_FILL_LEVEL.VALUE4</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">FX087_FILL_LEVEL.VALUE5</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">FX087_FILL_LEVEL.VALUE6</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">FX087_FILL_LEVEL.VISU</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100102DE" Crc32="2729228048" LastChange="2018-05-25T18:55:28">FX193_LTEST_V2000</Name>
			<PrgInfo>
				<CodeIndex>310</CodeIndex>
				<Symbol>
					<Name PrgParameter="Input">FX193_LTEST_V2000.ENABLE</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100119BF" Crc32="1843684117" LastChange="2018-05-25T18:55:28">OB010_OPERATING</Name>
			<PrgInfo>
				<CodeIndex>311</CodeIndex>
				<Symbol>
					<Name>OB010_OPERATING.RT_RESET1</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10000000" Crc32="2826790393" LastChange="2018-05-25T18:55:28">OB020_CABINET</Name>
			<PrgInfo>
				<CodeIndex>312</CodeIndex>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10000000" Crc32="3618737609" LastChange="2018-05-25T18:55:28">OB050_SUPPLY</Name>
			<PrgInfo>
				<CodeIndex>313</CodeIndex>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10091273" Crc32="1410139327" LastChange="2018-05-25T18:55:28">PB012_OPERATING_MODE</Name>
			<PrgInfo>
				<CodeIndex>315</CodeIndex>
				<Symbol>
					<Name>PB012_OPERATING_MODE.TON_RESET_NOT_STARTED</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.TON_STOP</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.RS_STOP</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.RS_AUTO</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.TON_AUTO</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.RS_RESERVOIR_FULL</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.RS_STOP_RESERVOIR_FULL</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.RS_PACKETS_IN_RESERVOIR</Name>
				</Symbol>
				<Symbol>
					<Name>PB012_OPERATING_MODE.SR_MESSAGE_RESERVOIR_FULL</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100125AA" Crc32="1090031400" LastChange="2018-05-25T18:55:28">PB019_ERRORS</Name>
			<PrgInfo>
				<CodeIndex>317</CodeIndex>
				<Symbol>
					<Name>PB019_ERRORS.RESERVOIR_REFEED_MODE_TOF</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100360A9" Crc32="0562870359" LastChange="2018-05-25T18:55:28">PB022_UPSTR_MACHINE</Name>
			<PrgInfo>
				<CodeIndex>318</CodeIndex>
				<Symbol>
					<Name>PB022_UPSTR_MACHINE.TOF_DRY_DRUM</Name>
				</Symbol>
				<Symbol>
					<Name>PB022_UPSTR_MACHINE.TON_INFEED_BLOCK</Name>
				</Symbol>
				<Symbol>
					<Name>PB022_UPSTR_MACHINE.SR_INFEED_BLOCK</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10000000" Crc32="1668284757" LastChange="2018-05-25T18:55:28">PB023_DOWNSTR_MACHINE</Name>
			<PrgInfo>
				<CodeIndex>319</CodeIndex>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1002428B" Crc32="2120983106" LastChange="2018-05-25T18:55:28">PB029_ERRORS</Name>
			<PrgInfo>
				<CodeIndex>320</CodeIndex>
				<Symbol>
					<Name>PB029_ERRORS.TON_E_STOP</Name>
				</Symbol>
				<Symbol>
					<Name>PB029_ERRORS.TON_SAFETY</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10000000" Crc32="1881187027" LastChange="2018-05-25T18:55:28">PB197_COUNTER</Name>
			<PrgInfo>
				<CodeIndex>325</CodeIndex>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1001241D" Crc32="1563016690" LastChange="2020-09-03T23:05:51">PB013_LAMP</Name>
			<PrgInfo>
				<CodeIndex>316</CodeIndex>
				<Symbol>
					<Name>PB013_LAMP.TON_FEEDING_POSSIBLE</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10047238" Crc32="2600057477" LastChange="2018-05-25T18:55:28">_INTERVAL</Name>
			<PrgInfo>
				<CodeIndex>300</CodeIndex>
				<Symbol>
					<Name>_INTERVAL.RT_IO</Name>
				</Symbol>
				<Symbol>
					<Name>_INTERVAL.CTD_IO</Name>
				</Symbol>
				<Symbol>
					<Name>_INTERVAL.FLASH</Name>
				</Symbol>
				<Symbol>
					<Name>_INTERVAL.FLASH_COUNTER</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1003CE1A" Crc32="2074717353" LastChange="2018-05-25T18:55:28">CPU1_PB030_CAMS</Name>
			<PrgInfo>
				<CodeIndex>301</CodeIndex>
				<Symbol>
					<Name>CPU1_PB030_CAMS.CAMBANK</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB030_CAMS.SR_CLOCK</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB030_CAMS.RT_CLOCK</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1004BBAE" Crc32="1780882719" LastChange="2018-05-25T18:55:28">CPU1_PB038_ERRORS</Name>
			<PrgInfo>
				<CodeIndex>302</CodeIndex>
				<Symbol>
					<Name>CPU1_PB038_ERRORS.X_RUN</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB038_ERRORS.CAMCONTROL2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB038_ERRORS.PARITY_CHECK2</Name>
				</Symbol>
				<Symbol>
					<Name>CPU1_PB038_ERRORS.PARITY_FAULT</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10012AA0" Crc32="2515532423" LastChange="2018-05-25T18:55:28">OB190_VISUALISATION</Name>
			<PrgInfo>
				<CodeIndex>314</CodeIndex>
				<Symbol>
					<Name>OB190_VISUALISATION.DB_ERRORS</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10014638" Crc32="2814327723" LastChange="2018-05-25T18:55:28">PB059_ERRORS</Name>
			<PrgInfo>
				<CodeIndex>321</CodeIndex>
				<Symbol>
					<Name>PB059_ERRORS.COMPRESSED_AIR</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100D653C" Crc32="3548261965" LastChange="2018-05-25T18:55:28">PB191_ERROR_EVALUATION</Name>
			<PrgInfo>
				<CodeIndex>322</CodeIndex>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.S1</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.S2</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.S3</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.S4</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.H1</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.H2</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.H3</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.H4</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.BLOCK1</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.BLOCK2</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.BLOCK3</Name>
				</Symbol>
				<Symbol>
					<Name>PB191_ERROR_EVALUATION.BLOCK4</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">PB191_ERROR_EVALUATION.DB_ERRORS</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1007285A" Crc32="1472891259" LastChange="2020-11-14T21:44:29">PB193_VISU_DATA</Name>
			<PrgInfo>
				<CodeIndex>323</CodeIndex>
				<Symbol>
					<Name>PB193_VISU_DATA.COPY_FAULTS</Name>
				</Symbol>
				<Symbol>
					<Name>PB193_VISU_DATA.VISU_RESET_COUNTER</Name>
				</Symbol>
				<Symbol>
					<Name>PB193_VISU_DATA.PRESET_1</Name>
				</Symbol>
				<Symbol>
					<Name>PB193_VISU_DATA.PRESET_3</Name>
				</Symbol>
				<Symbol>
					<Name>PB193_VISU_DATA.TOF_RESTART</Name>
				</Symbol>
				<Symbol>
					<Name>PB193_VISU_DATA.TOF_COLD_RESTART</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">PB193_VISU_DATA.DB_ERRORS</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="1016B1FB" Crc32="4007104119" LastChange="2018-05-25T18:55:28">PB195_DBSAVE</Name>
			<PrgInfo>
				<CodeIndex>324</CodeIndex>
				<Symbol>
					<Name>PB195_DBSAVE.SAVE_DB51</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.BUSY_DB51</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.ERROR_DB51</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.SAVE_DB61</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.BUSY_DB61</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.ERROR_DB61</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.SAVE_DB91</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.BUSY_DB91</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.ERROR_DB91</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.SAVE_DB121</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.BUSY_DB121</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.ERROR_DB121</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.SAVE_DB341</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.BUSY_DB341</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.ERROR_DB341</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.FT_CAMS</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.RT_DB51</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.RT_DB61</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.RT_DB91</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.RT_DB121</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.RT_DB341</Name>
				</Symbol>
				<Symbol>
					<Name>PB195_DBSAVE.SR_DATA_FAULT</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100E8D4F" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB_CLEAN_VISU</Name>
			<PrgInfo>
				<CodeIndex>54</CodeIndex>
				<Symbol>
					<Name>S_FB_CLEAN_VISU.TON_READY</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_CLEAN_VISU.READY</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_CLEAN_VISU.LAUF</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_CLEAN_VISU.COUNTER32</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB_CLEAN_VISU.MACHINE_TYPE</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_1</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_2</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_3</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_41</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_43</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_44</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_80</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_100</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB_CLEAN_VISU.DB_120</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100BCF58" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB_WATCHDOG</Name>
			<PrgInfo>
				<CodeIndex>130</CodeIndex>
				<Symbol>
					<Name>S_FB_WATCHDOG.RT</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_WATCHDOG.FT</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_WATCHDOG.DELAY</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_WATCHDOG.TON_READY</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_WATCHDOG.X</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB_WATCHDOG.POINT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB_WATCHDOG.EXTERNAL_WATCHDOG</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB_WATCHDOG.HIGH_OK</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB_WATCHDOG.LOW_OK</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB_WATCHDOG.TOGGLE_OUT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB_WATCHDOG.IO_OFF</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100D8395" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB192_ERROR_STAT</Name>
			<PrgInfo>
				<CodeIndex>143</CodeIndex>
				<Symbol>
					<Name>S_FB192_ERROR_STAT.SR_HAND</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB192_ERROR_STAT.SR_OK</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB192_ERROR_STAT.FT_OK</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB192_ERROR_STAT.T_OK</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB192_ERROR_STAT.HAND</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB192_ERROR_STAT.DOOR</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB192_ERROR_STAT.STOP</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB192_ERROR_STAT.RESET</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB192_ERROR_STAT.START</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB192_ERROR_STAT.DOOR_HAND</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB192_ERROR_STAT.ERROR</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB192_ERROR_STAT.OK</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB192_ERROR_STAT.OK_PULSE</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="101B395E" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB196_DATA_COLLECTION</Name>
			<PrgInfo>
				<CodeIndex>144</CodeIndex>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.DCS_FUF</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.DCS_BUFFER</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.VISU_BUFFER</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.ERROR</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.READY</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.TIMER</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.DELAY_RESET</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.RT_RI</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.FT_RI</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.TOF_RI</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.RESET_IMPULS</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.SIMULATE_DOWNSTREAM_OK_TIMER</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB196_DATA_COLLECTION.MASK</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.STOP_DCS</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.STOP_UP</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.STOP_DOWN</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.RUN</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.AUTO</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.RESET</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.NET_ERROR</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.VISU</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB196_DATA_COLLECTION.DCS</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB196_DATA_COLLECTION.SIMULATE_DOWNSTREAM_OK</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB196_DATA_COLLECTION.PLC_READY</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB196_DATA_COLLECTION.OVERRIDE</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB196_DATA_COLLECTION.DB_A</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB196_DATA_COLLECTION.DB_V</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10061669" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB220_ADD32BIT</Name>
			<PrgInfo>
				<CodeIndex>149</CodeIndex>
				<Symbol>
					<Name>S_FB220_ADD32BIT.ZWI</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB220_ADD32BIT.WERT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB220_ADD32BIT.ENABLE</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB220_ADD32BIT.RESET</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB220_ADD32BIT.DW1</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB220_ADD32BIT.DW2</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10061669" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB221_SUB32BIT</Name>
			<PrgInfo>
				<CodeIndex>150</CodeIndex>
				<Symbol>
					<Name>S_FB221_SUB32BIT.ZWI</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB221_SUB32BIT.WERT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB221_SUB32BIT.ENABLE</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB221_SUB32BIT.RESET</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB221_SUB32BIT.DW1</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB221_SUB32BIT.DW2</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10055989" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB24_STAT_V2000</Name>
			<PrgInfo>
				<CodeIndex>153</CodeIndex>
				<Symbol>
					<Name>S_FB24_STAT_V2000.POINT</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB24_STAT_V2000.MAX_ADRESS</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB24_STAT_V2000.MAX_MEM</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB24_STAT_V2000.ENABLE</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB24_STAT_V2000.DB</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100B26F9" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB61_SETPOINT_V2000</Name>
			<PrgInfo>
				<CodeIndex>176</CodeIndex>
				<Symbol>
					<Name>S_FB61_SETPOINT_V2000.START</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB61_SETPOINT_V2000.MINW</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB61_SETPOINT_V2000.MASK</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB61_SETPOINT_V2000.TEST</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB61_SETPOINT_V2000.POINT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB61_SETPOINT_V2000.EIN</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB61_SETPOINT_V2000.FAKTOR</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB61_SETPOINT_V2000.VISU2000</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB61_SETPOINT_V2000.SOLL</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB61_SETPOINT_V2000.PRESET</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_FB61_SETPOINT_V2000.DB_GRENZ</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="100D4682" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_FB85_DRYING_REVOLVER</Name>
			<PrgInfo>
				<CodeIndex>189</CodeIndex>
				<Symbol>
					<Name>S_FB85_DRYING_REVOLVER.OUT</Name>
				</Symbol>
				<Symbol>
					<Name>S_FB85_DRYING_REVOLVER.TRIGGER</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.SPEED</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.SPEED_LIMIT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.FAKTOR</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.STOP</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.FULL</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.MIN_SPEED</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.OFFSET</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_FB85_DRYING_REVOLVER.DRIFT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB85_DRYING_REVOLVER.SETPOINT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB85_DRYING_REVOLVER.MONITOR</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_FB85_DRYING_REVOLVER.COMPENSATE</Name>
				</Symbol>
			</PrgInfo>
		</Program>
		<Program>
			<Name Decoration="10219B79" IsDefinedInLibrary="1" Library="C:\TWINCAT\PLC\LIB\FC800.lib">S_PB28_COM_SERVO</Name>
			<PrgInfo>
				<CodeIndex>193</CodeIndex>
				<Symbol>
					<Name>S_PB28_COM_SERVO.AddressIn</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.AddressOut</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.AxisIn</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.AxisOut</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.CheckNoOut</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.CheckSumIn</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.CheckSumE</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.CheckSumOut</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.CheckSumOutH</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.CheckSumOutL</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.CopyPointer</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.Init</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.INIT_TIME</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.MaxAddress</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.OffsetIn</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.OffsetOut</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.ReadNo</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.ResetExternal</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.ResetInternal</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.ResetInternalTime</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.UnSyncs</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.TimeCtrlOut</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.TimeCtrlRead</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.TimeOutWrite</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.TimeOutRead</Name>
				</Symbol>
				<Symbol>
					<Name>S_PB28_COM_SERVO.WriteNo</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_PB28_COM_SERVO.NO_OF_AXIS</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_PB28_COM_SERVO.RESET</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Input">S_PB28_COM_SERVO.E_COM</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_PB28_COM_SERVO.FAULT</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="Output">S_PB28_COM_SERVO.FAULT_NAME</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_PB28_COM_SERVO.A_COM</Name>
				</Symbol>
				<Symbol>
					<Name PrgParameter="InOut">S_PB28_COM_SERVO.DataMem</Name>
				</Symbol>
			</PrgInfo>
		</Program>
	</Programs>
	<Symbols>
		<Symbol>
			<Name TaskPrio="1">_CPU1.RT_RESTART</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>792</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">_CPU1.TOF_RESTART</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>795</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">_CPU2.RT_CLOCK</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>810</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">_CPU2.TOGGLE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>813</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB083_MOTORS.RT_AUTO1</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>6740</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB083_MOTORS.TOF_BELTMOTOR</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>6743</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB083_MOTORS.RS_DISCH_POS</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6758</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE.RS_FEED_POSSIBLE</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6761</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE.RS_ROT_FOR_REFEED</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6764</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE.DRUM_ROT_FOR_REFEED</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6767</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE.RS_ROT_DISCH</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6768</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE.CTUD_STOP_DRUM</Name>
			<Type Decoration="100A13D0">CTUD</Type>
			<IGroup>16448</IGroup>
			<IOffset>6771</IOffset>
			<BitSize>96</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE.COUNTER_STOP_DRUM</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6783</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE.TP_RESET_GUARD</Name>
			<Type Decoration="10050B9B">TP</Type>
			<IGroup>16448</IGroup>
			<IOffset>6784</IOffset>
			<BitSize>112</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RT_PACKETS_FEEDING_2</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>6798</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RT_FEEDING_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6801</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RS_FEEDING_2</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6802</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.FEEDING_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6805</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RS_FEEDING_ENABLE_2</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6806</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.FEEDING_ENABLE_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6809</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RS_FEEDING_ACTIVE_2</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6810</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RS_AF_ROT_FOR_REFEED_2</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6813</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.AF_DRUM_ROT_FOR_REFEED_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6816</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RS_ROT_FOR_REFEED_2</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6817</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RT_STOP_DRUM_FILL_2</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>6820</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.CTUD_STOP_DRUM_FILL_2</Name>
			<Type Decoration="100A13D0">CTUD</Type>
			<IGroup>16448</IGroup>
			<IOffset>6823</IOffset>
			<BitSize>96</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.COUNTER_STOP_DRUM_FILL_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6835</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RT_ROT_DISCH_2</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>6836</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.TON_FEEDING</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>6839</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.FT_FEEDING_2</Name>
			<Type Decoration="1003051C">F_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>6854</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.RS_ROT_DISCH_2</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6857</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.CTUD_STOP_DRUM_CLEAR_2</Name>
			<Type Decoration="100A13D0">CTUD</Type>
			<IGroup>16448</IGroup>
			<IOffset>6860</IOffset>
			<BitSize>96</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB084_REFEED_MODE_2.COUNTER_STOP_DRUM_CLEAR_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6872</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.RS_FIRST_LAYER_DISCH</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6873</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.FIRST_LAYER_DISCH</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6876</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.SR_PREP_STOP</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>6877</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.PREP_STOP</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6880</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.TON_PREP_STOP</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>6881</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.TON_PREP_STOP_2ND_LAYER</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6896</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.RS_STOP_DISCHARGE</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6897</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.TON_WAIT</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>6900</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.RESERVOIR</Name>
			<Type Decoration="102F59AF">SFC_RESERVOIR</Type>
			<IGroup>16448</IGroup>
			<IOffset>6915</IOffset>
			<BitSize>376</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.TON_CLEAR</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>6962</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.SR_UPPER_BELT_INTERLOCK</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>6977</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.TON_UPPER_BELT</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>6980</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.RS_UPPER_BELT</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>6995</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.UPPER_BELT_LIFTED</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6998</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB085_VALVE_CONTROL.TOF_UPPER_BELT</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>6999</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name>CPU1_PB087_VARIABLE_LEVEL.RT_PACKETS_FEEDING</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>7014</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name>CPU1_PB087_VARIABLE_LEVEL.RT_FEEDING</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7017</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name>CPU1_PB087_VARIABLE_LEVEL.TON_FEEDING</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7018</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name>CPU1_PB087_VARIABLE_LEVEL.RS_VARIABLE</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7033</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.RT_INC</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>7036</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.INC_COUNTER</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7039</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.RT_DEC</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>7040</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.DEC_COUNTER</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7043</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.CTUD_FILL_LEVEL</Name>
			<Type Decoration="100A13D0">CTUD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7044</IOffset>
			<BitSize>96</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SETPOINT_1</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7056</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SETPOINT_2</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7058</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SETPOINT_3</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7060</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SETPOINT_4</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7062</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SETPOINT_5</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7064</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SETPOINT_6</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7066</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_0</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7068</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_0</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7069</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_LT_SETP</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7070</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_LE_SETP</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7071</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_SETP</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7072</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_GE_SETP_HYST</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7073</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_LE_N1</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7074</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_N2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7075</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.LEVEL_GT_MAX</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7076</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SR_CLEARING_ENABLE</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7077</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.TOF_PACK_IN_RESERVOIR</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>7080</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SR_FILLING_POSSIBLE</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7095</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.TON_BACK_UP</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7098</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.TON_BACK_UP_DISCHARGE</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7113</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SR_PREPARE_CLEAR</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7128</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SR_ENABLE</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7131</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.TOF_ENABLE</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>7134</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.TON_START_CLEAR</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7149</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.TON_LEVEL_0</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7164</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.DELAY_LEVEL_0</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7179</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SR_CLEARING_POSSIBLE</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7180</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.SR_NO_SYNCHRON</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7183</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.TON_SYNCHRON</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7186</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.RS_CELLO_STOP</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7201</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.CTUD_STOP_PACKER</Name>
			<Type Decoration="100A13D0">CTUD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7204</IOffset>
			<BitSize>96</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB087_VARIABLE_LEVEL.COUNTER_STOP_PACKER</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7216</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB088_ERRORS.TON_BACK_UP_INFEED</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7217</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB088_ERRORS.SR_BACK_UP_INFEED</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7232</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB088_ERRORS.TON_BACK_UP_DISCHARGE</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7235</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB088_ERRORS.TON_DISCHARGE_BLOCK</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7250</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.SETPOINT</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7265</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.COUNTER</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7267</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.FACTOR</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7269</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.N1</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7271</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.N2</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7273</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.N3</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7275</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.HYSTERESIS</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7277</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.VALUE1</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[DW1 Setpoint 1]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7279</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.VALUE2</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[DW2 Setpoint 2]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7281</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.VALUE3</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[DW3 Setpoint 3]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7283</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.VALUE4</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[DW4 Setpoint 4]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7285</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.VALUE5</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[DW5 Setpoint 5]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7287</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.VALUE6</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[DW6 Setpoint 6]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7289</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">FX087_FILL_LEVEL.VISU</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[value for the visualisation]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7291</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">FX193_LTEST_V2000.ENABLE</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Lampentest / lamp test]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>7293</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">OB010_OPERATING.RT_RESET1</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>7294</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.TON_RESET_NOT_STARTED</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7809</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.TON_STOP</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7824</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.RS_STOP</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7839</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.RS_AUTO</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7842</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.TON_AUTO</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7845</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.RS_RESERVOIR_FULL</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7860</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.RS_STOP_RESERVOIR_FULL</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7863</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.RS_PACKETS_IN_RESERVOIR</Name>
			<Type Decoration="100306C8">RS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7866</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB012_OPERATING_MODE.SR_MESSAGE_RESERVOIR_FULL</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7869</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB019_ERRORS.RESERVOIR_REFEED_MODE_TOF</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>7887</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB022_UPSTR_MACHINE.TOF_DRY_DRUM</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>7902</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB022_UPSTR_MACHINE.TON_INFEED_BLOCK</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7917</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB022_UPSTR_MACHINE.SR_INFEED_BLOCK</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>7932</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB029_ERRORS.TON_E_STOP</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7935</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB029_ERRORS.TON_SAFETY</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7950</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB013_LAMP.TON_FEEDING_POSSIBLE</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>7872</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="4">_INTERVAL.RT_IO</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>814</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="4">_INTERVAL.CTD_IO</Name>
			<Type Decoration="10060AFD">CTD</Type>
			<IGroup>16448</IGroup>
			<IOffset>817</IOffset>
			<BitSize>64</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="4">_INTERVAL.FLASH</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>825</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="4">_INTERVAL.FLASH_COUNTER</Name>
			<Type Decoration="101222B0">WORD_BIT</Type>
			<IGroup>16448</IGroup>
			<IOffset>827</IOffset>
			<BitSize>152</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB030_CAMS.CAMBANK</Name>
			<Type Decoration="10148508">S_FB31_HD12CAM</Type>
			<IGroup>16448</IGroup>
			<IOffset>846</IOffset>
			<BitSize>46408</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB030_CAMS.SR_CLOCK</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>6647</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB030_CAMS.RT_CLOCK</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>6650</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB038_ERRORS.X_RUN</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6653</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB038_ERRORS.CAMCONTROL2</Name>
			<Type Decoration="101663EC">S_FB34_CAMCONTROL2</Type>
			<IGroup>16448</IGroup>
			<IOffset>6654</IOffset>
			<BitSize>488</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB038_ERRORS.PARITY_CHECK2</Name>
			<Type Decoration="100B1FB5">S_FB39_PARITY2</Type>
			<IGroup>16448</IGroup>
			<IOffset>6715</IOffset>
			<BitSize>192</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">CPU1_PB038_ERRORS.PARITY_FAULT</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>6739</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">OB190_VISUALISATION.DB_ERRORS</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>7297</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB059_ERRORS.COMPRESSED_AIR</Name>
			<Type Decoration="100D2C0E">S_FB_PRESSURE_FAULT</Type>
			<IGroup>16448</IGroup>
			<IOffset>7965</IOffset>
			<BitSize>152</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.S1</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7984</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.S2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7985</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.S3</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7986</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.S4</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7987</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.H1</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7988</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.H2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7989</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.H3</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7990</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.H4</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>7991</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.BLOCK1</Name>
			<Type Decoration="101A7D13">S_FB191_ERRORS</Type>
			<IGroup>16448</IGroup>
			<IOffset>7992</IOffset>
			<BitSize>592</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.BLOCK2</Name>
			<Type Decoration="101A7D13">S_FB191_ERRORS</Type>
			<IGroup>16448</IGroup>
			<IOffset>8066</IOffset>
			<BitSize>592</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.BLOCK3</Name>
			<Type Decoration="101A7D13">S_FB191_ERRORS</Type>
			<IGroup>16448</IGroup>
			<IOffset>8140</IOffset>
			<BitSize>592</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.BLOCK4</Name>
			<Type Decoration="101A7D13">S_FB191_ERRORS</Type>
			<IGroup>16448</IGroup>
			<IOffset>8214</IOffset>
			<BitSize>592</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB191_ERROR_EVALUATION.DB_ERRORS</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>8288</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB193_VISU_DATA.COPY_FAULTS</Name>
			<Type Decoration="10093330">S_FB75_DBCOPY</Type>
			<IGroup>16448</IGroup>
			<IOffset>8292</IOffset>
			<BitSize>168</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB193_VISU_DATA.VISU_RESET_COUNTER</Name>
			<Type Decoration="101222B0">WORD_BIT</Type>
			<IGroup>16448</IGroup>
			<IOffset>8313</IOffset>
			<BitSize>152</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB193_VISU_DATA.PRESET_1</Name>
			<Type Decoration="101222B0">WORD_BIT</Type>
			<IGroup>16448</IGroup>
			<IOffset>8332</IOffset>
			<BitSize>152</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB193_VISU_DATA.PRESET_3</Name>
			<Type Decoration="101222B0">WORD_BIT</Type>
			<IGroup>16448</IGroup>
			<IOffset>8351</IOffset>
			<BitSize>152</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB193_VISU_DATA.TOF_RESTART</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>8370</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB193_VISU_DATA.TOF_COLD_RESTART</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>8385</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB193_VISU_DATA.DB_ERRORS</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>8386</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.SAVE_DB51</Name>
			<Type Decoration="1025E07C">S_FB_FILE_DB256</Type>
			<IGroup>16448</IGroup>
			<IOffset>8390</IOffset>
			<BitSize>13624</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.BUSY_DB51</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>10093</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.ERROR_DB51</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>10094</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.SAVE_DB61</Name>
			<Type Decoration="1025E07C">S_FB_FILE_DB256</Type>
			<IGroup>16448</IGroup>
			<IOffset>10095</IOffset>
			<BitSize>13624</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.BUSY_DB61</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>11798</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.ERROR_DB61</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>11799</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.SAVE_DB91</Name>
			<Type Decoration="1025E22A">S_FB_FILE_DB512</Type>
			<IGroup>16448</IGroup>
			<IOffset>11800</IOffset>
			<BitSize>21816</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.BUSY_DB91</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>14527</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.ERROR_DB91</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>14528</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.SAVE_DB121</Name>
			<Type Decoration="1025E07C">S_FB_FILE_DB256</Type>
			<IGroup>16448</IGroup>
			<IOffset>14529</IOffset>
			<BitSize>13624</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.BUSY_DB121</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>16232</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.ERROR_DB121</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>16233</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.SAVE_DB341</Name>
			<Type Decoration="1025E22A">S_FB_FILE_DB512</Type>
			<IGroup>16448</IGroup>
			<IOffset>16234</IOffset>
			<BitSize>21816</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.BUSY_DB341</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>18961</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.ERROR_DB341</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>18962</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.FT_CAMS</Name>
			<Type Decoration="1003051C">F_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>18963</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.RT_DB51</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>18966</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.RT_DB61</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>18969</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.RT_DB91</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>18972</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.RT_DB121</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>18975</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.RT_DB341</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>18978</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">PB195_DBSAVE.SR_DATA_FAULT</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>18981</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.ADSLOG_MSGTYPE_HINT</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>0</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.ADSLOG_MSGTYPE_WARN</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>4</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.ADSLOG_MSGTYPE_ERROR</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>8</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.ADSLOG_MSGTYPE_LOG</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>12</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.ADSLOG_MSGTYPE_MSGBOX</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>16</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.ADSLOG_MSGTYPE_RESOURCE</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>20</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.ADSLOG_MSGTYPE_STRING</Name>
			<Type>DWORD</Type>
			<Comment>
				<![CDATA[file operation constants]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>24</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.FILE_OPENCREATE</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>28</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.FILE_OPENREAD</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>32</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.FILE_OPENWRITE</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>36</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.FILE_READ</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>40</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.FILE_WRITE</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>44</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.FILE_SEEKBEGIN</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>48</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.FILE_SEEKEND</Name>
			<Type>DWORD</Type>
			<Comment>
				<![CDATA[boot data constants (-> SYSTEMINFOTYPE.bootDataFlags)]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>52</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.BOOTDATAFLAGS_RETAIN_LOADED</Name>
			<Type>BYTE</Type>
			<IGroup>16448</IGroup>
			<IOffset>56</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.BOOTDATAFLAGS_RETAIN_INVALID</Name>
			<Type>BYTE</Type>
			<IGroup>16448</IGroup>
			<IOffset>57</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.BOOTDATAFLAGS_RETAIN_REQUESTED</Name>
			<Type>BYTE</Type>
			<IGroup>16448</IGroup>
			<IOffset>58</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.BOOTDATAFLAGS_PERSISTENT_LOADED</Name>
			<Type>BYTE</Type>
			<IGroup>16448</IGroup>
			<IOffset>59</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.BOOTDATAFLAGS_PERSISTENT_INVALID</Name>
			<Type>BYTE</Type>
			<Comment>
				<![CDATA[system state constants (-> SYSTEMINFOTYPE.systemStateFlags)]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>60</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.SYSTEMSTATEFLAGS_BSOD</Name>
			<Type>BYTE</Type>
			<Comment>
				<![CDATA[blue screen of death]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>61</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1">.SYSTEMSTATEFLAGS_RTVIOLATION</Name>
			<Type>BYTE</Type>
			<Comment>
				<![CDATA[realtime violation - latency time]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>62</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.FPH_STOP_MACHINE</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[FPH: Parameteraustausch aktiv: Maschine Stop		/	FPH: processing parameter changes, machine stop]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>19022</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1" Static="MArea">.SystemInfo</Name>
			<Type Decoration="10066081">SYSTEMINFOTYPE</Type>
			<IGroup>16416</IGroup>
			<IOffset>32768</IOffset>
			<BitSize>320</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1" Static="MArea">.SystemTaskInfoArr</Name>
			<Type Decoration="20017954">ARRAY [1..4] OF SYSTEMTASKINFOTYPE</Type>
			<IGroup>16416</IGroup>
			<IOffset>32832</IOffset>
			<BitSize>1056</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_1_16</Name>
			<Type>WORD</Type>
			<IGroup>16416</IGroup>
			<IOffset>50</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Not-Aus-Kreis                     			/	emergency stop circuit]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>400</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Sicherheitskreis       				/	safety circuit]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>401</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Spannungsversorgung        			/	power supply]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>402</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Motorschutzschalter       				/	motor circuit breaker]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>403</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>404</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>405</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Watchdog						/	watchdog]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>406</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_8</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>407</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_9</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Datentransfer        					/	data transfer]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>408</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_10</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Kurvenfehler                      			/	cam fault]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>409</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_11</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber         				/	absolute encoder]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>410</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_12</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>411</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_13</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>412</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_14</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>413</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_15</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>414</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_16</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[S Sicherheitskreis       				/	s safety circuit]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>415</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_17_32</Name>
			<Type>WORD</Type>
			<IGroup>16416</IGroup>
			<IOffset>52</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_17</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Stop-Taster             					/	stop button]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>416</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_18</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Haube Speicher         				/	guard,reservoir]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>417</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_19</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Haube Nachlegeschacht			/	guard,refeed pocket]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>418</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_20</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Haube Einlauf                  				/	guard,infeed]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>419</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_21</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Deckel Einschieber             			/	cover,infeed pusher]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>420</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_22</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Sicherheitsschalter Obergurt   		/	safety switch upper belt]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>421</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_23</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Seitentür                     				/	side door]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>422</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_24</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>423</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_25</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Not-Aus                   					/	emergency stop]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>424</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="3">.ERROR_26</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Druckluft                  					/	compressed air]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>425</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_27</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>426</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_28</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>427</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_29</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>428</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_30</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speichermotor nicht betriebsbereit	/	reservoir motor not ready for oper.]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>429</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_31</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Thermokontakt Gurtmotor			/	thermal contact belt motor]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>430</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_32</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Thermokontakt Speichermotor		/	thermal contact reservoir motor]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>431</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_33_48</Name>
			<Type>WORD</Type>
			<IGroup>16416</IGroup>
			<IOffset>54</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_33</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Handrad                       				/	handwheel]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>432</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_34</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einschieber nicht in Position			/	infeed pusher out of position]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>433</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_35</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ausschieber nicht in Position  		/	discharge pusher out of position]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>434</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_36</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einschieber              				/	infeed pusher]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>435</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_37</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ausschieber               				/	discharge pusher]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>436</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_38</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Stau Einlauf                  				/	back-up at infeed]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>437</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_39</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Stau Auslauf                  				/	back up at discharge]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>438</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_40</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurt                      				/	upper belt]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>439</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_41</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[S Paketfühler                				/	s packet feeler ph'cell]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>440</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_42</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[S LS Auslaufsperre            			/	s discharge stop ph'cell]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>441</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.ERROR_43</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Stau Lichtschranke Auslaufsperre	/	back-up discharge stop photocell]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>442</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_44</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>443</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_45</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>444</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_46</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>445</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_47</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>446</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_48</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>447</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="2">.ERROR_49_64</Name>
			<Type>WORD</Type>
			<IGroup>16416</IGroup>
			<IOffset>56</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_49</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>448</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_50</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>449</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_51</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>450</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_52</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>451</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_53</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>452</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_54</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>453</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_55</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>454</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_56</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>455</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_57</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>456</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_58</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>457</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_59</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>458</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_60</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>459</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_61</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>460</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_62</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>461</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_63</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>462</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.ERROR_64</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>463</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_1_32</Name>
			<Type>DWORD</Type>
			<IGroup>16416</IGroup>
			<IOffset>80</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="3">.CAM_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Endstellung Füllen        			/ 	final position, filling]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>640</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="3">.CAM_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Endstellung Entleeren       		/ 	final position, discharge]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>641</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Gurt Anheben beim Füllen   	 	/ 	belt lifting during filling]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>642</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Gurt Anheben beim Entleeren  	/ 	belt lifting during discharge]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>643</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einlaufsperre beim Füllen  		/ 	infeed stop during filling]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>644</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einlaufsperre beim Entleeren 	/ 	infeed stop during discharge]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>645</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Auslaufsperre beim Entleeren 	/ 	exit stop during discharge]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>646</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_8</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einschieber                 			/ 	infeed pusher]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>647</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_9</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Auschieber                  			/ 	discharge pusher]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>648</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_10</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Paketführung beim Füllen  		/ 	packet guide during filling]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>649</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_11</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Zähler vorwärts           			/ 	pulse counter incrementation]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>650</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea" TaskPrio="1">.CAM_12</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Zähler rückwärts      	   		/ 	pulse counter decrementation]]>
			</Comment>
			<IGroup>16417</IGroup>
			<IOffset>651</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_13</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>652</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_14</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>653</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_15</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>654</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_16</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>655</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_17</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>656</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_18</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>657</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_19</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>658</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_20</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>659</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_21</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>660</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_22</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>661</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_23</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>662</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_24</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>663</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_25</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>664</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_26</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>665</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_27</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>666</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_28</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>667</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_29</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>668</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_30</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>669</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_31</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>670</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="MArea">.CAM_32</Name>
			<Type>BOOL</Type>
			<IGroup>16417</IGroup>
			<IOffset>671</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.ANGLE</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>19023</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.STEP</Name>
			<Type>WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>19025</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.AUTO</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19027</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.BACK_UP_DISCHARGE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19028</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.CLEARING_ENABLE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19029</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.CLEARING_POSSIBLE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19030</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.COLD_RESTART</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19031</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.CPU1_CLOCK</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19032</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.CPU1_RESET</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19033</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.CPU2_RESET</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19034</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.DIRECTION_CLEARING</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19035</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.DIRECTION_FILLING</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19036</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.DOWNSTR_MACH_NOT_READY</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19037</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.DRUM_ROT_FOR_REFEED_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19038</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.DRY_DRUM_RUN</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19039</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.FAULT_BACK_UP_DISCHARGE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19040</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.FAULT_BACK_UP_INFEED</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19041</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.FAULT_CAM</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19042</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.FAULT_DATA_TRANSFER</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19043</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.FAULT_GUARD_RESERVOIR</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19044</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.FAULT_INFEED_BLOCK</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19045</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.FEEDING_ACTIVE_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19046</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.FEEDING_POSSIBLE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19047</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.FEEDING_POSSIBLE_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19048</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.FILLING_POSSIBLE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19049</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="4">.FLASH_100</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19050</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="4">.FLASH_200</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19051</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="4">.FLASH_400</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19052</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="6">.FLASH_800</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19053</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.INCHING</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19054</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.INCHING_CLEAR</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19055</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.INCHING_FILL</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19056</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.INIT_CAMS</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19057</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="7">.IO_READY</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19058</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.LEVEL_UNDER_N3</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19059</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.LEVEL_UNDER_SETPOINT</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19060</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.LEVEL_OVER_SETPOINT</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19061</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.MESSAGE_CLEARING</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19062</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.MESSAGE_RESERVOIR_FULL</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19063</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.PACKETS_IN_RESERVOIR</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19064</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.PACKETS_REFEED</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19065</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.PACKETS_REFEED_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19066</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.PREP_CONT_DISCH_ON</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19067</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.PREPARE_CLEAR</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19068</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.PRESET_LAMP_TEST</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19069</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.PRESET_RESET_SAFETY</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19070</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.PRESET_VARIABLE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19071</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.PRESET_VARIABLE_GRAPHIC</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>27831</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.RESERVOIR_RUN</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19072</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.RESET_COUNTER</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19073</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.RESET_NOT_STARTED</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19074</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.RESET_REJECT</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19075</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.RESET_REJECT_FLAG</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19076</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.ROTATION_CLEARING</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19077</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.ROTATION_FILLING</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19078</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.RT_AUTO</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19079</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.RT_RESET</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19080</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.RT_MACH_CLOCK</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19081</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.RT_MACH_CLOCK_CPU2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19082</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.SAFETY_CIRCUIT</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19083</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.START_CLEAR</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19084</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.STOP_DCS</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19085</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.STOP_DISCHARGE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19086</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.STOP_END</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19087</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.STOP_FAST</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19088</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.STOP_RESERVOIR_FULL</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19089</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.SUM_FS</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19090</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.SUM_PS</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19091</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.SYNCHRON</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19092</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.TO_FINAL_POS_FILL</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19093</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.TO_FINAL_POS_DISCH</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19094</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.TON_CLEAR_BELT</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19095</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.TON_WAIT_NEXT_DISCH</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19096</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.UPSTR_MACH_NOT_READY</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19097</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="3">.VARIABLE</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19098</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.WATCHDOG</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19099</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="1">.DRUM_ROT_FOR_RFEED_2</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>19100</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="1">.FILL_LEVEL</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>19101</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.GRAY</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61472</IGroup>
			<IOffset>70</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>560</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>561</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>562</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>563</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>564</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>565</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>566</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E70_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>567</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E71_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>568</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E71_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber (parity) 				/	absolute encoder (parity)]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>569</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E71_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Absolutwertgeber  						/	absolute encoder]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>570</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E71_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>571</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E71_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>572</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E71_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>573</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E71_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>574</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E71_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Watchdog -A90.31						/	watchdog -A90.31]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>575</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E72_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Paketfühler 1							/	packet sensor 1]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>576</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E72_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Paketfühler 2							/	packet sensor 2]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>577</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E72_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Drehrichtung Entleeren					/	direction of rotation clearing]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>578</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E72_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Drehrichtung Füllen					/	direction of rotation filling]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>579</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E72_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurtverriegelung					/	upper belt interlock]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>580</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E72_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Handrad								/	handwheel]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>581</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E72_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Stau im Einlauf						/	back-up infeed]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>582</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E72_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Nachlegeschacht voll					/	refeed pocket full]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>583</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E73_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Stau im Auslauf						/	back-up discharge]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>584</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E73_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Auslaufsperre							/	exit stop]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>585</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E73_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einlaufsperre							/	infeed stop]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>586</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E73_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Schacht voll							/	pocket full]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>587</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E73_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speicher voll							/	reservoir full]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>588</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E73_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einschieber							/	infeed pusher]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>589</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E73_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ausschieber							/	discharge pusher]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>590</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E73_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[2. Schacht voll						/	2nd pocket full]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>591</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E74_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Not-Aus								/	emergency stop]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>592</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E74_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Haube Speicher						/	guard reservoir]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>593</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E74_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Sicherheitsschalter Obergurt			/	safety switch upper belt]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>594</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E74_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Haube Einlauf						/	guard infeed]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>595</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E74_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Maschine Aus 						/	reservoir off]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>596</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E74_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Maschine Ein  						/	reservoir on]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>597</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E74_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Füllen								/	reservoir fill]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>598</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E74_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Entleeren 							/	reservoir clear]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>599</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E75_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Automatik 							/	automatic]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>600</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E75_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einrichten 							/	inching]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>601</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E75_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Kontrollen Löschen 					/	reset]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>602</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E75_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Pakete Nachlegen					/	packets refeed]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>603</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E75_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Thermokontakt Gurtmotor				/	thermal contact belt motor]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>604</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E75_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Thermokontakt Speichermotor			/	thermal contact reservoir motor]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>605</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E75_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Seitentür								/	side door]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>606</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E75_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Deckel Einschieber					/	cover at infeed pusher]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>607</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einschieber Bruch						/	infeed pusher jam]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>608</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ausschieber Bruch					/	discharge pusher jam]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>609</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Auslaufsperre							/	exit stop]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>610</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einschieber geperrt					/	infeed pusher inhibited]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>611</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurt anheben rechts				/	raise upper belt right]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>612</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurt absenken rechts				/	lower upper belt right]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>613</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurt anheben links					/	raise upper belt left]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>614</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E76_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurt absenken links				/	lower upper belt left]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>615</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>616</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>617</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>618</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>619</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>620</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>621</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>622</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E77_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>623</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E78_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Sicherheitskreis Speicher				/	safety circuit reservoir]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>624</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E78_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Motorschutzschalter					/	motor circuit breaker]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>625</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E78_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Betrieb Speicher						/	operation reservoir]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>626</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E78_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Rückmeldung Gurtmotor				/	feedback beltmotor]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>627</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E78_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Rückmeldung Speicher Füllen			/	feedback reservoir filling]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>628</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E78_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Rückmeldung Speicher Entleeren		/	feedback reservoir clearing]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>629</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E78_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Watchdog -A90.30						/	watchdog -A90.30]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>630</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E78_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Nachlegeschacht Sicherheitskreis		/	safety circuit refeed pocket]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>631</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.EW190</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[Druckluft								/	compressed air]]>
			</Comment>
			<IGroup>61472</IGroup>
			<IOffset>190</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.EW192</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61472</IGroup>
			<IOffset>192</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN</Name>
			<Type>WORD</Type>
			<IGroup>61472</IGroup>
			<IOffset>940</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E_DOWN_M_PREP_CLEAR</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speicher entleeren vorbereiten		/	prepare reservoir clearing]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7520</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.E_DOWN_M_AUTO</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Cello in Automatik  				/	cello in automatic]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7521</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E_DOWN_M_CLEAR</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Start Speicher entleeren			/	start reservoir clearing]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7522</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E_DOWN_M_START_BELT</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Start Gurt		   					/	start belt]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7523</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E_DOWN_M_BACK_UP_MIN</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einlaufgurt Cello Stau min.			/	infeed belt cello back-up min.]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7524</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.E_DOWN_M_AUTO_DCS</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Cello betriebsbereit	 			/	cello ready for operation]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7525</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_MASTER</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Cello als Master					/	cello is master]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7526</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7527</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E_DOWN_M_CONTINOUS_CLEAR</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Dauerentleeren vorbereiten  		/	prepare continuous clearing]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7528</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_9</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7529</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.E_DOWN_M_BACK_UP_MAX</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einlaufgurt Cello Stau max. 			/	infeed belt cello back-up max.]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7530</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_11</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7531</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_12</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7532</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_13</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7533</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_14</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7534</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.E_DOWN_M_15</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61473</IGroup>
			<IOffset>7535</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.PACKER_READY</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12000</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.PACKER_INCHING</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12001</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.PACKER_ENABLE</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12002</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.PACKER_DRY_DRUM</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12003</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.PACKER_N_0</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12004</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.PACKER_RUN_WO_P</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12005</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.PACKER_WATCHDOG</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12006</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.PACKER_MACH_CLOCK</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12007</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.PACKER_CLEARING_END</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12008</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.PACKER_LOW_SPEED</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12009</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="3">.PACKER_LOCK_RESERVOIR</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12010</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.PACKER_BC_ACTIVE</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12011</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.PACKER_CLEAR_FILL</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12013</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input">.PACKER_BC_RESERVOIR_EMPTY</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12014</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.PACKER_EMERGENCY_CIRCUIT</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12016</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="2">.PACKER_POWER_SUPPLY</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12017</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.PACKER_ENABLE_CLEAR_RESERVOIR</Name>
			<Type>BOOL</Type>
			<IGroup>61473</IGroup>
			<IOffset>12020</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Input" TaskPrio="1">.PACKER_CLEAR_LEVEL</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[------------     DIGITAL 	OUTPUTS		--------------]]>
			</Comment>
			<IGroup>61472</IGroup>
			<IOffset>1505</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.A70_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Sperre Einlauf						/	infeed block]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>560</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.A70_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Sperre Auslauf						/	exit block]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>561</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A70_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurt anheben						/	raise upper belt]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>562</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A70_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurt von Hand anheben			/	raise upper belt manually]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>563</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A70_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Obergurtverriegelung					/	upper belt interlock]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>564</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A70_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Paketseitenführung					/	side guide]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>565</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A70_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Lampe Pakete nachlegen				/	lamp packets refeed]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>566</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A70_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Lampe Bedienpult						/	lamp on main operator's panel]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>567</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A71_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Einschieber bereit						/	infeed pusher ready]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>569</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A71_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>570</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A71_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ampel: Pakete nachlegen				/	lamp colomn: refeeding possible]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>571</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A71_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ampel: Speicher dreht					/	lamp colomn: reservoir run]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>572</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A71_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ampel: Standby						/	lamp colomn: standby]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>573</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A71_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Ampel: Stop							/	lamp colomn: stop]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>574</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A71_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>575</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.A74_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Gurtmotor							/	beltmotor]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>592</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A74_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speicher Füllen						/	reservoir fill]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>593</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A74_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speicher Entleeren					/	reservoir clear]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>594</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A74_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>595</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A74_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speichermotor Freigabe				/	reservoir motor enable]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>596</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A74_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speichermotor Entleeren				/	reservoir motor clearing]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>597</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A74_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>598</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A74_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>599</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>600</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>601</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>602</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>603</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>604</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>605</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>606</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A75_7</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>607</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A76_0</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Bremse Speichermotor					/	brake]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>608</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A76_1</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Kontrollen Löschen					/	reset]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>609</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A76_2</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Speichermotor Reset					/	reservoir motor reset]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>610</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A76_3</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>611</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output">.A76_4</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[/]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>612</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.A76_5</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Stopp Schütz							/	stop contactor]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>613</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.A76_6</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[Kontrollen Löschen					/	reset]]>
			</Comment>
			<IGroup>61489</IGroup>
			<IOffset>614</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.RESERVOIR_AUTO</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12080</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.RESERVOIR_FULL</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12081</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.RESERVOIR_WITH_PACKETS</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12082</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.RESERVOIR_START_BELT</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12083</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.RESERVOIR_DCS_N_OK</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12084</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.RESERVOIR_DISABLE_CELLO</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12085</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.RESERVOIR_RED_SPEED</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12086</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.RESERVOIR_CLEARING</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12087</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.RESERVOIR_VARIABLE_ON</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12088</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.RESERVOIR_BACK_UP</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12089</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.RESERVOIR_LEVEL_N1</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12090</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.RESERVOIR_LEVEL_N3</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12091</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.RESERVOIR_GUARD</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12092</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.RESERVOIR_FULL_CLEARING</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12093</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.RESERVOIR_EMERGENCY_STOP</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12096</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="2">.RESERVOIR_SAFETY_CIRCUIT</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12097</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="3">.RESERVOIR_REFEED_MODE</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12098</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.RESERVOIR_START_CLEAR</Name>
			<Type>BOOL</Type>
			<IGroup>61489</IGroup>
			<IOffset>12100</IOffset>
			<BitSize>1</BitSize>
		</Symbol>
		<Symbol>
			<Name Static="Output" TaskPrio="1">.RESERVOIR_FILLING_LEVEL</Name>
			<Type>WORD</Type>
			<IGroup>61488</IGroup>
			<IOffset>1515</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1">.DB5</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Auswurfzähler  				/ 	reject counter]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>19103</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="6">.DB6</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Warnungen  					/ 	warnings]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>19615</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="6">.DB7</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Erstwertfehler  				/ 	first-up detection]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>20127</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="7">.DB8</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Materialzähler,  Meßwerte 		/ 	material counter]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>20639</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="4">.DB41</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Profibus-Diagnose			/ 	profibus diagnostics]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>21151</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="4">.DB43</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 PC - Diagnose				/ 	PC - diagnostics]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>21663</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="4">.DB44</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 PC - Diagnose				/ 	PC - diagnostics]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>22175</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="2">.DB51</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Voreinstellungen  				/  	preselections]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>22687</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="3">.DB61</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Drehzahlen, Grenzwerte  		/  	limits + setpoint values]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>23199</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="6">.DB81</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Status						/  	status]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>23711</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="3">.DB91</Name>
			<Type Decoration="2001034D">ARRAY [0..511] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Kurven 						/ 	cams]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>24223</IOffset>
			<BitSize>8192</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="4">.DB101</Name>
			<Type Decoration="2001034D">ARRAY [0..511] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Heizungen  					/	heaters]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>25247</IOffset>
			<BitSize>8192</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="6">.DB121</Name>
			<Type Decoration="2001024D">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Manometer  					/ 	manometers]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>26271</IOffset>
			<BitSize>4096</BitSize>
		</Symbol>
		<Symbol>
			<Name Persistent="1" TaskPrio="3">.DB341</Name>
			<Type Decoration="2001034D">ARRAY [0..511] OF WORD</Type>
			<Comment>
				<![CDATA[V2000 M2 Service Voreinstellungen		/	service presets]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>26783</IOffset>
			<BitSize>8192</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.PRESET_VARIABLE_A</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>27807</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.PRESET_VARIABLE_TON</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>27808</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name TaskPrio="2">.PRESET_VARIABLE_CTU</Name>
			<Type Decoration="10060B75">CTU</Type>
			<IGroup>16448</IGroup>
			<IOffset>27823</IOffset>
			<BitSize>64</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.TON_READY</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>63</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.READY</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>78</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.LAUF</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>79</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.COUNTER32</Name>
			<Type>INT</Type>
			<Comment>
				<![CDATA[Anzahl 32-Bit Zähler
							/ number of 32-bit counters 
							/ nombres de compteurs 32 bits]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>81</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.MACHINE_TYPE</Name>
			<Type>INT</Type>
			<Comment>
				<![CDATA[D:	Maschinentyp:	z.B. 700 für M700]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>83</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_1</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	Symbole
							GB: 	Symbols					
							F:	Symboles]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>85</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_2</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	Störungen
							GB:	Errors					
							F:	Défauts]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>89</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_3</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	Zähler
							GB:	Counters					
							F:	Compteurs]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>93</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_41</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	Profibus-Diagnose
							GB:	Profibus Diagnostics		
							F:	Diagnostic Profibus]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>97</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_43</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	PC-Diagnose
							GB:	PC-diagnostics			
							F:	Diagnostic ordinateur personnel]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>101</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_44</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	PC-Diagnose
							GB:	PC-diagnostics			
							F:	Diagnostic ordinateur personnel]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>105</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_80</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D: 	SPS-Status
							GB:	PLC-Status 				
							F:	Etat API]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>109</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_100</Name>
			<Type Decoration="2001034D" Pointer="1">ARRAY [0..511] OF WORD</Type>
			<Comment>
				<![CDATA[D: 	Heizungen
							GB:	Heaters					
							F:	Chauffages]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>113</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="4">S_FB_CLEAN_VISU.DB_120</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D: 	Manometer
							GB:	Air pressure measurement 	
							F:	Manomètres]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>117</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.RT</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>121</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.FT</Name>
			<Type Decoration="1003051C">F_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>124</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.DELAY</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>127</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.TON_READY</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>142</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.X</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>157</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.POINT</Name>
			<Type Decoration="2001028C" Pointer="1">ARRAY [0..249] OF DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>159</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.EXTERNAL_WATCHDOG</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	IO's gestört --> alle Ausgänge abschalten
									GB:	IO malfunction --> disable all outputs	
									E:	ES malfuncion --> anular todas salidas
									F:	IO-erreurs --> Débrancher tout les sorties]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>163</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.HIGH_OK</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Alle Überwachungs-Eingänge sind "TRUE"
									GB:	All control-Inputs have "TRUE"-condition
									E:	Todas las entradas en tienen condicion activa
									F:	Tout les entrées de évaluation sont en condition 
										"FALSE"]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>164</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.LOW_OK</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	Alle Überwachungs-Eingänge sind "FALSE"
									GB:	All control-Inputs have "FALSE" condition	
									E:	Todas las entradas tienen condicion desactivadas
									F:	Tout les entrées de évaluation sont en condition 
										"FALSE"]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>165</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.TOGGLE_OUT</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	"Toggle"-Bit für Kontrollausgänge
									GB:	"Toggle"-Bit for control-outputs
									E:	"Toggle"-Bit para control de salidas
									F:	Bit de change de Evaluation d'erreur]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>166</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB_WATCHDOG.IO_OFF</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	Alle Ausgänge AB 0 ... AB999 abgeschaltet
									GB:	All outputs QB0 ... QB999 set to NULL		
									E:	Todas las salidas 0 ... 999 se ponen a cero
									F:	Tout les sorties sont mis a zero]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>167</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.SR_HAND</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>168</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.SR_OK</Name>
			<Type Decoration="100306C6">SR</Type>
			<IGroup>16448</IGroup>
			<IOffset>171</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.FT_OK</Name>
			<Type Decoration="1003051C">F_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>174</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.T_OK</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>177</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.HAND</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Handrad / GB: handwheel disengaged		
								E: Rueda de mano	/ F: volant]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>192</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.DOOR</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:Tür offen oder Materialmangel				
								GB:  Door open or material shortage			
								E:  	Puerta abierta o escasez de material	
								F:	Porte ouverte ou manque de matériel]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>193</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.STOP</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Störung vorhanden / GB: error present
								E:  Condición de avería / F: erreur existante]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>194</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.RESET</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: RESET / GB: RESET						
								 E: RESETEO	 / F: RAZ]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>195</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.START</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: START / GB: START								
								 E: ARRANQUE / F: DEMARRAGE]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>196</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.DOOR_HAND</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Tür oder  Handrad   
								GB:  DOOR or  HANDWHEEL	
								E:  	Puerta /rueda de mano 
								F:	porte / volant]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>197</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.ERROR</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Fehler vorhanden / GB: error exists		
								E: Fallo presente / F: erreur existante]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>198</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.OK</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Zustand "ok" / GB: condition  "ok"			
								E:  Estado "ok" / F: situation "ok"]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>199</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB192_ERROR_STAT.OK_PULSE</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: verlängertes OK-Signal	
								GB: 	Extended "OK" pulse 		
								F:	Signal OK prolongé]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>200</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.DCS_FUF</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[GB: DCS first up fault 		// D: EWF für BDE]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>201</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.DCS_BUFFER</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[GB: DCS state  internal 	// D: BDE Status intern]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>203</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.VISU_BUFFER</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[GB: Visu first up fault internal	//]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>205</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.ERROR</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[GB: machine error		// D: Stopgrund liegt vor]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>207</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.READY</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[GB: DCS state is defined	// D: BDE Status steht fest]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>208</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.TIMER</Name>
			<Type Decoration="10060D24">TON</Type>
			<IGroup>16448</IGroup>
			<IOffset>209</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.DELAY_RESET</Name>
			<Type Decoration="10060D24">TON</Type>
			<Comment>
				<![CDATA[GB: Reset signal with delay // D:Verzögerter Reset]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>224</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.RT_RI</Name>
			<Type Decoration="1003051C">R_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>239</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.FT_RI</Name>
			<Type Decoration="1003051C">F_TRIG</Type>
			<IGroup>16448</IGroup>
			<IOffset>242</IOffset>
			<BitSize>24</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.TOF_RI</Name>
			<Type Decoration="10060D24">TOF</Type>
			<IGroup>16448</IGroup>
			<IOffset>245</IOffset>
			<BitSize>120</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.RESET_IMPULS</Name>
			<Type>BOOL</Type>
			<IGroup>16448</IGroup>
			<IOffset>260</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.SIMULATE_DOWNSTREAM_OK_TIMER</Name>
			<Type Decoration="10050B9B">TP</Type>
			<IGroup>16448</IGroup>
			<IOffset>261</IOffset>
			<BitSize>112</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.MASK</Name>
			<Type Decoration="2001015D">ARRAY [0..15] OF WORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>275</IOffset>
			<BitSize>256</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.STOP_DCS</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: BDE deaktiviert
							GB:	Data collection disabeld    					
							E:	ADP no activo						
							F:	Acquisition de données désactivée]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>307</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.STOP_UP</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Stop vorlaufende Maschine
							GB:  Upstream machine is in STOP-mode		
							E:	Parada de máquina precedente			
							F:	Machine amont est en mode STOP]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>308</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.STOP_DOWN</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	Parada de máquina precedente
							GB:	Downstream machine is in STOP-mode	
							E:	Parada de máquina siguiente			
							F:	Machine aval est en mode STOP]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>309</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.RUN</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	Maschine läuft
							 GB:	Machine is running						
							E:	Máquina en funcionamiento				
							F:	Machine fonctionne]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>310</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.AUTO</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	Automatikbetrieb
							GB:	Automatic mode active													
							E:	Modo automático activo				
							F:	Fonctionnement automatique actif]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>311</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.RESET</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	Überschreibgrund zurücksetzen
							GB:	Reset the override reason       									
							E:	Reseteo ADP							
							F:	Remise à zéro acquisition de données]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>312</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.NET_ERROR</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	In dem Fall, dass das BDE über ein Netzwerk
								auf die Maschine zurgreift, zeigt dieses Flag 
								an, dass das Netz unterbrochen ist -> Daten ungültig   
							GB:	In case, that the DCS gets the machine data
								data via a network, this flag shows a network 
								failure -> data not valid        
							E:	Fallo de red ADP						
							F:	Panne de réseau acquisition de données]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>313</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.VISU</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[D:	Element Pointer auf VISU-EWF (Index)
							GB:	Index of VISU "first up"-error data 										
							E:	Indicador procesa VISU fallo primer valor	
							F:	Pointeur sur  valeur primaire dans VISU]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>314</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.DCS</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[D:	Pointer auf BDE-Maschinen Status (Index)
							GB:	Index of data collection machine state  		
							E:	Indicador procesa fallo primer valor de ADP	
							F:	Pointeur sur  valeur primaire dans acquis. données]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>316</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.SIMULATE_DOWNSTREAM_OK</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[
	D:	Solange dieses Signal TRUE ist sollte die vorlaufende Maschine das
		Signal 'nachlaufende Maschinen OK' bekommen 					
	GB:  As long this signal is true the up-
		stream machine should get the signal that all down strem machines are OK
	E:	Red en funcionamiento						
	F:	Réseau fonctionne]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>318</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.PLC_READY</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[PLC-READY SIGNAL]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>319</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.OVERRIDE</Name>
			<Type Pointer="1">WORD</Type>
			<Comment>
				<![CDATA[D:	Überschreibgrund
							GB:	Override-reason 			
							E:	Elemento de dato de "motivo override 
							F:	Index de la "motivation de override" (surinscription)]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>321</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.DB_A</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	DB des BDE-Systems
							GB:	Data Block of DCS-system			
							E:	DB del sistema ADP					
							F:	Bloc du système d'acquisition de données]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>325</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB196_DATA_COLLECTION.DB_V</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D: Visualisierungs DB
							GB:	Data Block from Visualisation			
							E:  	DB de visualización					
							F:	Bloc de visualisation]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>329</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB220_ADD32BIT.ZWI</Name>
			<Type>DWORD</Type>
			<IGroup>16448</IGroup>
			<IOffset>333</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB220_ADD32BIT.WERT</Name>
			<Type>WORD</Type>
			<Comment>
				<![CDATA[D: Wert, der addiert werden soll 
								GB: 	Value to be added 
								E:  	Valor a añadir 
								F:	Valeur à additionner]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>337</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB220_ADD32BIT.ENABLE</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: Nur bei HIGH wird Zähler um Wert erhöht			
								GB:  "High-level" --> counter is increased by "VALUE"
								E:  	Contador se incrementa por valor en caso de HIGH	
								F:	En cas de HIGH, le compteur s'incrémente d'une valeur]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>339</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB220_ADD32BIT.RESET</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D: RESET löscht den Zähler  
								GB: 	Reset clears the counter 
								E: 	RESET pone el contador a cero  
								F:	RESET efface le compteur]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>340</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB220_ADD32BIT.DW1</Name>
			<Type Pointer="1">WORD</Type>
			<Comment>
				<![CDATA[D: Niederwertiges Datenwort
								GB: 	Less significant word		
								E: 	Dato elemental menos significativo de 32 bits 
								F:	Mot de données moins significatif]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>341</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB220_ADD32BIT.DW2</Name>
			<Type Pointer="1">WORD</Type>
			<Comment>
				<![CDATA[D: Höherwertiges Datenwort
								GB: 	Significant word		
								E: 	Dato elemental significativo de 32 bits 
								F:	Mot de données significatif]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>345</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB24_STAT_V2000.POINT</Name>
			<Type Pointer="1">BYTE</Type>
			<IGroup>16448</IGroup>
			<IOffset>365</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1" TaskPrio="2">S_FB24_STAT_V2000.MAX_ADRESS</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>369</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name Constant="1" IsDefinedInLibrary="1" TaskPrio="2">S_FB24_STAT_V2000.MAX_MEM</Name>
			<Type>INT</Type>
			<IGroup>16448</IGroup>
			<IOffset>371</IOffset>
			<BitSize>16</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB24_STAT_V2000.ENABLE</Name>
			<Type>BOOL</Type>
			<Comment>
				<![CDATA[D:	Status aktiv	
								GB:	Enable status mode	
								E:	Estado activo					
								F:	état actif]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>373</IOffset>
			<BitSize>8</BitSize>
		</Symbol>
		<Symbol>
			<Name IsDefinedInLibrary="1" TaskPrio="2">S_FB24_STAT_V2000.DB</Name>
			<Type Decoration="2001024D" Pointer="1">ARRAY [0..255] OF WORD</Type>
			<Comment>
				<![CDATA[D:	Datenbaustein mit Parametern
								GB:	Block for data-exchange 
								E:	Bloque de datos con parámetros	
								F:	Bloc de données avec paramètres]]>
			</Comment>
			<IGroup>16448</IGroup>
			<IOffset>374</IOffset>
			<BitSize>32</BitSize>
		</Symbol>
	</Symbols>
	<VarConfigs/>
</PlcProjectInfo>