{"text_format":"3","workbook":"xls","n_sheets":128,"sheets":["CommonDirect","Standard","StandardAllgemein","ProfiBus_Standard","FibreOptic_Standard","PC_Diagnostics","EtherCAT","PLCPresets","ManualMovement","Speed","X851_Speed","TimerCounter","PLCStatus","Cam","Heater","X350_GlueJet","X350_GlueJet_3","X355_GlueJet","X400_GlueJet","X401_GlueJet","X401_GlueJetCoupon","X407_GlueJet","X407_GlueJetLabel","X407_GlueJet_LongSeal","X407_GlueJet_LongSeal1","X407_GlueJetPaper","X409_GlueJet","X409_GlueJetBOW","X409_GlueJetBOWDB","X409_GlueJetJumbo","X409_GlueJetJumboMax","X409_GlueJetPaper","X411_GlueJetBOW","X411_GlueJetPaper","X550_GlueJet","X550_GlueJet_3","X550_GlueJet_PacketTrack","X700_GlueJet","X700_GlueJet_3","X701_GlueJet","X701_GlueJet_3","X707_GlueJet_LongSeal1","X707_GlueJetLabel","X725_GlueJet","X726_GlueJet","X751_GlueJet","X751_GlueJetOnsert","X752_GlueJet","X778_GlueJet","X778_GlueJetPaper","X778_GlueJetPaperMax4","X779_GlueJet","X779_GlueJetPaper","X779_GlueJetLabel","Manometer","ManometerExt","Servo","DiagnosticRegister","ParcelDimensions","SpeedDependentParameter","LooseEndDetector","Weigher","Bobbin","Bobbin4x","Parameters32","407_GlueJetPaperMax4","CasePackerParameter","CasePackerParameter2","HeaterSpecial","Heater48","HeaterImpulse","Functions_Palletizer","Palletizer_TargetPos","TaxStampMonitoring","TaxStampMonitoring2","DCS_MainPicture","ServicePresets","CamExt","PLCPresetsExt","ManualMovementExt","OnsertMonitoring2","Register","MaterialMechanism","IO-Link","HotMeltTank","StampInspection","StampInspectionBoxer","TopFold","FPI","Frequenzumrichter","ClosureStampInspection","LED_Diag","LED_Diag_Sensitiv","X520_MainPicture","ConveyorSensor","PortalPallet","ABSPalletSettings","LooseEndCalibrate","WeigherFormat","251_13_MainPicture","251_13_24_MainPicture","WeigherTobaccoBlock","ConveyorTimer","WeigherHistogram","PortalParameter","BobDepalSettings","X545_MainPicture","X794_MainPicture","X930_ScanCode","ServiceIntervalDisplay","PortalAGV","ServoRes","BucketChain","DCS_Trend","leer (3)","MaterialChange","RecipeManagement","MaterialChangeStep","StepSequence","Sonder RJR 531","Sonder RJR","Sonder Countdown","ReserviertFürSPS","Printer001","Printer002","Printer003","Printer004","Beispiel"],"not_rendered":{"macros":1,"external_links":1,"defined_names":349},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CommonDirect","index":0,"n_rows":28,"n_cols":4,"rows_kept":28,"flags":["formulas_cached_only"]}
["CommonDirect","MASCHINENABHAENGIG"]
["CommonDirect A1","Description of","Main","Print view"]
["CommonDirect A2","Interface Allocation","Overview","Normal view"]
["CommonDirect A3","concerning Visualisation","CommonDirect C3","CommonDirect D3"]
["CommonDirect A4","Machine","CommonDirect C4","CommonDirect D4"]
["CommonDirect A5","CommonDirect B5","CommonDirect C5","CommonDirect D5"]
["CommonDirect A6","CommonDirect B6","CommonDirect C6","CommonDirect D6"]
["CommonDirect A7","CommonDirect B7","CommonDirect C7","CommonDirect D7"]
["CommonDirect A8","CommonDirect B8","CommonDirect C8","CommonDirect D8"]
["CommonDirect A9","CommonDirect B9","CommonDirect C9","CommonDirect D9"]
["CommonDirect A10","CommonDirect B10","CommonDirect C10","CommonDirect D10"]
["CommonDirect A11","CommonDirect B11","CommonDirect C11","CommonDirect D11"]
["CommonDirect A12","CommonDirect B12","CommonDirect C12","CommonDirect D12"]
["CommonDirect A13","CommonDirect B13","CommonDirect C13","CommonDirect D13"]
["CommonDirect A14","CommonDirect B14","CommonDirect C14","CommonDirect D14"]
["CommonDirect A15","CommonDirect B15","CommonDirect C15","CommonDirect D15"]
["CommonDirect A16","CommonDirect B16","CommonDirect C16","CommonDirect D16"]
["CommonDirect A17","CommonDirect B17","CommonDirect C17","CommonDirect D17"]
["CommonDirect A18","CommonDirect B18","CommonDirect C18","CommonDirect D18"]
["CommonDirect A19","CommonDirect B19","CommonDirect C19","CommonDirect D19"]
["CommonDirect A20","CommonDirect B20","CommonDirect C20","CommonDirect D20"]
["CommonDirect A21","CommonDirect B21","CommonDirect C21","CommonDirect D21"]
["CommonDirect A22","CommonDirect B22","CommonDirect C22","CommonDirect D22"]
["CommonDirect A23","CommonDirect B23","CommonDirect C23","CommonDirect D23"]
["CommonDirect A24","CommonDirect B24","CommonDirect C24","CommonDirect D24"]
["CommonDirect A25","CommonDirect B25","CommonDirect C25","CommonDirect D25"]
["CommonDirect A26","CommonDirect B26","CommonDirect C26","CommonDirect D26"]
["CommonDirect A27","CommonDirect B27","CommonDirect C27","CommonDirect D27"]

{"sheet":"Standard","index":1,"n_rows":820,"n_cols":7,"rows_kept":820,"flags":["formulas_cached_only"]}
["Standard","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 0-24","Cyclic Process Data"]
[41,"DB 0-4","Cyclic Process Data 1st Machine"]
[41,"DB 0 ","Cyclic Process Data 1st Machine Reject event counter"]
[42,null,"DW 000–015","Reject event counter1-16"]
[42,null,"DW 016","16 Bits for „rejection has taken place“"]
[42,null,"DW 017-032","Reject event counter17-32"]
[42,null,"DW 033","16 Bits for „rejection has taken place“"]
[42,null,"DW 034–049","Reject event counter33-48"]
[42,null,"DW 050","16 Bits for „rejection has taken place“"]
[41,"DB 1 ","Cyclic Process Data 1st Machine Warnings"]
[42,null,"DW 000-002","standard icons"]
[42,null,"DW 003","machine icons"]
[42,null,"DW 004","graphic"]
[42,null,"DW 005","reserve text"]
[42,null,"DW 006-015","supplementary aggregates (are represented by an arrow)"]
[41,"DB 2 ","Cyclic Process Data 1st Machine Faults"]
[42,null,"DW 000","first-up fault "]
[42,null,"DW 001","first-up fault, DCS"]
[42,null,"DW 010-025","bitmap for faults "]
[42,null,"DW 255","Pause word for DCS"]
[41,"DB 3 ","Common Cyclic Processdata 1st Machine"]
[42,null,"DD 000-028","32 bit material counter"]
[42,null,"DD 060-068","32 bit measured values"]
[42,null,"DW 070-150","Miscellaneous"]
[42,null,"DW 150","PC -> PLC"]
["###IF MITAUSWURFZAEHLERN###41","DB 4","Cyclic Process Data 1st Machine Reject counter"]
["###IF MITAUSWURFZAEHLERN###42",null,"DW 000","16 Bits for „reject exists“"]
["###IF MITAUSWURFZAEHLERN###42",null,"DW 001","16 Bits for „rejection has taken place“"]
["###IF MITAUSWURFZAEHLERN###42",null,"DD 008–038","Reject counter 1-16"]
["###IF MITAUSWURFZAEHLERN###42",null,"DW 040","16 Bits for „reject exists“"]
["###IF MITAUSWURFZAEHLERN###42",null,"DW 041","16 Bits for „rejection has taken place“"]
["###IF MITAUSWURFZAEHLERN###42",null,"DD 048–078","Reject event counter 17-32"]
["###IF MITAUSWURFZAEHLERN###42",null,"DW 080","16 Bits for „reject exists“"]
["###IF MITAUSWURFZAEHLERN###42",null,"DW 081","16 Bits for „rejection has taken place“"]
["###IF MITAUSWURFZAEHLERN###42",null,"DD 088–118","Reject counter 33-48"]
[41,"DB 5-9","Cyclic Process Data 2nd Machine"]
[41,"DB 10-14","Cyclic Process Data 3rd Machine"]
[41,"DB 15-19","Cyclic Process Data 4th Machine"]
[41,"DB 20-24","Cyclic Process Data 5th Machine"]
[1,"###MAIN"]
[1,"Common Process Data ###MNR"]
[21,"DB ###ADDR:0+5[MNR]+10[PLC]:ADDR","Reject Events ###MNR"]
[41,"DW 0",null,"Reject event 1 ","Rejects.###MNR.1","###INDEX:Rejects.###MNR.1:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_01>[W]{p}"]
[41,"DW 1",null,"Reject event  2","Rejects.###MNR.2","###INDEX:Rejects.###MNR.2:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_02>[W]{p}"]
[41,"DW 2",null,"Reject event 3","Rejects.###MNR.3","###INDEX:Rejects.###MNR.3:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_03>[W]{p}"]
[41,"DW 3",null,"Reject event 4","Rejects.###MNR.4","###INDEX:Rejects.###MNR.4:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_04>[W]{p}"]
[41,"DW 4",null,"Reject event 5","Rejects.###MNR.5","###INDEX:Rejects.###MNR.5:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_05>[W]{p}"]
[41,"DW 5",null,"Reject event 6","Rejects.###MNR.6","###INDEX:Rejects.###MNR.6:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_06>[W]{p}"]
[41,"DW 6",null,"Reject event 7","Rejects.###MNR.7","###INDEX:Rejects.###MNR.7:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_07>[W]{p}"]
[41,"DW 7",null,"Reject event 8","Rejects.###MNR.8","###INDEX:Rejects.###MNR.8:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_08>[W]{p}"]
[41,"DW 8 ",null,"Reject event 9","Rejects.###MNR.9","###INDEX:Rejects.###MNR.9:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_09>[W]{p}"]
[41,"DW 9",null,"Reject event 10","Rejects.###MNR.10 ","###INDEX:Rejects.###MNR.10:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_10>[W]{p}"]
[41,"DW 10",null,"Reject event 11","Rejects.###MNR.11","###INDEX:Rejects.###MNR.11:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_11>[W]{p}"]
[41,"DW 11",null,"Reject event 12","Rejects.###MNR.12","###INDEX:Rejects.###MNR.12:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_12>[W]{p}"]
[41,"DW 12",null,"Reject event 13","Rejects.###MNR.13","###INDEX:Rejects.###MNR.13:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_13>[W]{p}"]
[41,"DW 13",null,"Reject event 14","Rejects.###MNR.14","###INDEX:Rejects.###MNR.14:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_14>[W]{p}"]
[41,"DW 14",null,"Reject event 15","Rejects.###MNR.15","###INDEX:Rejects.###MNR.15:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_15>[W]{p}"]
[41,"DW 15",null,"Reject event 16","Rejects.###MNR.16","###INDEX:Rejects.###MNR.16:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_16>[W]{p}"]
[41,"DW 16","Bit 0-16","Reject event 1-16 has taken place ",null,null,"Ch1.###MNR_T_auswurf<.m###MNR_ausw_statt_1>[W]{p}"]
[41,"DW 17",null,"Reject event 17","Rejects.###MNR.17","###INDEX:Rejects.###MNR.17:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_17>[W]{p}"]
[41,"DW 18",null,"Reject event 18","Rejects.###MNR.18","###INDEX:Rejects.###MNR.18:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_18>[W]{p}"]
[41,"DW 19",null,"Reject event 19","Rejects.###MNR.19","###INDEX:Rejects.###MNR.19:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_19>[W]{p}"]
[41,"DW 20",null,"Reject event 20","Rejects.###MNR.20","###INDEX:Rejects.###MNR.20:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_20>[W]{p}"]
[41,"DW 21",null,"Reject event 21","Rejects.###MNR.21","###INDEX:Rejects.###MNR.21:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_21>[W]{p}"]
[41,"DW 22",null,"Reject event 22","Rejects.###MNR.22","###INDEX:Rejects.###MNR.22:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_22>[W]{p}"]
[41,"DW 23",null,"Reject event 23","Rejects.###MNR.23","###INDEX:Rejects.###MNR.23:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_23>[W]{p}"]
[41,"DW 24",null,"Reject event 24","Rejects.###MNR.24","###INDEX:Rejects.###MNR.24:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_24>[W]{p}"]
[41,"DW 25",null,"Reject event 25","Rejects.###MNR.25","###INDEX:Rejects.###MNR.25:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_25>[W]{p}"]
[41,"DW 26",null,"Reject event 26","Rejects.###MNR.26","###INDEX:Rejects.###MNR.26:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_26>[W]{p}"]
[41,"DW 27",null,"Reject event 27","Rejects.###MNR.27","###INDEX:Rejects.###MNR.27:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_27>[W]{p}"]
[41,"DW 28",null,"Reject event 28","Rejects.###MNR.28","###INDEX:Rejects.###MNR.28:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_28>[W]{p}"]
[41,"DW 39",null,"Reject event 29","Rejects.###MNR.29","###INDEX:Rejects.###MNR.29:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_29>[W]{p}"]
[41,"DW 30",null,"Reject event 30","Rejects.###MNR.30","###INDEX:Rejects.###MNR.30:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_30>[W]{p}"]
[41,"DW 31",null,"Reject event 31","Rejects.###MNR.31","###INDEX:Rejects.###MNR.31:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_31>[W]{p}"]
[41,"DW 32",null,"Reject event 32","Rejects.###MNR.32","###INDEX:Rejects.###MNR.32:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_32>[W]{p}"]
[41,"DW 33","Bit 0-16","Reject event 17-32 has taken place",null,null,"Ch1.###MNR_T_auswurf<.m###MNR_ausw_statt_2>[W]{p}"]
[41,"DW 34",null,"Reject event 33","Rejects.###MNR.33","###INDEX:Rejects.###MNR.33:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_33>[W]{p}"]
[41,"DW 35",null,"Reject event 34","Rejects.###MNR.34","###INDEX:Rejects.###MNR.34:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_34>[W]{p}"]
[41,"DW 36",null,"Reject event 35","Rejects.###MNR.35","###INDEX:Rejects.###MNR.35:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_35>[W]{p}"]
[41,"DW 37",null,"Reject event 36","Rejects.###MNR.36","###INDEX:Rejects.###MNR.36:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_36>[W]{p}"]
[41,"DW 38",null,"Reject event 37","Rejects.###MNR.37","###INDEX:Rejects.###MNR.37:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_37>[W]{p}"]
[41,"DW 39",null,"Reject event 38","Rejects.###MNR.38","###INDEX:Rejects.###MNR.38:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_38>[W]{p}"]
[41,"DW 40",null,"Reject event 39","Rejects.###MNR.39","###INDEX:Rejects.###MNR.39:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_39>[W]{p}"]
[41,"DW 41",null,"Reject event 40","Rejects.###MNR.40","###INDEX:Rejects.###MNR.40:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_40>[W]{p}"]
[41,"DW 42",null,"Reject event 41","Rejects.###MNR.41","###INDEX:Rejects.###MNR.41:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_41>[W]{p}"]
[41,"DW 43",null,"Reject event 42","Rejects.###MNR.42","###INDEX:Rejects.###MNR.42:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_42>[W]{p}"]
[41,"DW 44",null,"Reject event 43","Rejects.###MNR.43","###INDEX:Rejects.###MNR.43:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_43>[W]{p}"]
[41,"DW 45",null,"Reject event 44","Rejects.###MNR.44","###INDEX:Rejects.###MNR.44:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_44>[W]{p}"]
[41,"DW 46",null,"Reject event 45","Rejects.###MNR.45","###INDEX:Rejects.###MNR.45:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_45>[W]{p}"]
[41,"DW 47",null,"Reject event 46","Rejects.###MNR.46","###INDEX:Rejects.###MNR.46:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_46>[W]{p}"]
[41,"DW 48",null,"Reject event 47","Rejects.###MNR.47","###INDEX:Rejects.###MNR.47:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_47>[W]{p}"]
[41,"DW 49",null,"Reject event 48","Rejects.###MNR.48","###INDEX:Rejects.###MNR.48:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_48>[W]{p}"]
[41,"DW 50","Bit 0-16","Reject event 33-48 has taken place",null,null,"Ch1.###MNR_T_auswurf<.m###MNR_ausw_statt_3>[W]{p}"]
[41,"###SDR[REJ]"]
[41,"DW ###ADDR:35+16[FREJ]:ADDR",null,"Reject event ###ADDR:33+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:33+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:33+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:33+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:36+16[FREJ]:ADDR",null,"Reject event ###ADDR:34+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:34+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:34+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:34+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:37+16[FREJ]:ADDR",null,"Reject event ###ADDR:35+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:35+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:35+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:35+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:38+16[FREJ]:ADDR",null,"Reject event ###ADDR:36+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:36+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:36+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:36+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:39+16[FREJ]:ADDR",null,"Reject event ###ADDR:37+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:37+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:37+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:37+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:41+16[FREJ]:ADDR",null,"Reject event ###ADDR:38+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:38+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:38+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:38+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:42+16[FREJ]:ADDR",null,"Reject event ###ADDR:39+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:39+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:39+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:39+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:43+16[FREJ]:ADDR",null,"Reject event ###ADDR:40+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:40+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:40+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:40+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:44+16[FREJ]:ADDR",null,"Reject event ###ADDR:41+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:41+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:41+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:41+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:45+16[FREJ]:ADDR",null,"Reject event ###ADDR:42+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:42+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:42+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:42+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:46+16[FREJ]:ADDR",null,"Reject event ###ADDR:43+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:43+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:43+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:43+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:47+16[FREJ]:ADDR",null,"Reject event ###ADDR:44+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:44+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:44+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:44+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:48+16[FREJ]:ADDR",null,"Reject event ###ADDR:45+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:45+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:45+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:45+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:49+16[FREJ]:ADDR",null,"Reject event ###ADDR:46+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:46+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:46+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:46+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:50+16[FREJ]:ADDR",null,"Reject event ###ADDR:47+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:47+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:47+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:47+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:51+16[FREJ]:ADDR",null,"Reject event ###ADDR:48+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:48+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:48+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurf<.m###MNR_ausw_###ADDR:48+16[FREJ]:ADDR>[W]{p}"]
[41,"DW ###ADDR:52+16[FREJ]:ADDR","Bit 0-16","Reject event ###ADDR:33+16[FREJ]:ADDR - ###ADDR:48+16[FREJ]:ADDR has taken place",null,null,"Ch1.###MNR_T_auswurf<.m###MNR_ausw_statt_###ADDR:3+1[FREJ]:ADDR>[W]{p}"]
[41,"###EDR[REJ]"]
[21,"DB ###ADDR:1+5[MNR]+10[PLC]:ADDR","Warnings ###MNR"]
[4,"Warnings as Standard Symbols"]
[41,"DW 0","Bit  0","Warning 1","Warnings.###MNR.1","###INDEX:Warnings.###MNR.1:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_01>[W]{p}"]
[41,null,"Bit  1","Warning 2","Warnings.###MNR.2","###INDEX:Warnings.###MNR.2:INDEX"]
[41,null,"Bit  2","Warning 3","Warnings.###MNR.3","###INDEX:Warnings.###MNR.3:INDEX"]
[41,null,"Bit  3","Warning 4","Warnings.###MNR.4","###INDEX:Warnings.###MNR.4:INDEX"]
[41,null,"Bit  4","Warning 5","Warnings.###MNR.5","###INDEX:Warnings.###MNR.5:INDEX"]
[41,null,"Bit  5","Warning 6","Warnings.###MNR.6","###INDEX:Warnings.###MNR.6:INDEX"]
[41,null,"Bit  6","Warning 7","Warnings.###MNR.7","###INDEX:Warnings.###MNR.7:INDEX"]
[41,null,"Bit  7","Warning 8","Warnings.###MNR.8","###INDEX:Warnings.###MNR.8:INDEX"]
[41,null,"Bit  8","Warning 9","Warnings.###MNR.9","###INDEX:Warnings.###MNR.9:INDEX"]
[41,null,"Bit  9","Warning 10","Warnings.###MNR.10","###INDEX:Warnings.###MNR.10:INDEX"]
[41,null,"Bit  10","Warning 11","Warnings.###MNR.11","###INDEX:Warnings.###MNR.11:INDEX"]
[41,null,"Bit  11","Warning 12","Warnings.###MNR.12","###INDEX:Warnings.###MNR.12:INDEX"]
[41,null,"Bit  12","Warning 13","Warnings.###MNR.13","###INDEX:Warnings.###MNR.13:INDEX"]
[41,null,"Bit  13","Warning 14","Warnings.###MNR.14","###INDEX:Warnings.###MNR.14:INDEX"]
[41,null,"Bit  14","Warning 15","Warnings.###MNR.15","###INDEX:Warnings.###MNR.15:INDEX"]
[41,null,"Bit  15","Warning 16","Warnings.###MNR.16","###INDEX:Warnings.###MNR.16:INDEX"]
[41,"DW 1","Bit  0","Warning 17","Warnings.###MNR.17","###INDEX:Warnings.###MNR.17:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_02>[W]{p}"]
[41,null,"Bit  1","Warning 18","Warnings.###MNR.18","###INDEX:Warnings.###MNR.18:INDEX"]
[41,null,"Bit  2","Warning 19","Warnings.###MNR.19","###INDEX:Warnings.###MNR.19:INDEX"]
[41,null,"Bit  3","Warning 20","Warnings.###MNR.20","###INDEX:Warnings.###MNR.20:INDEX"]
[41,null,"Bit  4","Warning 21","Warnings.###MNR.21","###INDEX:Warnings.###MNR.21:INDEX"]
[41,null,"Bit  5","Warning 22","Warnings.###MNR.22","###INDEX:Warnings.###MNR.22:INDEX"]
[41,null,"Bit  6","Warning 23","Warnings.###MNR.23","###INDEX:Warnings.###MNR.23:INDEX"]
[41,null,"Bit  7","Warning 24","Warnings.###MNR.24","###INDEX:Warnings.###MNR.24:INDEX"]
[41,null,"Bit  8","Warning 25","Warnings.###MNR.25","###INDEX:Warnings.###MNR.25:INDEX"]
[41,null,"Bit  9","Warning 26","Warnings.###MNR.26","###INDEX:Warnings.###MNR.26:INDEX"]
[41,null,"Bit  10","Warning 27","Warnings.###MNR.27","###INDEX:Warnings.###MNR.27:INDEX"]
[41,null,"Bit  11","Warning 28","Warnings.###MNR.28","###INDEX:Warnings.###MNR.28:INDEX"]
[41,null,"Bit  12","Warning 29","Warnings.###MNR.29","###INDEX:Warnings.###MNR.29:INDEX"]
[41,null,"Bit  13","Warning 30","Warnings.###MNR.30","###INDEX:Warnings.###MNR.30:INDEX"]
[41,null,"Bit  14","Warning 31","Warnings.###MNR.31","###INDEX:Warnings.###MNR.31:INDEX"]
[41,null,"Bit  15","Warning 32","Warnings.###MNR.32","###INDEX:Warnings.###MNR.32:INDEX"]
[41,"DW 2","Bit  0","Warning 33","Warnings.###MNR.33","###INDEX:Warnings.###MNR.33:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_03>[W]{p}"]
[41,null,"Bit  1","Warning 34","Warnings.###MNR.34","###INDEX:Warnings.###MNR.34:INDEX"]
[41,null,"Bit  2","Warning 35","Warnings.###MNR.35","###INDEX:Warnings.###MNR.35:INDEX"]
[41,null,"Bit  3","Warning 36","Warnings.###MNR.36","###INDEX:Warnings.###MNR.36:INDEX"]
[41,null,"Bit  4","Warning 37","Warnings.###MNR.37","###INDEX:Warnings.###MNR.37:INDEX"]
[41,null,"Bit  5","Warning 38","Warnings.###MNR.38","###INDEX:Warnings.###MNR.38:INDEX"]
[41,null,"Bit  6","Warning 39","Warnings.###MNR.39","###INDEX:Warnings.###MNR.39:INDEX"]
[41,null,"Bit  7","Warning 40","Warnings.###MNR.40","###INDEX:Warnings.###MNR.40:INDEX"]
[41,null,"Bit  8","Warning 41","Warnings.###MNR.41","###INDEX:Warnings.###MNR.41:INDEX"]
[41,null,"Bit  9","Warning 42","Warnings.###MNR.42","###INDEX:Warnings.###MNR.42:INDEX"]
[41,null,"Bit  10","Warning 43","Warnings.###MNR.43","###INDEX:Warnings.###MNR.43:INDEX"]
[41,null,"Bit  11","Warning 44","Warnings.###MNR.44","###INDEX:Warnings.###MNR.44:INDEX"]
[41,null,"Bit  12","Warning 45","Warnings.###MNR.45","###INDEX:Warnings.###MNR.45:INDEX"]
[41,null,"Bit  13","Warning 46","Warnings.###MNR.46","###INDEX:Warnings.###MNR.46:INDEX"]
[41,null,"Bit  14","Warning 47","Warnings.###MNR.47","###INDEX:Warnings.###MNR.47:INDEX"]
[41,null,"Bit  15","Warning 48","Warnings.###MNR.48","###INDEX:Warnings.###MNR.48:INDEX"]
[4,"Warnings as Machine-Symbols"]
[41,"DW 3","Bit  0","Warning 49","Warnings.###MNR.49","###INDEX:Warnings.###MNR.49:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_04>[W]{p}"]
[41,null,"Bit  1","Warning 50","Warnings.###MNR.50","###INDEX:Warnings.###MNR.50:INDEX"]
[41,null,"Bit  2","Warning 51","Warnings.###MNR.51","###INDEX:Warnings.###MNR.51:INDEX"]
[41,null,"Bit  3","Warning 52","Warnings.###MNR.52","###INDEX:Warnings.###MNR.52:INDEX"]
[41,null,"Bit  4","Warning 53","Warnings.###MNR.53","###INDEX:Warnings.###MNR.53:INDEX"]
[41,null,"Bit  5","Warning 54","Warnings.###MNR.54","###INDEX:Warnings.###MNR.54:INDEX"]
[41,null,"Bit  6","Warning 55","Warnings.###MNR.55","###INDEX:Warnings.###MNR.55:INDEX"]
[41,null,"Bit  7","Warning 56","Warnings.###MNR.56","###INDEX:Warnings.###MNR.56:INDEX"]
[41,null,"Bit  8","Warning 57","Warnings.###MNR.57","###INDEX:Warnings.###MNR.57:INDEX"]
[41,null,"Bit  9","Warning 58","Warnings.###MNR.58","###INDEX:Warnings.###MNR.58:INDEX"]
[41,null,"Bit  10","Warning 59","Warnings.###MNR.59","###INDEX:Warnings.###MNR.59:INDEX"]
[41,null,"Bit  11","Warning 60","Warnings.###MNR.60","###INDEX:Warnings.###MNR.60:INDEX"]
[41,null,"Bit  12","Warning 61","Warnings.###MNR.61","###INDEX:Warnings.###MNR.61:INDEX"]
[41,null,"Bit  13","Warning 62","Warnings.###MNR.62","###INDEX:Warnings.###MNR.62:INDEX"]
[41,null,"Bit  14","Warning 63","Warnings.###MNR.63","###INDEX:Warnings.###MNR.63:INDEX"]
[41,null,"Bit  15","Warning 64","Warnings.###MNR.64","###INDEX:Warnings.###MNR.64:INDEX"]
[4,"Warnings as Graphic"]
[41,"DW 4","Bit  0","Warning 65","Warnings.###MNR.65","###INDEX:Warnings.###MNR.65:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_05>[W]{p}"]
[41,null,"Bit  1","Warning 66","Warnings.###MNR.66","###INDEX:Warnings.###MNR.66:INDEX"]
[41,null,"Bit  2","Warning 67","Warnings.###MNR.67","###INDEX:Warnings.###MNR.67:INDEX"]
[41,null,"Bit  3","Warning 68","Warnings.###MNR.68","###INDEX:Warnings.###MNR.68:INDEX"]
[41,null,"Bit  4","Warning 69","Warnings.###MNR.69","###INDEX:Warnings.###MNR.69:INDEX"]
[41,null,"Bit  5","Warning 70","Warnings.###MNR.70","###INDEX:Warnings.###MNR.70:INDEX"]
[41,null,"Bit  6","Warning 71","Warnings.###MNR.71","###INDEX:Warnings.###MNR.71:INDEX"]
[41,null,"Bit  7","Warning 72","Warnings.###MNR.72","###INDEX:Warnings.###MNR.72:INDEX"]
[41,null,"Bit  8","Warning 73","Warnings.###MNR.73","###INDEX:Warnings.###MNR.73:INDEX"]
[41,null,"Bit  9","Warning 74","Warnings.###MNR.74","###INDEX:Warnings.###MNR.74:INDEX"]
[41,null,"Bit  10","Warning 75","Warnings.###MNR.75","###INDEX:Warnings.###MNR.75:INDEX"]
[41,null,"Bit  11","Warning 76","Warnings.###MNR.76","###INDEX:Warnings.###MNR.76:INDEX"]
[41,null,"Bit  12","Warning 77","Warnings.###MNR.77","###INDEX:Warnings.###MNR.77:INDEX"]
[41,null,"Bit  13","Warning 78","Warnings.###MNR.78","###INDEX:Warnings.###MNR.78:INDEX"]
[41,null,"Bit  14","Warning 79","Warnings.###MNR.79","###INDEX:Warnings.###MNR.79:INDEX"]
[41,null,"Bit  15","Warning 80","Warnings.###MNR.80","###INDEX:Warnings.###MNR.80:INDEX"]
[4,"Warnings as Reserved-Text"]
[41,"DW 5","Bit  0","Warning 81","Warnings.###MNR.81","###INDEX:Warnings.###MNR.81:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_06>[W]{p}"]
[41,null,"Bit  1","Warning 82","Warnings.###MNR.82","###INDEX:Warnings.###MNR.82:INDEX"]
[41,null,"Bit  2","Warning 83","Warnings.###MNR.83","###INDEX:Warnings.###MNR.83:INDEX"]
[41,null,"Bit  3","Warning 84","Warnings.###MNR.84","###INDEX:Warnings.###MNR.84:INDEX"]
[41,null,"Bit  4","Warning 85","Warnings.###MNR.85","###INDEX:Warnings.###MNR.85:INDEX"]
[41,null,"Bit  5","Warning 86","Warnings.###MNR.86","###INDEX:Warnings.###MNR.86:INDEX"]
[41,null,"Bit  6","Warning 87","Warnings.###MNR.87","###INDEX:Warnings.###MNR.87:INDEX"]
[41,null,"Bit  7","Warning 88","Warnings.###MNR.88","###INDEX:Warnings.###MNR.88:INDEX"]
[41,null,"Bit  8","Warning 89","Warnings.###MNR.89","###INDEX:Warnings.###MNR.89:INDEX"]
[41,null,"Bit  9","Warning 90","Warnings.###MNR.90","###INDEX:Warnings.###MNR.90:INDEX"]
[41,null,"Bit  10","Warning 91","Warnings.###MNR.91","###INDEX:Warnings.###MNR.91:INDEX"]
[41,null,"Bit  11","Warning 92","Warnings.###MNR.92","###INDEX:Warnings.###MNR.92:INDEX"]
[41,null,"Bit  12","Warning 93","Warnings.###MNR.93","###INDEX:Warnings.###MNR.93:INDEX"]
[41,null,"Bit  13","Warning 94","Warnings.###MNR.94","###INDEX:Warnings.###MNR.94:INDEX"]
[41,null,"Bit  14","Warning 95","Warnings.###MNR.95","###INDEX:Warnings.###MNR.95:INDEX"]
[41,null,"Bit  15","Warning 96","Warnings.###MNR.96","###INDEX:Warnings.###MNR.96:INDEX"]
[4,"Warnings for Supplement Aggregates (Arrows)"]
[41,"DW 6","Bit  0","Warning 97","Warnings.###MNR.97","###INDEX:Warnings.###MNR.97:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_07>[W]{p}"]
[41,null,"Bit  1","Warning 98","Warnings.###MNR.98","###INDEX:Warnings.###MNR.98:INDEX"]
[41,null,"Bit  2","Warning 99","Warnings.###MNR.99","###INDEX:Warnings.###MNR.99:INDEX"]
[41,null,"Bit  3","Warning 100","Warnings.###MNR.100","###INDEX:Warnings.###MNR.100:INDEX"]
[41,null,"Bit  4","Warning 101","Warnings.###MNR.101","###INDEX:Warnings.###MNR.101:INDEX"]
[41,null,"Bit  5","Warning 102","Warnings.###MNR.102","###INDEX:Warnings.###MNR.102:INDEX"]
[41,null,"Bit  6","Warning 103","Warnings.###MNR.103","###INDEX:Warnings.###MNR.103:INDEX"]
[41,null,"Bit  7","Warning 104","Warnings.###MNR.104","###INDEX:Warnings.###MNR.104:INDEX"]
[41,null,"Bit  8","Warning 105","Warnings.###MNR.105","###INDEX:Warnings.###MNR.105:INDEX"]
[41,null,"Bit  9","Warning 106","Warnings.###MNR.106","###INDEX:Warnings.###MNR.106:INDEX"]
[41,null,"Bit  10","Warning 107","Warnings.###MNR.107","###INDEX:Warnings.###MNR.107:INDEX"]
[41,null,"Bit  11","Warning 108","Warnings.###MNR.108","###INDEX:Warnings.###MNR.108:INDEX"]
[41,null,"Bit  12","Warning 109","Warnings.###MNR.109","###INDEX:Warnings.###MNR.109:INDEX"]
[41,null,"Bit  13","Warning 110","Warnings.###MNR.110","###INDEX:Warnings.###MNR.110:INDEX"]
[41,null,"Bit  14","Warning 111","Warnings.###MNR.111","###INDEX:Warnings.###MNR.111:INDEX"]
[41,null,"Bit  15","Warning 112","Warnings.###MNR.112","###INDEX:Warnings.###MNR.112:INDEX"]
[41,"DW 7","Bit  0","Warning 113","Warnings.###MNR.113","###INDEX:Warnings.###MNR.113:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_08>[W]{p}"]
[41,null,"Bit  1","Warning 114","Warnings.###MNR.114","###INDEX:Warnings.###MNR.114:INDEX"]
[41,null,"Bit  2","Warning 115","Warnings.###MNR.115","###INDEX:Warnings.###MNR.115:INDEX"]
[41,null,"Bit  3","Warning 116","Warnings.###MNR.116","###INDEX:Warnings.###MNR.116:INDEX"]
[41,null,"Bit  4","Warning 117","Warnings.###MNR.117","###INDEX:Warnings.###MNR.117:INDEX"]
[41,null,"Bit  5","Warning 118","Warnings.###MNR.118","###INDEX:Warnings.###MNR.118:INDEX"]
[41,null,"Bit  6","Warning 119","Warnings.###MNR.119","###INDEX:Warnings.###MNR.119:INDEX"]
[41,null,"Bit  7","Warning 120","Warnings.###MNR.120","###INDEX:Warnings.###MNR.120:INDEX"]
[41,null,"Bit  8","Warning 121","Warnings.###MNR.121","###INDEX:Warnings.###MNR.121:INDEX"]
[41,null,"Bit  9","Warning 122","Warnings.###MNR.122","###INDEX:Warnings.###MNR.122:INDEX"]
[41,null,"Bit  10","Warning 123","Warnings.###MNR.123","###INDEX:Warnings.###MNR.123:INDEX"]
[41,null,"Bit  11","Warning 124","Warnings.###MNR.124","###INDEX:Warnings.###MNR.124:INDEX"]
[41,null,"Bit  12","Warning 125","Warnings.###MNR.125","###INDEX:Warnings.###MNR.125:INDEX"]
[41,null,"Bit  13","Warning 126","Warnings.###MNR.126","###INDEX:Warnings.###MNR.126:INDEX"]
[41,null,"Bit  14","Warning 127","Warnings.###MNR.127","###INDEX:Warnings.###MNR.127:INDEX"]
[41,null,"Bit  15","Warning 128","Warnings.###MNR.128","###INDEX:Warnings.###MNR.128:INDEX"]
[41,"DW 8","Bit  0","Warning 129","Warnings.###MNR.129","###INDEX:Warnings.###MNR.129:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_09>[W]{p}"]
[41,null,"Bit  1","Warning 130","Warnings.###MNR.130","###INDEX:Warnings.###MNR.130:INDEX"]
[41,null,"Bit  2","Warning 131","Warnings.###MNR.131","###INDEX:Warnings.###MNR.131:INDEX"]
[41,null,"Bit  3","Warning 132","Warnings.###MNR.132","###INDEX:Warnings.###MNR.132:INDEX"]
[41,null,"Bit  4","Warning 133","Warnings.###MNR.133","###INDEX:Warnings.###MNR.133:INDEX"]
[41,null,"Bit  5","Warning 134","Warnings.###MNR.134","###INDEX:Warnings.###MNR.134:INDEX"]
[41,null,"Bit  6","Warning 135","Warnings.###MNR.135","###INDEX:Warnings.###MNR.135:INDEX"]
[41,null,"Bit  7","Warning 136","Warnings.###MNR.136","###INDEX:Warnings.###MNR.136:INDEX"]
[41,null,"Bit  8","Warning 137","Warnings.###MNR.137","###INDEX:Warnings.###MNR.137:INDEX"]
[41,null,"Bit  9","Warning 138","Warnings.###MNR.138","###INDEX:Warnings.###MNR.138:INDEX"]
[41,null,"Bit  10","Warning 139","Warnings.###MNR.139","###INDEX:Warnings.###MNR.139:INDEX"]
[41,null,"Bit  11","Warning 140","Warnings.###MNR.140","###INDEX:Warnings.###MNR.140:INDEX"]
[41,null,"Bit  12","Warning 141","Warnings.###MNR.141","###INDEX:Warnings.###MNR.141:INDEX"]
[41,null,"Bit  13","Warning 142","Warnings.###MNR.142","###INDEX:Warnings.###MNR.142:INDEX"]
[41,null,"Bit  14","Warning 143","Warnings.###MNR.143","###INDEX:Warnings.###MNR.143:INDEX"]
[41,null,"Bit  15","Warning 144","Warnings.###MNR.144","###INDEX:Warnings.###MNR.144:INDEX"]
[41,"DW 9","Bit  0","Warning 145","Warnings.###MNR.145","###INDEX:Warnings.###MNR.145:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_10>[W]{p}"]
[41,null,"Bit  1","Warning 146","Warnings.###MNR.146","###INDEX:Warnings.###MNR.146:INDEX"]
[41,null,"Bit  2","Warning 147","Warnings.###MNR.147","###INDEX:Warnings.###MNR.147:INDEX"]
[41,null,"Bit  3","Warning 148","Warnings.###MNR.148","###INDEX:Warnings.###MNR.148:INDEX"]
[41,null,"Bit  4","Warning 149","Warnings.###MNR.149","###INDEX:Warnings.###MNR.149:INDEX"]
[41,null,"Bit  5","Warning 150","Warnings.###MNR.150","###INDEX:Warnings.###MNR.150:INDEX"]
[41,null,"Bit  6","Warning 151","Warnings.###MNR.151","###INDEX:Warnings.###MNR.151:INDEX"]
[41,null,"Bit  7","Warning 152","Warnings.###MNR.152","###INDEX:Warnings.###MNR.152:INDEX"]
[41,null,"Bit  8","Warning 153","Warnings.###MNR.153","###INDEX:Warnings.###MNR.153:INDEX"]
[41,null,"Bit  9","Warning 154","Warnings.###MNR.154","###INDEX:Warnings.###MNR.154:INDEX"]
[41,null,"Bit  10","Warning 155","Warnings.###MNR.155","###INDEX:Warnings.###MNR.155:INDEX"]
[41,null,"Bit  11","Warning 156","Warnings.###MNR.156","###INDEX:Warnings.###MNR.156:INDEX"]
[41,null,"Bit  12","Warning 157","Warnings.###MNR.157","###INDEX:Warnings.###MNR.157:INDEX"]
[41,null,"Bit  13","Warning 158","Warnings.###MNR.158","###INDEX:Warnings.###MNR.158:INDEX"]
[41,null,"Bit  14","Warning 159","Warnings.###MNR.159","###INDEX:Warnings.###MNR.159:INDEX"]
[41,null,"Bit  15","Warning 160","Warnings.###MNR.160","###INDEX:Warnings.###MNR.160:INDEX"]
[41,"DW 10","Bit  0","Warning 161","Warnings.###MNR.161","###INDEX:Warnings.###MNR.161:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_11>[W]{p}"]
[41,null,"Bit  1","Warning 162","Warnings.###MNR.162","###INDEX:Warnings.###MNR.162:INDEX"]
[41,null,"Bit  2","Warning 163","Warnings.###MNR.163","###INDEX:Warnings.###MNR.163:INDEX"]
[41,null,"Bit  3","Warning 164","Warnings.###MNR.164","###INDEX:Warnings.###MNR.164:INDEX"]
[41,null,"Bit  4","Warning 165","Warnings.###MNR.165","###INDEX:Warnings.###MNR.165:INDEX"]
[41,null,"Bit  5","Warning 166","Warnings.###MNR.166","###INDEX:Warnings.###MNR.166:INDEX"]
[41,null,"Bit  6","Warning 167","Warnings.###MNR.167","###INDEX:Warnings.###MNR.167:INDEX"]
[41,null,"Bit  7","Warning 168","Warnings.###MNR.168","###INDEX:Warnings.###MNR.168:INDEX"]
[41,null,"Bit  8","Warning 169","Warnings.###MNR.169","###INDEX:Warnings.###MNR.169:INDEX"]
[41,null,"Bit  9","Warning 170","Warnings.###MNR.170","###INDEX:Warnings.###MNR.170:INDEX"]
[41,null,"Bit  10","Warning 171","Warnings.###MNR.171","###INDEX:Warnings.###MNR.171:INDEX"]
[41,null,"Bit  11","Warning 172","Warnings.###MNR.172","###INDEX:Warnings.###MNR.172:INDEX"]
[41,null,"Bit  12","Warning 173","Warnings.###MNR.173","###INDEX:Warnings.###MNR.173:INDEX"]
[41,null,"Bit  13","Warning 174","Warnings.###MNR.174","###INDEX:Warnings.###MNR.174:INDEX"]
[41,null,"Bit  14","Warning 175","Warnings.###MNR.175","###INDEX:Warnings.###MNR.175:INDEX"]
[41,null,"Bit  15","Warning 176","Warnings.###MNR.176","###INDEX:Warnings.###MNR.176:INDEX"]
[41,"DW 11","Bit  0","Warning 177","Warnings.###MNR.177","###INDEX:Warnings.###MNR.177:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_12>[W]{p}"]
[41,null,"Bit  1","Warning 178","Warnings.###MNR.178","###INDEX:Warnings.###MNR.178:INDEX"]
[41,null,"Bit  2","Warning 179","Warnings.###MNR.179","###INDEX:Warnings.###MNR.179:INDEX"]
[41,null,"Bit  3","Warning 180","Warnings.###MNR.180","###INDEX:Warnings.###MNR.180:INDEX"]
[41,null,"Bit  4","Warning 181","Warnings.###MNR.181","###INDEX:Warnings.###MNR.181:INDEX"]
[41,null,"Bit  5","Warning 182","Warnings.###MNR.182","###INDEX:Warnings.###MNR.182:INDEX"]
[41,null,"Bit  6","Warning 183","Warnings.###MNR.183","###INDEX:Warnings.###MNR.183:INDEX"]
[41,null,"Bit  7","Warning 184","Warnings.###MNR.184","###INDEX:Warnings.###MNR.184:INDEX"]
[41,null,"Bit  8","Warning 185","Warnings.###MNR.185","###INDEX:Warnings.###MNR.185:INDEX"]
[41,null,"Bit  9","Warning 186","Warnings.###MNR.186","###INDEX:Warnings.###MNR.186:INDEX"]
[41,null,"Bit  10","Warning 187","Warnings.###MNR.187","###INDEX:Warnings.###MNR.187:INDEX"]
[41,null,"Bit  11","Warning 188","Warnings.###MNR.188","###INDEX:Warnings.###MNR.188:INDEX"]
[41,null,"Bit  12","Warning 189","Warnings.###MNR.189","###INDEX:Warnings.###MNR.189:INDEX"]
[41,null,"Bit  13","Warning 190","Warnings.###MNR.190","###INDEX:Warnings.###MNR.190:INDEX"]
[41,null,"Bit  14","Warning 191","Warnings.###MNR.191","###INDEX:Warnings.###MNR.191:INDEX"]
[41,null,"Bit  15","Warning 192","Warnings.###MNR.192","###INDEX:Warnings.###MNR.192:INDEX"]
[41,"DW 12","Bit  0","Warning 193","Warnings.###MNR.193","###INDEX:Warnings.###MNR.193:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_13>[W]{p}"]
[41,null,"Bit  1","Warning 194","Warnings.###MNR.194","###INDEX:Warnings.###MNR.194:INDEX"]
[41,null,"Bit  2","Warning 195","Warnings.###MNR.195","###INDEX:Warnings.###MNR.195:INDEX"]
[41,null,"Bit  3","Warning 196","Warnings.###MNR.196","###INDEX:Warnings.###MNR.196:INDEX"]
[41,null,"Bit  4","Warning 197","Warnings.###MNR.197","###INDEX:Warnings.###MNR.197:INDEX"]
[41,null,"Bit  5","Warning 198","Warnings.###MNR.198","###INDEX:Warnings.###MNR.198:INDEX"]
[41,null,"Bit  6","Warning 199","Warnings.###MNR.199","###INDEX:Warnings.###MNR.199:INDEX"]
[41,null,"Bit  7","Warning 200","Warnings.###MNR.200","###INDEX:Warnings.###MNR.200:INDEX"]
[41,null,"Bit  8","Warning 201","Warnings.###MNR.201","###INDEX:Warnings.###MNR.201:INDEX"]
[41,null,"Bit  9","Warning 202","Warnings.###MNR.202","###INDEX:Warnings.###MNR.202:INDEX"]
[41,null,"Bit  10","Warning 203","Warnings.###MNR.203","###INDEX:Warnings.###MNR.203:INDEX"]
[41,null,"Bit  11","Warning 204","Warnings.###MNR.204","###INDEX:Warnings.###MNR.204:INDEX"]
[41,null,"Bit  12","Warning 205","Warnings.###MNR.205","###INDEX:Warnings.###MNR.205:INDEX"]
[41,null,"Bit  13","Warning 206","Warnings.###MNR.206","###INDEX:Warnings.###MNR.206:INDEX"]
[41,null,"Bit  14","Warning 207","Warnings.###MNR.207","###INDEX:Warnings.###MNR.207:INDEX"]
[41,null,"Bit  15","Warning 208","Warnings.###MNR.208","###INDEX:Warnings.###MNR.208:INDEX"]
[41,"DW 13","Bit  0","Warning 209","Warnings.###MNR.209","###INDEX:Warnings.###MNR.209:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_14>[W]{p}"]
[41,null,"Bit  1","Warning 210","Warnings.###MNR.210","###INDEX:Warnings.###MNR.210:INDEX"]
[41,null,"Bit  2","Warning 211","Warnings.###MNR.211","###INDEX:Warnings.###MNR.211:INDEX"]
[41,null,"Bit  3","Warning 212","Warnings.###MNR.212","###INDEX:Warnings.###MNR.212:INDEX"]
[41,null,"Bit  4","Warning 213","Warnings.###MNR.213","###INDEX:Warnings.###MNR.213:INDEX"]
[41,null,"Bit  5","Warning 214","Warnings.###MNR.214","###INDEX:Warnings.###MNR.214:INDEX"]
[41,null,"Bit  6","Warning 215","Warnings.###MNR.215","###INDEX:Warnings.###MNR.215:INDEX"]
[41,null,"Bit  7","Warning 216","Warnings.###MNR.216","###INDEX:Warnings.###MNR.216:INDEX"]
[41,null,"Bit  8","Warning 217","Warnings.###MNR.217","###INDEX:Warnings.###MNR.217:INDEX"]
[41,null,"Bit  9","Warning 218","Warnings.###MNR.218","###INDEX:Warnings.###MNR.218:INDEX"]
[41,null,"Bit  10","Warning 219","Warnings.###MNR.219","###INDEX:Warnings.###MNR.219:INDEX"]
[41,null,"Bit  11","Warning 220","Warnings.###MNR.220","###INDEX:Warnings.###MNR.220:INDEX"]
[41,null,"Bit  12","Warning 221","Warnings.###MNR.221","###INDEX:Warnings.###MNR.221:INDEX"]
[41,null,"Bit  13","Warning 222","Warnings.###MNR.222","###INDEX:Warnings.###MNR.222:INDEX"]
[41,null,"Bit  14","Warning 223","Warnings.###MNR.223","###INDEX:Warnings.###MNR.223:INDEX"]
[41,null,"Bit  15","Warning 224","Warnings.###MNR.224","###INDEX:Warnings.###MNR.224:INDEX"]
[41,"DW 14","Bit  0","Warning 225","Warnings.###MNR.225","###INDEX:Warnings.###MNR.225:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_15>[W]{p}"]
[41,null,"Bit  1","Warning 226","Warnings.###MNR.226","###INDEX:Warnings.###MNR.226:INDEX"]
[41,null,"Bit  2","Warning 227","Warnings.###MNR.227","###INDEX:Warnings.###MNR.227:INDEX"]
[41,null,"Bit  3","Warning 228","Warnings.###MNR.228","###INDEX:Warnings.###MNR.228:INDEX"]
[41,null,"Bit  4","Warning 229","Warnings.###MNR.229","###INDEX:Warnings.###MNR.229:INDEX"]
[41,null,"Bit  5","Warning 230","Warnings.###MNR.230","###INDEX:Warnings.###MNR.230:INDEX"]
[41,null,"Bit  6","Warning 231","Warnings.###MNR.231","###INDEX:Warnings.###MNR.231:INDEX"]
[41,null,"Bit  7","Warning 232","Warnings.###MNR.232","###INDEX:Warnings.###MNR.232:INDEX"]
[41,null,"Bit  8","Warning 233","Warnings.###MNR.233","###INDEX:Warnings.###MNR.233:INDEX"]
[41,null,"Bit  9","Warning 234","Warnings.###MNR.234","###INDEX:Warnings.###MNR.234:INDEX"]
[41,null,"Bit  10","Warning 235","Warnings.###MNR.235","###INDEX:Warnings.###MNR.235:INDEX"]
[41,null,"Bit  11","Warning 236","Warnings.###MNR.236","###INDEX:Warnings.###MNR.236:INDEX"]
[41,null,"Bit  12","Warning 237","Warnings.###MNR.237","###INDEX:Warnings.###MNR.237:INDEX"]
[41,null,"Bit  13","Warning 238","Warnings.###MNR.238","###INDEX:Warnings.###MNR.238:INDEX"]
[41,null,"Bit  14","Warning 239","Warnings.###MNR.239","###INDEX:Warnings.###MNR.239:INDEX"]
[41,null,"Bit  15","Warning 240","Warnings.###MNR.240","###INDEX:Warnings.###MNR.240:INDEX"]
[41,"DW 15","Bit  0","Warning 241","Warnings.###MNR.241","###INDEX:Warnings.###MNR.241:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_16>[W]{p}"]
[41,null,"Bit  1","Warning 242","Warnings.###MNR.242","###INDEX:Warnings.###MNR.242:INDEX"]
[41,null,"Bit  2","Warning 243","Warnings.###MNR.243","###INDEX:Warnings.###MNR.243:INDEX"]
[41,null,"Bit  3","Warning 244","Warnings.###MNR.244","###INDEX:Warnings.###MNR.244:INDEX"]
[41,null,"Bit  4","Warning 245","Warnings.###MNR.245","###INDEX:Warnings.###MNR.245:INDEX"]
[41,null,"Bit  5","Warning 246","Warnings.###MNR.246","###INDEX:Warnings.###MNR.246:INDEX"]
[41,null,"Bit  6","Warning 247","Warnings.###MNR.247","###INDEX:Warnings.###MNR.247:INDEX"]
[41,null,"Bit  7","Warning 248","Warnings.###MNR.248","###INDEX:Warnings.###MNR.248:INDEX"]
[41,null,"Bit  8","Warning 249","Warnings.###MNR.249","###INDEX:Warnings.###MNR.249:INDEX"]
[41,null,"Bit  9","Warning 250","Warnings.###MNR.250","###INDEX:Warnings.###MNR.250:INDEX"]
[41,null,"Bit  10","Warning 251","Warnings.###MNR.251","###INDEX:Warnings.###MNR.251:INDEX"]
[41,null,"Bit  11","Warning 252","Warnings.###MNR.252","###INDEX:Warnings.###MNR.252:INDEX"]
[41,null,"Bit  12","Warning 253","Warnings.###MNR.253","###INDEX:Warnings.###MNR.253:INDEX"]
[41,null,"Bit  13","Warning 254","Warnings.###MNR.254","###INDEX:Warnings.###MNR.254:INDEX"]
[41,null,"Bit  14","Warning 255","Warnings.###MNR.255","###INDEX:Warnings.###MNR.255:INDEX"]
[41,null,"Bit  15","Warning 256","Warnings.###MNR.256","###INDEX:Warnings.###MNR.256:INDEX"]
[41,"###SDR[WAR]"]
[41,"DW ###ADDR:15+1[FWAR]:ADDR","Bit  0","Warning ###ADDR:241+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:241+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:241+16[FWAR]:ADDR:INDEX","Ch1.###MNR_T_warnung<.m###MNR_warn_###ADDR:16+1[FREJ]:ADDR>[W]{p}"]
[41,null,"Bit  1","Warning ###ADDR:242+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:242+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:242+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  2","Warning ###ADDR:243+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:243+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:243+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  3","Warning ###ADDR:244+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:244+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:244+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  4","Warning ###ADDR:245+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:245+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:245+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  5","Warning ###ADDR:246+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:246+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:246+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  6","Warning ###ADDR:247+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:247+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:247+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  7","Warning ###ADDR:248+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:248+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:248+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  8","Warning ###ADDR:249+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:249+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:249+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  9","Warning ###ADDR:250+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:250+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:250+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  10","Warning ###ADDR:251+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:251+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:251+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  11","Warning ###ADDR:252+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:252+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:252+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  12","Warning ###ADDR:253+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:253+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:253+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  13","Warning ###ADDR:254+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:254+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:254+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  14","Warning ###ADDR:255+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:255+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:255+16[FWAR]:ADDR:INDEX"]
[41,null,"Bit  15","Warning ###ADDR:256+16[FWAR]:ADDR","Warnings.###MNR.###ADDR:256+16[FWAR]:ADDR","###INDEX:Warnings.###MNR.###ADDR:256+16[FWAR]:ADDR:INDEX"]
[41,"###EDR[WAR]"]
[21,"DB ###ADDR:2+5[MNR]+10[PLC]:ADDR","Faults ###MNR"]
[41,"DW 0",null,"First-up value as number",null,null,"Ch1.###MNR_T_zyk_fehler<.m###MNR_erstwert>[W]{p}"]
[41,"DW 1",null,"First-up value as number for DCS (is presetas long as machine is at standstill)",null,null,"Ch1.###MNR_T_zyk_fehler<.m###MNR_erstwert_bde>[W]{p}"]
[41]
[41,"DW 10","Bit  0","Fault 1","Alarms.###MNR.1","###INDEX:Alarms.###MNR.1:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_01>[W]{p}"]
[41,null,"Bit  1","Fault 2","Alarms.###MNR.2","###INDEX:Alarms.###MNR.2:INDEX"]
[41,null,"Bit  2","Fault 3","Alarms.###MNR.3","###INDEX:Alarms.###MNR.3:INDEX"]
[41,null,"Bit  3","Fault 4","Alarms.###MNR.4","###INDEX:Alarms.###MNR.4:INDEX"]
[41,null,"Bit  4","Fault 5","Alarms.###MNR.5","###INDEX:Alarms.###MNR.5:INDEX"]
[41,null,"Bit  5","Fault 6","Alarms.###MNR.6","###INDEX:Alarms.###MNR.6:INDEX"]
[41,null,"Bit  6","Fault 7","Alarms.###MNR.7","###INDEX:Alarms.###MNR.7:INDEX"]
[41,null,"Bit  7","Fault 8","Alarms.###MNR.8","###INDEX:Alarms.###MNR.8:INDEX"]
[41,null,"Bit  8","Fault 9","Alarms.###MNR.9","###INDEX:Alarms.###MNR.9:INDEX"]
[41,null,"Bit  9","Fault 10","Alarms.###MNR.10","###INDEX:Alarms.###MNR.10:INDEX"]
[41,null,"Bit  10","Fault 11","Alarms.###MNR.11","###INDEX:Alarms.###MNR.11:INDEX"]
[41,null,"Bit  11","Fault 12","Alarms.###MNR.12","###INDEX:Alarms.###MNR.12:INDEX"]
[41,null,"Bit  12","Fault 13","Alarms.###MNR.13","###INDEX:Alarms.###MNR.13:INDEX"]
[41,null,"Bit  13","Fault 14","Alarms.###MNR.14","###INDEX:Alarms.###MNR.14:INDEX"]
[41,null,"Bit  14","Fault 15","Alarms.###MNR.15","###INDEX:Alarms.###MNR.15:INDEX"]
[41,null,"Bit  15","Fault 16","Alarms.###MNR.16","###INDEX:Alarms.###MNR.16:INDEX"]
[41,"DW 11","Bit  0","Fault 17","Alarms.###MNR.17","###INDEX:Alarms.###MNR.17:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_02>[W]{p}"]
[41,null,"Bit  1","Fault 18","Alarms.###MNR.18","###INDEX:Alarms.###MNR.18:INDEX"]
[41,null,"Bit  2","Fault 19","Alarms.###MNR.19","###INDEX:Alarms.###MNR.19:INDEX"]
[41,null,"Bit  3","Fault 20","Alarms.###MNR.20","###INDEX:Alarms.###MNR.20:INDEX"]
[41,null,"Bit  4","Fault 21","Alarms.###MNR.21","###INDEX:Alarms.###MNR.21:INDEX"]
[41,null,"Bit  5","Fault 22","Alarms.###MNR.22","###INDEX:Alarms.###MNR.22:INDEX"]
[41,null,"Bit  6","Fault 23","Alarms.###MNR.23","###INDEX:Alarms.###MNR.23:INDEX"]
[41,null,"Bit  7","Fault 24","Alarms.###MNR.24","###INDEX:Alarms.###MNR.24:INDEX"]
[41,null,"Bit  8","Fault 25","Alarms.###MNR.25","###INDEX:Alarms.###MNR.25:INDEX"]
[41,null,"Bit  9","Fault 26","Alarms.###MNR.26","###INDEX:Alarms.###MNR.26:INDEX"]
[41,null,"Bit  10","Fault 27","Alarms.###MNR.27","###INDEX:Alarms.###MNR.27:INDEX"]
[41,null,"Bit  11","Fault 28","Alarms.###MNR.28","###INDEX:Alarms.###MNR.28:INDEX"]
[41,null,"Bit  12","Fault 29","Alarms.###MNR.29","###INDEX:Alarms.###MNR.29:INDEX"]
[41,null,"Bit  13","Fault 30","Alarms.###MNR.30","###INDEX:Alarms.###MNR.30:INDEX"]
[41,null,"Bit  14","Fault 31","Alarms.###MNR.31","###INDEX:Alarms.###MNR.31:INDEX"]
[41,null,"Bit  15","Fault 32","Alarms.###MNR.32","###INDEX:Alarms.###MNR.32:INDEX"]
[41,"DW 12","Bit  0","Fault 33","Alarms.###MNR.33","###INDEX:Alarms.###MNR.33:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_03>[W]{p}"]
[41,null,"Bit  1","Fault 34","Alarms.###MNR.34","###INDEX:Alarms.###MNR.34:INDEX"]
[41,null,"Bit  2","Fault 35","Alarms.###MNR.35","###INDEX:Alarms.###MNR.35:INDEX"]
[41,null,"Bit  3","Fault 36","Alarms.###MNR.36","###INDEX:Alarms.###MNR.36:INDEX"]
[41,null,"Bit  4","Fault 37","Alarms.###MNR.37","###INDEX:Alarms.###MNR.37:INDEX"]
[41,null,"Bit  5","Fault 38","Alarms.###MNR.38","###INDEX:Alarms.###MNR.38:INDEX"]
[41,null,"Bit  6","Fault 39","Alarms.###MNR.39","###INDEX:Alarms.###MNR.39:INDEX"]
[41,null,"Bit  7","Fault 40","Alarms.###MNR.40","###INDEX:Alarms.###MNR.40:INDEX"]
[41,null,"Bit  8","Fault 41","Alarms.###MNR.41","###INDEX:Alarms.###MNR.41:INDEX"]
[41,null,"Bit  9","Fault 42","Alarms.###MNR.42","###INDEX:Alarms.###MNR.42:INDEX"]
[41,null,"Bit  10","Fault 43","Alarms.###MNR.43","###INDEX:Alarms.###MNR.43:INDEX"]
[41,null,"Bit  11","Fault 44","Alarms.###MNR.44","###INDEX:Alarms.###MNR.44:INDEX"]
[41,null,"Bit  12","Fault 45","Alarms.###MNR.45","###INDEX:Alarms.###MNR.45:INDEX"]
[41,null,"Bit  13","Fault 46","Alarms.###MNR.46","###INDEX:Alarms.###MNR.46:INDEX"]
[41,null,"Bit  14","Fault 47","Alarms.###MNR.47","###INDEX:Alarms.###MNR.47:INDEX"]
[41,null,"Bit  15","Fault 48","Alarms.###MNR.48","###INDEX:Alarms.###MNR.48:INDEX"]
[41,"DW 13","Bit  0","Fault 49","Alarms.###MNR.49","###INDEX:Alarms.###MNR.49:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_04>[W]{p}"]
[41,null,"Bit  1","Fault 50","Alarms.###MNR.50","###INDEX:Alarms.###MNR.50:INDEX"]
[41,null,"Bit  2","Fault 51","Alarms.###MNR.51","###INDEX:Alarms.###MNR.51:INDEX"]
[41,null,"Bit  3","Fault 52","Alarms.###MNR.52","###INDEX:Alarms.###MNR.52:INDEX"]
[41,null,"Bit  4","Fault 53","Alarms.###MNR.53","###INDEX:Alarms.###MNR.53:INDEX"]
[41,null,"Bit  5","Fault 54","Alarms.###MNR.54","###INDEX:Alarms.###MNR.54:INDEX"]
[41,null,"Bit  6","Fault 55","Alarms.###MNR.55","###INDEX:Alarms.###MNR.55:INDEX"]
[41,null,"Bit  7","Fault 56","Alarms.###MNR.56","###INDEX:Alarms.###MNR.56:INDEX"]
[41,null,"Bit  8","Fault 57","Alarms.###MNR.57","###INDEX:Alarms.###MNR.57:INDEX"]
[41,null,"Bit  9","Fault 58","Alarms.###MNR.58","###INDEX:Alarms.###MNR.58:INDEX"]
[41,null,"Bit  10","Fault 59","Alarms.###MNR.59","###INDEX:Alarms.###MNR.59:INDEX"]
[41,null,"Bit  11","Fault 60","Alarms.###MNR.60","###INDEX:Alarms.###MNR.60:INDEX"]
[41,null,"Bit  12","Fault 61","Alarms.###MNR.61","###INDEX:Alarms.###MNR.61:INDEX"]
[41,null,"Bit  13","Fault 62","Alarms.###MNR.62","###INDEX:Alarms.###MNR.62:INDEX"]
[41,null,"Bit  14","Fault 63","Alarms.###MNR.63","###INDEX:Alarms.###MNR.63:INDEX"]
[41,null,"Bit  15","Fault 64","Alarms.###MNR.64","###INDEX:Alarms.###MNR.64:INDEX"]
[41,"DW 14","Bit  0","Fault 65","Alarms.###MNR.65","###INDEX:Alarms.###MNR.65:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_05>[W]{p}"]
[41,null,"Bit  1","Fault 66","Alarms.###MNR.66","###INDEX:Alarms.###MNR.66:INDEX"]
[41,null,"Bit  2","Fault 67","Alarms.###MNR.67","###INDEX:Alarms.###MNR.67:INDEX"]
[41,null,"Bit  3","Fault 68","Alarms.###MNR.68","###INDEX:Alarms.###MNR.68:INDEX"]
[41,null,"Bit  4","Fault 69","Alarms.###MNR.69","###INDEX:Alarms.###MNR.69:INDEX"]
[41,null,"Bit  5","Fault 70","Alarms.###MNR.70","###INDEX:Alarms.###MNR.70:INDEX"]
[41,null,"Bit  6","Fault 71","Alarms.###MNR.71","###INDEX:Alarms.###MNR.71:INDEX"]
[41,null,"Bit  7","Fault 72","Alarms.###MNR.72","###INDEX:Alarms.###MNR.72:INDEX"]
[41,null,"Bit  8","Fault 73","Alarms.###MNR.73","###INDEX:Alarms.###MNR.73:INDEX"]
[41,null,"Bit  9","Fault 74","Alarms.###MNR.74","###INDEX:Alarms.###MNR.74:INDEX"]
[41,null,"Bit  10","Fault 75","Alarms.###MNR.75","###INDEX:Alarms.###MNR.75:INDEX"]
[41,null,"Bit  11","Fault 76","Alarms.###MNR.76","###INDEX:Alarms.###MNR.76:INDEX"]
[41,null,"Bit  12","Fault 77","Alarms.###MNR.77","###INDEX:Alarms.###MNR.77:INDEX"]
[41,null,"Bit  13","Fault 78","Alarms.###MNR.78","###INDEX:Alarms.###MNR.78:INDEX"]
[41,null,"Bit  14","Fault 79","Alarms.###MNR.79","###INDEX:Alarms.###MNR.79:INDEX"]
[41,null,"Bit  15","Fault 80","Alarms.###MNR.80","###INDEX:Alarms.###MNR.80:INDEX"]
[41,"DW 15","Bit  0","Fault 81","Alarms.###MNR.81","###INDEX:Alarms.###MNR.81:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_06>[W]{p}"]
[41,null,"Bit  1","Fault 82","Alarms.###MNR.82","###INDEX:Alarms.###MNR.82:INDEX"]
[41,null,"Bit  2","Fault 83","Alarms.###MNR.83","###INDEX:Alarms.###MNR.83:INDEX"]
[41,null,"Bit  3","Fault 84","Alarms.###MNR.84","###INDEX:Alarms.###MNR.84:INDEX"]
[41,null,"Bit  4","Fault 85","Alarms.###MNR.85","###INDEX:Alarms.###MNR.85:INDEX"]
[41,null,"Bit  5","Fault 86","Alarms.###MNR.86","###INDEX:Alarms.###MNR.86:INDEX"]
[41,null,"Bit  6","Fault 87","Alarms.###MNR.87","###INDEX:Alarms.###MNR.87:INDEX"]
[41,null,"Bit  7","Fault 88","Alarms.###MNR.88","###INDEX:Alarms.###MNR.88:INDEX"]
[41,null,"Bit  8","Fault 89","Alarms.###MNR.89","###INDEX:Alarms.###MNR.89:INDEX"]
[41,null,"Bit  9","Fault 90","Alarms.###MNR.90","###INDEX:Alarms.###MNR.90:INDEX"]
[41,null,"Bit  10","Fault 91","Alarms.###MNR.91","###INDEX:Alarms.###MNR.91:INDEX"]
[41,null,"Bit  11","Fault 92","Alarms.###MNR.92","###INDEX:Alarms.###MNR.92:INDEX"]
[41,null,"Bit  12","Fault 93","Alarms.###MNR.93","###INDEX:Alarms.###MNR.93:INDEX"]
[41,null,"Bit  13","Fault 94","Alarms.###MNR.94","###INDEX:Alarms.###MNR.94:INDEX"]
[41,null,"Bit  14","Fault 95","Alarms.###MNR.95","###INDEX:Alarms.###MNR.95:INDEX"]
[41,null,"Bit  15","Fault 96","Alarms.###MNR.96","###INDEX:Alarms.###MNR.96:INDEX"]
[41,"DW 16","Bit  0","Fault 97","Alarms.###MNR.97","###INDEX:Alarms.###MNR.97:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_07>[W]{p}"]
[41,null,"Bit  1","Fault 98","Alarms.###MNR.98","###INDEX:Alarms.###MNR.98:INDEX"]
[41,null,"Bit  2","Fault 99","Alarms.###MNR.99","###INDEX:Alarms.###MNR.99:INDEX"]
[41,null,"Bit  3","Fault 100","Alarms.###MNR.100","###INDEX:Alarms.###MNR.100:INDEX"]
[41,null,"Bit  4","Fault 101","Alarms.###MNR.101","###INDEX:Alarms.###MNR.101:INDEX"]
[41,null,"Bit  5","Fault 102","Alarms.###MNR.102","###INDEX:Alarms.###MNR.102:INDEX"]
[41,null,"Bit  6","Fault 103","Alarms.###MNR.103","###INDEX:Alarms.###MNR.103:INDEX"]
[41,null,"Bit  7","Fault 104","Alarms.###MNR.104","###INDEX:Alarms.###MNR.104:INDEX"]
[41,null,"Bit  8","Fault 105","Alarms.###MNR.105","###INDEX:Alarms.###MNR.105:INDEX"]
[41,null,"Bit  9","Fault 106","Alarms.###MNR.106","###INDEX:Alarms.###MNR.106:INDEX"]
[41,null,"Bit  10","Fault 107","Alarms.###MNR.107","###INDEX:Alarms.###MNR.107:INDEX"]
[41,null,"Bit  11","Fault 108","Alarms.###MNR.108","###INDEX:Alarms.###MNR.108:INDEX"]
[41,null,"Bit  12","Fault 109","Alarms.###MNR.109","###INDEX:Alarms.###MNR.109:INDEX"]
[41,null,"Bit  13","Fault 110","Alarms.###MNR.110","###INDEX:Alarms.###MNR.110:INDEX"]
[41,null,"Bit  14","Fault 111","Alarms.###MNR.111","###INDEX:Alarms.###MNR.111:INDEX"]
[41,null,"Bit  15","Fault 112","Alarms.###MNR.112","###INDEX:Alarms.###MNR.112:INDEX"]
[41,"DW 17","Bit  0","Fault 113","Alarms.###MNR.113","###INDEX:Alarms.###MNR.113:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_08>[W]{p}"]
[41,null,"Bit  1","Fault 114","Alarms.###MNR.114","###INDEX:Alarms.###MNR.114:INDEX"]
[41,null,"Bit  2","Fault 115","Alarms.###MNR.115","###INDEX:Alarms.###MNR.115:INDEX"]
[41,null,"Bit  3","Fault 116","Alarms.###MNR.116","###INDEX:Alarms.###MNR.116:INDEX"]
[41,null,"Bit  4","Fault 117","Alarms.###MNR.117","###INDEX:Alarms.###MNR.117:INDEX"]
[41,null,"Bit  5","Fault 118","Alarms.###MNR.118","###INDEX:Alarms.###MNR.118:INDEX"]
[41,null,"Bit  6","Fault 119","Alarms.###MNR.119","###INDEX:Alarms.###MNR.119:INDEX"]
[41,null,"Bit  7","Fault 120","Alarms.###MNR.120","###INDEX:Alarms.###MNR.120:INDEX"]
[41,null,"Bit  8","Fault 121","Alarms.###MNR.121","###INDEX:Alarms.###MNR.121:INDEX"]
[41,null,"Bit  9","Fault 122","Alarms.###MNR.122","###INDEX:Alarms.###MNR.122:INDEX"]
[41,null,"Bit  10","Fault 123","Alarms.###MNR.123","###INDEX:Alarms.###MNR.123:INDEX"]
[41,null,"Bit  11","Fault 124","Alarms.###MNR.124","###INDEX:Alarms.###MNR.124:INDEX"]
[41,null,"Bit  12","Fault 125","Alarms.###MNR.125","###INDEX:Alarms.###MNR.125:INDEX"]
[41,null,"Bit  13","Fault 126","Alarms.###MNR.126","###INDEX:Alarms.###MNR.126:INDEX"]
[41,null,"Bit  14","Fault 127","Alarms.###MNR.127","###INDEX:Alarms.###MNR.127:INDEX"]
[41,null,"Bit  15","Fault 128","Alarms.###MNR.128","###INDEX:Alarms.###MNR.128:INDEX"]
[41,"DW 18","Bit  0","Fault 129","Alarms.###MNR.129","###INDEX:Alarms.###MNR.129:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_09>[W]{p}"]
[41,null,"Bit  1","Fault 130","Alarms.###MNR.130","###INDEX:Alarms.###MNR.130:INDEX"]
[41,null,"Bit  2","Fault 131","Alarms.###MNR.131","###INDEX:Alarms.###MNR.131:INDEX"]
[41,null,"Bit  3","Fault 132","Alarms.###MNR.132","###INDEX:Alarms.###MNR.132:INDEX"]
[41,null,"Bit  4","Fault 133","Alarms.###MNR.133","###INDEX:Alarms.###MNR.133:INDEX"]
[41,null,"Bit  5","Fault 134","Alarms.###MNR.134","###INDEX:Alarms.###MNR.134:INDEX"]
[41,null,"Bit  6","Fault 135","Alarms.###MNR.135","###INDEX:Alarms.###MNR.135:INDEX"]
[41,null,"Bit  7","Fault 136","Alarms.###MNR.136","###INDEX:Alarms.###MNR.136:INDEX"]
[41,null,"Bit  8","Fault 137","Alarms.###MNR.137","###INDEX:Alarms.###MNR.137:INDEX"]
[41,null,"Bit  9","Fault 138","Alarms.###MNR.138","###INDEX:Alarms.###MNR.138:INDEX"]
[41,null,"Bit  10","Fault 139","Alarms.###MNR.139","###INDEX:Alarms.###MNR.139:INDEX"]
[41,null,"Bit  11","Fault 140","Alarms.###MNR.140","###INDEX:Alarms.###MNR.140:INDEX"]
[41,null,"Bit  12","Fault 141","Alarms.###MNR.141","###INDEX:Alarms.###MNR.141:INDEX"]
[41,null,"Bit  13","Fault 142","Alarms.###MNR.142","###INDEX:Alarms.###MNR.142:INDEX"]
[41,null,"Bit  14","Fault 143","Alarms.###MNR.143","###INDEX:Alarms.###MNR.143:INDEX"]
[41,null,"Bit  15","Fault 144","Alarms.###MNR.144","###INDEX:Alarms.###MNR.144:INDEX"]
[41,"DW 19","Bit  0","Fault 145","Alarms.###MNR.145","###INDEX:Alarms.###MNR.145:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_10>[W]{p}"]
[41,null,"Bit  1","Fault 146","Alarms.###MNR.146","###INDEX:Alarms.###MNR.146:INDEX"]
[41,null,"Bit  2","Fault 147","Alarms.###MNR.147","###INDEX:Alarms.###MNR.147:INDEX"]
[41,null,"Bit  3","Fault 148","Alarms.###MNR.148","###INDEX:Alarms.###MNR.148:INDEX"]
[41,null,"Bit  4","Fault 149","Alarms.###MNR.149","###INDEX:Alarms.###MNR.149:INDEX"]
[41,null,"Bit  5","Fault 150","Alarms.###MNR.150","###INDEX:Alarms.###MNR.150:INDEX"]
[41,null,"Bit  6","Fault 151","Alarms.###MNR.151","###INDEX:Alarms.###MNR.151:INDEX"]
[41,null,"Bit  7","Fault 152","Alarms.###MNR.152","###INDEX:Alarms.###MNR.152:INDEX"]
[41,null,"Bit  8","Fault 153","Alarms.###MNR.153","###INDEX:Alarms.###MNR.153:INDEX"]
[41,null,"Bit  9","Fault 154","Alarms.###MNR.154","###INDEX:Alarms.###MNR.154:INDEX"]
[41,null,"Bit  10","Fault 155","Alarms.###MNR.155","###INDEX:Alarms.###MNR.155:INDEX"]
[41,null,"Bit  11","Fault 156","Alarms.###MNR.156","###INDEX:Alarms.###MNR.156:INDEX"]
[41,null,"Bit  12","Fault 157","Alarms.###MNR.157","###INDEX:Alarms.###MNR.157:INDEX"]
[41,null,"Bit  13","Fault 158","Alarms.###MNR.158","###INDEX:Alarms.###MNR.158:INDEX"]
[41,null,"Bit  14","Fault 159","Alarms.###MNR.159","###INDEX:Alarms.###MNR.159:INDEX"]
[41,null,"Bit  15","Fault 160","Alarms.###MNR.160","###INDEX:Alarms.###MNR.160:INDEX"]
[41,"DW 20","Bit  0","Fault 161","Alarms.###MNR.161","###INDEX:Alarms.###MNR.161:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_11>[W]{p}"]
[41,null,"Bit  1","Fault 162","Alarms.###MNR.162","###INDEX:Alarms.###MNR.162:INDEX"]
[41,null,"Bit  2","Fault 163","Alarms.###MNR.163","###INDEX:Alarms.###MNR.163:INDEX"]
[41,null,"Bit  3","Fault 164","Alarms.###MNR.164","###INDEX:Alarms.###MNR.164:INDEX"]
[41,null,"Bit  4","Fault 165","Alarms.###MNR.165","###INDEX:Alarms.###MNR.165:INDEX"]
[41,null,"Bit  5","Fault 166","Alarms.###MNR.166","###INDEX:Alarms.###MNR.166:INDEX"]
[41,null,"Bit  6","Fault 167","Alarms.###MNR.167","###INDEX:Alarms.###MNR.167:INDEX"]
[41,null,"Bit  7","Fault 168","Alarms.###MNR.168","###INDEX:Alarms.###MNR.168:INDEX"]
[41,null,"Bit  8","Fault 169","Alarms.###MNR.169","###INDEX:Alarms.###MNR.169:INDEX"]
[41,null,"Bit  9","Fault 170","Alarms.###MNR.170","###INDEX:Alarms.###MNR.170:INDEX"]
[41,null,"Bit  10","Fault 171","Alarms.###MNR.171","###INDEX:Alarms.###MNR.171:INDEX"]
[41,null,"Bit  11","Fault 172","Alarms.###MNR.172","###INDEX:Alarms.###MNR.172:INDEX"]
[41,null,"Bit  12","Fault 173","Alarms.###MNR.173","###INDEX:Alarms.###MNR.173:INDEX"]
[41,null,"Bit  13","Fault 174","Alarms.###MNR.174","###INDEX:Alarms.###MNR.174:INDEX"]
[41,null,"Bit  14","Fault 175","Alarms.###MNR.175","###INDEX:Alarms.###MNR.175:INDEX"]
[41,null,"Bit  15","Fault 176","Alarms.###MNR.176","###INDEX:Alarms.###MNR.176:INDEX"]
[41,"DW 21","Bit  0","Fault 177","Alarms.###MNR.177","###INDEX:Alarms.###MNR.177:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_12>[W]{p}"]
[41,null,"Bit  1","Fault 178","Alarms.###MNR.178","###INDEX:Alarms.###MNR.178:INDEX"]
[41,null,"Bit  2","Fault 179","Alarms.###MNR.179","###INDEX:Alarms.###MNR.179:INDEX"]
[41,null,"Bit  3","Fault 180","Alarms.###MNR.180","###INDEX:Alarms.###MNR.180:INDEX"]
[41,null,"Bit  4","Fault 181","Alarms.###MNR.181","###INDEX:Alarms.###MNR.181:INDEX"]
[41,null,"Bit  5","Fault 182","Alarms.###MNR.182","###INDEX:Alarms.###MNR.182:INDEX"]
[41,null,"Bit  6","Fault 183","Alarms.###MNR.183","###INDEX:Alarms.###MNR.183:INDEX"]
[41,null,"Bit  7","Fault 184","Alarms.###MNR.184","###INDEX:Alarms.###MNR.184:INDEX"]
[41,null,"Bit  8","Fault 185","Alarms.###MNR.185","###INDEX:Alarms.###MNR.185:INDEX"]
[41,null,"Bit  9","Fault 186","Alarms.###MNR.186","###INDEX:Alarms.###MNR.186:INDEX"]
[41,null,"Bit  10","Fault 187","Alarms.###MNR.187","###INDEX:Alarms.###MNR.187:INDEX"]
[41,null,"Bit  11","Fault 188","Alarms.###MNR.188","###INDEX:Alarms.###MNR.188:INDEX"]
[41,null,"Bit  12","Fault 189","Alarms.###MNR.189","###INDEX:Alarms.###MNR.189:INDEX"]
[41,null,"Bit  13","Fault 190","Alarms.###MNR.190","###INDEX:Alarms.###MNR.190:INDEX"]
[41,null,"Bit  14","Fault 191","Alarms.###MNR.191","###INDEX:Alarms.###MNR.191:INDEX"]
[41,null,"Bit  15","Fault 192","Alarms.###MNR.192","###INDEX:Alarms.###MNR.192:INDEX"]
[41,"DW 22","Bit  0","Fault 193","Alarms.###MNR.193","###INDEX:Alarms.###MNR.193:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_13>[W]{p}"]
[41,null,"Bit  1","Fault 194","Alarms.###MNR.194","###INDEX:Alarms.###MNR.194:INDEX"]
[41,null,"Bit  2","Fault 195","Alarms.###MNR.195","###INDEX:Alarms.###MNR.195:INDEX"]
[41,null,"Bit  3","Fault 196","Alarms.###MNR.196","###INDEX:Alarms.###MNR.196:INDEX"]
[41,null,"Bit  4","Fault 197","Alarms.###MNR.197","###INDEX:Alarms.###MNR.197:INDEX"]
[41,null,"Bit  5","Fault 198","Alarms.###MNR.198","###INDEX:Alarms.###MNR.198:INDEX"]
[41,null,"Bit  6","Fault 199","Alarms.###MNR.199","###INDEX:Alarms.###MNR.199:INDEX"]
[41,null,"Bit  7","Fault 200","Alarms.###MNR.200","###INDEX:Alarms.###MNR.200:INDEX"]
[41,null,"Bit  8","Fault 201","Alarms.###MNR.201","###INDEX:Alarms.###MNR.201:INDEX"]
[41,null,"Bit  9","Fault 202","Alarms.###MNR.202","###INDEX:Alarms.###MNR.202:INDEX"]
[41,null,"Bit  10","Fault 203","Alarms.###MNR.203","###INDEX:Alarms.###MNR.203:INDEX"]
[41,null,"Bit  11","Fault 204","Alarms.###MNR.204","###INDEX:Alarms.###MNR.204:INDEX"]
[41,null,"Bit  12","Fault 205","Alarms.###MNR.205","###INDEX:Alarms.###MNR.205:INDEX"]
[41,null,"Bit  13","Fault 206","Alarms.###MNR.206","###INDEX:Alarms.###MNR.206:INDEX"]
[41,null,"Bit  14","Fault 207","Alarms.###MNR.207","###INDEX:Alarms.###MNR.207:INDEX"]
[41,null,"Bit  15","Fault 208","Alarms.###MNR.208","###INDEX:Alarms.###MNR.208:INDEX"]
[41,"DW 23","Bit  0","Fault 209","Alarms.###MNR.209","###INDEX:Alarms.###MNR.209:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_14>[W]{p}"]
[41,null,"Bit  1","Fault 210","Alarms.###MNR.210","###INDEX:Alarms.###MNR.210:INDEX"]
[41,null,"Bit  2","Fault 211","Alarms.###MNR.211","###INDEX:Alarms.###MNR.211:INDEX"]
[41,null,"Bit  3","Fault 212","Alarms.###MNR.212","###INDEX:Alarms.###MNR.212:INDEX"]
[41,null,"Bit  4","Fault 213","Alarms.###MNR.213","###INDEX:Alarms.###MNR.213:INDEX"]
[41,null,"Bit  5","Fault 214","Alarms.###MNR.214","###INDEX:Alarms.###MNR.214:INDEX"]
[41,null,"Bit  6","Fault 215","Alarms.###MNR.215","###INDEX:Alarms.###MNR.215:INDEX"]
[41,null,"Bit  7","Fault 216","Alarms.###MNR.216","###INDEX:Alarms.###MNR.216:INDEX"]
[41,null,"Bit  8","Fault 217","Alarms.###MNR.217","###INDEX:Alarms.###MNR.217:INDEX"]
[41,null,"Bit  9","Fault 218","Alarms.###MNR.218","###INDEX:Alarms.###MNR.218:INDEX"]
[41,null,"Bit  10","Fault 219","Alarms.###MNR.219","###INDEX:Alarms.###MNR.219:INDEX"]
[41,null,"Bit  11","Fault 220","Alarms.###MNR.220","###INDEX:Alarms.###MNR.220:INDEX"]
[41,null,"Bit  12","Fault 221","Alarms.###MNR.221","###INDEX:Alarms.###MNR.221:INDEX"]
[41,null,"Bit  13","Fault 222","Alarms.###MNR.222","###INDEX:Alarms.###MNR.222:INDEX"]
[41,null,"Bit  14","Fault 223","Alarms.###MNR.223","###INDEX:Alarms.###MNR.223:INDEX"]
[41,null,"Bit  15","Fault 224","Alarms.###MNR.224","###INDEX:Alarms.###MNR.224:INDEX"]
[41,"DW 24","Bit  0","Fault 225","Alarms.###MNR.225","###INDEX:Alarms.###MNR.225:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_15>[W]{p}"]
[41,null,"Bit  1","Fault 226","Alarms.###MNR.226","###INDEX:Alarms.###MNR.226:INDEX"]
[41,null,"Bit  2","Fault 227","Alarms.###MNR.227","###INDEX:Alarms.###MNR.227:INDEX"]
[41,null,"Bit  3","Fault 228","Alarms.###MNR.228","###INDEX:Alarms.###MNR.228:INDEX"]
[41,null,"Bit  4","Fault 229","Alarms.###MNR.229","###INDEX:Alarms.###MNR.229:INDEX"]
[41,null,"Bit  5","Fault 230","Alarms.###MNR.230","###INDEX:Alarms.###MNR.230:INDEX"]
[41,null,"Bit  6","Fault 231","Alarms.###MNR.231","###INDEX:Alarms.###MNR.231:INDEX"]
[41,null,"Bit  7","Fault 232","Alarms.###MNR.232","###INDEX:Alarms.###MNR.232:INDEX"]
[41," ","Bit  8","Fault 233","Alarms.###MNR.233","###INDEX:Alarms.###MNR.233:INDEX"]
[41,null,"Bit  9","Fault 234","Alarms.###MNR.234","###INDEX:Alarms.###MNR.234:INDEX"]
[41,null,"Bit  10","Fault 235","Alarms.###MNR.235","###INDEX:Alarms.###MNR.235:INDEX"]
[41,null,"Bit  11","Fault 236","Alarms.###MNR.236","###INDEX:Alarms.###MNR.236:INDEX"]
[41,null,"Bit  12","Fault 237","Alarms.###MNR.237","###INDEX:Alarms.###MNR.237:INDEX"]
[41,null,"Bit  13","Fault 238","Alarms.###MNR.238","###INDEX:Alarms.###MNR.238:INDEX"]
[41,null,"Bit  14","Fault 239","Alarms.###MNR.239","###INDEX:Alarms.###MNR.239:INDEX"]
[41,null,"Bit  15","Fault 240","Alarms.###MNR.240","###INDEX:Alarms.###MNR.240:INDEX"]
[41,"DW 25","Bit  0","Fault 241","Alarms.###MNR.241","###INDEX:Alarms.###MNR.241:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_16>[W]{p}"]
[41,null,"Bit  1","Fault 242","Alarms.###MNR.242","###INDEX:Alarms.###MNR.242:INDEX"]
[41,null,"Bit  2","Fault 243","Alarms.###MNR.243","###INDEX:Alarms.###MNR.243:INDEX"]
[41,null,"Bit  3","Fault 244","Alarms.###MNR.244","###INDEX:Alarms.###MNR.244:INDEX"]
[41,null,"Bit  4","Fault 245","Alarms.###MNR.245","###INDEX:Alarms.###MNR.245:INDEX"]
[41,null,"Bit  5","Fault 246","Alarms.###MNR.246","###INDEX:Alarms.###MNR.246:INDEX"]
[41,null,"Bit  6","Fault 247","Alarms.###MNR.247","###INDEX:Alarms.###MNR.247:INDEX"]
[41,null,"Bit  7","Fault 248","Alarms.###MNR.248","###INDEX:Alarms.###MNR.248:INDEX"]
[41,null,"Bit  8","Fault 249","Alarms.###MNR.249","###INDEX:Alarms.###MNR.249:INDEX"]
[41,null,"Bit  9","Fault 250","Alarms.###MNR.250","###INDEX:Alarms.###MNR.250:INDEX"]
[41,null,"Bit  10","Fault 251","Alarms.###MNR.251","###INDEX:Alarms.###MNR.251:INDEX"]
[41,null,"Bit  11","Fault 252","Alarms.###MNR.252","###INDEX:Alarms.###MNR.252:INDEX"]
[41,null,"Bit  12","Fault 253","Alarms.###MNR.253","###INDEX:Alarms.###MNR.253:INDEX"]
[41,null,"Bit  13","Fault 254","Alarms.###MNR.254","###INDEX:Alarms.###MNR.254:INDEX"]
[41,null,"Bit  14","Fault 255","Alarms.###MNR.255","###INDEX:Alarms.###MNR.255:INDEX"]
[41,null,"Bit  15","Fault 256","Alarms.###MNR.256","###INDEX:Alarms.###MNR.256:INDEX"]
[41,"###SDR[ALA]"]
[41,"DW ###ADDR:25+1[FALA]:ADDR","Bit  0","Fault ###ADDR:241+16[FALA]:ADDR","Alarms.###MNR.###ADDR:241+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:241+16[FALA]:ADDR:INDEX","Ch1.###MNR_T_zyk_fehler<.m###MNR_fehler_###ADDR:16+1[FREJ]:ADDR>[W]{p}"]
[41,null,"Bit  1","Fault ###ADDR:242+16[FALA]:ADDR","Alarms.###MNR.###ADDR:242+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:242+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  2","Fault ###ADDR:243+16[FALA]:ADDR","Alarms.###MNR.###ADDR:243+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:243+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  3","Fault ###ADDR:244+16[FALA]:ADDR","Alarms.###MNR.###ADDR:244+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:244+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  4","Fault ###ADDR:245+16[FALA]:ADDR","Alarms.###MNR.###ADDR:245+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:245+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  5","Fault ###ADDR:246+16[FALA]:ADDR","Alarms.###MNR.###ADDR:246+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:246+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  6","Fault ###ADDR:247+16[FALA]:ADDR","Alarms.###MNR.###ADDR:247+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:247+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  7","Fault ###ADDR:248+16[FALA]:ADDR","Alarms.###MNR.###ADDR:248+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:248+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  8","Fault ###ADDR:249+16[FALA]:ADDR","Alarms.###MNR.###ADDR:249+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:249+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  9","Fault ###ADDR:250+16[FALA]:ADDR","Alarms.###MNR.###ADDR:250+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:250+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  10","Fault ###ADDR:251+16[FALA]:ADDR","Alarms.###MNR.###ADDR:251+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:251+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  11","Fault ###ADDR:252+16[FALA]:ADDR","Alarms.###MNR.###ADDR:252+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:252+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  12","Fault ###ADDR:253+16[FALA]:ADDR","Alarms.###MNR.###ADDR:253+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:253+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  13","Fault ###ADDR:254+16[FALA]:ADDR","Alarms.###MNR.###ADDR:254+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:254+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  14","Fault ###ADDR:255+16[FALA]:ADDR","Alarms.###MNR.###ADDR:255+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:255+16[FALA]:ADDR:INDEX"]
[41,null,"Bit  15","Fault ###ADDR:256+16[FALA]:ADDR","Alarms.###MNR.###ADDR:256+16[FALA]:ADDR","###INDEX:Alarms.###MNR.###ADDR:256+16[FALA]:ADDR:INDEX"]
[41,"###EDR[ALA]"]
[21,"DB ###ADDR:3+5[MNR]+10[PLC]:ADDR","Common Data ###MNR"]
[31,"DW 0-59","32-Bit-Counter"]
[41,"DD 0",null,"Good packets",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_p_gut>[DW]{p}"]
[41,"DD 4",null,"Bad packets",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_p_sch>[DW]{p}"]
[41,"DD 6",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_unicounter_01>[DW]{p}"]
[41,"DD 8",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_unicounter_02>[DW]{p}"]
[41,"DD 10",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_unicounter_03>[DW]{p}"]
[4,"350/700/725 only "]
[41,"DD 4",null,"Cigarette end detector",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_unicounter_01>[DW]{p}"]
[31,"DW 60-68","32-Bit-Measured Values"]
[41,"DD 60",null,"Clock counter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_takt>[DW]{p}"]
[41,"DD 62",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_ddmesswert_1>[DW]{p}"]
[41,"DD 64",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_ddmesswert_2>[DW]{p}"]
[41,"DD 66",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_ddmesswert_3>[DW]{p}"]
[4,"Capricornr only"]
[41,"DD 62",null,"Fill level, Capricorn cigarettes",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_ddmesswert_1>[DW]{p}"]
[41,"DD 64",null,"Fill level, Capricorn, as percentage",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_ddmesswert_2>[DW]{p}"]
[31,"DW 70-149","16-Bit-Measured Values"]
[41,"DW 70",null,"Speed",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_drehzahl>[W]{p}"]
[41,"DW 71",null,"Temperature cabinet",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_temperatur>[W]{p}"]
[41,"DW 73",null,"Maindrive current",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_zusatz_1>[W]{p}"]
[41,"DW 74",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_zusatz_2>[W]{p}"]
[41,"DW 75",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_zusatz_3>[W]{p}"]
[41,"DW 76",null,"Unicounter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_zusatz_4>[W]{p}"]
[4,"016 only"]
[41,"DW 73",null,"Packet counter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_zusatz_1>[W]{p}"]
[41,"DW 90","Bit 0","Enable packet counter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_bit_1>[B]{p}"]
[41,null,"Bit 1","Packet counter modified",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_bit_2>[B]{p}"]
[41,"DW 92","Bit 0","SPS-Ready",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_sps_ready>[B]{p}"]
[41,"DW 100",null,"setpoint from upstream machine",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_v_drehzahl>[W]{p}"]
[4,"Machines with Splicer only"]
[41,"DW 101",null,"16 bit from splicer",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_1>[W]{p}"]
[null,null,"Bit 1","Foil, red"]
[null,null,"Bit 2","Foil, white"]
[null,null,"Bit 3","Foil, yellow"]
[null,null,"Bit 4","Foil splice, yellow"]
[null,null,"Bit 5","Paper, red"]
[null,null,"Bit 6","Paper, white"]
[null,null,"Bit 7","Paper, yellow"]
[null,null,"Bit 8","Paper splice, yellow"]
[null,null,"Bit 9","Tax stamp, red"]
[null,null,"Bit 10","Tax stamp, white"]
[null,null,"Bit 11","Tax stamp, yellow"]
[null,null,"Bit 12","Tax stamp splice, yellow"]
[4,"Capricornr only"]
[41,"DW 101",null,"Speed Maker",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_1>[W]{p}"]
[41,"DW 102",null,"Speed Packer",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_2>[W]{p}"]
[41,"DW 103",null,"Remaining time packer in minutes",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_3>[W]{p}"]
[41,"DW 104",null,"Remaining time packer in seconds",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_4>[W]{p}"]
[41,"DW 105",null,"Remaining time maker in minutes",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_5>[W]{p}"]
[41,"DW 106",null,"Remaining time maker in seconds",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_6>[W]{p}"]
[41,"DW 107",null,"Position packer in procent",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_7>[W]{p}"]
[41,"DW 108",null,"Position maker in procent",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_messwert_8>[W]{p}"]
[31,"DW 150","Visualization -> PLC"]
[41,"DW 150","Bit 0","Reset production counter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_resetprod>[B]{w}"]
[41,null,"Bit 1","Reset reject counter",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_resetauswurf>[B]{w}"]
[41,null,"Bit 2","Reset reject message",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_100t_reset>[B]{w}"]
[31,"DW 160","Material change"]
[41,"DW 160","Bit 0","Materia change started -> PLC",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_mw_visubits>[W]{w}"]
[41,null,"Bit 1","Material selection confirmed > PLC"]
[41,null,"Bit 2","Cancel material change -> PLC"]
[41,null,"Bit 3","Confirmation of manual intervention > PLC"]
[41,null,"Bit 4","Start permitted"]
[41,null,"Bit 5","Schritt abbrechen"]
[41,null,"Bit 6","Schritt Wiederholen"]
[41,"DW 161",null,"Bitmap of materials to be changed",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_mw_matbits>[W]{w}"]
[41,"DW 162","Bit 0","mit Restproduktion",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_mw_mitrest>[B]{r}"]
[41,"DD 163",null,"Restproduktion",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_mw_rest>[DW]{r}"]
[41,"DW 170","Bit 0","Material change started -> Visu (confirmation)",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_mw_spsbits>[W]{r}"]
[41,null,"Bit 1","Material selected -> Visu"]
[41,null,"Bit 2 ","Cancelation permitted"]
[31,"DW 180","Verschiedenes"]
[41,"DW 180-199",null,"Markencode",null,null,"Ch1.###MNR_T_zyk_allge<.m###MNR_markencode>[W 0-19]{r}"]
["###IF MITAUSWURFZAEHLERN###21","DB ###ADDR:4+5[MNR]+10[PLC]:ADDR","Reject Counters ###MNR"]
["###IF MITAUSWURFZAEHLERN###41","DW 0","Bit 0-16","Reject counter 1-16 exist",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_vorhanden_1>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DW 1","Bit 0-16","Reject counter 1-16 has taken place ",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_statt_1>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 08",null,"Reject counter 1 ","Rejects.###MNR.1","###INDEX:Rejects.###MNR.1:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_01>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 10",null,"Reject counter 2","Rejects.###MNR.2","###INDEX:Rejects.###MNR.2:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_02>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 12",null,"Reject counter 3","Rejects.###MNR.3","###INDEX:Rejects.###MNR.3:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_03>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 14",null,"Reject counter 4","Rejects.###MNR.4","###INDEX:Rejects.###MNR.4:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_04>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 16",null,"Reject counter 5","Rejects.###MNR.5","###INDEX:Rejects.###MNR.5:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_05>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 18",null,"Reject counter 6","Rejects.###MNR.6","###INDEX:Rejects.###MNR.6:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_06>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 20",null,"Reject counter 7","Rejects.###MNR.7","###INDEX:Rejects.###MNR.7:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_07>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 22",null,"Reject counter 8","Rejects.###MNR.8","###INDEX:Rejects.###MNR.8:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_08>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 24",null,"Reject counter 9","Rejects.###MNR.9","###INDEX:Rejects.###MNR.9:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_09>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 26",null,"Reject counter 10","Rejects.###MNR.10 ","###INDEX:Rejects.###MNR.10:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_10>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 28",null,"Reject counter 11","Rejects.###MNR.11","###INDEX:Rejects.###MNR.11:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_11>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 30",null,"Reject counter 12","Rejects.###MNR.12","###INDEX:Rejects.###MNR.12:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_12>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 32",null,"Reject counter 13","Rejects.###MNR.13","###INDEX:Rejects.###MNR.13:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_13>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 34",null,"Reject counter 14","Rejects.###MNR.14","###INDEX:Rejects.###MNR.14:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_14>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 36",null,"Reject counter 15","Rejects.###MNR.15","###INDEX:Rejects.###MNR.15:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_15>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 38",null,"Reject counter 16","Rejects.###MNR.16","###INDEX:Rejects.###MNR.16:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_16>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DW 40","Bit 0-16","Reject counter 17-32 exist",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_vorhanden_2>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DW 41","Bit 0-16","Reject counter 17-32 has taken place ",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_statt_2>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 48",null,"Reject counter 17","Rejects.###MNR.17","###INDEX:Rejects.###MNR.17:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_17>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 50",null,"Reject counter 18","Rejects.###MNR.18","###INDEX:Rejects.###MNR.18:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_18>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 52",null,"Reject counter 19","Rejects.###MNR.19","###INDEX:Rejects.###MNR.19:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_19>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 54",null,"Reject counter 20","Rejects.###MNR.20","###INDEX:Rejects.###MNR.20:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_20>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 56",null,"Reject counter 21","Rejects.###MNR.21","###INDEX:Rejects.###MNR.21:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_21>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 58",null,"Reject counter 22","Rejects.###MNR.22","###INDEX:Rejects.###MNR.22:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_22>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 60",null,"Reject counter 23","Rejects.###MNR.23","###INDEX:Rejects.###MNR.23:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_23>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 62",null,"Reject counter 24","Rejects.###MNR.24","###INDEX:Rejects.###MNR.24:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_24>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 64",null,"Reject counter 25","Rejects.###MNR.25","###INDEX:Rejects.###MNR.25:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_25>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 66",null,"Reject counter 26","Rejects.###MNR.26","###INDEX:Rejects.###MNR.26:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_26>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 68",null,"Reject counter 27","Rejects.###MNR.27","###INDEX:Rejects.###MNR.27:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_27>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 70",null,"Reject counter 28","Rejects.###MNR.28","###INDEX:Rejects.###MNR.28:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_28>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 72",null,"Reject counter 29","Rejects.###MNR.29","###INDEX:Rejects.###MNR.29:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_29>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 74",null,"Reject counter 30","Rejects.###MNR.30","###INDEX:Rejects.###MNR.30:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_30>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 76",null,"Reject counter 31","Rejects.###MNR.31","###INDEX:Rejects.###MNR.31:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_31>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 78",null,"Reject counter 32","Rejects.###MNR.32","###INDEX:Rejects.###MNR.32:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_32>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DW 80","Bit 0-16","Reject counter 33-48 exist",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_vorhanden_3>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DW 81","Bit 0-16","Reject counter 33-48 has taken place ",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_statt_3>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 88",null,"Reject counter 33","Rejects.###MNR.33","###INDEX:Rejects.###MNR.33:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_33>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 90",null,"Reject counter 34","Rejects.###MNR.34","###INDEX:Rejects.###MNR.34:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_34>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 92",null,"Reject counter 35","Rejects.###MNR.35","###INDEX:Rejects.###MNR.35:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_35>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 94",null,"Reject counter 36","Rejects.###MNR.36","###INDEX:Rejects.###MNR.36:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_36>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 96",null,"Reject counter 37","Rejects.###MNR.37","###INDEX:Rejects.###MNR.37:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_37>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 98",null,"Reject counter 38","Rejects.###MNR.38","###INDEX:Rejects.###MNR.38:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_38>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 100",null,"Reject counter 39","Rejects.###MNR.39","###INDEX:Rejects.###MNR.39:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_39>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 102",null,"Reject counter 40","Rejects.###MNR.40","###INDEX:Rejects.###MNR.40:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_40>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 104",null,"Reject counter 41","Rejects.###MNR.41","###INDEX:Rejects.###MNR.41:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_41>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 106",null,"Reject counter 42","Rejects.###MNR.42","###INDEX:Rejects.###MNR.42:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_42>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 108",null,"Reject counter 43","Rejects.###MNR.43","###INDEX:Rejects.###MNR.43:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_43>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 110",null,"Reject counter 44","Rejects.###MNR.44","###INDEX:Rejects.###MNR.44:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_44>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 112",null,"Reject counter 45","Rejects.###MNR.45","###INDEX:Rejects.###MNR.45:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_45>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 114",null,"Reject counter 46","Rejects.###MNR.46","###INDEX:Rejects.###MNR.46:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_46>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 116",null,"Reject counter 47","Rejects.###MNR.47","###INDEX:Rejects.###MNR.47:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_47>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD 118",null,"Reject counter 48","Rejects.###MNR.48","###INDEX:Rejects.###MNR.48:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_48>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","###SDR[REJ]"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:104+16[FREJ]:ADDR","Bit 0-16","Rejectcounter  ###ADDR:33+16[FREJ]:ADDR - ###ADDR:48+16[FREJ]:ADDR has taken place",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_vorhanden_####ADDR:3+1[FREJ]:ADDR>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:105+16[FREJ]:ADDR","Bit 0-16","Rejectcounter  ###ADDR:33+16[FREJ]:ADDR - ###ADDR:48+16[FREJ]:ADDR has taken place",null,null,"Ch1.###MNR_T_auswurfz<.m###MNR_auswz_statt_###ADDR:3+1[FREJ]:ADDR>[W]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:112+16[FREJ]:ADDR",null,"Reject counter ###ADDR:33+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:33+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:33+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:33+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:114+16[FREJ]:ADDR",null,"Reject counter ###ADDR:34+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:34+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:34+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:34+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:116+16[FREJ]:ADDR",null,"Reject counter ###ADDR:35+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:35+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:35+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:35+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:118+16[FREJ]:ADDR",null,"Reject counter ###ADDR:36+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:36+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:36+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:36+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:120+16[FREJ]:ADDR",null,"Reject counter ###ADDR:37+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:37+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:37+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:37+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:122+16[FREJ]:ADDR",null,"Reject counter ###ADDR:38+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:38+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:38+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:38+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:124+16[FREJ]:ADDR",null,"Reject counter ###ADDR:39+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:39+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:39+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:39+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:126+16[FREJ]:ADDR",null,"Reject counter ###ADDR:40+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:40+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:40+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:40+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:128+16[FREJ]:ADDR",null,"Reject counter ###ADDR:41+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:41+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:41+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:41+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:130+16[FREJ]:ADDR",null,"Reject counter ###ADDR:42+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:42+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:42+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:42+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:132+16[FREJ]:ADDR",null,"Reject counter ###ADDR:43+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:43+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:43+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:43+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:134+16[FREJ]:ADDR",null,"Reject counter ###ADDR:44+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:44+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:44+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:44+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:136+16[FREJ]:ADDR",null,"Reject counter ###ADDR:45+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:45+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:45+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:45+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:138+16[FREJ]:ADDR",null,"Reject counter ###ADDR:46+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:46+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:46+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:46+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:140+16[FREJ]:ADDR",null,"Reject counter ###ADDR:47+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:47+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:47+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:47+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","DD ###ADDR:142+16[FREJ]:ADDR",null,"Reject counter ###ADDR:48+16[FREJ]:ADDR","Rejects.###MNR.###ADDR:48+16[FREJ]:ADDR","###INDEX:Rejects.###MNR.###ADDR:48+16[FREJ]:ADDR:INDEX","Ch1.###MNR_T_auswurfz<.m###MNR_auswz_###ADDR:48+16[FREJ]:ADDR>[DW]{p}"]
["###IF MITAUSWURFZAEHLERN###41","###EDR[REJ]"]

{"sheet":"StandardAllgemein","index":2,"n_rows":23,"n_cols":7,"rows_kept":23,"flags":["formulas_cached_only"]}
["Common Standard"]
[1,"###OVERVIEW"]
[21,"DB 40: ","Cyclic process data of the machine line "]
[1,"###MAIN"]
[1,"DB 40 Allgemeine Prozeßdaten"]
[41,"DW 0","Bit 0","Key-operated switch 1",null,null,"Ch1.T_zyk_linie<.schluessel_1>[B]{p}"]
[41,null,"Bit 1","Key-operated switch 2",null,null,"Ch1.T_zyk_linie<.schluessel_2>[B]{p}"]
[41,null,"Bit 2","Key-operated switch 3",null,null,"Ch1.T_zyk_linie<.schluessel_3>[B]{p}"]
[41,null,"Bit 5","special symbol for the malfunction line",null,null,"Ch1.T_zyk_linie<.achtung>[B]{p}"]
[41,"DW 10",null,"Lifecounter to PLC Steuerung",null,null,"Ch1.T_zyk_linie<.leben_hin>[W]{p}"]
[41,"DW 11",null,"Lifecounter from PLC Steuerung",null,null,"Ch1.T_zyk_linie<.leben_zur>[W]{p}"]
[31,"DW 20-22","Materialchange"]
[41,"DW 20",null,"Current machine  (1-5)",null,null,"Ch1.T_zyk_linie<.mw_aktmaschine>[W]{r}"]
[41,"DW 21",null,"Step chain number (1000...5999)",null,null,"Ch1.T_zyk_linie<.mw_schritt_am>[W]{r}"]
[41,"DW 22",null,"Manual intervention",null,null,"Ch1.T_zyk_linie<.mw_handein>[W]{r}"]
[41,"DW 22","Bit 0","Hand",null,null,"Ch1.T_zyk_linie<.mw_handein>[W]{r}"]
[41,null,"Bit 1","Service hand"]
[41,null,"Bit 2","Reset"]
[41,null,"Bit 3","Start"]
[41,null,"Bit 4","Sichtkontrolle"]
[41,null,"Bit 8","With confirmation"]
[41,"DW 23","Bit 0","Eingaben sperren",null,null,"Ch1.T_zyk_linie<.mw_keineeing>[B]{r}"]
[41,"DW 35","Bit 0","Sperre Bildsprung",null,null,"Ch1.T_zyk_linie<.li_bildsprung>[B]{r}"]

{"sheet":"ProfiBus_Standard","index":3,"n_rows":110,"n_cols":7,"rows_kept":110,"flags":["formulas_cached_only"]}
["ProfiBus_Standard","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 41: ","Profibus"]
[1,"###MAIN"]
[1,"DB 41 Profibus"]
[41,"Bit 0",null,"Module exists"]
[41,"Bit 1",null,"Module does not respond"]
[41,"Bit 2",null,"Module fault"]
[41,"Bit 3",null,"Bus fault"]
[41,"Bit 8-15",null,"Fault byte"]
[21,"DB41","Profibus Machine ###MNR"]
[41,"DW ###ADDR:1+100[MNR]:ADDR",null,"Module 1","Profibus.###MNR.1","###INDEX:Profibus.###MNR.1:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:0+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:2+100[MNR]:ADDR",null,"Module 2","Profibus.###MNR.2","###INDEX:Profibus.###MNR.2:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:1+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:3+100[MNR]:ADDR",null,"Module 3","Profibus.###MNR.3","###INDEX:Profibus.###MNR.3:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:2+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:4+100[MNR]:ADDR",null,"Module 4","Profibus.###MNR.4","###INDEX:Profibus.###MNR.4:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:3+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:5+100[MNR]:ADDR",null,"Module 5","Profibus.###MNR.5","###INDEX:Profibus.###MNR.5:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:4+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:6+100[MNR]:ADDR",null,"Module 6","Profibus.###MNR.6","###INDEX:Profibus.###MNR.6:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:5+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:7+100[MNR]:ADDR",null,"Module 7","Profibus.###MNR.7","###INDEX:Profibus.###MNR.7:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:6+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:8+100[MNR]:ADDR",null,"Module 8","Profibus.###MNR.8","###INDEX:Profibus.###MNR.8:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:7+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:9+100[MNR]:ADDR",null,"Module 9","Profibus.###MNR.9","###INDEX:Profibus.###MNR.9:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:8+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:10+100[MNR]:ADDR",null,"Module 10","Profibus.###MNR.10","###INDEX:Profibus.###MNR.10:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:9+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:11+100[MNR]:ADDR",null,"Module 11","Profibus.###MNR.11","###INDEX:Profibus.###MNR.11:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:10+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:12+100[MNR]:ADDR",null,"Module 12","Profibus.###MNR.12","###INDEX:Profibus.###MNR.12:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:11+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:13+100[MNR]:ADDR",null,"Module 13","Profibus.###MNR.13","###INDEX:Profibus.###MNR.13:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:12+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:14+100[MNR]:ADDR",null,"Module 14","Profibus.###MNR.14","###INDEX:Profibus.###MNR.14:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:13+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:15+100[MNR]:ADDR",null,"Module 15","Profibus.###MNR.15","###INDEX:Profibus.###MNR.15:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:14+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:16+100[MNR]:ADDR",null,"Module 16","Profibus.###MNR.16","###INDEX:Profibus.###MNR.16:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:15+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:17+100[MNR]:ADDR",null,"Module 17","Profibus.###MNR.17","###INDEX:Profibus.###MNR.17:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:16+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:18+100[MNR]:ADDR",null,"Module 18","Profibus.###MNR.18","###INDEX:Profibus.###MNR.18:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:17+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:19+100[MNR]:ADDR",null,"Module 19","Profibus.###MNR.19","###INDEX:Profibus.###MNR.19:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:18+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:20+100[MNR]:ADDR",null,"Module 20","Profibus.###MNR.20","###INDEX:Profibus.###MNR.20:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:19+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:21+100[MNR]:ADDR",null,"Module 21","Profibus.###MNR.21","###INDEX:Profibus.###MNR.21:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:20+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:22+100[MNR]:ADDR",null,"Module 22","Profibus.###MNR.22","###INDEX:Profibus.###MNR.22:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:21+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:23+100[MNR]:ADDR",null,"Module 23","Profibus.###MNR.23","###INDEX:Profibus.###MNR.23:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:22+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:24+100[MNR]:ADDR",null,"Module 24","Profibus.###MNR.24","###INDEX:Profibus.###MNR.24:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:23+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:25+100[MNR]:ADDR",null,"Module 25","Profibus.###MNR.25","###INDEX:Profibus.###MNR.25:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:24+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:26+100[MNR]:ADDR",null,"Module 26","Profibus.###MNR.26","###INDEX:Profibus.###MNR.26:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:25+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:27+100[MNR]:ADDR",null,"Module 27","Profibus.###MNR.27","###INDEX:Profibus.###MNR.27:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:26+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:28+100[MNR]:ADDR",null,"Module 28","Profibus.###MNR.28","###INDEX:Profibus.###MNR.28:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:27+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:29+100[MNR]:ADDR",null,"Module 29","Profibus.###MNR.29","###INDEX:Profibus.###MNR.29:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:28+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:30+100[MNR]:ADDR",null,"Module 30","Profibus.###MNR.30","###INDEX:Profibus.###MNR.30:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:29+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:31+100[MNR]:ADDR",null,"Module 31","Profibus.###MNR.31","###INDEX:Profibus.###MNR.31:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:30+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:32+100[MNR]:ADDR",null,"Module 32","Profibus.###MNR.32","###INDEX:Profibus.###MNR.32:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:31+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:33+100[MNR]:ADDR",null,"Module 33","Profibus.###MNR.33","###INDEX:Profibus.###MNR.33:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:32+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:34+100[MNR]:ADDR",null,"Module 34","Profibus.###MNR.34","###INDEX:Profibus.###MNR.34:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:33+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:35+100[MNR]:ADDR",null,"Module 35","Profibus.###MNR.35","###INDEX:Profibus.###MNR.35:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:34+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:36+100[MNR]:ADDR",null,"Module 36","Profibus.###MNR.36","###INDEX:Profibus.###MNR.36:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:35+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:37+100[MNR]:ADDR",null,"Module 37","Profibus.###MNR.37","###INDEX:Profibus.###MNR.37:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:36+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:38+100[MNR]:ADDR",null,"Module 38","Profibus.###MNR.38","###INDEX:Profibus.###MNR.38:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:37+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:39+100[MNR]:ADDR",null,"Module 39","Profibus.###MNR.39","###INDEX:Profibus.###MNR.39:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:38+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:40+100[MNR]:ADDR",null,"Module 40","Profibus.###MNR.40","###INDEX:Profibus.###MNR.40:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:39+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:41+100[MNR]:ADDR",null,"Module 41","Profibus.###MNR.41","###INDEX:Profibus.###MNR.41:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:40+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:42+100[MNR]:ADDR",null,"Module 42","Profibus.###MNR.42","###INDEX:Profibus.###MNR.42:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:41+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:43+100[MNR]:ADDR",null,"Module 43","Profibus.###MNR.43","###INDEX:Profibus.###MNR.43:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:42+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:44+100[MNR]:ADDR",null,"Module 44","Profibus.###MNR.44","###INDEX:Profibus.###MNR.44:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:43+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:45+100[MNR]:ADDR",null,"Module 45","Profibus.###MNR.45","###INDEX:Profibus.###MNR.45:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:44+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:46+100[MNR]:ADDR",null,"Module 46","Profibus.###MNR.46","###INDEX:Profibus.###MNR.46:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:45+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:47+100[MNR]:ADDR",null,"Module 47","Profibus.###MNR.47","###INDEX:Profibus.###MNR.47:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:46+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:48+100[MNR]:ADDR",null,"Module 48","Profibus.###MNR.48","###INDEX:Profibus.###MNR.48:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:47+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:49+100[MNR]:ADDR",null,"Module 49","Profibus.###MNR.49","###INDEX:Profibus.###MNR.49:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:48+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:50+100[MNR]:ADDR",null,"Module 50","Profibus.###MNR.50","###INDEX:Profibus.###MNR.50:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:49+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:51+100[MNR]:ADDR",null,"Module 51","Profibus.###MNR.51","###INDEX:Profibus.###MNR.51:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:50+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:52+100[MNR]:ADDR",null,"Module 52","Profibus.###MNR.52","###INDEX:Profibus.###MNR.52:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:51+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:53+100[MNR]:ADDR",null,"Module 53","Profibus.###MNR.53","###INDEX:Profibus.###MNR.53:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:52+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:54+100[MNR]:ADDR",null,"Module 54","Profibus.###MNR.54","###INDEX:Profibus.###MNR.54:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:53+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:55+100[MNR]:ADDR",null,"Module 55","Profibus.###MNR.55","###INDEX:Profibus.###MNR.55:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:54+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:56+100[MNR]:ADDR",null,"Module 56","Profibus.###MNR.56","###INDEX:Profibus.###MNR.56:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:55+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:57+100[MNR]:ADDR",null,"Module 57","Profibus.###MNR.57","###INDEX:Profibus.###MNR.57:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:56+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:58+100[MNR]:ADDR",null,"Module 58","Profibus.###MNR.58","###INDEX:Profibus.###MNR.58:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:57+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:59+100[MNR]:ADDR",null,"Module 59","Profibus.###MNR.59","###INDEX:Profibus.###MNR.59:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:58+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:60+100[MNR]:ADDR",null,"Module 60","Profibus.###MNR.60","###INDEX:Profibus.###MNR.60:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:59+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:61+100[MNR]:ADDR",null,"Module 61","Profibus.###MNR.61","###INDEX:Profibus.###MNR.61:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:60+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:62+100[MNR]:ADDR",null,"Module 62","Profibus.###MNR.62","###INDEX:Profibus.###MNR.62:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:61+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:63+100[MNR]:ADDR",null,"Module 63","Profibus.###MNR.63","###INDEX:Profibus.###MNR.63:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:62+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:64+100[MNR]:ADDR",null,"Module 64","Profibus.###MNR.64","###INDEX:Profibus.###MNR.64:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:63+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:65+100[MNR]:ADDR",null,"Module 65","Profibus.###MNR.65","###INDEX:Profibus.###MNR.65:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:64+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:66+100[MNR]:ADDR",null,"Module 66","Profibus.###MNR.66","###INDEX:Profibus.###MNR.66:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:65+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:67+100[MNR]:ADDR",null,"Module 67","Profibus.###MNR.67","###INDEX:Profibus.###MNR.67:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:66+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:68+100[MNR]:ADDR",null,"Module 68","Profibus.###MNR.68","###INDEX:Profibus.###MNR.68:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:67+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:69+100[MNR]:ADDR",null,"Module 69","Profibus.###MNR.69","###INDEX:Profibus.###MNR.69:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:68+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:70+100[MNR]:ADDR",null,"Module 70","Profibus.###MNR.70","###INDEX:Profibus.###MNR.70:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:69+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:71+100[MNR]:ADDR",null,"Module 71","Profibus.###MNR.71","###INDEX:Profibus.###MNR.71:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:70+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:72+100[MNR]:ADDR",null,"Module 72","Profibus.###MNR.72","###INDEX:Profibus.###MNR.72:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:71+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:73+100[MNR]:ADDR",null,"Module 73","Profibus.###MNR.73","###INDEX:Profibus.###MNR.73:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:72+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:74+100[MNR]:ADDR",null,"Module 74","Profibus.###MNR.74","###INDEX:Profibus.###MNR.74:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:73+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:75+100[MNR]:ADDR",null,"Module 75","Profibus.###MNR.75","###INDEX:Profibus.###MNR.75:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:74+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:76+100[MNR]:ADDR",null,"Module 76","Profibus.###MNR.76","###INDEX:Profibus.###MNR.76:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:75+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:77+100[MNR]:ADDR",null,"Module 77","Profibus.###MNR.77","###INDEX:Profibus.###MNR.77:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:76+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:78+100[MNR]:ADDR",null,"Module 78","Profibus.###MNR.78","###INDEX:Profibus.###MNR.78:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:77+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:79+100[MNR]:ADDR",null,"Module 79","Profibus.###MNR.79","###INDEX:Profibus.###MNR.79:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:78+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:80+100[MNR]:ADDR",null,"Module 80","Profibus.###MNR.80","###INDEX:Profibus.###MNR.80:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:79+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:81+100[MNR]:ADDR",null,"Module 81","Profibus.###MNR.81","###INDEX:Profibus.###MNR.81:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:80+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:82+100[MNR]:ADDR",null,"Module 82","Profibus.###MNR.82","###INDEX:Profibus.###MNR.82:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:81+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:83+100[MNR]:ADDR",null,"Module 83","Profibus.###MNR.83","###INDEX:Profibus.###MNR.83:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:82+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:84+100[MNR]:ADDR",null,"Module 84","Profibus.###MNR.84","###INDEX:Profibus.###MNR.84:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:83+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:85+100[MNR]:ADDR",null,"Module 85","Profibus.###MNR.85","###INDEX:Profibus.###MNR.85:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:84+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:86+100[MNR]:ADDR",null,"Module 86","Profibus.###MNR.86","###INDEX:Profibus.###MNR.86:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:85+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:87+100[MNR]:ADDR",null,"Module 87","Profibus.###MNR.87","###INDEX:Profibus.###MNR.87:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:86+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:88+100[MNR]:ADDR",null,"Module 88","Profibus.###MNR.88","###INDEX:Profibus.###MNR.88:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:87+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:89+100[MNR]:ADDR",null,"Module 89","Profibus.###MNR.89","###INDEX:Profibus.###MNR.89:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:88+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:90+100[MNR]:ADDR",null,"Module 90","Profibus.###MNR.90","###INDEX:Profibus.###MNR.90:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:89+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:91+100[MNR]:ADDR",null,"Module 91","Profibus.###MNR.91","###INDEX:Profibus.###MNR.91:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:90+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:92+100[MNR]:ADDR",null,"Module 92","Profibus.###MNR.92","###INDEX:Profibus.###MNR.92:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:91+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:93+100[MNR]:ADDR",null,"Module 93","Profibus.###MNR.93","###INDEX:Profibus.###MNR.93:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:92+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:94+100[MNR]:ADDR",null,"Module 94","Profibus.###MNR.94","###INDEX:Profibus.###MNR.94:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:93+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:95+100[MNR]:ADDR",null,"Module 95","Profibus.###MNR.95","###INDEX:Profibus.###MNR.95:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:94+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:96+100[MNR]:ADDR",null,"Module 96","Profibus.###MNR.96","###INDEX:Profibus.###MNR.96:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:95+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:97+100[MNR]:ADDR",null,"Module 97","Profibus.###MNR.97","###INDEX:Profibus.###MNR.97:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:96+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:98+100[MNR]:ADDR",null,"Module 98","Profibus.###MNR.98","###INDEX:Profibus.###MNR.98:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:97+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:99+100[MNR]:ADDR",null,"Module 99","Profibus.###MNR.99","###INDEX:Profibus.###MNR.99:INDEX","Ch1.T_profibus<.profibus>[W ###ADDR:98+100[MNR]:ADDR]{p}"]

{"sheet":"FibreOptic_Standard","index":4,"n_rows":110,"n_cols":7,"rows_kept":110,"flags":["formulas_cached_only"]}
["FibreOptic_Standard","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 42: ","Fibre Optic"]
[1,"###MAIN"]
[2,"DB 42 Fibre Optic"]
[41,"Bit 0",null,"Module exists"]
[41,"Bit 1",null,"Module does not respond"]
[41,"Bit 2",null,"Module fault"]
[41,"Bit 3",null,"Bus fault"]
[41,"Bit 8-15",null,"Fault byte"]
[21,"Fibre Optic Machine ###MNR"]
[41,"DW ###ADDR:1+100[MNR]:ADDR",null,"Module 1","FibreOptic.###MNR.1","###INDEX:FibreOptic.###MNR.1:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:0+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:2+100[MNR]:ADDR",null,"Module 2","FibreOptic.###MNR.2","###INDEX:FibreOptic.###MNR.2:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:1+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:3+100[MNR]:ADDR",null,"Module 3","FibreOptic.###MNR.3","###INDEX:FibreOptic.###MNR.3:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:2+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:4+100[MNR]:ADDR",null,"Module 4","FibreOptic.###MNR.4","###INDEX:FibreOptic.###MNR.4:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:3+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:5+100[MNR]:ADDR",null,"Module 5","FibreOptic.###MNR.5","###INDEX:FibreOptic.###MNR.5:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:4+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:6+100[MNR]:ADDR",null,"Module 6","FibreOptic.###MNR.6","###INDEX:FibreOptic.###MNR.6:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:5+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:7+100[MNR]:ADDR",null,"Module 7","FibreOptic.###MNR.7","###INDEX:FibreOptic.###MNR.7:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:6+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:8+100[MNR]:ADDR",null,"Module 8","FibreOptic.###MNR.8","###INDEX:FibreOptic.###MNR.8:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:7+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:9+100[MNR]:ADDR",null,"Module 9","FibreOptic.###MNR.9","###INDEX:FibreOptic.###MNR.9:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:8+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:10+100[MNR]:ADDR",null,"Module 10","FibreOptic.###MNR.10","###INDEX:FibreOptic.###MNR.10:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:9+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:11+100[MNR]:ADDR",null,"Module 11","FibreOptic.###MNR.11","###INDEX:FibreOptic.###MNR.11:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:10+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:12+100[MNR]:ADDR",null,"Module 12","FibreOptic.###MNR.12","###INDEX:FibreOptic.###MNR.12:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:11+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:13+100[MNR]:ADDR",null,"Module 13","FibreOptic.###MNR.13","###INDEX:FibreOptic.###MNR.13:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:12+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:14+100[MNR]:ADDR",null,"Module 14","FibreOptic.###MNR.14","###INDEX:FibreOptic.###MNR.14:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:13+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:15+100[MNR]:ADDR",null,"Module 15","FibreOptic.###MNR.15","###INDEX:FibreOptic.###MNR.15:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:14+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:16+100[MNR]:ADDR",null,"Module 16","FibreOptic.###MNR.16","###INDEX:FibreOptic.###MNR.16:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:15+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:17+100[MNR]:ADDR",null,"Module 17","FibreOptic.###MNR.17","###INDEX:FibreOptic.###MNR.17:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:16+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:18+100[MNR]:ADDR",null,"Module 18","FibreOptic.###MNR.18","###INDEX:FibreOptic.###MNR.18:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:17+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:19+100[MNR]:ADDR",null,"Module 19","FibreOptic.###MNR.19","###INDEX:FibreOptic.###MNR.19:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:18+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:20+100[MNR]:ADDR",null,"Module 20","FibreOptic.###MNR.20","###INDEX:FibreOptic.###MNR.20:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:19+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:21+100[MNR]:ADDR",null,"Module 21","FibreOptic.###MNR.21","###INDEX:FibreOptic.###MNR.21:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:20+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:22+100[MNR]:ADDR",null,"Module 22","FibreOptic.###MNR.22","###INDEX:FibreOptic.###MNR.22:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:21+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:23+100[MNR]:ADDR",null,"Module 23","FibreOptic.###MNR.23","###INDEX:FibreOptic.###MNR.23:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:22+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:24+100[MNR]:ADDR",null,"Module 24","FibreOptic.###MNR.24","###INDEX:FibreOptic.###MNR.24:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:23+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:25+100[MNR]:ADDR",null,"Module 25","FibreOptic.###MNR.25","###INDEX:FibreOptic.###MNR.25:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:24+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:26+100[MNR]:ADDR",null,"Module 26","FibreOptic.###MNR.26","###INDEX:FibreOptic.###MNR.26:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:25+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:27+100[MNR]:ADDR",null,"Module 27","FibreOptic.###MNR.27","###INDEX:FibreOptic.###MNR.27:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:26+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:28+100[MNR]:ADDR",null,"Module 28","FibreOptic.###MNR.28","###INDEX:FibreOptic.###MNR.28:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:27+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:29+100[MNR]:ADDR",null,"Module 29","FibreOptic.###MNR.29","###INDEX:FibreOptic.###MNR.29:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:28+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:30+100[MNR]:ADDR",null,"Module 30","FibreOptic.###MNR.30","###INDEX:FibreOptic.###MNR.30:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:29+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:31+100[MNR]:ADDR",null,"Module 31","FibreOptic.###MNR.31","###INDEX:FibreOptic.###MNR.31:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:30+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:32+100[MNR]:ADDR",null,"Module 32","FibreOptic.###MNR.32","###INDEX:FibreOptic.###MNR.32:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:31+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:33+100[MNR]:ADDR",null,"Module 33","FibreOptic.###MNR.33","###INDEX:FibreOptic.###MNR.33:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:32+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:34+100[MNR]:ADDR",null,"Module 34","FibreOptic.###MNR.34","###INDEX:FibreOptic.###MNR.34:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:33+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:35+100[MNR]:ADDR",null,"Module 35","FibreOptic.###MNR.35","###INDEX:FibreOptic.###MNR.35:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:34+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:36+100[MNR]:ADDR",null,"Module 36","FibreOptic.###MNR.36","###INDEX:FibreOptic.###MNR.36:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:35+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:37+100[MNR]:ADDR",null,"Module 37","FibreOptic.###MNR.37","###INDEX:FibreOptic.###MNR.37:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:36+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:38+100[MNR]:ADDR",null,"Module 38","FibreOptic.###MNR.38","###INDEX:FibreOptic.###MNR.38:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:37+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:39+100[MNR]:ADDR",null,"Module 39","FibreOptic.###MNR.39","###INDEX:FibreOptic.###MNR.39:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:38+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:40+100[MNR]:ADDR",null,"Module 40","FibreOptic.###MNR.40","###INDEX:FibreOptic.###MNR.40:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:39+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:41+100[MNR]:ADDR",null,"Module 41","FibreOptic.###MNR.41","###INDEX:FibreOptic.###MNR.41:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:40+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:42+100[MNR]:ADDR",null,"Module 42","FibreOptic.###MNR.42","###INDEX:FibreOptic.###MNR.42:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:41+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:43+100[MNR]:ADDR",null,"Module 43","FibreOptic.###MNR.43","###INDEX:FibreOptic.###MNR.43:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:42+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:44+100[MNR]:ADDR",null,"Module 44","FibreOptic.###MNR.44","###INDEX:FibreOptic.###MNR.44:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:43+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:45+100[MNR]:ADDR",null,"Module 45","FibreOptic.###MNR.45","###INDEX:FibreOptic.###MNR.45:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:44+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:46+100[MNR]:ADDR",null,"Module 46","FibreOptic.###MNR.46","###INDEX:FibreOptic.###MNR.46:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:45+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:47+100[MNR]:ADDR",null,"Module 47","FibreOptic.###MNR.47","###INDEX:FibreOptic.###MNR.47:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:46+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:48+100[MNR]:ADDR",null,"Module 48","FibreOptic.###MNR.48","###INDEX:FibreOptic.###MNR.48:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:47+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:49+100[MNR]:ADDR",null,"Module 49","FibreOptic.###MNR.49","###INDEX:FibreOptic.###MNR.49:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:48+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:50+100[MNR]:ADDR",null,"Module 50","FibreOptic.###MNR.50","###INDEX:FibreOptic.###MNR.50:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:49+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:51+100[MNR]:ADDR",null,"Module 51","FibreOptic.###MNR.51","###INDEX:FibreOptic.###MNR.51:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:50+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:52+100[MNR]:ADDR",null,"Module 52","FibreOptic.###MNR.52","###INDEX:FibreOptic.###MNR.52:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:51+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:53+100[MNR]:ADDR",null,"Module 53","FibreOptic.###MNR.53","###INDEX:FibreOptic.###MNR.53:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:52+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:54+100[MNR]:ADDR",null,"Module 54","FibreOptic.###MNR.54","###INDEX:FibreOptic.###MNR.54:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:53+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:55+100[MNR]:ADDR",null,"Module 55","FibreOptic.###MNR.55","###INDEX:FibreOptic.###MNR.55:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:54+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:56+100[MNR]:ADDR",null,"Module 56","FibreOptic.###MNR.56","###INDEX:FibreOptic.###MNR.56:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:55+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:57+100[MNR]:ADDR",null,"Module 57","FibreOptic.###MNR.57","###INDEX:FibreOptic.###MNR.57:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:56+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:58+100[MNR]:ADDR",null,"Module 58","FibreOptic.###MNR.58","###INDEX:FibreOptic.###MNR.58:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:57+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:59+100[MNR]:ADDR",null,"Module 59","FibreOptic.###MNR.59","###INDEX:FibreOptic.###MNR.59:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:58+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:60+100[MNR]:ADDR",null,"Module 60","FibreOptic.###MNR.60","###INDEX:FibreOptic.###MNR.60:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:59+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:61+100[MNR]:ADDR",null,"Module 61","FibreOptic.###MNR.61","###INDEX:FibreOptic.###MNR.61:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:60+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:62+100[MNR]:ADDR",null,"Module 62","FibreOptic.###MNR.62","###INDEX:FibreOptic.###MNR.62:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:61+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:63+100[MNR]:ADDR",null,"Module 63","FibreOptic.###MNR.63","###INDEX:FibreOptic.###MNR.63:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:62+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:64+100[MNR]:ADDR",null,"Module 64","FibreOptic.###MNR.64","###INDEX:FibreOptic.###MNR.64:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:63+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:65+100[MNR]:ADDR",null,"Module 65","FibreOptic.###MNR.65","###INDEX:FibreOptic.###MNR.65:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:64+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:66+100[MNR]:ADDR",null,"Module 66","FibreOptic.###MNR.66","###INDEX:FibreOptic.###MNR.66:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:65+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:67+100[MNR]:ADDR",null,"Module 67","FibreOptic.###MNR.67","###INDEX:FibreOptic.###MNR.67:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:66+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:68+100[MNR]:ADDR",null,"Module 68","FibreOptic.###MNR.68","###INDEX:FibreOptic.###MNR.68:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:67+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:69+100[MNR]:ADDR",null,"Module 69","FibreOptic.###MNR.69","###INDEX:FibreOptic.###MNR.69:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:68+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:70+100[MNR]:ADDR",null,"Module 70","FibreOptic.###MNR.70","###INDEX:FibreOptic.###MNR.70:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:69+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:71+100[MNR]:ADDR",null,"Module 71","FibreOptic.###MNR.71","###INDEX:FibreOptic.###MNR.71:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:70+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:72+100[MNR]:ADDR",null,"Module 72","FibreOptic.###MNR.72","###INDEX:FibreOptic.###MNR.72:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:71+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:73+100[MNR]:ADDR",null,"Module 73","FibreOptic.###MNR.73","###INDEX:FibreOptic.###MNR.73:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:72+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:74+100[MNR]:ADDR",null,"Module 74","FibreOptic.###MNR.74","###INDEX:FibreOptic.###MNR.74:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:73+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:75+100[MNR]:ADDR",null,"Module 75","FibreOptic.###MNR.75","###INDEX:FibreOptic.###MNR.75:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:74+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:76+100[MNR]:ADDR",null,"Module 76","FibreOptic.###MNR.76","###INDEX:FibreOptic.###MNR.76:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:75+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:77+100[MNR]:ADDR",null,"Module 77","FibreOptic.###MNR.77","###INDEX:FibreOptic.###MNR.77:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:76+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:78+100[MNR]:ADDR",null,"Module 78","FibreOptic.###MNR.78","###INDEX:FibreOptic.###MNR.78:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:77+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:79+100[MNR]:ADDR",null,"Module 79","FibreOptic.###MNR.79","###INDEX:FibreOptic.###MNR.79:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:78+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:80+100[MNR]:ADDR",null,"Module 80","FibreOptic.###MNR.80","###INDEX:FibreOptic.###MNR.80:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:79+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:81+100[MNR]:ADDR",null,"Module 81","FibreOptic.###MNR.81","###INDEX:FibreOptic.###MNR.81:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:80+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:82+100[MNR]:ADDR",null,"Module 82","FibreOptic.###MNR.82","###INDEX:FibreOptic.###MNR.82:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:81+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:83+100[MNR]:ADDR",null,"Module 83","FibreOptic.###MNR.83","###INDEX:FibreOptic.###MNR.83:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:82+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:84+100[MNR]:ADDR",null,"Module 84","FibreOptic.###MNR.84","###INDEX:FibreOptic.###MNR.84:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:83+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:85+100[MNR]:ADDR",null,"Module 85","FibreOptic.###MNR.85","###INDEX:FibreOptic.###MNR.85:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:84+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:86+100[MNR]:ADDR",null,"Module 86","FibreOptic.###MNR.86","###INDEX:FibreOptic.###MNR.86:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:85+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:87+100[MNR]:ADDR",null,"Module 87","FibreOptic.###MNR.87","###INDEX:FibreOptic.###MNR.87:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:86+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:88+100[MNR]:ADDR",null,"Module 88","FibreOptic.###MNR.88","###INDEX:FibreOptic.###MNR.88:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:87+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:89+100[MNR]:ADDR",null,"Module 89","FibreOptic.###MNR.89","###INDEX:FibreOptic.###MNR.89:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:88+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:90+100[MNR]:ADDR",null,"Module 90","FibreOptic.###MNR.90","###INDEX:FibreOptic.###MNR.90:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:89+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:91+100[MNR]:ADDR",null,"Module 91","FibreOptic.###MNR.91","###INDEX:FibreOptic.###MNR.91:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:90+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:92+100[MNR]:ADDR",null,"Module 92","FibreOptic.###MNR.92","###INDEX:FibreOptic.###MNR.92:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:91+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:93+100[MNR]:ADDR",null,"Module 93","FibreOptic.###MNR.93","###INDEX:FibreOptic.###MNR.93:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:92+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:94+100[MNR]:ADDR",null,"Module 94","FibreOptic.###MNR.94","###INDEX:FibreOptic.###MNR.94:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:93+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:95+100[MNR]:ADDR",null,"Module 95","FibreOptic.###MNR.95","###INDEX:FibreOptic.###MNR.95:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:94+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:96+100[MNR]:ADDR",null,"Module 96","FibreOptic.###MNR.96","###INDEX:FibreOptic.###MNR.96:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:95+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:97+100[MNR]:ADDR",null,"Module 97","FibreOptic.###MNR.97","###INDEX:FibreOptic.###MNR.97:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:96+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:98+100[MNR]:ADDR",null,"Module 98","FibreOptic.###MNR.98","###INDEX:FibreOptic.###MNR.98:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:97+100[MNR]:ADDR]{p}"]
[41,"DW ###ADDR:99+100[MNR]:ADDR",null,"Module 99","FibreOptic.###MNR.99","###INDEX:FibreOptic.###MNR.99:INDEX","Ch1.T_lwl<.lwl>[W ###ADDR:98+100[MNR]:ADDR]{p}"]

{"sheet":"PC_Diagnostics","index":5,"n_rows":57,"n_cols":7,"rows_kept":57,"flags":["formulas_cached_only"]}
["PC_Diagnostics"]
[1,"###OVERVIEW"]
[21,"DB 43: ","PC Diagnostics"]
[1,"###MAIN"]
[1,"DB 43 PC Diagnostics"]
[21,"DB 43","PC Diagnostics"]
[41,"DW 10",null,"Actual value corevoltage processor",null,null,"Ch1.T_diagnose<.mb_vccp1>[W]{p}"]
[41,"DW 11",null,"Setpoint corevoltage processor",null,null,"Ch1.T_diagnose<.mb_vccp1_set>[W]{p}"]
[41,"DW 12",null,"Internal"]
[41,"DW 13",null,"Internal"]
[41,"DW 14",null,"Internal"]
[41,"DW 15",null,"Internal"]
[41,"DW 16",null,"Actual value + 3,3 V",null,null,"Ch1.T_diagnose<.mb_volt_3_3>[W]{p}"]
[41,"DW 17",null,"Setpoint + 3,3 V",null,null,"Ch1.T_diagnose<.mb_volt_3_3_set>[W]{p}"]
[41,"DW 18",null,"Actual value + 5,0 V",null,null,"Ch1.T_diagnose<.mb_volt_5>[W]{p}"]
[41,"DW 19",null,"Setpoint + 5,0 V",null,null,"Ch1.T_diagnose<.mb_volt_5_set>[W]{p}"]
[41,"DW 20",null,"Actual value + 12,0 V",null,null,"Ch1.T_diagnose<.mb_volt_12>[W]{p}"]
[41,"DW 21",null,"Setpoint + 12,0 V",null,null,"Ch1.T_diagnose<.mb_volt_12_set>[W]{p}"]
[41,"DW 22",null,"Actual value - 12,0 V",null,null,"Ch1.T_diagnose<.mb_volt_12a>[W]{p}"]
[41,"DW 23",null,"Setpoint - 12,0 V",null,null,"Ch1.T_diagnose<.mb_volt_12a_set>[W]{p}"]
[41,"DW 24",null,"Actual value - 5,0 V",null,null,"Ch1.T_diagnose<.mb_volt_5a>[W]{p}"]
[41,"DW 25",null,"Setpoint - 5,0 V",null,null,"Ch1.T_diagnose<.mb_volt_5a_set>[W]{p}"]
[41,"DW 26",null,"Actual value buffer battery",null,null,"Ch1.T_diagnose<.mb_vbat>[W]{p}"]
[41,"DW 27",null,"Setpoint buffer battery",null,null,"Ch1.T_diagnose<.mb_vbat_set>[W]{p}"]
[41,"DW 28",null,"Actual value Temperatur 1",null,null,"Ch1.T_diagnose<.mb_temp_0>[W]{p}"]
[41,"DW 29",null,"Setpoint Temperatur 1",null,null,"Ch1.T_diagnose<.mb_temp_0_set>[W]{p}"]
[41,"DW 30",null,"Actual value Temperatur 2",null,null,"Ch1.T_diagnose<.mb_temp_1>[W]{p}"]
[41,"DW 31",null,"Setpoint Temperatur 2",null,null,"Ch1.T_diagnose<.mb_temp_1_set>[W]{p}"]
[41,"DW 32",null,"Actual value Temperatur 3",null,null,"Ch1.T_diagnose<.mb_temp_2>[W]{p}"]
[41,"DW 33",null,"Setpoint Temperatur 3",null,null,"Ch1.T_diagnose<.mb_temp_2_set>[W]{p}"]
[41,"DW 34",null,"Actual value Temperatur 4",null,null,"Ch1.T_diagnose<.mb_temp_3>[W]{p}"]
[41,"DW 35",null,"Setpoint Temperatur 4",null,null,"Ch1.T_diagnose<.mb_temp_3_set>[W]{p}"]
[41,"DW 36",null,"Actual value Temperatur 5",null,null,"Ch1.T_diagnose<.mb_temp_4>[W]{p}"]
[41,"DW 37",null,"Setpoint Temperatur 5",null,null,"Ch1.T_diagnose<.mb_temp_4_set>[W]{p}"]
[41,"DW 38",null,"Actual value Temperatur 6",null,null,"Ch1.T_diagnose<.mb_temp_5>[W]{p}"]
[41,"DW 39",null,"Setpoint Temperatur 6",null,null,"Ch1.T_diagnose<.mb_temp_5_set>[W]{p}"]
[41,"DW 40",null,"Actual value Temperatur 7",null,null,"Ch1.T_diagnose<.mb_temp_6>[W]{p}"]
[41,"DW 41",null,"Setpoint Temperatur 7",null,null,"Ch1.T_diagnose<.mb_temp_6_set>[W]{p}"]
[41,"DW 42",null,"Actual value Temperatur 8",null,null,"Ch1.T_diagnose<.mb_temp_7>[W]{p}"]
[41,"DW 43",null,"Setpoint Temperatur 8",null,null,"Ch1.T_diagnose<.mb_temp_7_set>[W]{p}"]
[41,"DW 44",null,"Actual value fan 1",null,null,"Ch1.T_diagnose<.mb_fan_0>[W]{p}"]
[41,"DW 45",null,"Setpoint fan 1",null,null,"Ch1.T_diagnose<.mb_fan_0_set>[W]{p}"]
[41,"DW 46",null,"Actual value fan 2",null,null,"Ch1.T_diagnose<.mb_fan_1>[W]{p}"]
[41,"DW 47",null,"Setpoint fan 2",null,null,"Ch1.T_diagnose<.mb_fan_1_set>[W]{p}"]
[41,"DW 48",null,"Actual value fan 3",null,null,"Ch1.T_diagnose<.mb_fan_2>[W]{p}"]
[41,"DW 49",null,"Setpoint fan 3",null,null,"Ch1.T_diagnose<.mb_fan_2_set>[W]{p}"]
[41,"DW 50",null,"Actual value fan 4",null,null,"Ch1.T_diagnose<.mb_fan_3>[W]{p}"]
[41,"DW 51",null,"Setpoint fan 4",null,null,"Ch1.T_diagnose<.mb_fan_3_set>[W]{p}"]
[21,"DB 44","PC Diagnostics"]
[41,"DW 10",null,"Temperature status",null,null,"Ch1.T_diagnose2<.mb_temp_ist>[W]{p}"]
[41,null,0,"Not enabled"]
[41,null,1,"Enabled and everything OK"]
[41,null,2,"Enabled and warning"]
[41,null,3,"Enabled and fault"]
[41,"DW 11",null,"Fan status",null,null,"Ch1.T_diagnose2<.mb_fan_ist>[W]{p}"]
[41,"DW 12",null,"Voltage status",null,null,"Ch1.T_diagnose2<.mb_volt_ist>[W]{p}"]
[41,"DW 13",null,"Battery status",null,null,"Ch1.T_diagnose2<.mb_batt_ist>[W]{p}"]

{"sheet":"EtherCAT","index":6,"n_rows":45,"n_cols":7,"rows_kept":45,"flags":["formulas_cached_only"]}
["EtherCAT"]
[1,"###OVERVIEW"]
[21,"DB 45: ","EtherCAT"]
[1,"###MAIN"]
[1,"DB 45 EtherCAT"]
[21,"DB 45","EtherCAT"]
[41,"DW 0","Bit 0","EtherCAT changed",null,null,"Ch1.T_ethercat<.ethercat_aender>[B]{w}"]
[41,null,"zur Steuerung"]
[41,"DW 10",null,"Module number",null,null,"Ch1.T_ethercat<.ethercat_nrzs>[W]{r}"]
[41,null,"von Steuerung"]
[41,"DW 20",null,"Module number",null,null,"Ch1.T_ethercat<.ethercat_nrvs>[W]{r}"]
[41,"DW 21-30",null,"Module name",null,null,"Ch1.T_ethercat<.ethercat_modulname>[S0-19]{r}"]
[41,null,"Fehlerbeschreibung"]
[41,"DW 40",null,"Klemme ist ok: Nummer",null,null,"Ch1.T_ethercat<.ethercat_f1nummer>[W]{r}"]
[41,"DW 41-50",null,"Klemme ist ok: Name",null,null,"Ch1.T_ethercat<.ethercat_f1name>[S0-19]{r}"]
[41]
[41,"DW 60",null,"Klemme gestört: Nummer",null,null,"Ch1.T_ethercat<.ethercat_f2nummer>[W]{r}"]
[41,"DW 61-70",null,"Klemme gestört: Name",null,null,"Ch1.T_ethercat<.ethercat_f2name>[S0-19]{r}"]
[41]
[41,"DW 80",null,"Modul gestört: Nummer",null,null,"Ch1.T_ethercat<.ethercat_f3nummer>[W]{r}"]
[41,"DW 81-90",null,"Modul gestört: Name",null,null,"Ch1.T_ethercat<.ethercat_f3name>[S0-19]{r}"]
[41,"DW 91",null,"Modul gestört: Klemmennummer",null,null,"Ch1.T_ethercat<.ethercat_f3knummer>[W]{r}"]
[41]
[41,"DW 200",null,"Module number position 1",null,null,"Ch1.T_ethercat<.ethercat>[W0]{r}"]
[41,"DW 201",null,"Status module position 1",null,null,"Ch1.T_ethercat<.ethercat>[W1]{r}"]
[41,null,"Bit 1","Warning"]
[41,null,"Bit 2","Fault"]
[41,null,"Bit 4","Link Fehler Verbindung nach oben"]
[41,null,"Bit 5","interner Link Fehler"]
[41,null,"Bit 6","Link Fehler Verbindung nach unten"]
[41,null,"Bit 7","interner Fehler / K-Busfehler"]
[41,null,"Bit 8-15","Fault byte"]
[41]
[41,"DW200-201",null,"Module postion 1",null,null,"Ch1.T_ethercat<.ethercat_data>[W0-1]{r}"]
[41,"DW202-203",null,"Module postion 2",null,null,"Ch1.T_ethercat<.ethercat_data>[W2-3]{r}"]
[41,"DW204-205",null,"Module postion 3",null,null,"Ch1.T_ethercat<.ethercat_data>[W4-5]{r}"]
[41,"DW206-207",null,"Module postion 4",null,null,"Ch1.T_ethercat<.ethercat_data>[W6-7]{r}"]
[41,"DW208-209",null,"Module postion 5",null,null,"Ch1.T_ethercat<.ethercat_data>[W8-9]{r}"]
[41,"DW210-211",null,"Module postion 6",null,null,"Ch1.T_ethercat<.ethercat_data>[W10-11]{r}"]
[41,"DW212-213",null,"Module postion 7",null,null,"Ch1.T_ethercat<.ethercat_data>[W12-13]{r}"]
[41,"DW214-215",null,"Module postion 8",null,null,"Ch1.T_ethercat<.ethercat_data>[W14-15]{r}"]
[41,"DW216-217",null,"Module postion 9",null,null,"Ch1.T_ethercat<.ethercat_data>[W16-17]{r}"]
[41,"DW218-219",null,"Module postion 10",null,null,"Ch1.T_ethercat<.ethercat_data>[W18-19]{r}"]
[41]
[41,"DW310-311",null,"Module postion 56",null,null,"Ch1.T_ethercat<.ethercat_data>[W110-111]{r}"]

{"sheet":"PLCPresets","index":7,"n_rows":59,"n_cols":7,"rows_kept":59,"flags":["formulas_cached_only"]}
["PLCPresets","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 50 - 54","Presets"]
[41,"DB 50 ","Presets 1st Machine "]
[41,"DW 010 –012","3*16 Bit Presets"]
[41,"DB 051-054","Presets Machine 2-5"]
[1,"###MAIN"]
[1,"DB 50-54 Presets"]
[21,"DB ###ADDR:50+1[MNR]:ADDR","Presets ###MNR"]
[41,"DW 0","Bit 0","Presets changed",null,null,"Ch1.###MNR_T_vorein<.m###MNR_voraender>[B]{w}"]
[41,"DW 9",null,"Reserved PLC"]
[41,"DW 10","Bit 0","Presetting   1","PLCPresets.###MNR.1","###INDEX:PLCPresets.###MNR.1:INDEX","Ch1.###MNR_T_vorein<.m###MNR_vorein_1>[W]{r}"]
[41,null,"Bit 1","Presetting   2","PLCPresets.###MNR.2","###INDEX:PLCPresets.###MNR.2:INDEX"]
[41,null,"Bit 2","Presetting   3","PLCPresets.###MNR.3","###INDEX:PLCPresets.###MNR.3:INDEX"]
[41,null,"Bit 3","Presetting   4","PLCPresets.###MNR.4","###INDEX:PLCPresets.###MNR.4:INDEX"]
[41,null,"Bit 4","Presetting   5","PLCPresets.###MNR.5","###INDEX:PLCPresets.###MNR.5:INDEX"]
[41,null,"Bit 5","Presetting   6","PLCPresets.###MNR.6","###INDEX:PLCPresets.###MNR.6:INDEX"]
[41,null,"Bit 6","Presetting   7","PLCPresets.###MNR.7","###INDEX:PLCPresets.###MNR.7:INDEX"]
[41,null,"Bit 7","Presetting   8","PLCPresets.###MNR.8","###INDEX:PLCPresets.###MNR.8:INDEX"]
[41,null,"Bit 8","Presetting   9","PLCPresets.###MNR.9","###INDEX:PLCPresets.###MNR.9:INDEX"]
[41,null,"Bit 9","Presetting   10","PLCPresets.###MNR.10","###INDEX:PLCPresets.###MNR.10:INDEX"]
[41,null,"Bit 10","Presetting   11","PLCPresets.###MNR.11","###INDEX:PLCPresets.###MNR.11:INDEX"]
[41,null,"Bit 11","Presetting   12","PLCPresets.###MNR.12","###INDEX:PLCPresets.###MNR.12:INDEX"]
[41,null,"Bit 12","Presetting   13","PLCPresets.###MNR.13","###INDEX:PLCPresets.###MNR.13:INDEX"]
[41,null,"Bit 13","Presetting   14","PLCPresets.###MNR.14","###INDEX:PLCPresets.###MNR.14:INDEX"]
[41,null,"Bit 14","Presetting   15","PLCPresets.###MNR.15","###INDEX:PLCPresets.###MNR.15:INDEX"]
[41,null,"Bit 15","Presetting   16","PLCPresets.###MNR.16","###INDEX:PLCPresets.###MNR.16:INDEX"]
[41,"DW 11","Bit 0","Presetting   17","PLCPresets.###MNR.21","###INDEX:PLCPresets.###MNR.21:INDEX","Ch1.###MNR_T_vorein<.m###MNR_vorein_2>[W]{r}"]
[41,null,"Bit 1","Presetting   18","PLCPresets.###MNR.22","###INDEX:PLCPresets.###MNR.22:INDEX"]
[41,null,"Bit 2","Presetting   19","PLCPresets.###MNR.23","###INDEX:PLCPresets.###MNR.23:INDEX"]
[41,null,"Bit 3","Presetting   20","PLCPresets.###MNR.24","###INDEX:PLCPresets.###MNR.24:INDEX"]
[41,null,"Bit 4","Presetting   21","PLCPresets.###MNR.25","###INDEX:PLCPresets.###MNR.25:INDEX"]
[41,null,"Bit 5","Presetting   22","PLCPresets.###MNR.26","###INDEX:PLCPresets.###MNR.26:INDEX"]
[41,null,"Bit 6","Presetting   23","PLCPresets.###MNR.27","###INDEX:PLCPresets.###MNR.27:INDEX"]
[41,null,"Bit 7","Presetting   24","PLCPresets.###MNR.28","###INDEX:PLCPresets.###MNR.28:INDEX"]
[41,null,"Bit 8","Presetting   25","PLCPresets.###MNR.29","###INDEX:PLCPresets.###MNR.29:INDEX"]
[41,null,"Bit 9","Presetting   26","PLCPresets.###MNR.30","###INDEX:PLCPresets.###MNR.30:INDEX"]
[41,null,"Bit 10","Presetting   27","PLCPresets.###MNR.31","###INDEX:PLCPresets.###MNR.31:INDEX"]
[41,null,"Bit 11","Presetting   28","PLCPresets.###MNR.32","###INDEX:PLCPresets.###MNR.32:INDEX"]
[41,null,"Bit 12","Presetting   29","PLCPresets.###MNR.33","###INDEX:PLCPresets.###MNR.33:INDEX"]
[41,null,"Bit 13","Presetting   30","PLCPresets.###MNR.34","###INDEX:PLCPresets.###MNR.34:INDEX"]
[41,null,"Bit 14","Presetting   31","PLCPresets.###MNR.35","###INDEX:PLCPresets.###MNR.35:INDEX"]
[41,null,"Bit 15","Presetting   32","PLCPresets.###MNR.36","###INDEX:PLCPresets.###MNR.36:INDEX"]
[41,"DW 12","Bit 0","Presetting   33","PLCPresets.###MNR.41","###INDEX:PLCPresets.###MNR.41:INDEX","Ch1.###MNR_T_vorein<.m###MNR_vorein_3>[W]{r}"]
[41,null,"Bit 1","Presetting   34","PLCPresets.###MNR.42","###INDEX:PLCPresets.###MNR.42:INDEX"]
[41,null,"Bit 2","Presetting   35","PLCPresets.###MNR.43","###INDEX:PLCPresets.###MNR.43:INDEX"]
[41,null,"Bit 3","Presetting   36","PLCPresets.###MNR.44","###INDEX:PLCPresets.###MNR.44:INDEX"]
[41,null,"Bit 4","Presetting   37","PLCPresets.###MNR.45","###INDEX:PLCPresets.###MNR.45:INDEX"]
[41,null,"Bit 5","Presetting   38","PLCPresets.###MNR.46","###INDEX:PLCPresets.###MNR.46:INDEX"]
[41,null,"Bit 6","Presetting   39","PLCPresets.###MNR.47","###INDEX:PLCPresets.###MNR.47:INDEX"]
[41,null,"Bit 7","Presetting   40","PLCPresets.###MNR.48","###INDEX:PLCPresets.###MNR.48:INDEX"]
[41,null,"Bit 8","Presetting   41","PLCPresets.###MNR.49","###INDEX:PLCPresets.###MNR.49:INDEX"]
[41,null,"Bit 9","Presetting   42","PLCPresets.###MNR.50","###INDEX:PLCPresets.###MNR.50:INDEX"]
[41,null,"Bit 10","Presetting   43","PLCPresets.###MNR.51","###INDEX:PLCPresets.###MNR.51:INDEX"]
[41,null,"Bit 11","Presetting   44","PLCPresets.###MNR.52","###INDEX:PLCPresets.###MNR.52:INDEX"]
[41,null,"Bit 12","Presetting   45","PLCPresets.###MNR.53","###INDEX:PLCPresets.###MNR.53:INDEX"]
[41,null,"Bit 13","Presetting   46","PLCPresets.###MNR.54","###INDEX:PLCPresets.###MNR.54:INDEX"]
[41,null,"Bit 14","Presetting   47","PLCPresets.###MNR.55","###INDEX:PLCPresets.###MNR.55:INDEX"]
[41,null,"Bit 15","Presetting   48","PLCPresets.###MNR.56","###INDEX:PLCPresets.###MNR.56:INDEX"]

{"sheet":"ManualMovement","index":8,"n_rows":35,"n_cols":7,"rows_kept":35,"flags":["formulas_cached_only"]}
["ManualMovement","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 50 - 54","Manual movement "]
[41,"DB 50 ","Manual movement 1st Machine "]
[42,"DW 020 –022","2*12 Bit Manual movement"]
[41,"DB 051-054","Manual movement Machine  2-5"]
[1,"###MAIN"]
[1,"DB 50-54 Manual movement "]
[21,"DB ###ADDR:50+1[MNR]:ADDR","Manual movement ###MNR"]
[41,"DW 20","Bit 0","Manual movement changed",null,null,"Ch1.###MNR_T_vorein<.m###MNR_handaender>[B]{w}"]
[41,null,"Bit 8","Manual enable","ManualMovement.###MNR.40","###INDEX:ManualMovement.###MNR.40:INDEX","Ch1.###MNR_T_vorein<.m###MNR_handbetrieb>[B]{r}"]
[41,"DW 30","Bit 0","Manual movement  ","ManualMovement.###MNR.1","###INDEX:ManualMovement.###MNR.1:INDEX","Ch1.###MNR_T_vorein<.m###MNR_handver_1>[W]{r}"]
[41,null,"Bit 1","Manual movement  ","ManualMovement.###MNR.2","###INDEX:ManualMovement.###MNR.2:INDEX"]
[41,null,"Bit 2","Manual movement  ","ManualMovement.###MNR.3","###INDEX:ManualMovement.###MNR.3:INDEX"]
[41,null,"Bit 3","Manual movement  ","ManualMovement.###MNR.4","###INDEX:ManualMovement.###MNR.4:INDEX"]
[41,null,"Bit 4","Manual movement  ","ManualMovement.###MNR.5","###INDEX:ManualMovement.###MNR.5:INDEX"]
[41,null,"Bit 5","Manual movement  ","ManualMovement.###MNR.6","###INDEX:ManualMovement.###MNR.6:INDEX"]
[41,null,"Bit 6","Manual movement  ","ManualMovement.###MNR.7","###INDEX:ManualMovement.###MNR.7:INDEX"]
[41,null,"Bit 7","Manual movement  ","ManualMovement.###MNR.8","###INDEX:ManualMovement.###MNR.8:INDEX"]
[41,null,"Bit 8","Manual movement  ","ManualMovement.###MNR.9","###INDEX:ManualMovement.###MNR.9:INDEX"]
[41,null,"Bit 9","Manual movement  ","ManualMovement.###MNR.10","###INDEX:ManualMovement.###MNR.10:INDEX"]
[41,null,"Bit 10","Manual movement  ","ManualMovement.###MNR.11","###INDEX:ManualMovement.###MNR.11:INDEX"]
[41,null,"Bit 11","Manual movement  ","ManualMovement.###MNR.12","###INDEX:ManualMovement.###MNR.12:INDEX"]
[41,"DW 31","Bit 0","Manual movement  ","ManualMovement.###MNR.21","###INDEX:ManualMovement.###MNR.21:INDEX","Ch1.###MNR_T_vorein<.m###MNR_handver_1>[W]{r}"]
[41,null,"Bit 1","Manual movement  ","ManualMovement.###MNR.22","###INDEX:ManualMovement.###MNR.22:INDEX"]
[41,null,"Bit 2","Manual movement  ","ManualMovement.###MNR.23","###INDEX:ManualMovement.###MNR.23:INDEX"]
[41,null,"Bit 3","Manual movement  ","ManualMovement.###MNR.24","###INDEX:ManualMovement.###MNR.24:INDEX"]
[41,null,"Bit 4","Manual movement  ","ManualMovement.###MNR.25","###INDEX:ManualMovement.###MNR.25:INDEX"]
[41,null,"Bit 5","Manual movement  ","ManualMovement.###MNR.26","###INDEX:ManualMovement.###MNR.26:INDEX"]
[41,null,"Bit 6","Manual movement  ","ManualMovement.###MNR.27","###INDEX:ManualMovement.###MNR.27:INDEX"]
[41,null,"Bit 7","Manual movement  ","ManualMovement.###MNR.28","###INDEX:ManualMovement.###MNR.28:INDEX"]
[41,null,"Bit 8","Manual movement  ","ManualMovement.###MNR.29","###INDEX:ManualMovement.###MNR.29:INDEX"]
[41,null,"Bit 9","Manual movement  ","ManualMovement.###MNR.30","###INDEX:ManualMovement.###MNR.30:INDEX"]
[41,null,"Bit 10","Manual movement  ","ManualMovement.###MNR.31","###INDEX:ManualMovement.###MNR.31:INDEX"]
[41,null,"Bit 11","Manual movement  ","ManualMovement.###MNR.32","###INDEX:ManualMovement.###MNR.32:INDEX"]

{"sheet":"Speed","index":9,"n_rows":44,"n_cols":7,"rows_kept":44,"flags":["formulas_cached_only"]}
["Speed","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 60 ","Speed 1st Machine "]
[41,null,"DW 019","Limit"]
[41,null,"DW 020","Angle of rotation after stop"]
[41,"DB 061-064","Speed Machine 2-5"]
[1,"###MAIN"]
[1,"DB 60-64 Speed"]
[21,"DB ###ADDR:60+1[MNR]:ADDR","Speed ###MNR"]
[41,"DW 0","Bit 0","Speed changed",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_drehaender>[B]{w}"]
[41,"DW 19",null,"Limit N>N max",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_grenze>[W]{p}"]
[41,"DW 20",null,"Angle of rotation after stop","Speed.###MNR.22","###INDEX:Speed.###MNR.22:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_drehstop>[W]{p}"]
[41,"DW 30",null,"Setpoint 1","Speed.###MNR.1","###INDEX:Speed.###MNR.1:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W0]{r}"]
[41,"DW 31",null,"Setpoint 2","Speed.###MNR.2","###INDEX:Speed.###MNR.2:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W1]{r}"]
[41,"DW 32",null,"Setpoint 3","Speed.###MNR.3","###INDEX:Speed.###MNR.3:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W2]{r}"]
[41,"DW 33",null,"Setpoint 4","Speed.###MNR.4","###INDEX:Speed.###MNR.4:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W3]{r}"]
[41,"DW 34",null,"Setpoint 5","Speed.###MNR.5","###INDEX:Speed.###MNR.5:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W4]{r}"]
[41,"DW 35",null,"Setpoint 6","Speed.###MNR.6","###INDEX:Speed.###MNR.6:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W5]{r}"]
[41,"DW 36",null,"Setpoint 7","Speed.###MNR.7","###INDEX:Speed.###MNR.7:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W6]{r}"]
[41,"DW 37",null,"Setpoint 8","Speed.###MNR.8","###INDEX:Speed.###MNR.8:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W7]{r}"]
[41,"DW 38",null,"Setpoint 9","Speed.###MNR.9","###INDEX:Speed.###MNR.9:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W8]{r}"]
[41,"DW 39",null,"Setpoint 10","Speed.###MNR.10","###INDEX:Speed.###MNR.10:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W9]{r}"]
[41,"DW 40",null,"Setpoint 11","Speed.###MNR.11","###INDEX:Speed.###MNR.11:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W10]{r}"]
[41,"DW 41",null,"Setpoint 12","Speed.###MNR.12","###INDEX:Speed.###MNR.12:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W11]{r}"]
[41,"DW 42",null,"Setpoint 13","Speed.###MNR.13","###INDEX:Speed.###MNR.13:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W12]{r}"]
[41,"DW 43",null,"Setpoint 14","Speed.###MNR.14","###INDEX:Speed.###MNR.14:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W13]{r}"]
[41,"DW 44",null,"Setpoint 15","Speed.###MNR.15","###INDEX:Speed.###MNR.15:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W14]{r}"]
[41,"DW 45",null,"Setpoint 16","Speed.###MNR.16","###INDEX:Speed.###MNR.16:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh>[W15]{r}"]
[41,"DW 50",null,"Additional input 1","Speed.###MNR.31","###INDEX:Speed.###MNR.31:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W0]{r}"]
[41,"DW 51",null,"Additional input 2","Speed.###MNR.33","###INDEX:Speed.###MNR.33:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W1]{r}"]
[41,"DW 52",null,"Additional input 3","Speed.###MNR.35","###INDEX:Speed.###MNR.35:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W2]{r}"]
[41,"DW 53",null,"Additional input 4","Speed.###MNR.37","###INDEX:Speed.###MNR.37:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W3]{r}"]
[41,"DW 54",null,"Additional input 5","Speed.###MNR.39","###INDEX:Speed.###MNR.39:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W4]{r}"]
[41,"DW 55",null,"Additional input 6","Speed.###MNR.41","###INDEX:Speed.###MNR.41:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W5]{r}"]
[41,"DW 56",null,"Additional input 7","Speed.###MNR.43","###INDEX:Speed.###MNR.43:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W6]{r}"]
[41,"DW 57",null,"Additional input 8","Speed.###MNR.45","###INDEX:Speed.###MNR.45:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zs>[W7]{r}"]
[41,"DW 60",null,"Additional output 1","Speed.###MNR.31","###INDEX:Speed.###MNR.31:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W0]{r}"]
[41,"DW 61",null,"Additional output 2","Speed.###MNR.33","###INDEX:Speed.###MNR.33:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W1]{r}"]
[41,"DW 62",null,"Additional output 3","Speed.###MNR.35","###INDEX:Speed.###MNR.35:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W2]{r}"]
[41,"DW 63",null,"Additional output 4","Speed.###MNR.37","###INDEX:Speed.###MNR.37:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W3]{r}"]
[41,"DW 64",null,"Additional output 5","Speed.###MNR.39","###INDEX:Speed.###MNR.39:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W4]{r}"]
[41,"DW 65",null,"Additional output 6","Speed.###MNR.41","###INDEX:Speed.###MNR.41:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W5]{r}"]
[41,"DW 66",null,"Additional output 7","Speed.###MNR.43","###INDEX:Speed.###MNR.43:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W6]{r}"]
[41,"DW 67",null,"Additional output 8","Speed.###MNR.45","###INDEX:Speed.###MNR.45:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_zi>[W7]{r}"]

{"sheet":"X851_Speed","index":10,"n_rows":20,"n_cols":7,"rows_kept":20,"flags":["formulas_cached_only"]}
["X851_Speed","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 60 ","Speed 1st Machine "]
[41,"DB 061-064","Speed Machine 2-5"]
[1,"###MAIN"]
[1,"DB 60-64 Speed"]
[21,"DB ###ADDR:60+1[MNR]:ADDR","Speed ###MNR"]
[41,"DW 0"]
[41,"Bit 0",null,"Speed changed",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_drehaender>[B]{w}"]
[41,"DW 10",null,"Speed motor 1 Actual value ","851_Speed.###MNR.10","###INDEX:851_Speed.###MNR.10:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_mo_1>[W]{r}"]
[41,"DW 11",null,"Speed motor 1 limit",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_dreh_gr_1>[W]{r}"]
[41,"DW 12",null,"Torque, Motor 1, actual value ","851_Speed.###MNR.11","###INDEX:851_Speed.###MNR.11:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_mome_mo_1>[W]{r}"]
[41,"DW 13",null,"Torque, Motor 1, limit value",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_mome_gr_1>[W]{r}"]
[41,"DW 20",null,"Speed motor 1 Setpoint",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_dreh_so_1>[W]{r}"]
[41,"DW 30",null,"Speed motor 2 Actual value ","851_Speed.###MNR.20","###INDEX:851_Speed.###MNR.20:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_dreh_mo_2>[W]{r}"]
[41,"DW 31",null,"Speed motor 2 limit",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_dreh_gr_2>[W]{r}"]
[41,"DW 32",null,"Torque, Motor 2, actual value ","851_Speed.###MNR.21","###INDEX:851_Speed.###MNR.21:INDEX","Ch1.###MNR_T_drehzahl<.m###MNR_mome_mo_2>[W]{r}"]
[41,"DW 33",null,"Torque, Motor 2, limit value",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_mome_gr_2>[W]{r}"]
[41,"DW 40",null,"Speed motor 2 setpoint",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_dreh_so_2>[W]{r}"]
[41,"DD50",null,"Operating hours",null,null,"Ch1.###MNR_T_drehzahl<.m###MNR_dreh_stun>[DW]{r}"]

{"sheet":"TimerCounter","index":11,"n_rows":40,"n_cols":7,"rows_kept":40,"flags":["formulas_cached_only"]}
["TimerCounter","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 70 ","Timer and Counter 1st Machine "]
[41,null,"DW 019","Limit"]
[41,null,"DW 020","Angle of rotation after stop"]
[41,"DB 071-074","Timer and Counter Machine 2-5"]
[1,"###MAIN"]
[1,"DB 70-74 Timer and Counter"]
[21,"DB ###ADDR:70+1[MNR]:ADDR","Timer and Counter ###MNR"]
[41,"DW 0","Bit 0","Timer and Counter changed",null,null,"Ch1.###MNR_T_zeiten<.m###MNR_zeiten_aender>[B]{w}"]
[41,"DD 10",null,"Timer 1","TimerCounter.###MNR.11","###INDEX:TimerCounter.###MNR.11:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW0]{r}"]
[41,"DD 12",null,"Timer 2","TimerCounter.###MNR.12","###INDEX:TimerCounter.###MNR.12:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW1]{r}"]
[41,"DD 14",null,"Timer 3","TimerCounter.###MNR.13","###INDEX:TimerCounter.###MNR.13:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW2]{r}"]
[41,"DD 16",null,"Timer 4","TimerCounter.###MNR.14","###INDEX:TimerCounter.###MNR.14:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW3]{r}"]
[41,"DD 18",null,"Timer 5","TimerCounter.###MNR.15","###INDEX:TimerCounter.###MNR.15:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW4]{r}"]
[41,"DD 20",null,"Timer 6","TimerCounter.###MNR.16","###INDEX:TimerCounter.###MNR.16:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW5]{r}"]
[41,"DD 22",null,"Timer 7","TimerCounter.###MNR.17","###INDEX:TimerCounter.###MNR.17:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW6]{r}"]
[41,"DD 24",null,"Timer 8","TimerCounter.###MNR.18","###INDEX:TimerCounter.###MNR.18:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW7]{r}"]
[41,"DD 26",null,"Timer 9","TimerCounter.###MNR.19","###INDEX:TimerCounter.###MNR.19:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW8]{r}"]
[41,"DD 28",null,"Timer 10","TimerCounter.###MNR.20","###INDEX:TimerCounter.###MNR.20:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW9]{r}"]
[41,"DD 30",null,"Timer 11","TimerCounter.###MNR.21","###INDEX:TimerCounter.###MNR.21:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW10]{r}"]
[41,"DD 32",null,"Timer 12","TimerCounter.###MNR.22","###INDEX:TimerCounter.###MNR.22:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW11]{r}"]
[41,"DD 34",null,"Timer 13","TimerCounter.###MNR.23","###INDEX:TimerCounter.###MNR.23:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW12]{r}"]
[41,"DD 36",null,"Timer 14","TimerCounter.###MNR.24","###INDEX:TimerCounter.###MNR.24:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW13]{r}"]
[41,"DD 38",null,"Timer 15","TimerCounter.###MNR.25","###INDEX:TimerCounter.###MNR.25:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW14]{r}"]
[41,"DD 40",null,"Timer 16","TimerCounter.###MNR.26","###INDEX:TimerCounter.###MNR.26:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zeiten>[DW15]{r}"]
[41,"DW 50",null,"16-Bit Counter 1","TimerCounter.###MNR.31","###INDEX:TimerCounter.###MNR.31:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W0]{r}"]
[41,"DW 51",null,"16-Bit Counter 2","TimerCounter.###MNR.32","###INDEX:TimerCounter.###MNR.32:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W1]{r}"]
[41,"DW 52",null,"16-Bit Counter 3","TimerCounter.###MNR.33","###INDEX:TimerCounter.###MNR.33:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W2]{r}"]
[41,"DW 53",null,"16-Bit Counter 4","TimerCounter.###MNR.34","###INDEX:TimerCounter.###MNR.34:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W3]{r}"]
[41,"DW 54",null,"16-Bit Counter 5","TimerCounter.###MNR.35","###INDEX:TimerCounter.###MNR.35:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W4]{r}"]
[41,"DW 55",null,"16-Bit Counter 6","TimerCounter.###MNR.36","###INDEX:TimerCounter.###MNR.36:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W5]{r}"]
[41,"DW 56",null,"16-Bit Counter 7","TimerCounter.###MNR.37","###INDEX:TimerCounter.###MNR.37:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W6]{r}"]
[41,"DW 57",null,"16-Bit Counter 8","TimerCounter.###MNR.38","###INDEX:TimerCounter.###MNR.38:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_zaehler>[W7]{r}"]
[41,"DD 60",null,"32-Bit Counter 1","TimerCounter.###MNR.41","###INDEX:TimerCounter.###MNR.41:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_ddzaehler_1>[DW]{r}"]
[41,"DD 62",null,"32-Bit Counter 2","TimerCounter.###MNR.42","###INDEX:TimerCounter.###MNR.42:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_ddzaehler_2>[DW]{r}"]
[41,"DD 64",null,"32-Bit Counter 3","TimerCounter.###MNR.43","###INDEX:TimerCounter.###MNR.43:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_ddzaehler_3>[DW]{r}"]
[41,"DD 66",null,"32-Bit Counter 4","TimerCounter.###MNR.44","###INDEX:TimerCounter.###MNR.44:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_ddzaehler_4>[DW]{r}"]
[41,"DD 68",null,"32-Bit Counter 5","TimerCounter.###MNR.45","###INDEX:TimerCounter.###MNR.45:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_ddzaehler_5>[DW]{r}"]
[41,"DD 70",null,"32-Bit Counter 6","TimerCounter.###MNR.46","###INDEX:TimerCounter.###MNR.46:INDEX","Ch1.###MNR_T_zeiten<.m###MNR_ddzaehler_6>[DW]{r}"]

{"sheet":"PLCStatus","index":12,"n_rows":40,"n_cols":7,"rows_kept":40,"flags":["formulas_cached_only"]}
["PLCStatus","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 80 ","PLC Status 1st Machine"]
[41,"DB 081-084","PLC Status Machine 2-5"]
[1,"###MAIN"]
[1,"DB 80-84 PLC Status"]
[21,"DB ###ADDR:80+1[MNR]:ADDR","PLC Status ###MNR"]
[41,"DW 0",null,"address of 1st input",null,null,"Ch1.###MNR_T_status<.m###MNR_st_ein_soll_1>[W]{r}"]
[41,"DW 1",null,"address of 2nd input",null,null,"Ch1.###MNR_T_status<.m###MNR_st_ein_soll_2>[W]{r}"]
[41,"DW 5",null,"content of 1st input",null,null,"Ch1.###MNR_T_status<.m###MNR_st_ein_ist_1>[W]{r}"]
[41,"DW 6",null,"content of 2nd input",null,null,"Ch1.###MNR_T_status<.m###MNR_st_ein_ist_2>[W]{r}"]
[41,"DW 9","Bit 0","input 1 not present",null,null,"Ch1.###MNR_T_status<.m###MNR_st_ein_kon_1>[B]{r}"]
[41,null,"Bit 1","input 2 not present",null,null,"Ch1.###MNR_T_status<.m###MNR_st_ein_kon_1>[B]{r}"]
[41,"DW 10",null,"address of 1st output",null,null,"Ch1.###MNR_T_status<.m###MNR_st_aus_soll_1>[W]{r}"]
[41,"DW 11",null,"address of 2nd output",null,null,"Ch1.###MNR_T_status<.m###MNR_st_aus_soll_2>[W]{r}"]
[41,"DW 15",null,"content of 1st output",null,null,"Ch1.###MNR_T_status<.m###MNR_st_aus_ist_1>[W]{r}"]
[41,"DW 16",null,"content of 2nd output",null,null,"Ch1.###MNR_T_status<.m###MNR_st_aus_ist_2>[W]{r}"]
[41,"DW 19","Bit 0","output 1 not present",null,null,"Ch1.###MNR_T_status<.m###MNR_st_aus_kon_1>[B]{r}"]
[41,null,"Bit 1","output 2 not present",null,null,"Ch1.###MNR_T_status<.m###MNR_st_aus_kon_2>[B]{r}"]
[41,"DW 20",null,"address of 1st flag",null,null,"Ch1.###MNR_T_status<.m###MNR_st_mer_soll_1>[W]{r}"]
[41,"DW 21",null,"address of 2nd flag",null,null,"Ch1.###MNR_T_status<.m###MNR_st_mer_soll_2>[W]{r}"]
[41,"DW 25",null,"content of 1st flag",null,null,"Ch1.###MNR_T_status<.m###MNR_st_mer_ist_1>[W]{r}"]
[41,"DW 26",null,"content of 2nd flag",null,null,"Ch1.###MNR_T_status<.m###MNR_st_mer_ist_2>[W]{r}"]
[41,"DW 29","Bit 0","flag 1 not present",null,null,"Ch1.###MNR_T_status<.m###MNR_st_mer_kon_1>[B]{r}"]
[41,null,"Bit 1","flag 2 not present",null,null,"Ch1.###MNR_T_status<.m###MNR_st_mer_kon_2>[B]{r}"]
[41]
[41,"DW 30","Bit 0","Checken ein",null,null,"Ch1.###MNR_T_status<.m###MNR_st_check_ein>[B]{r}"]
[41]
[41,"DW 31","Bit 0","Aktuelle Bits","PLCStatus.###MNR.30","###INDEX:PLCStatus.###MNR.30:INDEX","Ch1.###MNR_T_status<.m###MNR_st_check_aktuell>[W]{r}"]
[41,null,"Bit 1","Aktuelle Bits","PLCStatus.###MNR.31","###INDEX:PLCStatus.###MNR.31:INDEX"]
[41,null,"Bit 2","Aktuelle Bits","PLCStatus.###MNR.33","###INDEX:PLCStatus.###MNR.32:INDEX"]
[41,null,"Bit 3","Aktuelle Bits","PLCStatus.###MNR.33","###INDEX:PLCStatus.###MNR.33:INDEX"]
[41,null,"Bit 4","Aktuelle Bits","PLCStatus.###MNR.34","###INDEX:PLCStatus.###MNR.34:INDEX"]
[41,null,"Bit 5","Aktuelle Bits","PLCStatus.###MNR.35","###INDEX:PLCStatus.###MNR.35:INDEX"]
[41,null,"Bit 6","Aktuelle Bits","PLCStatus.###MNR.36","###INDEX:PLCStatus.###MNR.36:INDEX"]
[41,null,"Bit 7","Aktuelle Bits","PLCStatus.###MNR.37","###INDEX:PLCStatus.###MNR.37:INDEX"]
[41,"DW 32","Bit 0 - 7","Auslöser",null,null,"Ch1.###MNR_T_status<.m###MNR_st_check_ausloeser>[W]{r}"]
[41]
[41,"DW 40",null,"Monitoring Word 1 - 30",null,null,"Ch1.###MNR_T_status<.m###MNR_mon_word>[W0]{r}"]
[41,"DW 41 - 69",null,"Monitoring Word 2 - 30",null,null,"Ch1.###MNR_T_status<.m###MNR_mon_word>[W1-29]{r}"]

{"sheet":"Cam","index":13,"n_rows":45,"n_cols":7,"rows_kept":45,"flags":["formulas_cached_only"]}
["Cam","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 90 ","Cams 1st Machine "]
[41,"DB 091-094","Cams Machine 2-5"]
[1,"###MAIN"]
[1,"DB 90-94 Cams"]
[21,"DB ###ADDR:90+1[MNR]:ADDR","DW ###ADDR:0+80[FLDNull]:ADDR-###ADDR:79+80[FLDNull]:ADDR Cams ###FLD ###MNR"]
[41,"DW ###ADDR:0+80[FLDNull]:ADDR","Bit 0","Cams changed",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_aend_###ADDR:0+1[FLD]:ADDR>[B]{w}"]
[41,"DW ###ADDR:1+80[FLDNull]:ADDR",null,"Cam position",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_stell_###ADDR:0+1[FLD]:ADDR>[W]"]
[41,"DW ###ADDR:10+80[FLDNull]:ADDR",null,"Cam 1 start","Cam.###MNR.###ADDR:1+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:1+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W0]{r}"]
[41,"DW ###ADDR:11+80[FLDNull]:ADDR",null,"Cam 1 end",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W1]{r}"]
[41,"DW ###ADDR:12+80[FLDNull]:ADDR",null,"Cam 2","Cam.###MNR.###ADDR:2+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:2+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W2]{r}"]
[41,"DW ###ADDR:14+80[FLDNull]:ADDR",null,"Cam 3","Cam.###MNR.###ADDR:3+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:3+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W4]{r}"]
[41,"DW ###ADDR:16+80[FLDNull]:ADDR",null,"Cam 4","Cam.###MNR.###ADDR:4+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:4+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W6]{r}"]
[41,"DW ###ADDR:18+80[FLDNull]:ADDR",null,"Cam 5","Cam.###MNR.###ADDR:5+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:5+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W8]{r}"]
[41,"DW ###ADDR:20+80[FLDNull]:ADDR",null,"Cam 6","Cam.###MNR.###ADDR:6+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:6+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W10]{r}"]
[41,"DW ###ADDR:22+80[FLDNull]:ADDR",null,"Cam 7","Cam.###MNR.###ADDR:7+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:7+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W12]{r}"]
[41,"DW ###ADDR:24+80[FLDNull]:ADDR",null,"Cam 8","Cam.###MNR.###ADDR:8+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:8+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W14]{r}"]
[41,"DW ###ADDR:26+80[FLDNull]:ADDR",null,"Cam 9","Cam.###MNR.###ADDR:9+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:9+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W16]{r}"]
[41,"DW ###ADDR:28+80[FLDNull]:ADDR",null,"Cam 10","Cam.###MNR.###ADDR:10+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:10+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W18]{r}"]
[41,"DW ###ADDR:30+80[FLDNull]:ADDR",null,"Cam 11","Cam.###MNR.###ADDR:11+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:11+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W20]{r}"]
[41,"DW ###ADDR: 32+80[FLDNull]:ADDR",null,"Cam 12","Cam.###MNR.###ADDR:12+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:12+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W22]{r}"]
[41,"DW ###ADDR:34+80[FLDNull]:ADDR",null,"Cam 13","Cam.###MNR.###ADDR:13+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:13+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W24]{r}"]
[41,"DW ###ADDR:36+80[FLDNull]:ADDR",null,"Cam 14","Cam.###MNR.###ADDR:14+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:14+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W26]{r}"]
[41,"DW ###ADDR:38+80[FLDNull]:ADDR",null,"Cam 15","Cam.###MNR.###ADDR:15+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:15+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W28]{r}"]
[41,"DW ###ADDR:40+80[FLDNull]:ADDR",null,"Cam 16","Cam.###MNR.###ADDR:16+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:16+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W30]{r}"]
[41,"DW ###ADDR:42+80[FLDNull]:ADDR",null,"Cam 17","Cam.###MNR.###ADDR:21+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:21+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W32]{r}"]
[41,"DW ###ADDR:44+80[FLDNull]:ADDR",null,"Cam 18","Cam.###MNR.###ADDR:22+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:22+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W34]{r}"]
[41,"DW ###ADDR:46+80[FLDNull]:ADDR",null,"Cam 19","Cam.###MNR.###ADDR:23+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:23+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W36]{r}"]
[41,"DW ###ADDR:48+80[FLDNull]:ADDR",null,"Cam 20","Cam.###MNR.###ADDR:24+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:24+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W38]{r}"]
[41,"DW ###ADDR:50+80[FLDNull]:ADDR",null,"Cam 21","Cam.###MNR.###ADDR:25+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:25+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W40]{r}"]
[41,"DW ###ADDR:52+80[FLDNull]:ADDR",null,"Cam 22","Cam.###MNR.###ADDR:26+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:26+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W42]{r}"]
[41,"DW ###ADDR:54+80[FLDNull]:ADDR",null,"Cam 23","Cam.###MNR.###ADDR:27+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:27+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W44]{r}"]
[41,"DW ###ADDR:56+80[FLDNull]:ADDR",null,"Cam 24","Cam.###MNR.###ADDR:28+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:28+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W46]{r}"]
[41,"DW ###ADDR:58+80[FLDNull]:ADDR",null,"Cam 25","Cam.###MNR.###ADDR:29+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:29+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W48]{r}"]
[41,"DW ###ADDR:60+80[FLDNull]:ADDR",null,"Cam 26","Cam.###MNR.###ADDR:30+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:30+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W50]{r}"]
[41,"DW ###ADDR:62+80[FLDNull]:ADDR",null,"Cam 27","Cam.###MNR.###ADDR:31+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:31+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W52]{r}"]
[41,"DW ###ADDR:64+80[FLDNull]:ADDR",null,"Cam 28","Cam.###MNR.###ADDR:32+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:32+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W54]{r}"]
[41,"DW ###ADDR:66+80[FLDNull]:ADDR",null,"Cam 29","Cam.###MNR.###ADDR:33+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:33+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W56]{r}"]
[41,"DW ###ADDR:68+80[FLDNull]:ADDR",null,"Cam 30","Cam.###MNR.###ADDR:34+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:34+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W58]{r}"]
[41,"DW ###ADDR:70+80[FLDNull]:ADDR",null,"Cam 31","Cam.###MNR.###ADDR:35+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:35+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W60]{r}"]
[41,"DW ###ADDR:72+80[FLDNull]:ADDR",null,"Cam 32","Cam.###MNR.###ADDR:36+40[FLDNull]:ADDR","###INDEX:Cam.###MNR.###ADDR:36+40[FLDNull]:ADDR:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv_###FLD>[W62]{r}"]
[41]
[41,"DW ###ADDR:75+80[FLDNull]:ADDR",null,"Cam 1- 16: Block Cam",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_sperr_###FLD>[W0]{r}"]
[41,"DW ###ADDR:76+80[FLDNull]:ADDR",null,"Cam 17- 32: Block Cam",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_sperr_###FLD>[W1]{r}"]

{"sheet":"Heater","index":14,"n_rows":76,"n_cols":7,"rows_kept":76,"flags":["formulas_cached_only"]}
["Heater","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 100 ","Heaters 1st Machine "]
[41,"DB 101-104","Heaters Machine 2-5"]
[1,"###MAIN"]
[1,"DB 100-104 Heaters"]
[41,"DW 0","Bit 0","Heaters changed",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heizaend>[B]{w}"]
[41,"DW 1",null,"Fault word",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W0]{p}"]
[41,null,1,"wire break","Heater.20","###INDEX:Heater.20:INDEX"]
[41,null,2,"short-circuit","Heater.21","###INDEX:Heater.21:INDEX"]
[41,null,3,"temperature > 215","Heater.22","###INDEX:Heater.22:INDEX"]
[41,null,4,"temperature too high","Heater.23","###INDEX:Heater.23:INDEX"]
[41,null,5,"temperture too low","Heater.24","###INDEX:Heater.24:INDEX"]
[41,"DW 2",null,"status word",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W1]{p}"]
[41,null,0,"inhibited","Heater.11","###INDEX:Heater.11:INDEX"]
[41,null,1,"active","Heater.10","###INDEX:Heater.10:INDEX"]
[41,null,2,"defective","Heater.12","###INDEX:Heater.12:INDEX"]
[41,"DW 5",null,"actual value","Heater.0","###INDEX:Heater.0:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W4]{p}"]
[41,"DW 6",null,"Y"]
[41,"DW 10",null,"Setpoint ","Heater.1","###INDEX:Heater.1:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W0]{r}"]
[41,"DW 11",null,"lower warning limit","Heater.2","###INDEX:Heater.2:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W1]{r}"]
[41,"DW 12",null,"upper warning limit","Heater.3","###INDEX:Heater.3:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W2]{r}"]
[41,"DW 13",null,"P",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W3]{r}"]
[41,"DW 14",null,"I",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W4]{r}"]
[41,"DW 15",null,"D",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W5]{r}"]
[41,"DW 16",null,"YN",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W6]{r}"]
[41,"DW 17",null,"Y0",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W7]{r}"]
[21,"DB ###ADDR:100+1[MNR]:ADDR","Heaters ###MNR"]
[41,"DW 1-6",null,"Heater 1 read","Heater.###MNR.1","###INDEX:Heater.###MNR.1:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W0-5]{r}"]
[41,"DW 10-15",null,"Heater 1 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W0-5]{r}"]
[41,"DW 21-26",null,"Heater 2 read","Heater.###MNR.2","###INDEX:Heater.###MNR.2:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_2>[W0-5]{r}"]
[41,"DW 30-35",null,"Heater 2 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_2>[W0-5]{r}"]
[41,"DW 41-46",null,"Heater 3 read","Heater.###MNR.3","###INDEX:Heater.###MNR.3:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_3>[W0-5]{r}"]
[41,"DW 50-55",null,"Heater 3 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_3>[W0-5]{r}"]
[41,"DW 61-66",null,"Heater 4 read","Heater.###MNR.4","###INDEX:Heater.###MNR.4:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_4>[W0-5]{r}"]
[41,"DW 70-75",null,"Heater 4 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_4>[W0-5]{r}"]
[41,"DW 81-86",null,"Heater 5 read","Heater.###MNR.5","###INDEX:Heater.###MNR.5:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_5>[W0-5]{r}"]
[41,"DW 90-95",null,"Heater 5 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_5>[W0-5]{r}"]
[41,"DW 101-106",null,"Heater 6 read","Heater.###MNR.6","###INDEX:Heater.###MNR.6:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_6>[W0-5]{r}"]
[41,"DW 110-115",null,"Heater 6 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_6>[W0-5]{r}"]
[41,"DW 121-126",null,"Heater 7 read","Heater.###MNR.10","###INDEX:Heater.###MNR.10:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_7>[W0-5]{r}"]
[41,"DW 130-135",null,"Heater 7 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_7>[W0-5]{r}"]
[41,"DW 141-146",null,"Heater 8 read","Heater.###MNR.11","###INDEX:Heater.###MNR.11:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_8>[W0-5]{r}"]
[41,"DW 150-155",null,"Heater 8 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_8>[W0-5]{r}"]
[41,"DW 161-166",null,"Heater 9 read","Heater.###MNR.12","###INDEX:Heater.###MNR.12:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_9>[W0-5]{r}"]
[41,"DW 170-175",null,"Heater 9 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_9>[W0-5]{r}"]
[41,"DW 181-186",null,"Heater 10 read","Heater.###MNR.13","###INDEX:Heater.###MNR.13:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_10>[W0-5]{r}"]
[41,"DW 190-195",null,"Heater 10 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_10>[W0-5]{r}"]
[41,"DW 201-206",null,"Heater 11 read","Heater.###MNR.14","###INDEX:Heater.###MNR.14:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_11>[W0-5]{r}"]
[41,"DW 210-215",null,"Heater 11 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_11>[W0-5]{r}"]
[41,"DW 221-226",null,"Heater 12 read","Heater.###MNR.15","###INDEX:Heater.###MNR.15:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_12>[W0-5]{r}"]
[41,"DW 230-235",null,"Heater 12 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_12>[W0-5]{r}"]
[41,"DW 241-246",null,"Heater 13 read","Heater.###MNR.20","###INDEX:Heater.###MNR.20:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_13>[W0-5]{r}"]
[41,"DW 250-255",null,"Heater 13 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_13>[W0-5]{r}"]
[41,"DW 261-266",null,"Heater 14 read","Heater.###MNR.21","###INDEX:Heater.###MNR.21:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_14>[W0-5]{r}"]
[41,"DW 270-275",null,"Heater 14 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_14>[W0-5]{r}"]
[41,"DW 281-286",null,"Heater 15 read","Heater.###MNR.22","###INDEX:Heater.###MNR.22:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_15>[W0-5]{r}"]
[41,"DW 290-295",null,"Heater 15 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_15>[W0-5]{r}"]
[41,"DW 301-306",null,"Heater 16 read","Heater.###MNR.23","###INDEX:Heater.###MNR.23:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_16>[W0-5]{r}"]
[41,"DW 310-315",null,"Heater 16 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_16>[W0-5]{r}"]
[41,"DW 321-326",null,"Heater 17 read","Heater.###MNR.24","###INDEX:Heater.###MNR.24:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_17>[W0-5]{r}"]
[41,"DW 330-335",null,"Heater 17 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_17>[W0-5]{r}"]
[41,"DW 341-346",null,"Heater 18 read","Heater.###MNR.25","###INDEX:Heater.###MNR.25:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_18>[W0-5]{r}"]
[41,"DW 350-355",null,"Heater 18 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_18>[W0-5]{r}"]
[41,"DW 361-366",null,"Heater 19 read","Heater.###MNR.30","###INDEX:Heater.###MNR.30:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_19>[W0-5]{r}"]
[41,"DW 370-375",null,"Heater 19 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_19>[W0-5]{r}"]
[41,"DW 381-386",null,"Heater 20 read","Heater.###MNR.31","###INDEX:Heater.###MNR.31:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_20>[W0-5]{r}"]
[41,"DW 390-395",null,"Heater 20 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_20>[W0-5]{r}"]
[41,"DW 401-406",null,"Heater 21 read","Heater.###MNR.32","###INDEX:Heater.###MNR.32:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_21>[W0-5]{r}"]
[41,"DW 410-415",null,"Heater 21 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_21>[W0-5]{r}"]
[41,"DW 421-426",null,"Heater 22 read","Heater.###MNR.33","###INDEX:Heater.###MNR.33:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_22>[W0-5]{r}"]
[41,"DW 430-435",null,"Heater 22 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_22>[W0-5]{r}"]
[41,"DW 441-446",null,"Heater 23 read","Heater.###MNR.34","###INDEX:Heater.###MNR.34:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_23>[W0-5]{r}"]
[41,"DW 450-455",null,"Heater 23 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_23>[W0-5]{r}"]
[41,"DW 461-466",null,"Heater 24 read","Heater.###MNR.35","###INDEX:Heater.###MNR.35:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_24>[W0-5]{r}"]
[41,"DW 470-475",null,"Heater 24 write",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_24>[W0-5]{r}"]

{"sheet":"X350_GlueJet","index":15,"n_rows":22,"n_cols":7,"rows_kept":22,"flags":["formulas_cached_only"]}
["X350_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-39",null,"19 values of Track 2","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41]
[41,"DW 90",null,"Glue min.","350_GlueJet.34","###INDEX:350_GlueJet.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","350_GlueJet.31","###INDEX:350_GlueJet.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","350_GlueJet.32","###INDEX:350_GlueJet.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","350_GlueJet.33","###INDEX:350_GlueJet.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","350_GlueJet.1","###INDEX:350_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","350_GlueJet.11","###INDEX:350_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X350_GlueJet_3","index":16,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
["X350_GlueJet_3","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-29",null,"9 values of Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41,"DW 31-49",null,"19 values of Track 3","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-49]{r}"]
[41]
[41,"DW 90",null,"Glue min.","350_GlueJet_3.34","###INDEX:350_GlueJet_3.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","350_GlueJet_3.31","###INDEX:350_GlueJet_3.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","350_GlueJet_3.32","###INDEX:350_GlueJet_3.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","350_GlueJet_3.33","###INDEX:350_GlueJet_3.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","350_GlueJet_3.1","###INDEX:350_GlueJet_3.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","350_GlueJet_3.11","###INDEX:350_GlueJet_3.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 122",null,"Offset, Track 3 (21)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X355_GlueJet","index":17,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
["X355_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-29",null,"9 values of Track 2","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-19]{r}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","355_GlueJet.1","###INDEX:355_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","355_GlueJet.11","###INDEX:355_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]v"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X400_GlueJet","index":18,"n_rows":26,"n_cols":7,"rows_kept":26,"flags":["formulas_cached_only"]}
["X400_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11",null,"Start of gluing, Track 1","* 100 / Factor(1) - Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1]{r}"]
[41,"DW 12",null,"End of gluing, Track 1","* 100 / Factor(1) – Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W2]{r}"]
[41,"DW 41",null,"Start of gluing, Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31]{r}"]
[41,"DW 42",null,"End of gluing, Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W32]{r}"]
[41,"DW 80",null,"Pressure, jet(1)","400_GlueJet.31","###INDEX:400_GlueJet.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesedruck_1>[W]{r}"]
[41,"DW 81",null,"Pilot control(1) on","400_GlueJet.41","###INDEX:400_GlueJet.41:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevorein_1>[W]{r}"]
[41,"DW 82",null,"Pilot control(1) off","400_GlueJet.42","###INDEX:400_GlueJet.42:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevoraus_1>[W]{r}"]
[41,"DW 90",null,"Pressure, jet(2)","400_GlueJet.32","###INDEX:400_GlueJet.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesedruck_2>[W]{r}"]
[41,"DW 91",null,"Pilot control(2) on","400_GlueJet.51","###INDEX:400_GlueJet.51:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevorein_2>[W]{r}"]
[41,"DW 92",null,"Pilot control(2) off","400_GlueJet.52","###INDEX:400_GlueJet.52:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevoraus_2>[W]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","400_GlueJet.1","###INDEX:400_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(2)","400_GlueJet.2","###INDEX:400_GlueJet.2:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 110",null,"Factor(1)","400_GlueJet.11","###INDEX:400_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 111",null,"Factor(2)","400_GlueJet.12","###INDEX:400_GlueJet.12:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_2>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (31)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"6 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"6 values of Track 2",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X401_GlueJet","index":19,"n_rows":26,"n_cols":7,"rows_kept":26,"flags":["formulas_cached_only"]}
["X401_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11",null,"Start of gluing, Track 1","* 100 / Factor(1) – Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1]{r}"]
[41,"DW 12",null,"End of gluing, Track 1","* 100 / Factor(1) – Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W2]{r}"]
[41,"DW 41",null,"Start of gluing, Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31]{r}"]
[41,"DW 42",null,"End of gluing, Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W32]{r}"]
[41,"DW 80",null,"Pressure, jet(1)","401_GlueJet.31","###INDEX:401_GlueJet.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesedruck_1>[W]{r}"]
[41,"DW 81",null,"Pilot control(1) on","401_GlueJet.41","###INDEX:401_GlueJet.41:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevorein_1>[W]{r}"]
[41,"DW 82",null,"Pilot control(1) off","401_GlueJet.42","###INDEX:401_GlueJet.42:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevoraus_1>[W]{r}"]
[41,"DW 90",null,"Pressure, jet(2)","401_GlueJet.32","###INDEX:401_GlueJet.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesedruck_2>[W]{r}"]
[41,"DW 91",null,"Pilot control(2) on","401_GlueJet.51","###INDEX:401_GlueJet.51:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevorein_2>[W]{r}"]
[41,"DW 92",null,"Pilot control(2) off","401_GlueJet.52","###INDEX:401_GlueJet.52:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesevoraus_2>[W]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","401_GlueJet.1","###INDEX:401_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(2)","401_GlueJet.2","###INDEX:401_GlueJet.2:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 110",null,"Factor(1)","401_GlueJet.11","###INDEX:401_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 111",null,"Factor(2)","401_GlueJet.12","###INDEX:401_GlueJet.12:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_2>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (31)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"6 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"6 values of Track 2",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X401_GlueJetCoupon","index":20,"n_rows":14,"n_cols":7,"rows_kept":14,"flags":["formulas_cached_only"]}
["X401_GlueJetCoupon","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-25",null,"5 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-5]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor","401_GlueJetCoupon.1","###INDEX:401_GlueJetCoupon.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","401_GlueJetCoupon.11","###INDEX:401_GlueJetCoupon.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (5)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]

{"sheet":"X407_GlueJet","index":21,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
["X407_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-25",null,"15 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-15]{r}"]
[41,"DW 26-30",null,"15 values of Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W16-30]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor","407_GlueJet.1","###INDEX:407_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","407_GlueJet.11","###INDEX:407_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (16)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X407_GlueJetLabel","index":22,"n_rows":18,"n_cols":7,"rows_kept":18,"flags":["formulas_cached_only"]}
["X407_GlueJetLabel","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabaender>[B]{w}"]
[41,"DW 11-30",null,"20 values of Track 1","* 100 / Factor - Distance(1)",null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W1-20]{r}"]
[41,"DW 31-50",null,"20 values of Track 2","* 100 / Factor - Distance(2)",null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W21-40]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor","407_GlueJetLabel.1","###INDEX:407_GlueJetLabel.1:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselababst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor","407_GlueJetLabel.2","###INDEX:407_GlueJetLabel.2:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselababst_2>[W]{r}"]
[41,"DW 110",null,"Factor","407_GlueJetLabel.11","###INDEX:407_GlueJetLabel.11:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselabfakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (21)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (20)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (20)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_2>[W]{r}"]

{"sheet":"X407_GlueJet_LongSeal","index":23,"n_rows":28,"n_cols":7,"rows_kept":28,"flags":["formulas_cached_only"]}
["X407_GlueJet_LongSeal","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 -119","Glue jets"]
[41,"DB 110 ","Glue jets 1st part 1st Machine "]
[41,"DB 111-114","Glue jets 1st part Machine  2-5"]
[41,"DB 115","Glue jets 2nd part 1st Machine "]
[41,"DB 116-119","Glue jets 2nd part Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-119 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-30",null,"20 values of Track 1","* 100 / Factor(1) - Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-20]{r}"]
[41,"DW 31-60",null,"30 values of Track 2","* 100 / Factor(2) - Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W21-50]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor","407_GlueJet_LongSeal.1","###INDEX:407_GlueJet_LongSeal.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor","407_GlueJet_LongSeal.1","###INDEX:407_GlueJet_LongSeal.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 110",null,"Factor(1)","407_GlueJet_LongSeal.11","###INDEX:407_GlueJet_LongSeal.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 111",null,"Factor(2)","407_GlueJet_LongSeal.11","###INDEX:407_GlueJet_LongSeal.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_2>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (21)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (20)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseaender2>[B]{w}"]
[41,"DW 11-70",null,"60 values of Track 3","* 100 / Factor(3) - Distance(3)",null,"Ch1.###MNR_T_duese2<.m###MNR_duese3>[W1-60]{r}"]
[41,"DW 100",null,"Distance(3) photocell-jet * 100 / Factor","407_GlueJet_LongSeal.1","###INDEX:407_GlueJet_LongSeal.1:INDEX","Ch1.###MNR_T_duese2<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 110",null,"Factor(3)","407_GlueJet_LongSeal.11","###INDEX:407_GlueJet_LongSeal.11:INDEX","Ch1.###MNR_T_duese2<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 120",null,"Offset, Track 3 (1)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 3 (60)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X407_GlueJet_LongSeal1","index":24,"n_rows":13,"n_cols":7,"rows_kept":13,"flags":["formulas_cached_only"]}
["X407_GlueJet_LongSeal1","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[41,"DB 116-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseaender2>[B]{w}"]
[41,"DW 11-70",null,"60 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese2<.m###MNR_duese3>[W1-60]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor","407_GlueJet_LongSeal1.1","###INDEX:407_GlueJet_LongSeal1.1:INDEX","Ch1.###MNR_T_duese2<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 110",null,"Factor","407_GlueJet_LongSeal1.11","###INDEX:407_GlueJet_LongSeal1.11:INDEX","Ch1.###MNR_T_duese2<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (60)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X407_GlueJetPaper","index":25,"n_rows":20,"n_cols":6,"rows_kept":20,"flags":["formulas_cached_only"]}
["X407_GlueJetPaper","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[41,"DB 115-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseaenderpap>[B]{w}"]
[41,"DW 11",null,"Start of gluing, Track 1","* 100 / Factor(1) - Distance(1)","Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W1]{r}"]
[41,"DW 12",null,"End of gluing, Track 1","* 100 / Factor(1) – Distance(1)","Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W2]{r}"]
[41,"DW 41",null,"Start of gluing, Track 2","* 100 / Factor(2) – Distance(2)","Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W31]{r}"]
[41,"DW 42",null,"End of gluing, Track 2","* 100 / Factor(2) – Distance(2)","Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W32]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","407_GlueJetPaper.1","Ch1.###MNR_T_duesepap<.m###MNR_dueseabstpap_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(2)","407_GlueJetPaper.1","Ch1.###MNR_T_duesepap<.m###MNR_dueseabstpap_2>[W]{r}"]
[41,"DW 110",null,"Factor(1)","407_GlueJetPaper.11","Ch1.###MNR_T_duesepap<.m###MNR_duesefaktpap_1>[W]{r}"]
[41,"DW 111",null,"Factor(2)","407_GlueJetPaper.11","Ch1.###MNR_T_duesepap<.m###MNR_duesefaktpap_2>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseoffsetpap_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (31)",null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseoffsetpap_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (2)",null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseanzahlpap_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (2)",null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseanzahlpap_2>[W]{r}"]

{"sheet":"X409_GlueJet","index":26,"n_rows":33,"n_cols":7,"rows_kept":33,"flags":["formulas_cached_only"]}
["X409_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 -119","Glue jets"]
[41,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[41,"DB 115 ","Glue jets 1st Machine "]
[41,"DB 116-119","Glue jets Machine 2-5"]
[1,"###MAIN"]
[1,"DB 110-119 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-30",null,"20 values of Track 1","* 100 / Factor(1) – Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-20]{r}"]
[41,"DW 31-60",null,"30 values of Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W21-50]{r}"]
[41,"DW 61-x",null,"1 to x value of Track 3","* 100 / Factor(3) – Distance(3)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W51-x]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","409_GlueJet.1","###INDEX:409_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(2)","409_GlueJet.1","###INDEX:409_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 102",null,"Distance(3) photocell-jet * 100 / Factor(3)","409_GlueJet.1","###INDEX:409_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_4>[W]{r}"]
[41,"DW 110",null,"Factor(1)","409_GlueJet.11","###INDEX:409_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 111",null,"Factor(2)","409_GlueJet.11","###INDEX:409_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 112",null,"Factor(3)","409_GlueJet.11","###INDEX:409_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_4>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (21)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 122",null,"Offset, Track 3 (59)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_4>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (20)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (x)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_4>[W]{r}"]
[21,"DB ###ADDR:115+1[MNR]:ADDR",null,"Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseaender2>[B]{w}"]
[41,"DW 11-70",null,"60 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese2<.m###MNR_duese2>[W1-60]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor ","409_GlueJet.1","###INDEX:409_GlueJet.1:INDEX","Ch1.###MNR_T_duese2<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 110",null,"Factor ","409_GlueJet.11","###INDEX:409_GlueJet.11:INDEX","Ch1.###MNR_T_duese2<.m###MNR_duesefakt_2>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots (60)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X409_GlueJetBOW","index":27,"n_rows":18,"n_cols":7,"rows_kept":18,"flags":["formulas_cached_only"]}
["X409_GlueJetBOW","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[41,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 31-60",null,"30 values of Track 1","* 100 / Factor(1) – Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W21-50]{r}"]
[41,"DW 69-x",null,"1 to x value of Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W51-x]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(1)","409_GlueJetBOW.1","###INDEX:409_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 102",null,"Distance(2) photocell-jet * 100 / Factor(2)","409_GlueJetBOW.1","###INDEX:409_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_4>[W]{r}"]
[41,"DW 111",null,"Factor(1)","409_GlueJetBOW.11","###INDEX:409_GlueJetBOW.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 112",null,"Factor(2)","409_GlueJetBOW.11","###INDEX:409_GlueJetBOW.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_4>[W]{r}"]
[41,"DW 121",null,"Offset, Track 1 (21)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 122",null,"Offset, Track 2  (59)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_4>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 1 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 2 (x)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_4>[W]{r}"]

{"sheet":"X409_GlueJetBOWDB","index":28,"n_rows":21,"n_cols":7,"rows_kept":21,"flags":["formulas_cached_only"]}
["X409_GlueJetBOWDB","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 -119","Glue jets"]
[41,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[41,"DB 115 ","Glue jets 1st Machine "]
[41,"DB 116-119","Glue jets Machine 2-5"]
[1,"###MAIN"]
[1,"DB 110-119 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-40",null,"30 values of Track 1","* 100 / Factor(1) – Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-30]{r}"]
[41,"DW 41-70",null,"30 values of Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-60]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","409_GlueJetBOWDB.1","###INDEX:409_GlueJetBOWDB.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(2)","409_GlueJetBOWDB.2","###INDEX:409_GlueJetBOWDB.2:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 110",null,"Factor(1)","409_GlueJetBOWDB.11","###INDEX:409_GlueJetBOWDB.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 111",null,"Factor(2)","409_GlueJetBOWDB.11","###INDEX:409_GlueJetBOWDB.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_2>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (31)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X409_GlueJetJumbo","index":29,"n_rows":36,"n_cols":7,"rows_kept":36,"flags":["formulas_cached_only"]}
["X409_GlueJetJumbo","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 -119","Glue jets"]
[41,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[41,"DB 115 ","Glue jets 1st Machine "]
[41,"DB 116-119","Glue jets Machine 2-5"]
[1,"###MAIN"]
[1,"DB 110-119 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-25",null,"15 values of Track 1","* 100 / Factor(1) – Distance(1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-15]{r}"]
[41,"DW 26-40",null,"15 values of Track 2","* 100 / Factor(2) – Distance(2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W16-300]{r}"]
[41,"DW 41-55",null,"15 values of Track 3","* 100 / Factor(3) – Distance(3)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-45]{r}"]
[41,"DW 56-70",null,"15 values of Track 4","* 100 / Factor(4) – Distance(4)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W46-60]{r}"]
[41,"DW 71-x",null,"1 to x value of Track 5","* 100 / Factor(5) – Distance(5)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W61-x]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","409_GlueJetJumbo.1","###INDEX:409_GlueJetJumbo.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(2)","409_GlueJetJumbo.1","###INDEX:409_GlueJetJumbo.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 102",null,"Distance(3) photocell-jet * 100 / Factor(3)","409_GlueJetJumbo.1","###INDEX:409_GlueJetJumbo.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 103",null,"Distance(4) photocell-jet * 100 / Factor(4)","409_GlueJetJumbo.1","###INDEX:409_GlueJetJumbo.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_4>[W]{r}"]
[41,"DW 104",null,"Distance(5) photocell-jet * 100 / Factor(5)","409_GlueJetJumbo.1","###INDEX:409_GlueJetJumbo.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_5>[W]{r}"]
[41,"DW 110",null,"Factor(1)","409_GlueJetJumbo.11","###INDEX:409_GlueJetJumbo.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 111",null,"Factor(2)","409_GlueJetJumbo.11","###INDEX:409_GlueJetJumbo.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_2>[W]{r}"]
[41,"DW 112",null,"Factor(3)","409_GlueJetJumbo.11","###INDEX:409_GlueJetJumbo.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 113",null,"Factor(4)","409_GlueJetJumbo.11","###INDEX:409_GlueJetJumbo.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_4>[W]{r}"]
[41,"DW 114",null,"Factor(5)","409_GlueJetJumbo.11","###INDEX:409_GlueJetJumbo.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_5>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (16)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 122",null,"Offset, Track 3 (31)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 123",null,"Offset, Track 4 (46)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_4>[W]{r}"]
[41,"DW 124",null,"Offset, Track 5 (61)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_5>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]
[41,"DW 133",null,"No. of glue dots, Track 4 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_4>[W]{r}"]
[41,"DW 134",null,"No. of glue dots, Track 5 (x)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_5>[W]{r}"]

{"sheet":"X409_GlueJetJumboMax","index":30,"n_rows":29,"n_cols":7,"rows_kept":29,"flags":["formulas_cached_only"]}
["X409_GlueJetJumboMax","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 10",null,"Distance(1) photocell-jet","411_GlueJetBOW.1","###INDEX:411_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_10>[W]{r}"]
[41,"DW 14",null,"Distance(5) photocell-jet","411_GlueJetBOW.1","###INDEX:411_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_14>[W]{r}"]
[41,"DW 15",null,"Distance(6) photocell-jet","411_GlueJetBOW.1","###INDEX:411_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_15>[W]{r}"]
[41,"DW 16",null,"Distance(7) photocell-jet","411_GlueJetBOW.1","###INDEX:411_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_16>[W]{r}"]
[41,"DW 17",null,"Distance(8) photocell-jet","411_GlueJetBOW.1","###INDEX:411_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_17>[W]{r}"]
[41,"DW 20",null,"Offset, Track 1 (60)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_20>[W]{r}"]
[41,"DW 24",null,"Offset, Track 5  (70)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_24>[W]{r}"]
[41,"DW 25",null,"Offset, Track 6  (90)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_25>[W]{r}"]
[41,"DW 26",null,"Offset, Track 7  (150)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_26>[W]{r}"]
[41,"DW 27",null,"Offset, Track 8  (170)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_27>[W]{r}"]
[41,"DW 30",null,"No. of glue dots, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_30>[W]{r}"]
[41,"DW 34",null,"No. of glue dots, Track 5 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_34>[W]{r}"]
[41,"DW 35",null,"No. of glue dots, Track 6 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_35>[W]{r}"]
[41,"DW 36",null,"No. of glue dots, Track 7 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_36>[W]{r}"]
[41,"DW 37",null,"No. of glue dots, Track 8 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_37>[W]{r}"]
[41]
[41,"DW 60",null,"1 value of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W0]{r}"]
[41,"DW 70-84",null,"15 values of Track 5",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W10-24]{r}"]
[41,"DW 90-105",null,"15 values of Track 6",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W30-44]{r}"]
[41,"DW 150-164",null,"15 values of Track 7",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W90-105]{r}"]
[41,"DW 170-184",null,"15 values of Track 8",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W110-124]{r}"]

{"sheet":"X409_GlueJetPaper","index":31,"n_rows":21,"n_cols":7,"rows_kept":21,"flags":["formulas_cached_only"]}
["X409_GlueJetPaper","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[41,"DB 115-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseaenderpap>[B]{w}"]
[41,"DW 11",null,"Start of gluing, Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W1]{r}"]
[41,"DW 12",null,"End of gluing, Track 1","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W2]{r}"]
[41,"DW 41",null,"Start of gluing, Track 2","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W31]{r}"]
[41,"DW 42",null,"End of gluing, Track 2","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W32]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor","409_GlueJetPaper.1","###INDEX:409_GlueJetPaper.1:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_dueseabstpap_1>[W]{r}"]
[41,"DW 110",null,"Factor","409_GlueJetPaper.11","###INDEX:409_GlueJetPaper.11:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_duesefaktpap_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1(1)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseoffsetpap_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (31)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseoffsetpap_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (2)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseanzahlpap_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (2)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseanzahlpap_2>[W]{r}"]
[41,"DW 140",null,"Glue quantity, jet","409_GlueJetPaper.14","###INDEX:409_GlueJetPaper.14:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_dueseleimmenge_1>[W]{r}"]
[41,"DW 141",null,"Glue quantity, jet","409_GlueJetPaper.14","###INDEX:409_GlueJetPaper.14:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_dueseleimmenge_1>[W]{r}"]
[{"$nulls":3},"Leimgröße","409_GlueJetPaper.17","###INDEX:409_GlueJetPaper.17:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_dueseleimmenge_2>[W]{r}"]

{"sheet":"X411_GlueJetBOW","index":32,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
["X411_GlueJetBOW","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[41,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 10",null,"Distance(1) photocell-jet","411_GlueJetBOW.1","###INDEX:411_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_10>[W]{r}"]
[41,"DW 11",null,"Distance(2) photocell-jet","411_GlueJetBOW.1","###INDEX:411_GlueJetBOW.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_11>[W]{r}"]
[41,"DW 20",null,"Offset, Track 1 (60)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_20>[W]{r}"]
[41,"DW 21",null,"Offset, Track 2  (100)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_21>[W]{r}"]
[41,"DW 30",null,"No. of glue dots, Track 1 (32)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_30>[W]{r}"]
[41,"DW 31",null,"No. of glue dots, Track 2 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_31>[W]{r}"]
[41]
[41,"DW 60-91",null,"32 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W0-31]{r}"]
[41,"DW 100",null,"1 value of Track 2",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W40]{r}"]

{"sheet":"X411_GlueJetPaper","index":33,"n_rows":21,"n_cols":7,"rows_kept":21,"flags":["formulas_cached_only"]}
["X411_GlueJetPaper","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 12",null,"Distance photocell-jet (1)","411_GlueJetPaper.1","###INDEX:411_GlueJetPaper.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_12>[W]{r}"]
[41,"DW 13",null,"Distance photocell-jet (2)","411_GlueJetPaper.1","###INDEX:411_GlueJetPaper.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_13>[W]{r}"]
[41,"DW 22",null,"Offset, Track 1 (110)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_22>[W]{r}"]
[41,"DW 23",null,"Offset, Track 2 (130)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_23>[W]{r}"]
[41,"DW 32",null,"No. of glue lines, Track 1 (6)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_32>[W]{r}"]
[41,"DW 33",null,"No. of glue lines, Track 2 (6)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_33>[W]{r}"]
[41,"DW 40",null,"Glue quantity, jet","411_GlueJetPaper.14","###INDEX:411_GlueJetPaper.14:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleimmenge>[W]{r}"]
[41,"DW 41",null,"Value 1","411_GlueJetPaper.15","###INDEX:411_GlueJetPaper.15:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesesonder1>[W]{r}"]
[41,"DW 42",null,"Value 2","411_GlueJetPaper.16","###INDEX:411_GlueJetPaper.16:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesesonder2>[W]{r}"]
[41,"DW 43",null,"Glue quantity, jet Track2","411_GlueJetPaper.17","###INDEX:411_GlueJetPaper.17:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleimmenge2>[W]{r}"]
[41]
[41,"DW 110-115",null,"6 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W50-55]{r}"]
[41,"DW 130-135",null,"6  values of Track 2",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W70-75]{r}"]

{"sheet":"X550_GlueJet","index":34,"n_rows":22,"n_cols":7,"rows_kept":22,"flags":["formulas_cached_only"]}
["X550_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-39",null,"19 values of Track 2","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41]
[41,"DW 90",null,"Glue min.","550_GlueJet.34","###INDEX:550_GlueJet.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","550_GlueJet.31","###INDEX:550_GlueJet.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","550_GlueJet.32","###INDEX:550_GlueJet.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","550_GlueJet.33","###INDEX:550_GlueJet.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","550_GlueJet.1","###INDEX:550_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","550_GlueJet.11","###INDEX:550_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X550_GlueJet_3","index":35,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
["X550_GlueJet_3","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-29",null,"9 values of Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41,"DW 31-49",null,"19 values of Track 3","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-49]{r}"]
[41]
[41,"DW 90",null,"Glue min.","550_GlueJet_3.34","###INDEX:550_GlueJet_3.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","550_GlueJet_3.31","###INDEX:550_GlueJet_3.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","550_GlueJet_3.32","###INDEX:550_GlueJet_3.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","550_GlueJet_3.33","###INDEX:550_GlueJet_3.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","550_GlueJet_3.1","###INDEX:550_GlueJet_3.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","550_GlueJet_3.11","###INDEX:550_GlueJet_3.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 122",null,"Offset, Track 3 (21)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X550_GlueJet_PacketTrack","index":36,"n_rows":35,"n_cols":7,"rows_kept":35,"flags":["formulas_cached_only"]}
["X550_GlueJet_PacketTrack","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[41,"DB 115-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptraender>[B]{w}"]
[41,"DW 10",null,"Distance photocell-jet (1)","550_GlueJet_PacketTrack.1","###INDEX:550_GlueJet_PacketTrack.1:INDEX","Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrabst_11>[W]{r}"]
[41,"DW 11",null,"Distance photocell-jet (2)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrabst_12>[W]{r}"]
[41,"DW 12",null,"Distance photocell-jet (3) (Hotmelt)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrabst_13>[W]{r}"]
[41,"DW 20",null,"Offset, Track 1 (60)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptroffset_20>[W]{r}"]
[41,"DW 21",null,"Offset, Track 2 (90)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptroffset_21>[W]{r}"]
[41,"DW 22",null,"Offset, Track 3 (120) (Hotmelt)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptroffset_22>[W]{r}"]
[41,"DW 30",null,"No. of glue dots, Track 1 (25)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptranzahl_30>[W]{r}"]
[41,"DW 31",null,"No. of glue dots, Track 2 (25)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptranzahl_31>[W]{r}"]
[41,"DW 32",null,"No. of glue dots, Track 2 (10)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptranzahl_32>[W]{r}"]
[41]
[41,"DW 40",null,"Abstand Düse 1 und 2",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR__dueseptrabst1_2>[W]{r}"]
[41]
[41,"DW 43",null,"Geschwindigkeitsgrenze 1 (0 - xxx)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrgeschw>[W0]{r}"]
[41,"DW 44",null,"Geschwindigkeitsgrenze 2 (xxx - yyy)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrgeschw>[W1]{r}"]
[41]
[41,"DW 50",null,"Zeit Kaltleim Bereich 1 (0 - xxx)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrzeitcold>[W0]{r}"]
[41,"DW 51",null,"Zeit Kaltleim Bereich 2 (xxx - yyy)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrzeitcold>[W1]{r}"]
[41,"DW 52",null,"Zeit Kaltleim Bereich 3 (yyy - )",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrzeitcold>[W2]{r}"]
[41]
[41,"DW 55",null,"Zeit Kaltleim Bereich 1 (0 - xxx)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrzeithot>[W0]{r}"]
[41,"DW 56",null,"Zeit Kaltleim Bereich 2 (xxx - yyy)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrzeithot>[W1]{r}"]
[41,"DW 57",null,"Zeit Kaltleim Bereich 3 (yyy - )",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptrzeithot>[W2]{r}"]
[41]
[41]
[41,"DW 60-84",null,"25 values of Track 1",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptr>[W0-24]{r}"]
[41,"DW 90-114",null,"25  values of Track 2",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptr>[W30-54]{r}"]
[41,"DW 120-129",null,"10  values of Track 3 (Hotmelt)",null,null,"Ch1.###MNR_T_dueseptr<.m###MNR_dueseptr>[W60-69]{r}"]

{"sheet":"X700_GlueJet","index":37,"n_rows":22,"n_cols":7,"rows_kept":22,"flags":["formulas_cached_only"]}
["X700_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-39",null,"19 values of Track 2","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41]
[41,"DW 90",null,"Glue min.","700_GlueJet.34","###INDEX:700_GlueJet.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","700_GlueJet.31","###INDEX:700_GlueJet.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","700_GlueJet.32","###INDEX:700_GlueJet.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","700_GlueJet.33","###INDEX:700_GlueJet.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","700_GlueJet.1","###INDEX:700_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","700_GlueJet.11","###INDEX:700_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X700_GlueJet_3","index":38,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
["X700_GlueJet_3","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-29",null,"9 values of Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41,"DW 31-49",null,"19 values of Track 3","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-49]{r}"]
[41]
[41,"DW 90",null,"Glue min.","700_GlueJet_3.34","###INDEX:700_GlueJet_3.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","700_GlueJet_3.31","###INDEX:700_GlueJet_3.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","700_GlueJet_3.32","###INDEX:700_GlueJet_3.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","700_GlueJet_3.33","###INDEX:700_GlueJet_3.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","700_GlueJet_3.1","###INDEX:700_GlueJet_3.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","700_GlueJet_3.11","###INDEX:700_GlueJet_3.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 122",null,"Offset, Track 3 (21)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X701_GlueJet","index":39,"n_rows":22,"n_cols":7,"rows_kept":22,"flags":["formulas_cached_only"]}
["X701_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-39",null,"19 values of Track 2","* 100 / Factor – Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41]
[41,"DW 90",null,"Glue min.","701_GlueJet.34","###INDEX:701_GlueJet.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","701_GlueJet.31","###INDEX:701_GlueJet.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","701_GlueJet.32","###INDEX:701_GlueJet.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","701_GlueJet.33","###INDEX:701_GlueJet.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","701_GlueJet.1","###INDEX:701_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","701_GlueJet.11","###INDEX:701_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X701_GlueJet_3","index":40,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
["X701_GlueJet_3","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-19",null,"9 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-9]{r}"]
[41,"DW 21-29",null,"9 values of Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-29]{r}"]
[41,"DW 31-49",null,"19 values of Track 3","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-49]{r}"]
[41]
[41,"DW 90",null,"Glue min.","701_GlueJet_3.34","###INDEX:701_GlueJet_3.34:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_min>[W]{r}"]
[41,"DW 91",null,"Glue max.","701_GlueJet_3.31","###INDEX:701_GlueJet_3.31:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_max>[W]{r}"]
[41,"DW 92",null,"Glue setpoint","701_GlueJet_3.32","###INDEX:701_GlueJet_3.32:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_soll>[W]{r}"]
[41,"DW 93",null,"Glue actual","701_GlueJet_3.33","###INDEX:701_GlueJet_3.33:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleim_ist>[W]{p}"]
[41]
[41,"DW 100",null,"Distance, photocell-jet * 100 / Factor","701_GlueJet_3.1","###INDEX:701_GlueJet_3.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","701_GlueJet_3.11","###INDEX:701_GlueJet_3.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 122",null,"Offset, Track 3 (21)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (19)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X707_GlueJet_LongSeal1","index":41,"n_rows":13,"n_cols":7,"rows_kept":13,"flags":["formulas_cached_only"]}
["X707_GlueJet_LongSeal1","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[41,"DB 116-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseaender2>[B]{w}"]
[41,"DW 11-70",null,"60 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese2<.m###MNR_duese3>[W1-60]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor","707_GlueJet_LongSeal1.1","###INDEX:707_GlueJet_LongSeal1.1:INDEX","Ch1.###MNR_T_duese2<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 110",null,"Factor","707_GlueJet_LongSeal1.11","###INDEX:707_GlueJet_LongSeal1.11:INDEX","Ch1.###MNR_T_duese2<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (60)",null,null,"Ch1.###MNR_T_duese2<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X707_GlueJetLabel","index":42,"n_rows":24,"n_cols":7,"rows_kept":24,"flags":["formulas_cached_only"]}
["X707_GlueJetLabel","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[]
[21,"DB 110 ","Glue jets 1st Machine "]
[41,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabaender>[B]{w}"]
[41,"DW 11-26",null,"16 values of Track 1","* 100 / Factor - Distance(1)",null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W1-16]{r}"]
[41,"DW 31-46",null,"16 values of Track 2","* 100 / Factor - Distance(2)",null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W21-36]{r}"]
[41,"DW 51-66",null,"16 values of Track 3","* 100 / Factor - Distance(1)",null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W41-56]{r}"]
[41,"DW 71-86",null,"16 values of Track 4","* 100 / Factor - Distance(2)",null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W61-76]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor","707_GlueJetLabel.1","###INDEX:707_GlueJetLabel.1:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselababst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor","707_GlueJetLabel.2","###INDEX:707_GlueJetLabel.2:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselababst_2>[W]{r}"]
[41,"DW 110",null,"Factor","707_GlueJetLabel.11","###INDEX:707_GlueJetLabel.11:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselabfakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_1>[W]{r}"]
[41,"DW 122",null,"Offset, Track 2",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_2>[W]{r}"]
[41,"DW 123",null,"Offset, Track 3",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_3>[W]{r}"]
[41,"DW 121",null,"Offset, Track 4",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_4>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_3>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_4>[W]{r}"]
[41,"DW 133",null,"No. of glue dots, Track 4",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_2>[W]{r}"]

{"sheet":"X725_GlueJet","index":43,"n_rows":22,"n_cols":7,"rows_kept":22,"flags":["formulas_cached_only"]}
["X725_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11",null,"1 value of Track 1","* 100 / Factor (1) – Distance (1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1]{r}"]
[41,"DW 21-32",null,"12 values of Track 2","* 100 / Factor (1) – Distance (2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-22]{r}"]
[41,"DW 41-54",null,"14 values of Track 3","* 100 / Factor (3) – Distance (3)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-44]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","725_GlueJet.1","###INDEX:725_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(1)","725_GlueJet.2","###INDEX:725_GlueJet.2:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 102",null,"Distance(3) photocell-jet * 100 / Factor(3)","725_GlueJet.3","###INDEX:725_GlueJet.3:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 110",null,"Factor(1)","725_GlueJet.11","###INDEX:725_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 112",null,"Factor(3)","725_GlueJet.13","###INDEX:725_GlueJet.13:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 121",null,"Offset, Track3 (31)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (12)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (14)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X726_GlueJet","index":44,"n_rows":22,"n_cols":7,"rows_kept":22,"flags":["formulas_cached_only"]}
["X726_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11",null,"1 value of Track 1","* 100 / Factor (1) – Distance (1)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1]{r}"]
[41,"DW 21-32",null,"12 values of Track 2","* 100 / Factor (1) – Distance (2)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W11-22]{r}"]
[41,"DW 41-54",null,"14 values of Track 3","* 100 / Factor (3) – Distance (3)",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-44]{r}"]
[41,"DW 100",null,"Distance(1) photocell-jet * 100 / Factor(1)","726_GlueJet.1","###INDEX:726_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 101",null,"Distance(2) photocell-jet * 100 / Factor(2)","726_GlueJet.2","###INDEX:726_GlueJet.2:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_2>[W]{r}"]
[41,"DW 102",null,"Distance(3) photocell-jet * 100 / Factor(3)","726_GlueJet.3","###INDEX:726_GlueJet.3:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_3>[W]{r}"]
[41,"DW 110",null,"Factor(1)","726_GlueJet.11","###INDEX:726_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 112",null,"Factor(3)","726_GlueJet.13","###INDEX:726_GlueJet.13:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_3>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (11)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 121",null,"Offset, Track3 (31)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_3>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (12)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]
[41,"DW 132",null,"No. of glue dots, Track 3 (14)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_3>[W]{r}"]

{"sheet":"X751_GlueJet","index":45,"n_rows":14,"n_cols":7,"rows_kept":14,"flags":["formulas_cached_only"]}
["X751_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 10",null,"Distance photocell-jet","751_GlueJet.1","###INDEX:751_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_10>[W]{r}"]
[41,"DW 20",null,"Offset, Track 1 (60)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_20>[W]{r}"]
[41,"DW 30",null,"No. of glue dots, Track 1 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_30>[W]{r}"]
[41,"DW 40",null,"Glue quantity, jet","751_GlueJet.3","###INDEX:751_GlueJet.3:INDEX","Ch1.###MNR_T_duese<.m###MNR_anzduese>[W]{r}"]
[41]
[41,"DW 60-74",null,"15 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W0-14]{r}"]

{"sheet":"X751_GlueJetOnsert","index":46,"n_rows":13,"n_cols":7,"rows_kept":13,"flags":["formulas_cached_only"]}
["X751_GlueJetOnsert","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 12",null,"Distance photocell-jet","751_GlueJetOnsert.1","###INDEX:751_GlueJetOnsert.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_12>[W]{r}"]
[41,"DW 22",null,"Offset, Track 1 (100)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_22>[W]{r}"]
[41,"DW 32",null,"No. of glue dots, Track 1 (10)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_32>[W]{r}"]
[41]
[41,"DW 100-109",null,"10 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W0-14]{r}"]

{"sheet":"X752_GlueJet","index":47,"n_rows":14,"n_cols":7,"rows_kept":14,"flags":["formulas_cached_only"]}
["X752_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 10",null,"Distance photocell-jet","752_GlueJet.1","###INDEX:752_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_10>[W]{r}"]
[41,"DW 20",null,"Offset, Track 1 (60)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_20>[W]{r}"]
[41,"DW 30",null,"No. of glue dots, Track 1 (15)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_30>[W]{r}"]
[41,"DW 40",null,"Glue quantity, jet","752_GlueJet.3","###INDEX:752_GlueJet.3:INDEX","Ch1.###MNR_T_duese<.m###MNR_anzduese>[W]{r}"]
[41]
[41,"DW 60-74",null,"15 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W0-14]{r}"]

{"sheet":"X778_GlueJet","index":48,"n_rows":16,"n_cols":7,"rows_kept":16,"flags":["formulas_cached_only"]}
["X778_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 11-40",null,"30 values of Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W1-30]{r}"]
[41,"DW 41-49",null,"9  values of Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W31-39]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor","778_GlueJet.1","###INDEX:778_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_1>[W]{r}"]
[41,"DW 110",null,"Factor","778_GlueJet.11","###INDEX:778_GlueJet.11:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesefakt_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (31)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_2>[W]{r}"]

{"sheet":"X778_GlueJetPaper","index":49,"n_rows":19,"n_cols":7,"rows_kept":19,"flags":["formulas_cached_only"]}
["X778_GlueJetPaper","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[41,"DB 115-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseaenderpap>[B]{w}"]
[41,"DW 11",null,"Start of gluing, Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W1]{r}"]
[41,"DW 12",null,"End of gluing, Track 1","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W2]{r}"]
[41,"DW 41",null,"Start of gluing, Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W31]{r}"]
[41,"DW 42",null,"End of gluing, Track 2","* 100 / Factor - Distance",null,"Ch1.###MNR_T_duesepap<.m###MNR_duesepap>[W32]{r}"]
[41,"DW 100",null,"Distance photocell-jet * 100 / Factor","778_GlueJetPaper.1","###INDEX:778_GlueJetPaper.1:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_dueseabstpap_1>[W]{r}"]
[41,"DW 110",null,"Factor","778_GlueJetPaper.11","###INDEX:778_GlueJetPaper.11:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_duesefaktpap_1>[W]{r}"]
[41,"DW 120",null,"Offset, Track 1 (1)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseoffsetpap_1>[W]{r}"]
[41,"DW 121",null,"Offset, Track 2 (31)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseoffsetpap_2>[W]{r}"]
[41,"DW 130",null,"No. of glue dots, Track 1 (2)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseanzahlpap_1>[W]{r}"]
[41,"DW 131",null,"No. of glue dots, Track 2 (2)",null,null,"Ch1.###MNR_T_duesepap<.m###MNR_dueseanzahlpap_2>[W]{r}"]
[41,"DW 140",null,"Glue quantity, jet","778_GlueJetPaper.14","###INDEX:778_GlueJetPaper.14:INDEX","Ch1.###MNR_T_duesepap<.m###MNR_dueseleimmenge_1>[W]{r}"]

{"sheet":"X778_GlueJetPaperMax4","index":50,"n_rows":20,"n_cols":7,"rows_kept":20,"flags":["formulas_cached_only"]}
["X778_GlueJetPaperMax4","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[null,"DB 116-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets",{"$nulls":3},"###INDEX:778_GlueJetPaper.1:INDEX"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4aender>[B]{w}"]
[41,"DW 12",null,"Distance photocell-jet (1)","778_GlueJetPaperMax4.1","###INDEX:778_GlueJetPaperMax4.1:INDEX","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4abst_12>[W]{r}"]
[41,"DW 13",null,"Distance photocell-jet (2)","778_GlueJetPaperMax4.1","###INDEX:778_GlueJetPaperMax4.1:INDEX","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4abst_13>[W]{r}"]
[41,"DW 22",null,"Offset, Track 1 (110)",null,null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4offset_22>[W]{r}"]
[41,"DW 23",null,"Offset, Track 2 (130)",null,null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4offset_23>[W]{r}"]
[41,"DW 32",null,"No. of glue lines, Track 1 (6)",null,null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4anzahl_32>[W]{r}"]
[41,"DW 33",null,"No. of glue lines, Track 2 (6)",null,null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4anzahl_33>[W]{r}"]
[41,"DW 40",null,"Glue quantity, jet","778_GlueJetPaperMax4.14","###INDEX:778_GlueJetPaperMax4.14:INDEX","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4leimmenge>[W]{r}"]
[41,"DW 41",null,"Value 1","778_GlueJetPaperMax4.15","###INDEX:778_GlueJetPaperMax4.15:INDEX","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4sonder1>[W]{r}"]
[41,"DW 42",null,"Value 2","778_GlueJetPaperMax4.16","###INDEX:778_GlueJetPaperMax4.16:INDEX","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4sonder2>[W]{r}"]
[41]
[41,"DW 110-115",null,"6 values of Track 1",null,null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4>[W50-55]{r}"]
[41,"DW 130-135",null,"6  values of Track 2",null,null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4>[W70-75]{r}"]

{"sheet":"X779_GlueJet","index":51,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
["X779_GlueJet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 10",null,"Distance photocell-jet (1)","779_GlueJet.1","###INDEX:779_GlueJet.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_10>[W]{r}"]
[41,"DW 11",null,"Distance photocell-jet (2)","779_GlueJet.2","###INDEX:779_GlueJet.2:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_11>[W]{r}"]
[41,"DW 20",null,"Offset, Track 1 (60)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_20>[W]{r}"]
[41,"DW 21",null,"Offset, Track 2 (100)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_21>[W]{r}"]
[41,"DW 30",null,"No. of glue dots, Track 1 (30)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_30>[W]{r}"]
[41,"DW 31",null,"No. of glue dots, Track 2 (9)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_31>[W]{r}"]
[41]
[41,"DW 60-89",null,"30 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W0-29]{r}"]
[41,"DW 100-108",null,"9  values of Track 2",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W40-48]{r}"]

{"sheet":"X779_GlueJetPaper","index":52,"n_rows":20,"n_cols":7,"rows_kept":20,"flags":["formulas_cached_only"]}
["X779_GlueJetPaper","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 110 ","Glue jets 1st Machine "]
[null,"DB 111-114","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 110-114 Glue jets"]
[21,"DB ###ADDR:110+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseaender>[B]{w}"]
[41,"DW 12",null,"Distance photocell-jet (1)","779_GlueJetPaper.1","###INDEX:779_GlueJetPaper.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_12>[W]{r}"]
[41,"DW 13",null,"Distance photocell-jet (2)","779_GlueJetPaper.1","###INDEX:779_GlueJetPaper.1:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseabst_13>[W]{r}"]
[41,"DW 22",null,"Offset, Track 1 (110)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_22>[W]{r}"]
[41,"DW 23",null,"Offset, Track 2 (130)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseoffset_23>[W]{r}"]
[41,"DW 32",null,"No. of glue lines, Track 1 (6)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_32>[W]{r}"]
[41,"DW 33",null,"No. of glue lines, Track 2 (6)",null,null,"Ch1.###MNR_T_duese<.m###MNR_dueseanzahl_33>[W]{r}"]
[41,"DW 40",null,"Glue quantity, jet","779_GlueJetPaper.14","###INDEX:779_GlueJetPaper.14:INDEX","Ch1.###MNR_T_duese<.m###MNR_dueseleimmenge>[W]{r}"]
[41,"DW 41",null,"Value 1","779_GlueJetPaper.15","###INDEX:779_GlueJetPaper.15:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesesonder1>[W]{r}"]
[41,"DW 42",null,"Value 2","779_GlueJetPaper.16","###INDEX:779_GlueJetPaper.16:INDEX","Ch1.###MNR_T_duese<.m###MNR_duesesonder2>[W]{r}"]
[41]
[41,"DW 110-112",null,"6 values of Track 1",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W50-55]{r}"]
[41,"DW 130-142",null,"6  values of Track 2",null,null,"Ch1.###MNR_T_duese<.m###MNR_duese>[W70-75]{r}"]

{"sheet":"X779_GlueJetLabel","index":53,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
["X779_GlueJetLabel","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 115","Glue jets 1st Machine "]
[41,"DB 115-119","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 115-119 Glue jets"]
[21,"DB ###ADDR:115+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabaender>[B]{w}"]
[41,"DW 10",null,"Distance photocell-jet (1)","779_GlueJetLabel.1","###INDEX:779_GlueJetLabel.1:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselababst_10>[W]{r}"]
[41,"DW 11",null,"Distance photocell-jet (2)","779_GlueJetLabel.2","###INDEX:779_GlueJetLabel.2:INDEX","Ch1.###MNR_T_dueselab<.m###MNR_dueselababst_11>[W]{r}"]
[41,"DW 20",null,"Offset, Track 1 (60)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_20>[W]{r}"]
[41,"DW 21",null,"Offset, Track 2 (80)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselaboffset_21>[W]{r}"]
[41,"DW 30",null,"No. of glue dots, Track 1 (20)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_30>[W]{r}"]
[41,"DW 31",null,"No. of glue dots, Track 2 (20)",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselabanzahl_31>[W]{r}"]
[41]
[41,"DW 60-79",null,"20 values of Track 1",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W0-19]{r}"]
[41,"DW 80-99",null,"20  values of Track 2",null,null,"Ch1.###MNR_T_dueselab<.m###MNR_dueselab>[W20-39]{r}"]

{"sheet":"Manometer","index":54,"n_rows":18,"n_cols":7,"rows_kept":18,"flags":["formulas_cached_only"]}
["Manometer","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 120 ","Manometer 1st Machine "]
[41,"DB 121-124","Manometer Machine  2-5"]
[1,"###MAIN"]
[1,"DB 120-124 Manometer"]
[21,"DB ###ADDR:120+1[MNR]:ADDR","Manometer ###MNR"]
[41,"DW 0","Bit 0","Manometer changed",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_aender>[B]{w}"]
[41,"DW 10",null,"Actual value 1","Manometer.###MNR.11","###INDEX:Manometer.###MNR.11:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W0]{p}"]
[41,"DW 11",null,"Actual value 2","Manometer.###MNR.12","###INDEX:Manometer.###MNR.12:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W1]{p}"]
[41,"DW 12",null,"Actual value 3","Manometer.###MNR.13","###INDEX:Manometer.###MNR.13:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W2]{p}"]
[41,"DW 13",null,"Actual value 4","Manometer.###MNR.14","###INDEX:Manometer.###MNR.14:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W3]{p}"]
[41,"DW 14",null,"Actual value 5","Manometer.###MNR.15","###INDEX:Manometer.###MNR.15:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W4]{p}"]
[41,"DW 15",null,"Actual value 6","Manometer.###MNR.16","###INDEX:Manometer.###MNR.16:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W5]{p}"]
[41,"DW 16",null,"Actual value 7","Manometer.###MNR.17","###INDEX:Manometer.###MNR.17:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W6]{p}"]
[41,"DW 17",null,"Actual value 8","Manometer.###MNR.18","###INDEX:Manometer.###MNR.18:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist>[W7]{p}"]
[41,"DW 20-27",null,"Setpoint 1-8",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_soll>[W0-7]{r}"]
[41,"DW 30-37",null,"2nd limit value 1-8",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_grenz>[W0-7]{r}"]

{"sheet":"ManometerExt","index":55,"n_rows":30,"n_cols":7,"rows_kept":30,"flags":["formulas_cached_only"]}
["ManometerExt","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 120 ","Manometer 1st Machine "]
[41,"DB 121-124","Manometer Machine  2-5"]
[1,"###MAIN"]
[1,"DB 120-124 Manometer"]
[21,"DB ###ADDR:120+1[MNR]:ADDR","Manometer ###MNR"]
[41,"DW 0","Bit 0","Manometer changed",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_aender>[B]{w}"]
[41,"DW 10",null,"Actual value 1","Manometer.###MNR.11","###INDEX:Manometer.###MNR.11:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W0]{p}"]
[41,"DW 11",null,"Actual value 2","Manometer.###MNR.12","###INDEX:Manometer.###MNR.12:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W1]{p}"]
[41,"DW 12",null,"Actual value 3","Manometer.###MNR.13","###INDEX:Manometer.###MNR.13:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W2]{p}"]
[41,"DW 13",null,"Actual value 4","Manometer.###MNR.14","###INDEX:Manometer.###MNR.14:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W3]{p}"]
[41,"DW 14",null,"Actual value 5","Manometer.###MNR.15","###INDEX:Manometer.###MNR.15:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W4]{p}"]
[41,"DW 15",null,"Actual value 6","Manometer.###MNR.16","###INDEX:Manometer.###MNR.16:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W5]{p}"]
[41,"DW 16",null,"Actual value 7","Manometer.###MNR.17","###INDEX:Manometer.###MNR.17:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W6]{p}"]
[41,"DW 17",null,"Actual value 8","Manometer.###MNR.18","###INDEX:Manometer.###MNR.18:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist1>[W7]{p}"]
[41,"DW 20-27",null,"Setpoint 1-8",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_soll1>[W0-7]{r}"]
[41,"DW 30-37",null,"2nd limit value 1-8",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_grenz1>[W0-7]{r}"]
[41,"DW 40",null,"Actual value 9","Manometer.###MNR.19","###INDEX:Manometer.###MNR.19:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W0]{p}"]
[41,"DW 41",null,"Actual value 10","Manometer.###MNR.20","###INDEX:Manometer.###MNR.20:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W1]{p}"]
[41,"DW 42",null,"Actual value11","Manometer.###MNR.21","###INDEX:Manometer.###MNR.21:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W2]{p}"]
[41,"DW 43",null,"Actual value 12","Manometer.###MNR.22","###INDEX:Manometer.###MNR.22:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W3]{p}"]
[41,"DW 44",null,"Actual value 13","Manometer.###MNR.23","###INDEX:Manometer.###MNR.23:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W4]{p}"]
[41,"DW 45",null,"Actual value 14","Manometer.###MNR.24","###INDEX:Manometer.###MNR.24:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W5]{p}"]
[41,"DW 46",null,"Actual value 15","Manometer.###MNR.25","###INDEX:Manometer.###MNR.25:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W6]{p}"]
[41,"DW 47",null,"Actual value 16","Manometer.###MNR.26","###INDEX:Manometer.###MNR.26:INDEX","Ch1.###MNR_T_manometer<.m###MNR_mano_ist2>[W7]{p}"]
[41,"DW 50-57",null,"Setpoint 9-16",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_soll2>[W0-7]{r}"]
[41,"DW 60-67",null,"2nd limit value 9-16",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_grenz2>[W0-7]{r}"]
[41]
[41,"DW 69","Bit 0 - 15","Manometer 1-16 exist",null,null,"Ch1.###MNR_T_manometer<.m###MNR_mano_vorhanden>[W]{r}"]

{"sheet":"Servo","index":56,"n_rows":97,"n_cols":7,"rows_kept":97,"flags":["formulas_cached_only"]}
["Servo","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 130 ","Servo 1, 1st Machine "]
[21,"DB 131-138","Servo 2-9 1st Machine "]
[21,"DB 140-178","Servo Machine 2-5"]
[21,"DB 540","Servo 11, 1st Machine "]
[21,"DB 541-579","Servo 12-50 1st Machine "]
[41,"DB 580-729","Servo Machine 2-5"]
[1,"###MAIN"]
[1,"DB 130-179 / 540-739 Servos"]
[21,"###IF FLD<11 ###THEN DB ###ADDR:129+10[MNR]+1[FLD]:ADDR###ELSE DB ###ADDR:529+40[MNR]+1[FLD]:ADDR###ENDIF","Servo ###FLD, ###MNR"]
[41,null,null,"###INDEX:Servo.###MNR.Servo###FLD.0:INDEX","Servo.###MNR.Servo###FLD.0","###INDEX:Servo.###MNR.Servo###FLD.0:INDEX"]
[41,"DW 0","Bit 0","Servo changed",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_servoaender_###FLD>[B]{w}"]
[41,"DW 1","Bit 0","Servo not active",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_servopassiv_###FLD>[B]{w}"]
[41,"DD 10",null,"Setpoint 1 ","Servo.###MNR.Servo###FLD.1","###INDEX:Servo.###MNR.Servo###FLD.1:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW0]{r}"]
[41,"DD 12",null,"Setpoint 2 ","Servo.###MNR.Servo###FLD.2","###INDEX:Servo.###MNR.Servo###FLD.2:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW1]{r}"]
[41,"DD 14",null,"Setpoint 3 ","Servo.###MNR.Servo###FLD.3","###INDEX:Servo.###MNR.Servo###FLD.3:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW2]{r}"]
[41,"DD 16",null,"Setpoint 4 ","Servo.###MNR.Servo###FLD.4","###INDEX:Servo.###MNR.Servo###FLD.4:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW3]{r}"]
[41,"DD 18",null,"Setpoint 5 ","Servo.###MNR.Servo###FLD.5","###INDEX:Servo.###MNR.Servo###FLD.5:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW4]{r}"]
[41,"DD 20",null,"Setpoint 6 ","Servo.###MNR.Servo###FLD.6","###INDEX:Servo.###MNR.Servo###FLD.6:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW5]{r}"]
[41,"DD 22",null,"Setpoint 7 ","Servo.###MNR.Servo###FLD.7","###INDEX:Servo.###MNR.Servo###FLD.7:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW6]{r}"]
[41,"DD 24",null,"Setpoint 8 ","Servo.###MNR.Servo###FLD.8","###INDEX:Servo.###MNR.Servo###FLD.8:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW7]{r}"]
[41,"DD 26",null,"Setpoint 9 ","Servo.###MNR.Servo###FLD.9","###INDEX:Servo.###MNR.Servo###FLD.9:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW8]{r}"]
[41,"DD 28",null,"Setpoint 10 ","Servo.###MNR.Servo###FLD.10","###INDEX:Servo.###MNR.Servo###FLD.10:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW9]{r}"]
[41,"DD 30",null,"Setpoint 11 ","Servo.###MNR.Servo###FLD.11","###INDEX:Servo.###MNR.Servo###FLD.11:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW10]{r}"]
[41,"DD 32",null,"Setpoint 12 ","Servo.###MNR.Servo###FLD.12","###INDEX:Servo.###MNR.Servo###FLD.12:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW11]{r}"]
[41,"DD 34",null,"Setpoint 13 ","Servo.###MNR.Servo###FLD.13","###INDEX:Servo.###MNR.Servo###FLD.13:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW12]{r}"]
[41,"DD 36",null,"Setpoint 14 ","Servo.###MNR.Servo###FLD.14","###INDEX:Servo.###MNR.Servo###FLD.14:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW13]{r}"]
[41,"DD 38",null,"Setpoint 15 ","Servo.###MNR.Servo###FLD.15","###INDEX:Servo.###MNR.Servo###FLD.15:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW14]{r}"]
[41,"DD 40",null,"Setpoint 16 ","Servo.###MNR.Servo###FLD.16","###INDEX:Servo.###MNR.Servo###FLD.16:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW15]{r}"]
[41,"DD 42",null,"Setpoint 17 ","Servo.###MNR.Servo###FLD.17","###INDEX:Servo.###MNR.Servo###FLD.17:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW16]{r}"]
[41,"DD 44",null,"Setpoint 18 ","Servo.###MNR.Servo###FLD.18","###INDEX:Servo.###MNR.Servo###FLD.18:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW17]{r}"]
[41,"DD 46",null,"Setpoint 19 ","Servo.###MNR.Servo###FLD.19","###INDEX:Servo.###MNR.Servo###FLD.19:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW18]{r}"]
[41,"DD 48",null,"Setpoint 20 ","Servo.###MNR.Servo###FLD.20","###INDEX:Servo.###MNR.Servo###FLD.20:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_###FLD>[DW19]{r}"]
[41,"DD 50-DD 109",null,"interne Reserve"]
[41,"DD 110-148",null,"Lower limit value 1-20",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_un_###FLD>[DW0-19]{p}"]
[41,"DW 150-189",null,"Fault text, Diagnosis 1",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_fetext_###FLD1>[S0-39]{p}"]
[41,"DW 190","Bit 0","Switch 1","Servo.###MNR.Servo###FLD.101","###INDEX:Servo.###MNR.Servo###FLD.101:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_schalt_###FLD>[DW]{r}"]
[41,null,"Bit 1","Switch 2","Servo.###MNR.Servo###FLD.102","###INDEX:Servo.###MNR.Servo###FLD.102:INDEX"]
[41,null,"Bit 2","Switch 3","Servo.###MNR.Servo###FLD.103","###INDEX:Servo.###MNR.Servo###FLD.103:INDEX"]
[41,null,"Bit 3","Switch 4","Servo.###MNR.Servo###FLD.104","###INDEX:Servo.###MNR.Servo###FLD.104:INDEX"]
[41,"DD 192",null,"Zeichnungsnummer 1","Servo.###MNR.Servo###FLD.121","###INDEX:Servo.###MNR.Servo###FLD.121:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_zeich_###FLD>[DW0]{r}"]
[41,"DD 194",null,"Zeichnungsnummer 2","Servo.###MNR.Servo###FLD.122","###INDEX:Servo.###MNR.Servo###FLD.122:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_zeich_###FLD>[DW1]{r}"]
[41,"DD 200",null,"Setpoint 21","Servo.###MNR.Servo###FLD.131","###INDEX:Servo.###MNR.Servo###FLD.131:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para2_###FLD>[DW0]{r}"]
[41,"DD 202",null,"Setpoint 22","Servo.###MNR.Servo###FLD.132","###INDEX:Servo.###MNR.Servo###FLD.132:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para2_###FLD>[DW1]{r}"]
[41,"DD 204",null,"Setpoint 23","Servo.###MNR.Servo###FLD.133","###INDEX:Servo.###MNR.Servo###FLD.133:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para2_###FLD>[DW2]{r}"]
[41,"DD 206",null,"Setpoint 24","Servo.###MNR.Servo###FLD.134","###INDEX:Servo.###MNR.Servo###FLD.134:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para2_###FLD>[DW3]{r}"]
[41,"DD 210-248",null,"Upper limit value 1-20",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para_ob_###FLD>[DW0-19]{p}"]
[41,"DW 250-289",null,"Fault text, Diagnosis 2",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_fetext_###FLD2>[S0-39]{p}"]
[41,"DD 290-296",null,"Lower limit value 21-24",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para2_un_###FLD>[DW0-3]{r}"]
[41,"DD 300-306",null,"Upper limit value 21-24",null,null,"Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_para2_ob_###FLD>[DW0-3]{r}"]
[41,"DD 310",null,"Diagnosis 1 / 1","Servo.###MNR.Servo###FLD.41","###INDEX:Servo.###MNR.Servo###FLD.41:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW0]{p}"]
[41,"DD 312",null,"Diagnosis 1 / 2 ","Servo.###MNR.Servo###FLD.42","###INDEX:Servo.###MNR.Servo###FLD.42:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW1]{p}"]
[41,"DD 314",null,"Diagnosis 1 / 3 ","Servo.###MNR.Servo###FLD.43","###INDEX:Servo.###MNR.Servo###FLD.43:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW2]{p}"]
[41,"DD 316",null,"Diagnosis 1 / 4 ","Servo.###MNR.Servo###FLD.44","###INDEX:Servo.###MNR.Servo###FLD.44:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW3]{p}"]
[41,"DD 318",null,"Diagnosis 1 / 5 ","Servo.###MNR.Servo###FLD.45","###INDEX:Servo.###MNR.Servo###FLD.45:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW4]{p}"]
[41,"DD 320",null,"Diagnosis 1 / 6 ","Servo.###MNR.Servo###FLD.46","###INDEX:Servo.###MNR.Servo###FLD.46:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW5]{p}"]
[41,"DD 322",null,"Diagnosis 1 / 7 ","Servo.###MNR.Servo###FLD.47","###INDEX:Servo.###MNR.Servo###FLD.47:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW6]{p}"]
[41,"DD 324",null,"Diagnosis 1 / 8 ","Servo.###MNR.Servo###FLD.48","###INDEX:Servo.###MNR.Servo###FLD.48:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW7]{p}"]
[41,"DD 326",null,"Diagnosis 1 / 9 ","Servo.###MNR.Servo###FLD.49","###INDEX:Servo.###MNR.Servo###FLD.49:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW8]{p}"]
[41,"DD 328",null,"Diagnosis 1 / 10","Servo.###MNR.Servo###FLD.50","###INDEX:Servo.###MNR.Servo###FLD.50:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW9]{p}"]
[41,"DD 330",null,"Diagnosis 1 / 11","Servo.###MNR.Servo###FLD.51","###INDEX:Servo.###MNR.Servo###FLD.51:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW10]{p}"]
[41,"DD 332",null,"Diagnosis 1 / 12","Servo.###MNR.Servo###FLD.52","###INDEX:Servo.###MNR.Servo###FLD.52:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW11]{p}"]
[41,"DD 334",null,"Diagnosis 1 / 13","Servo.###MNR.Servo###FLD.53","###INDEX:Servo.###MNR.Servo###FLD.53:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW12]{p}"]
[41,"DD 336",null,"Diagnosis 1 / 14","Servo.###MNR.Servo###FLD.54","###INDEX:Servo.###MNR.Servo###FLD.54:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW13]{p}"]
[41,"DD 338",null,"Diagnosis 1 / 15","Servo.###MNR.Servo###FLD.55","###INDEX:Servo.###MNR.Servo###FLD.55:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW14]{p}"]
[41,"DD 340",null,"Diagnosis 1 / 16","Servo.###MNR.Servo###FLD.56","###INDEX:Servo.###MNR.Servo###FLD.56:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW15]{p}"]
[41,"DD 342",null,"Diagnosis 1 / 17","Servo.###MNR.Servo###FLD.57","###INDEX:Servo.###MNR.Servo###FLD.57:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW16]{p}"]
[41,"DD 344",null,"Diagnosis 1 / 18","Servo.###MNR.Servo###FLD.58","###INDEX:Servo.###MNR.Servo###FLD.58:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW17]{p}"]
[41,"DD 346",null,"Diagnosis 1 / 19","Servo.###MNR.Servo###FLD.59","###INDEX:Servo.###MNR.Servo###FLD.59:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW18]{p}"]
[41,"DD 348",null,"Diagnosis 1 / 20","Servo.###MNR.Servo###FLD.60","###INDEX:Servo.###MNR.Servo###FLD.60:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD1>[DW19]{p}"]
[41,"DD 350-368",null,"Diagnosis 1 / Tabelle 1","Servo.###MNR.Servo###FLD.31","###INDEX:Servo.###MNR.Servo###FLD.31:INDEX"]
[41,"DD 370-388",null,"Diagnosis 1 / Tabelle 2","Servo.###MNR.Servo###FLD.32","###INDEX:Servo.###MNR.Servo###FLD.32:INDEX"]
[41,"DD 390-DD 408",null,"interne Reserve"]
[41,"DD 410",null,"Diagnosis 2 / 1","Servo.###MNR.Servo###FLD.81","###INDEX:Servo.###MNR.Servo###FLD.81:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW0]{p}"]
[41,"DD 412",null,"Diagnosis 2 / 2 ","Servo.###MNR.Servo###FLD.82","###INDEX:Servo.###MNR.Servo###FLD.82:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW1]{p}"]
[41,"DD 414",null,"Diagnosis 2 / 3 ","Servo.###MNR.Servo###FLD.83","###INDEX:Servo.###MNR.Servo###FLD.83:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW2]{p}"]
[41,"DD 416",null,"Diagnosis 2 / 4 ","Servo.###MNR.Servo###FLD.84","###INDEX:Servo.###MNR.Servo###FLD.84:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW3]{p}"]
[41,"DD 418",null,"Diagnosis 2 / 5 ","Servo.###MNR.Servo###FLD.85","###INDEX:Servo.###MNR.Servo###FLD.85:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW4]{p}"]
[41,"DD 420",null,"Diagnosis 2 / 6 ","Servo.###MNR.Servo###FLD.86","###INDEX:Servo.###MNR.Servo###FLD.86:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW5]{p}"]
[41,"DD 422",null,"Diagnosis 2 / 7 ","Servo.###MNR.Servo###FLD.87","###INDEX:Servo.###MNR.Servo###FLD.87:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW6]{p}"]
[41,"DD 424",null,"Diagnosis 2 / 8 ","Servo.###MNR.Servo###FLD.88","###INDEX:Servo.###MNR.Servo###FLD.88:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW7]{p}"]
[41,"DD 426",null,"Diagnosis 2 / 9 ","Servo.###MNR.Servo###FLD.89","###INDEX:Servo.###MNR.Servo###FLD.89:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW8]{p}"]
[41,"DD 428",null,"Diagnosis 2 / 10","Servo.###MNR.Servo###FLD.90","###INDEX:Servo.###MNR.Servo###FLD.90:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW9]{p}"]
[41,"DD 430",null,"Diagnosis 2 / 11","Servo.###MNR.Servo###FLD.91","###INDEX:Servo.###MNR.Servo###FLD.91:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW10]{p}"]
[41,"DD 432",null,"Diagnosis 2 / 12","Servo.###MNR.Servo###FLD.92","###INDEX:Servo.###MNR.Servo###FLD.92:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW11]{p}"]
[41,"DD 434",null,"Diagnosis 2 / 13","Servo.###MNR.Servo###FLD.93","###INDEX:Servo.###MNR.Servo###FLD.93:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW12]{p}"]
[41,"DD 436",null,"Diagnosis 2 / 14","Servo.###MNR.Servo###FLD.94","###INDEX:Servo.###MNR.Servo###FLD.94:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW13]{p}"]
[41,"DD 438",null,"Diagnosis 2 / 15","Servo.###MNR.Servo###FLD.95","###INDEX:Servo.###MNR.Servo###FLD.95:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW14]{p}"]
[41,"DD 440",null,"Diagnosis 2 / 16","Servo.###MNR.Servo###FLD.96","###INDEX:Servo.###MNR.Servo###FLD.96:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW15]{p}"]
[41,"DD 442",null,"Diagnosis 2 / 17","Servo.###MNR.Servo###FLD.97","###INDEX:Servo.###MNR.Servo###FLD.97:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW16]{p}"]
[41,"DD 444",null,"Diagnosis 2 / 18","Servo.###MNR.Servo###FLD.98","###INDEX:Servo.###MNR.Servo###FLD.98:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW17]{p}"]
[41,"DD 446",null,"Diagnosis 2 / 19","Servo.###MNR.Servo###FLD.99","###INDEX:Servo.###MNR.Servo###FLD.99:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW18]{p}"]
[41,"DD 448",null,"Diagnosis 2 / 20","Servo.###MNR.Servo###FLD.100","###INDEX:Servo.###MNR.Servo###FLD.100:INDEX","Ch1.###MNR_T_servo_###FLD<.m###MNR_servo_diag_###FLD2>[DW19]{p}"]
[41,"DD 450-468",null,"Diagnosis 2 / Tabelle 1","Servo.###MNR.Servo###FLD.71","###INDEX:Servo.###MNR.Servo###FLD.71:INDEX"]
[41,"DD 470-488",null,"Diagnosis 2 / Tabelle 2","Servo.###MNR.Servo###FLD.72","###INDEX:Servo.###MNR.Servo###FLD.72:INDEX"]
[41,"DD 490-DD 508",null,"interne Reserve"]

{"sheet":"DiagnosticRegister","index":57,"n_rows":40,"n_cols":7,"rows_kept":40,"flags":["formulas_cached_only"]}
["DiagnosticRegister","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 180","Registerdiagnose, 1st Machine "]
[41,"DB 181-184","Registerdiagnose, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 180-184 Registerdiagnose","Registerdiagnose"]
[21,"DB 180","Registerdiagnose ###MNR"]
[41,"DW 0","Bit 0","Registerdiagnose changed",null,null,"Ch1.###MNR_T_register<.m###MNR_regaender>[B]{w}"]
[null,"DW10-49",null,"Part1","Bobbin.10","###INDEX:Bobbin.10:INDEX"]
[41,"DW 10",null,"Setpoint 1 ","Bobbin.11","###INDEX:Bobbin.11:INDEX","Ch1.###MNR_T_register<.m###MNR_reg1soll>[W0]{r}"]
[41,"DW 11",null,"Setpoint 2 ","Bobbin.12","###INDEX:Bobbin.12:INDEX","Ch1.###MNR_T_register<.m###MNR_reg1soll>[W1]{r}"]
[41,"DW 12",null,"Setpoint 3 ","Bobbin.13","###INDEX:Bobbin.13:INDEX","Ch1.###MNR_T_register<.m###MNR_reg1soll>[W2]{r}"]
[41,"DW 13",null,"Setpoint 4 ","Bobbin.14","###INDEX:Bobbin.14:INDEX","Ch1.###MNR_T_register<.m###MNR_reg1soll>[W3]{r}"]
[41,"DW 20",null,"Limit min",null,null,"Ch1.###MNR_T_register<.m###MNR_reg1min>[W]{p}"]
[41,"DW 21",null,"Limit max",null,null,"Ch1.###MNR_T_register<.m###MNR_reg1max>[W]{p}"]
[41,"DW 22",null,"Pointer",null,null,"Ch1.###MNR_T_register<.m###MNR_reg1zeiger>[W]{p}"]
[41,"DW 23",null,"Actual value",null,null,"Ch1.###MNR_T_register<.m###MNR_reg1istzeiger>[W]{p}"]
[41,"DW30-49",null,"Register",null,null,"Ch1.###MNR_T_register<.m###MNR_reg1ist>[W0-19]{p}"]
[41]
[41,"DW 50-89",null,"Part 2","Bobbin.20","###INDEX:Bobbin.20:INDEX"]
[41,"DW 50",null,"Setpoint 1 ","Bobbin.21","###INDEX:Bobbin.21:INDEX","Ch1.###MNR_T_register<.m###MNR_reg2soll>[W0]{r}"]
[41,"DW 51",null,"Setpoint 2 ","Bobbin.22","###INDEX:Bobbin.22:INDEX","Ch1.###MNR_T_register<.m###MNR_reg2soll>[W1]{r}"]
[41,"DW 52",null,"Setpoint 3 ","Bobbin.23","###INDEX:Bobbin.23:INDEX","Ch1.###MNR_T_register<.m###MNR_reg2soll>[W2]{r}"]
[41,"DW 53",null,"Setpoint 4 ","Bobbin.24","###INDEX:Bobbin.24:INDEX","Ch1.###MNR_T_register<.m###MNR_reg2soll>[W3]{r}"]
[41,"DW 60",null,"Limit min",null,null,"Ch1.###MNR_T_register<.m###MNR_reg2min>[W]{p}"]
[41,"DW 61",null,"Limit max",null,null,"Ch1.###MNR_T_register<.m###MNR_reg2max>[W]{p}"]
[41,"DW 62",null,"Pointer",null,null,"Ch1.###MNR_T_register<.m###MNR_reg2zeiger>[W]{p}"]
[41,"DW 63",null,"Actual value",null,null,"Ch1.###MNR_T_register<.m###MNR_reg2istzeiger>[W]{p}"]
[41,"DW70-89",null,"Register",null,null,"Ch1.###MNR_T_register<.m###MNR_reg2ist>[W0-19]{p}"]
[41]
[41,"DW 90-129",null,"Part 3","Bobbin.30","###INDEX:Bobbin.30:INDEX"]
[41,"DW 90",null,"Setpoint 1 ","Bobbin.31","###INDEX:Bobbin.31:INDEX","Ch1.###MNR_T_register<.m###MNR_reg3soll>[W0]{r}"]
[41,"DW 91",null,"Setpoint 2 ","Bobbin.32","###INDEX:Bobbin.32:INDEX","Ch1.###MNR_T_register<.m###MNR_reg3soll>[W1]{r}"]
[41,"DW 92",null,"Setpoint 3 ","Bobbin.33","###INDEX:Bobbin.33:INDEX","Ch1.###MNR_T_register<.m###MNR_reg3soll>[W2]{r}"]
[41,"DW 93",null,"Setpoint 4 ","Bobbin.34","###INDEX:Bobbin.34:INDEX","Ch1.###MNR_T_register<.m###MNR_reg3soll>[W3]{r}"]
[41,"DW 100",null,"Limit min",null,null,"Ch1.###MNR_T_register<.m###MNR_reg3min>[W]{p}"]
[41,"DW 101",null,"Limit max",null,null,"Ch1.###MNR_T_register<.m###MNR_reg3max>[W]{p}"]
[41,"DW 102",null,"Pointer",null,null,"Ch1.###MNR_T_register<.m###MNR_reg3zeiger>[W]{p}"]
[41,"DW 103",null,"Actual value",null,null,"Ch1.###MNR_T_register<.m###MNR_reg3istzeiger>[W]{p}"]
[41,"DW110-129",null,"Register",null,null,"Ch1.###MNR_T_register<.m###MNR_reg3ist>[W0-19]{p}"]

{"sheet":"ParcelDimensions","index":58,"n_rows":19,"n_cols":7,"rows_kept":19,"flags":["formulas_cached_only"]}
["ParcelDimensions","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 190","Parcel Dimensions, 1st Machine "]
[41,"DB 191-194","Parcel Dimensions, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 190-194 Parcel Dimensions"]
[21,"DB 190","Parcel Dimensions ###MNR"]
[41,"DW 0","Bit 0","Parcel dimensions changed",null,null,"Ch1.###MNR_T_geb_par<.m###MNR_geb_par_aender>[B]{w}"]
[]
[41,"DW 10",null,"Gebindebreite","ParcelDimensions.10","###INDEX:ParcelDimensions.10:INDEX","Ch1.###MNR_T_geb_par<.m###MNR_geb_data>[W0]{r}"]
[41,"DW 11",null,"Gebindehöhe","ParcelDimensions.11","###INDEX:ParcelDimensions.11:INDEX","Ch1.###MNR_T_geb_par<.m###MNR_geb_data>[W1]{r}"]
[41,"DW 12",null,"Gebindelänge","ParcelDimensions.12","###INDEX:ParcelDimensions.12:INDEX","Ch1.###MNR_T_geb_par<.m###MNR_geb_data>[W2]{r}"]
[41,"DW 13",null,"Beuterl pro Gebinde","ParcelDimensions.13","###INDEX:ParcelDimensions.13:INDEX","Ch1.###MNR_T_geb_par<.m###MNR_geb_data>[W3]{r}"]
[41,"DW 14",null,"Beuteldicke","ParcelDimensions.14","###INDEX:ParcelDimensions.14:INDEX","Ch1.###MNR_T_geb_par<.m###MNR_geb_data>[W4]{r}"]
[41,"DW 15",null,"Zuschnittlänge","ParcelDimensions.15","###INDEX:ParcelDimensions.15:INDEX","Ch1.###MNR_T_geb_par<.m###MNR_geb_data>[W5]{r}"]
[41]
[41,"DW 20",null,"Auswurfrichtung gute Produkte",null,null,"Ch1.###MNR_T_geb_par<.m###MNR_geb_richtung>[W0]{r}"]
[41,"DW 21",null,"Auswurfrichtung schlechte Produkte",null,null,"Ch1.###MNR_T_geb_par<.m###MNR_geb_richtung>[W1]{r}"]
[41,"DW 22",null,"Auswurfrichtung manueller Auswurf",null,null,"Ch1.###MNR_T_geb_par<.m###MNR_geb_richtung>[W2]{r}"]

{"sheet":"SpeedDependentParameter","index":59,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
["SpeedDependentPar","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 200","Speed Dependent Parameter, 1st Machine "]
[41,"DB 201-204","Speed Dependent Parameter, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 200-204 Speed Dependent Parameter"]
[21,"DB 200","Speed Dependent Parameter ###MNR"]
[41,"DW 0","Bit 0","Speed Dependent Parameter changed",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_geb_par_aender>[B]{w}"]
[]
[41,"DW 10-49",null,"Teil 1","SpeedDependentPar.10","###INDEX:SpeedDependentParameter.10:INDEX"]
[41,"DW 11-19",null,"Drehzahlgrenze Nr. 2-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_dreh_1>[W0-9]{r}"]
[41,"DW 20-29",null,"Sellwert",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_soll_1>[W0-9]{r}"]
[41,"DW 30",null,"Zeiger Drehzahlbereich 1-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_zeig_1>[W]{p}"]
[41,"DW 50-89",null,"Teil 2","SpeedDependentPar.20","###INDEX:SpeedDependentParameter.20:INDEX"]
[41,"DW 51-59",null,"Drehzahlgrenze Nr. 2-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_dreh_2>[W0-9]{r}"]
[41,"DW 60-69",null,"Sellwert",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_soll_2>[W0-9]{r}"]
[41,"DW 70",null,"Zeiger Drehzahlbereich 1-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_zeig_2>[W]{p}"]
[41,"DW 90-129",null,"Teil 3","SpeedDependentPar.30","###INDEX:SpeedDependentParameter.30:INDEX"]
[41,"DW 91-99",null,"Drehzahlgrenze Nr. 2-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_dreh_3>[W0-9]{r}"]
[41,"DW 100-109",null,"Sellwert",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_soll_3>[W0-9]{r}"]
[41,"DW 110",null,"Zeiger Drehzahlbereich 1-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_zeig_3>[W]{p}"]
[41,"DW 120-159",null,"Teil 4","SpeedDependentPar.40","###INDEX:SpeedDependentParameter.40:INDEX"]
[41,"DW 131-139",null,"Drehzahlgrenze Nr. 2-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_dreh_4>[W0-9]{r}"]
[41,"DW 140-149",null,"Sellwert",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_soll_4>[W0-9]{r}"]
[41,"DW 150",null,"Zeiger Drehzahlbereich 1-10",null,null,"Ch1.###MNR_T_drehabh<.m###MNR_dreha_zeig_4>[W]{p}"]

{"sheet":"LooseEndDetector","index":60,"n_rows":71,"n_cols":7,"rows_kept":71,"flags":["formulas_cached_only"]}
["LooseEndDetector","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 210 ","LooseEndDetector"]
[41,"DB 211-214","Loose End Detector Machine  2-5"]
[21,"DB 215 ","DirtyFilter"]
[41,"DB 216-219","DirtyFilter Machine  2-5"]
[1,"###MAIN"]
[1,"DB210-214 Loose End Detector"]
[21,"DB ###ADDR:210+1[MNR]:ADDR","Loose End Detector ###MNR"]
[41,"DW 0","Bit 0","Loose End Detector changed",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loend_geaen>[B]{w}"]
[41,"DW 10",null,"Mask cigarettes row 1",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendmaskezig1>[W]{r}"]
[41,"DW 11",null,"Mask cigarettes row 2",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendmaskezig2>[W]{r}"]
[41,"DW 12",null,"Mask cigarettes row 3",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendmaskezig3>[W]{r}"]
[41,"DW 13",null,"Mask cigarettes row 4",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendmaskezig4>[W]{r}"]
[41,"DW 14",null,"Mask cigarettes row 5",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendmaskezig5>[W]{r}"]
[41]
[41,"DW15",null,"Shift type row 1",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendversch1>[W]{r}"]
[41,"DW16",null,"Shift type row 2",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendversch2>[W]{r}"]
[41,"DW17",null,"Shift type row 3",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendversch3>[W]{r}"]
[41,"DW18",null,"Shift type row 4",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendversch4>[W]{r}"]
[41,"DW19",null,"Shift type row 5",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendversch5>[W]{r}"]
[41]
[41,"DW 20",null,"possible cigarettes to deactivate row 1",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loenddeakt1>[W]{r}"]
[41,"DW 21",null,"possible cigarettes to deactivate row 2",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loenddeakt2>[W]{r}"]
[41,"DW 22",null,"possible cigarettes to deactivate row 3",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loenddeakt3>[W]{r}"]
[41,"DW 23",null,"possible cigarettes to deactivate row 4",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loenddeakt4>[W]{r}"]
[41,"DW 24",null,"possible cigarettes to deactivate row 5",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loenddeakt5>[W]{r}"]
[41]
[41,"DW 30",null,"Start B1",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendstartb1>[DW]{r}"]
[41,"DW 31",null,"Stop B1",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendstopb1>[DW]{r}"]
[41,"DW 32",null,"Start P2",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendstartp2>[DW]{r}"]
[41,"DW 33",null,"Stop P2",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendstopp2>[DW]{r}"]
[41,"DW 34",null,"Total length",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendtotall>[DW]{r}"]
[41]
[41,"DW 40",null,"Error code",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loenderrorcode>[W]{r}"]
[41,"DW 50",null,"Version 1",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendver1>[W]{r}"]
[41,"DW 51",null,"Version 2",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendver2>[W]{r}"]
[41,"DW 52",null,"CX Version 1",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendcxver1>[W]{r}"]
[41,"DW 53",null,"CX Version 2",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendcxver2>[W]{r}"]
[41,"DW 54",null,"Visu tpye",null,null,"Ch1.###MNR_T_looseend<.m###MNR_visutype>[W]{r}"]
[41,"DW 55",null,"Visu parameter",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendvorgabe>[W]{r}"]
[41,null,"Bit 0","Dirty filter"]
[41,null,"Bit 1","Holo filter"]
[41]
[41,"DW 60-69",null,"Version string PLC-Visu",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendfile>[S0-19]{p}"]
[41]
[41,"DW 100",null,"Row 1 active cigarettes",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendaktiv1>[W]{w}"]
[41,"DW 101",null,"Row 2 active cigarettes",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendaktiv2>[W]{w}"]
[41,"DW 102",null,"Row 3 active cigarettes",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendaktiv3>[W]{w}"]
[41,"DW 103",null,"Row 4 active cigarettes",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendaktiv4>[W]{w}"]
[41,"DW 104",null,"Row 5 active cigarettes",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendaktiv5>[W]{w}"]
[41]
[41,"DW 110",null,"Sensitivity",null,null,"Ch1.###MNR_T_looseend<.m###MNR_loendsensitiv>[W]{w}"]
[41,"DW 120-129",null,"Version string PLC-LED"]
[41]
[41,"DW 150-155",null,"Reserved for LED"]
[41]
[1,"DB215-219 Dirty Filter"]
[21,"DB ###ADDR:215+1[MNR]:ADDR","Dirty Filter ###MNR"]
[41,"DW 0","Bit 0","Dirty Filter changed",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_geaen>[B]{w}"]
[41,"DW 1","Bit 0","Dirty Filter changed",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_geaen>[B]{w}"]
[41,"DW 10",null,"status communication",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_zustand>[W]{r}"]
[41,"DD 20-59",null,"data from PLC"]
[41,null,"DD 20","Auftragsnummer",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_datavs>[DW0]{r}"]
[41,null,"DD 22","Dreckfläche",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_datavs>[DW1]{r}"]
[41]
[41,"DD 100-139",null,"data to PLC"]
[41,null,"DD 100","Auftragsnummer",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_datazs>[DW0]{r}"]
[41,null,"DD 102","Max Dreckfläche",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_datazs>[DW1]{r}"]
[41,null,"DD 104","Min Dreckfläche",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_datazs>[DW2]{r}"]
[41,null,"DD 106","Anz Zigaretten",null,null,"Ch1.###MNR_T_dirtyfilter<.m###MNR_df_datazs>[DW3]{r}"]

{"sheet":"Weigher","index":61,"n_rows":23,"n_cols":7,"rows_kept":23,"flags":["formulas_cached_only"]}
["Weigher","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 220 ","Vollzähligkeitskontrolle 1st Machine "]
[41,"DB 221-224","Vollzähligkeitskontrolle Machine  2-5"]
[1,"###MAIN"]
[1,"DB220-224 Vollzähligkeitskontrolle"]
[21,"DB ###ADDR:220+1[MNR]:ADDR","Vollzähligkeitskontrolle ###MNR"]
[41,"DW 0","Bit 0","Checkweigher changed",null,null,"Ch1.###MNR_T_waage<.m###MNR_waage_aend>[B]{w}"]
[41,"DW 10","Bit 0","Teach value",null,null,"Ch1.###MNR_T_waage<.m###MNR_waage_teach>[B]{r}"]
[41,null,"Bit 1","Set zero",null,null,"Ch1.###MNR_T_waage<.m###MNR_waage_teanul>[B]{r}"]
[41,"DW 11",null,"Minimum limit value","Weigher.14","###INDEX:Weigher.14:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_min_1>[W]{r}"]
[41,"DW 12",null,"Maximum limit value","Weigher.10","###INDEX:Weigher.10:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_max_1>[W]{r}"]
[41,"DW 13",null,"Minimum deviation as percentage","Weigher.13","###INDEX:Weigher.13:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_mip_1>[W]{r}"]
[41,"DW 14",null,"Maximum deviation as percentage","Weigher.11","###INDEX:Weigher.11:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_plp_1>[W]{r}"]
[41,"DW 15",null,"Set teach value","Weigher.12","###INDEX:Weigher.12:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_vor_1>[W]{r}"]
[41,"DW 16",null,"Empty cycle threshold","Weigher.15","###INDEX:Weigher.15:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_leer_1>[W]{r}"]
[41,"DW 17",null,"No. of average values","Weigher.16","###INDEX:Weigher.16:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_anzm_1>[W]{r}"]
[41,"DW 18",null,"Set tara","Weigher.17","###INDEX:Weigher.17:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_tara_1>[W]{r}"]
[41,"DW 20","Bit 0","Ready to teach",null,null,"Ch1.###MNR_T_waage<.m###MNR_waage_teachok_1>[B]{r}"]
[41,"DW 21",null,"Actual value","Weigher.20","###INDEX:Weigher.20:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_ist_1>[W]{p}"]
[41,"DW 22",null,"Average value","Weigher.21","###INDEX:Weigher.21:INDEX","Ch1.###MNR_T_waage<.m###MNR_waage_mit_1>[W]{p}"]
[41,"DW 30-79",null,"Last 50 values measured on weigher",null,null,"Ch1.###MNR_T_waage<.m###MNR_waage_wert_1>[W0-49]{p}"]
[41,"DW 80-129",null,"Last 50 averages",null,null,"Ch1.###MNR_T_waage<.m###MNR_waage_mitt_1>[W0-49]{p}"]

{"sheet":"Bobbin","index":62,"n_rows":40,"n_cols":7,"rows_kept":40,"flags":["formulas_cached_only"]}
["Bobbin","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 230 ","Bobbin control, 1st Machine "]
[41,"DB 231-234","Bobbin control, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 230-234 Bobinensteuerung"]
[21,"DB 230","Bobbin control ###MNR"]
[41,"DW 0","Bit 0","Bobbin control changed",null,null,"Ch1.###MNR_T_bobine<.m###MNR_bobine_aender>[B]{w}"]
[41,"DW 10",null,"Full bobbin diameter","Bobbin.11","###INDEX:Bobbin.11:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_durchmax>[W]{r}"]
[41,"DW 11",null,"Empty bobbin diameter","Bobbin.12","###INDEX:Bobbin.12:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_durchmin>[W]{r}"]
[41,"DW 12",null,"Actual bobbin diameter","Bobbin.13","###INDEX:Bobbin.13:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_durchist>[W]{p}"]
[41,"DW 13",null,"Blank length (optional)","Bobbin.14","###INDEX:Bobbin.14:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_zuschnitt>[W]{r}"]
[41,"DW 20",null,"Tensioning arm, setpoint position","Bobbin.21","###INDEX:Bobbin.21:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_pendmax>[W]{r}"]
[41,"DW 21",null,"Tensioning arm, splicing position","Bobbin.22","###INDEX:Bobbin.22:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_pendmin>[W]{r}"]
[41,"DW 22",null,"Actual tensioning arm position","Bobbin.23","###INDEX:Bobbin.23:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_pendist>[W]{p}"]
[41,"DW 50",null,"Splicer, left / right",null,null,"Ch1.###MNR_T_bobine<.m###MNR_bobine_wechlr>[W]{p}"]
[41,null,"Bit 0","Limit switch, left"]
[41,null,"Bit 1","End position, left"]
[41,null,"Bit 2","Middle position, left"]
[41,null,"Bit 3","Middle position, right"]
[41,null,"Bit 4","End position, right"]
[41,null,"Bit 5","Limit switch, right"]
[41,"DW 51",null,"Splicer, up / down",null,null,"Ch1.###MNR_T_bobine<.m###MNR_bobine_wechou>[W]{p}"]
[41,null,"Bit 0","Limit switch, top"]
[41,null,"Bit 1","End position, top"]
[41,null,"Bit 2","Middle position"]
[41,null,"Bit 3","End position, bottom"]
[41,null,"Bit 4","Limit switch, bottom"]
[41,"DW 52",null,"Splicer, forward / back",null,null,"Ch1.###MNR_T_bobine<.m###MNR_bobine_wechvz>[W]{p}"]
[41,null,"Bit 0","Limit switch, front"]
[41,null,"Bit 1","End position, front"]
[41,null,"Bit 2","Middle position"]
[41,null,"Bit 3","End position, rear"]
[41,null,"Bit 4","Limit switch, rear"]
[41,"DW 53","Bit 0","Status, splicer","Bobbin.###MNR.1","###INDEX:Bobbin.###MNR.1:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_wechbit>[W]{p}"]
[41,null,"Bit 1","Status, splicer","Bobbin.###MNR.2","###INDEX:Bobbin.###MNR.2:INDEX"]
[41,null,"Bit 2","Status, splicer","Bobbin.###MNR.3","###INDEX:Bobbin.###MNR.3:INDEX"]
[41,null,"Bit 3","Status, splicer","Bobbin.###MNR.4","###INDEX:Bobbin.###MNR.4:INDEX"]
[41,null,"Bit 4","Status, splicer","Bobbin.###MNR.5","###INDEX:Bobbin.###MNR.5:INDEX"]
[41,"DW 55",null,"Step chain, splicer","Bobbin.41","###INDEX:Bobbin.41:INDEX","Ch1.###MNR_T_bobine<.m###MNR_bobine_wechist>[W]{p}"]

{"sheet":"Bobbin4x","index":63,"n_rows":74,"n_cols":7,"rows_kept":74,"flags":["formulas_cached_only"]}
["Bobbin4x","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 230 ","Bobbin control, 1st Machine "]
[41,"DB 231-234","Bobbin control, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 230-234 Bobinensteuerung"]
[21,"DB 230","Bobbin control ###MNR"]
[41,"DW 0","Bit 0","Bobbin control changed",null,null,"Ch1.###MNR_T_bobine4x<.m###MNR_bobine_aender>[B]{w}"]
[41,"DW 50",null,"Splicer, left / right",null,null,"Ch1.###MNR_T_bobine4x<.m###MNR_bobine_wechlr>[W]{p}"]
[41,null,"Bit 0","Limit switch, left"]
[41,null,"Bit 1","End position, left"]
[41,null,"Bit 2","Middle position, left"]
[41,null,"Bit 3","Middle position, right"]
[41,null,"Bit 4","End position, right"]
[41,null,"Bit 5","Limit switch, right"]
[41,"DW 51",null,"Splicer, up / down",null,null,"Ch1.###MNR_T_bobine4x<.m###MNR_bobine_wechou>[W]{p}"]
[41,null,"Bit 0","Limit switch, top"]
[41,null,"Bit 1","End position, top"]
[41,null,"Bit 2","Middle position"]
[41,null,"Bit 3","End position, bottom"]
[41,null,"Bit 4","Limit switch, bottom"]
[41,"DW 52",null,"Splicer, forward / back",null,null,"Ch1.###MNR_T_bobine4x<.m###MNR_bobine_wechvz>[W]{p}"]
[41,null,"Bit 0","Limit switch, front"]
[41,null,"Bit 1","End position, front"]
[41,null,"Bit 2","Middle position"]
[41,null,"Bit 3","End position, rear"]
[41,null,"Bit 4","Limit switch, rear"]
[41,"DW 53","Bit 0","Status, splicer","Bobbin4x.###MNR.1","###INDEX:Bobbin4x.###MNR.1:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine_wechbit>[W]{p}"]
[41,null,"Bit 1","Status, splicer","Bobbin4x.###MNR.2","###INDEX:Bobbin4x.###MNR.2:INDEX"]
[41,null,"Bit 2","Status, splicer","Bobbin4x.###MNR.3","###INDEX:Bobbin4x.###MNR.3:INDEX"]
[41,null,"Bit 3","Status, splicer","Bobbin4x.###MNR.4","###INDEX:Bobbin4x.###MNR.4:INDEX"]
[41,null,"Bit 4","Status, splicer","Bobbin4x.###MNR.5","###INDEX:Bobbin4x.###MNR.5:INDEX"]
[41,"DW 55",null,"Step chain, splicer","Bobbin4x.41","###INDEX:Bobbin4x.41:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine_wechist>[W]{p}"]
[41]
[41,"DW60-109","Bobbin1"]
[41,"DW 60",null,"Full bobbin diameter","Bobbin4x.11","###INDEX:Bobbin4x.11:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine1_durchmax>[W]{r}"]
[41,"DW 61",null,"Empty bobbin diameter","Bobbin4x.12","###INDEX:Bobbin4x.12:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine1_durchmin>[W]{r}"]
[41,"DW 62",null,"Actual bobbin diameter","Bobbin4x.13","###INDEX:Bobbin4x.13:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine1_durchist>[W]{p}"]
[41,"DW 63",null,"Blank length (optional)","Bobbin4x.14","###INDEX:Bobbin4x.14:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine1_zuschnitt>[W]{r}"]
[41,"DW 70",null,"Tensioning arm, setpoint position","Bobbin4x.21","###INDEX:Bobbin4x.21:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine1_pendmax>[W]{r}"]
[41,"DW 71",null,"Tensioning arm, splicing position","Bobbin4x.22","###INDEX:Bobbin4x.22:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine1_pendmin>[W]{r}"]
[41,"DW 72",null,"Actual tensioning arm position","Bobbin4x.23","###INDEX:Bobbin4x.23:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine1_pendist>[W]{p}"]
[41,"DW80-109",null,"Reserviert für Steuerung"]
[41]
[41,"DW110-159","Bobbin2"]
[41,"DW 110",null,"Full bobbin diameter","Bobbin4x.11","###INDEX:Bobbin4x.11:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine2_durchmax>[W]{r}"]
[41,"DW 111",null,"Empty bobbin diameter","Bobbin4x.12","###INDEX:Bobbin4x.12:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine2_durchmin>[W]{r}"]
[41,"DW 112",null,"Actual bobbin diameter","Bobbin4x.13","###INDEX:Bobbin4x.13:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine2_durchist>[W]{p}"]
[41,"DW 113",null,"Blank length (optional)","Bobbin4x.14","###INDEX:Bobbin4x.14:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine2_zuschnitt>[W]{r}"]
[41,"DW 120",null,"Tensioning arm, setpoint position","Bobbin4x.21","###INDEX:Bobbin4x.21:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine2_pendmax>[W]{r}"]
[41,"DW 121",null,"Tensioning arm, splicing position","Bobbin4x.22","###INDEX:Bobbin4x.22:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine2_pendmin>[W]{r}"]
[41,"DW 122",null,"Actual tensioning arm position","Bobbin4x.23","###INDEX:Bobbin4x.23:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine2_pendist>[W]{p}"]
[41,"DW130-159",null,"Reserviert für Steuerung"]
[41]
[41,"DW160-209","Bobbin3"]
[41,"DW 160",null,"Full bobbin diameter","Bobbin4x.11","###INDEX:Bobbin4x.11:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine3_durchmax>[W]{r}"]
[41,"DW 161",null,"Empty bobbin diameter","Bobbin4x.12","###INDEX:Bobbin4x.12:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine3_durchmin>[W]{r}"]
[41,"DW 162",null,"Actual bobbin diameter","Bobbin4x.13","###INDEX:Bobbin4x.13:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine3_durchist>[W]{p}"]
[41,"DW 163",null,"Blank length (optional)","Bobbin4x.14","###INDEX:Bobbin4x.14:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine3_zuschnitt>[W]{r}"]
[41,"DW 170",null,"Tensioning arm, setpoint position","Bobbin4x.21","###INDEX:Bobbin4x.21:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine3_pendmax>[W]{r}"]
[41,"DW 171",null,"Tensioning arm, splicing position","Bobbin4x.22","###INDEX:Bobbin4x.22:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine3_pendmin>[W]{r}"]
[41,"DW 172",null,"Actual tensioning arm position","Bobbin4x.23","###INDEX:Bobbin4x.23:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine3_pendist>[W]{p}"]
[41,"DW180-209",null,"Reserviert für Steuerung"]
[41]
[41,"DW210-259","Bobbin4"]
[41,"DW 210",null,"Full bobbin diameter","Bobbin4x.11","###INDEX:Bobbin4x.11:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine4_durchmax>[W]{r}"]
[41,"DW 211",null,"Empty bobbin diameter","Bobbin4x.12","###INDEX:Bobbin4x.12:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine4_durchmin>[W]{r}"]
[41,"DW 212",null,"Actual bobbin diameter","Bobbin4x.13","###INDEX:Bobbin4x.13:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine4_durchist>[W]{p}"]
[41,"DW 213",null,"Blank length (optional)","Bobbin4x.14","###INDEX:Bobbin4x.14:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine4_zuschnitt>[W]{r}"]
[41,"DW 220",null,"Tensioning arm, setpoint position","Bobbin4x.21","###INDEX:Bobbin4x.21:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine4_pendmax>[W]{r}"]
[41,"DW 221",null,"Tensioning arm, splicing position","Bobbin4x.22","###INDEX:Bobbin4x.22:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine4_pendmin>[W]{r}"]
[41,"DW 222",null,"Actual tensioning arm position","Bobbin4x.23","###INDEX:Bobbin4x.23:INDEX","Ch1.###MNR_T_bobine4x<.m###MNR_bobine4_pendist>[W]{p}"]
[41,"DW230-259",null,"Reserviert für Steuerung"]
[41]

{"sheet":"Parameters32","index":64,"n_rows":40,"n_cols":7,"rows_kept":40,"flags":["formulas_cached_only"]}
["Parameters32","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 240 ","32 Parameter  1st Machine "]
[41,"DB 241-244","32 Parameter Machine 2-5"]
[1,"###MAIN"]
[1,"DB 240-244 32 Parameter"]
[21,"DB ###ADDR:240+1[MNR]:ADDR","32 Parameter ###MNR"]
[41,"DW 0","Bit 0","Parameter changed",null,null,"Ch1.###MNR_T_parameter<.m###MNR_parameter_aend>[B]{w}"]
[41,"DD 10",null,"Parameter 1","Parameters32.###MNR.1","###INDEX:Parameters32.###MNR.1:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW0]{r}"]
[41,"DD 12",null,"Parameter 2","Parameters32.###MNR.2","###INDEX:Parameters32.###MNR.2:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW1]{r}"]
[41,"DD 14",null,"Parameter 3","Parameters32.###MNR.3","###INDEX:Parameters32.###MNR.3:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW2]{r}"]
[41,"DD 16",null,"Parameter 4","Parameters32.###MNR.4","###INDEX:Parameters32.###MNR.4:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW3]{r}"]
[41,"DD 18",null,"Parameter 5","Parameters32.###MNR.5","###INDEX:Parameters32.###MNR.5:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW4]{r}"]
[41,"DD 20",null,"Parameter 6","Parameters32.###MNR.6","###INDEX:Parameters32.###MNR.6:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW5]{r}"]
[41,"DD 22",null,"Parameter 7","Parameters32.###MNR.7","###INDEX:Parameters32.###MNR.7:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW6]{r}"]
[41,"DD 24",null,"Parameter 8","Parameters32.###MNR.8","###INDEX:Parameters32.###MNR.8:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW7]{r}"]
[41,"DD 26",null,"Parameter 9","Parameters32.###MNR.9","###INDEX:Parameters32.###MNR.9:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW8]{r}"]
[41,"DD 28",null,"Parameter 10","Parameters32.###MNR.10","###INDEX:Parameters32.###MNR.10:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW9]{r}"]
[41,"DD 30",null,"Parameter 11","Parameters32.###MNR.11","###INDEX:Parameters32.###MNR.11:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW10]{r}"]
[41,"DD 32",null,"Parameter 12","Parameters32.###MNR.12","###INDEX:Parameters32.###MNR.12:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW11]{r}"]
[41,"DD 34",null,"Parameter 13","Parameters32.###MNR.13","###INDEX:Parameters32.###MNR.13:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW12]{r}"]
[41,"DD 36",null,"Parameter 14","Parameters32.###MNR.14","###INDEX:Parameters32.###MNR.14:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW13]{r}"]
[41,"DD 38",null,"Parameter 15","Parameters32.###MNR.15","###INDEX:Parameters32.###MNR.15:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW14]{r}"]
[41,"DD 40",null,"Parameter 16","Parameters32.###MNR.16","###INDEX:Parameters32.###MNR.16:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW15]{r}"]
[41,"DD 42",null,"Parameter 17","Parameters32.###MNR.17","###INDEX:Parameters32.###MNR.17:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW16]{r}"]
[41,"DD 44",null,"Parameter 18","Parameters32.###MNR.18","###INDEX:Parameters32.###MNR.18:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW17]{r}"]
[41,"DD 46",null,"Parameter 19","Parameters32.###MNR.19","###INDEX:Parameters32.###MNR.19:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW18]{r}"]
[41,"DD 48",null,"Parameter 20","Parameters32.###MNR.20","###INDEX:Parameters32.###MNR.20:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW19]{r}"]
[41,"DD 50",null,"Parameter 21","Parameters32.###MNR.21","###INDEX:Parameters32.###MNR.21:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW20]{r}"]
[41,"DD 52",null,"Parameter 22","Parameters32.###MNR.22","###INDEX:Parameters32.###MNR.22:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW21]{r}"]
[41,"DD 54",null,"Parameter 23","Parameters32.###MNR.23","###INDEX:Parameters32.###MNR.23:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW22]{r}"]
[41,"DD 56",null,"Parameter 24","Parameters32.###MNR.24","###INDEX:Parameters32.###MNR.24:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW23]{r}"]
[41,"DD 58",null,"Parameter 25","Parameters32.###MNR.25","###INDEX:Parameters32.###MNR.25:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW24]{r}"]
[41,"DD 60",null,"Parameter 26","Parameters32.###MNR.26","###INDEX:Parameters32.###MNR.26:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW25]{r}"]
[41,"DD 62",null,"Parameter 27","Parameters32.###MNR.27","###INDEX:Parameters32.###MNR.27:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW26]{r}"]
[41,"DD 64",null,"Parameter 28","Parameters32.###MNR.28","###INDEX:Parameters32.###MNR.28:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW27]{r}"]
[41,"DD 66",null,"Parameter 29","Parameters32.###MNR.29","###INDEX:Parameters32.###MNR.29:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW28]{r}"]
[41,"DD 68",null,"Parameter 30","Parameters32.###MNR.30","###INDEX:Parameters32.###MNR.30:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW29]{r}"]
[41,"DD 70",null,"Parameter 31","Parameters32.###MNR.31","###INDEX:Parameters32.###MNR.31:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW30]{r}"]
[41,"DD 72",null,"Parameter 32","Parameters32.###MNR.32","###INDEX:Parameters32.###MNR.32:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW31]{r}"]

{"sheet":"407_GlueJetPaperMax4","index":65,"n_rows":20,"n_cols":6,"rows_kept":20,"flags":["formulas_cached_only"]}
["407_GlueJetPaperMax4","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 250","Glue jets 1st Machine "]
[null,"DB 251-254","Glue jets Machine  2-5"]
[1,"###MAIN"]
[1,"DB 250-254 Glue jets"]
[21,"DB ###ADDR:250+1[MNR]:ADDR","Glue jets ###MNR"]
[41,"DW 0","Bit 0","Glue jets changed",null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4aender>[B]{w}"]
[41,"DW 12",null,"Distance photocell-jet (1)","407_GlueJetPaperMax4.1","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4abst_12>[W]{r}"]
[41,"DW 13",null,"Distance photocell-jet (2)","407_GlueJetPaperMax4.1","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4abst_13>[W]{r}"]
[41,"DW 22",null,"Offset, Track 1 (110)",null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4offset_22>[W]{r}"]
[41,"DW 23",null,"Offset, Track 2 (130)",null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4offset_23>[W]{r}"]
[41,"DW 32",null,"No. of glue lines, Track 1 (6)",null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4anzahl_32>[W]{r}"]
[41,"DW 33",null,"No. of glue lines, Track 2 (6)",null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4anzahl_33>[W]{r}"]
[41,"DW 40",null,"Glue quantity, jet","407_GlueJetPaperMax4.14","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4leimmenge>[W]{r}"]
[41,"DW 41",null,"Value 1","407_GlueJetPaperMax4.15","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4sonder1>[W]{r}"]
[41,"DW 42",null,"Value 2","407_GlueJetPaperMax4.16","Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4sonder2>[W]{r}"]
[41]
[41,"DW 110-121",null,"6 values of Track 1",null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4>[W50-55]{r}"]
[41,"DW 130-141",null,"6  values of Track 2",null,"Ch1.###MNR_T_duesepamax4<.m###MNR_duesepamax4>[W70-75]{r}"]

{"sheet":"CasePackerParameter","index":66,"n_rows":29,"n_cols":7,"rows_kept":29,"flags":["formulas_cached_only"]}
["CasePackerParameter","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 260 ","Casepacker parameters"]
[41,"DB 261-264","Casepacker parameters, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 260-264 Casepacker Parameters"]
[21,"DB ###ADDR:260+1[MNR]:ADDR","Casepacker parameters ###MNR"]
[41,"DW 0","Bit 0","Parameter changed",null,null,"Ch1.###MNR_T_casepacker<.m###MNR_casepa_aender>[B]{w}"]
[41,"DW 10",null,"Parameter 1 Main Drive ","CasePackerParameter.###MNR.10","###INDEX:CasePackerParameter.###MNR.10:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_haupt>[W0]{r}"]
[41,"DW 11",null,"Parameter 2 Main Drive","CasePackerParameter.###MNR.11","###INDEX:CasePackerParameter.###MNR.11:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_haupt>[W1]{r}"]
[41,"DW 12",null,"Parameter 3 Main Drive","CasePackerParameter.###MNR.12","###INDEX:CasePackerParameter.###MNR.12:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_haupt>[W2]{r}"]
[41,"DW 13",null,"Parameter 4 Main Drive","CasePackerParameter.###MNR.13","###INDEX:CasePackerParameter.###MNR.13:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_haupt>[W3]{r}"]
[41,"DW 14",null,"Parameter 5 Main Drive","CasePackerParameter.###MNR.14","###INDEX:CasePackerParameter.###MNR.14:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_haupt>[W4]{r}"]
[41,"DW 20",null,"Parameter 1 Infeed Pusher","CasePackerParameter.###MNR.20","###INDEX:CasePackerParameter.###MNR.20:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_ein>[W0]{r}"]
[41,"DW 21",null,"Parameter 2 Infeed Pusher","CasePackerParameter.###MNR.21","###INDEX:CasePackerParameter.###MNR.21:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_ein>[W1]{r}"]
[41,"DW 22",null,"Parameter 3 Infeed Pusher","CasePackerParameter.###MNR.22","###INDEX:CasePackerParameter.###MNR.22:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_ein>[W2]{r}"]
[41,"DW 23",null,"Parameter 4 Infeed Pusher","CasePackerParameter.###MNR.23","###INDEX:CasePackerParameter.###MNR.23:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_ein>[W3]{r}"]
[41,"DW 30",null,"Parameter 1 Mouthpiece","CasePackerParameter.###MNR.30","###INDEX:CasePackerParameter.###MNR.30:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_mund>[W0]{r}"]
[41,"DW 31",null,"Parameter 2 Mouthpiece","CasePackerParameter.###MNR.31","###INDEX:CasePackerParameter.###MNR.31:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_mund>[1]{r}"]
[41,"DW 32",null,"Parameter 3 Mouthpiece","CasePackerParameter.###MNR.32","###INDEX:CasePackerParameter.###MNR.32:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_mund>[W2]{r}"]
[41,"DW 40",null,"Parameter 1 Stacker","CasePackerParameter.###MNR.40","###INDEX:CasePackerParameter.###MNR.40:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_stap>[W0]{r}"]
[41,"DW 41",null,"Parameter 2 Stacker","CasePackerParameter.###MNR.41","###INDEX:CasePackerParameter.###MNR.41:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_stap>[W1]{r}"]
[41,"DW 42",null,"Parameter 3 Stacker","CasePackerParameter.###MNR.42","###INDEX:CasePackerParameter.###MNR.42:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_stap>[W2]{r}"]
[41,"DW 43",null,"Parameter 4 Stacker","CasePackerParameter.###MNR.43","###INDEX:CasePackerParameter.###MNR.43:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_stap>[W3]{r}"]
[41,"DW 50","Bit 0","Switch 1","CasePackerParameter.###MNR.50","###INDEX:CasePackerParameter.###MNR.50:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_bits>[W]{r}"]
[41,null,"Bit 1","Switch 2","CasePackerParameter.###MNR.51","###INDEX:CasePackerParameter.###MNR.51:INDEX"]
[41,null,"Bit 2","Switch 3","CasePackerParameter.###MNR.52","###INDEX:CasePackerParameter.###MNR.52:INDEX"]
[41,null,"Bit 3","Switch 4","CasePackerParameter.###MNR.53","###INDEX:CasePackerParameter.###MNR.53:INDEX"]
[41,null,"Bit 4","Switch 5","CasePackerParameter.###MNR.54","###INDEX:CasePackerParameter.###MNR.54:INDEX"]

{"sheet":"CasePackerParameter2","index":67,"n_rows":36,"n_cols":7,"rows_kept":36,"flags":["formulas_cached_only"]}
["CasePackerParameter2","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 260 ","Casepacker parameters"]
[41,"DB 261-264","Casepacker parameters, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 260-264 Casepacker Parameters"]
[21,"DB ###ADDR:260+1[MNR]:ADDR","Casepacker parameters ###MNR"]
[41,"DW 0","Bit 0","Parameter changed",null,null,"Ch1.###MNR_T_casepacker<.m###MNR_casepa_aender>[B]{w}"]
[41,"DW 60",null,"Parameter 1 Drive","CasePackerParameter2.###MNR.10","###INDEX:CasePackerParameter2.###MNR.10:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_antr>[W0]{r}"]
[41,"DW 61",null,"Parameter 2 Drive","CasePackerParameter2.###MNR.11","###INDEX:CasePackerParameter2.###MNR.11:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_antr>[W1]{r}"]
[41,"DW 62",null,"Parameter 3 Drive","CasePackerParameter2.###MNR.12","###INDEX:CasePackerParameter2.###MNR.12:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_antr>[W2]{r}"]
[41,"DW 63",null,"Parameter 4 Drive","CasePackerParameter2.###MNR.13","###INDEX:CasePackerParameter2.###MNR.13:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_antr>[W3]{r}"]
[41,"DW 64",null,"Parameter 5 Drive","CasePackerParameter2.###MNR.14","###INDEX:CasePackerParameter2.###MNR.14:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_antr>[W4]{r}"]
[41,"DW 70",null,"Parameter 1 / 1","CasePackerParameter2.###MNR.20","###INDEX:CasePackerParameter2.###MNR.20:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W0]{r}"]
[41,"DW 71",null,"Parameter 1 / 2","CasePackerParameter2.###MNR.21","###INDEX:CasePackerParameter2.###MNR.21:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W1]{r}"]
[41,"DW 72",null,"Parameter 1 / 3","CasePackerParameter2.###MNR.22","###INDEX:CasePackerParameter2.###MNR.22:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W2]{r}"]
[41,"DW 73",null,"Parameter 1 / 4","CasePackerParameter2.###MNR.23","###INDEX:CasePackerParameter2.###MNR.23:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W3]{r}"]
[41,"DW 74",null,"Parameter 1 / 5","CasePackerParameter2.###MNR.24","###INDEX:CasePackerParameter2.###MNR.24:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W4]{r}"]
[41,"DW 75",null,"Parameter 1 / 6","CasePackerParameter2.###MNR.25","###INDEX:CasePackerParameter2.###MNR.25:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W5]{r}"]
[41,"DW 76",null,"Parameter 1 / 7","CasePackerParameter2.###MNR.26","###INDEX:CasePackerParameter2.###MNR.26:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W6]{r}"]
[41,"DW 77",null,"Parameter 1 / 8","CasePackerParameter2.###MNR.27","###INDEX:CasePackerParameter2.###MNR.27:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa1>[W7]{r}"]
[41,"DW 80",null,"Parameter 2 / 1","CasePackerParameter2.###MNR.30","###INDEX:CasePackerParameter2.###MNR.30:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W0]{r}"]
[41,"DW 81",null,"Parameter 2 / 2","CasePackerParameter2.###MNR.31","###INDEX:CasePackerParameter2.###MNR.31:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W1]{r}"]
[41,"DW 82",null,"Parameter 2 / 3","CasePackerParameter2.###MNR.32","###INDEX:CasePackerParameter2.###MNR.32:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W2]{r}"]
[41,"DW 83",null,"Parameter 2 / 4","CasePackerParameter2.###MNR.33","###INDEX:CasePackerParameter2.###MNR.33:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W3]{r}"]
[41,"DW 84",null,"Parameter 2 / 5","CasePackerParameter2.###MNR.34","###INDEX:CasePackerParameter2.###MNR.34:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W4]{r}"]
[41,"DW 85",null,"Parameter 2 / 6","CasePackerParameter2.###MNR.35","###INDEX:CasePackerParameter2.###MNR.35:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W5]{r}"]
[41,"DW 86",null,"Parameter 2 / 7","CasePackerParameter2.###MNR.36","###INDEX:CasePackerParameter2.###MNR.36:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W6]{r}"]
[41,"DW 87",null,"Parameter 2 / 8","CasePackerParameter2.###MNR.37","###INDEX:CasePackerParameter2.###MNR.37:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W7]{r}"]
[41,"DW 88",null,"Parameter 2 / 9","CasePackerParameter2.###MNR.38","###INDEX:CasePackerParameter2.###MNR.38:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W8]{r}"]
[41,"DW 89",null,"Parameter 2 / 10","CasePackerParameter2.###MNR.39","###INDEX:CasePackerParameter2.###MNR.39:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W9]{r}"]
[41,"DW 90",null,"Parameter 2 / 11","CasePackerParameter2.###MNR.40","###INDEX:CasePackerParameter2.###MNR.40:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W10]{r}"]
[41,"DW 91",null,"Parameter 2 / 12","CasePackerParameter2.###MNR.41","###INDEX:CasePackerParameter2.###MNR.41:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W11]{r}"]
[41,"DW 92",null,"Parameter 2 / 13","CasePackerParameter2.###MNR.42","###INDEX:CasePackerParameter2.###MNR.42:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W12]{r}"]
[41,"DW 93",null,"Parameter 2 / 14","CasePackerParameter2.###MNR.43","###INDEX:CasePackerParameter2.###MNR.43:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W13]{r}"]
[41,"DW 94",null,"Parameter 2 / 15","CasePackerParameter2.###MNR.44","###INDEX:CasePackerParameter2.###MNR.44:INDEX","Ch1.###MNR_T_casepacker<.m###MNR_casepa_pa2>[W14]{r}"]

{"sheet":"HeaterSpecial","index":68,"n_rows":41,"n_cols":7,"rows_kept":41,"flags":["formulas_cached_only"]}
["HeaterSpecial","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 270 ","Heaters 1st Machine "]
[41,"DB 271-272","Heaters Machine 2-5"]
[1,"###MAIN"]
[1,"DB 270-274 Heaters"]
[41,"DW 0","Bit 0","Heaters changed",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizspaend>[B]{w}"]
[41,"DW 10",null,"Fault word",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_l_1>[W0]{p}"]
[41,null,1,"Wire break ","HeaterSpecial.20","###INDEX:HeaterSpecial.20:INDEX"]
[41,null,2,"Short circuit","HeaterSpecial.21","###INDEX:HeaterSpecial.21:INDEX"]
[41,null,3,"Temperature > 250","HeaterSpecial.22","###INDEX:HeaterSpecial.22:INDEX"]
[41,null,4,"Overtemperature","HeaterSpecial.23","###INDEX:HeaterSpecial.23:INDEX"]
[41,null,5,"Undertemperature","HeaterSpecial.24","###INDEX:HeaterSpecial.24:INDEX"]
[41,"DW 11",null,"Status word",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_l_1>[W1]{p}"]
[41,null,0," Inhibited","HeaterSpecial.11","###INDEX:HeaterSpecial.11:INDEX"]
[41,null,1," Active","HeaterSpecial.10","###INDEX:HeaterSpecial.10:INDEX"]
[41,null,2,"Defect","HeaterSpecial.12","###INDEX:HeaterSpecial.12:INDEX"]
[41,"DW 12",null,"Active speed range (1-5)",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_l_1>[W2]{p}"]
[41,"DW 14",null,"Actual value","HeaterSpecial.0","###INDEX:HeaterSpecial.0:INDEX","Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_l_1>[W4]{p}"]
[41,"DW 15",null,"Y",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_l_1>[W5]{r}"]
[41,"DW 16",null,"Active setpoint",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_l_1>[W6]{r}"]
[41,"DW 31",null,"Lower warning limit","HeaterSpecial.2","###INDEX:HeaterSpecial.2:INDEX","Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W0]{r}"]
[41,"DW 32",null,"Upper warning limit Warngrenze","HeaterSpecial.3","###INDEX:HeaterSpecial.3:INDEX","Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W1]{r}"]
[41,"DW 33",null,"P",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W2]{r}"]
[41,"DW 34",null,"I",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W3]{r}"]
[41,"DW 35",null,"D",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W4]{r}"]
[41,"DW 36",null,"Speed limit 2",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W5]{r}"]
[41,"DW 37",null,"Speed limit 3",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W6]{r}"]
[41,"DW 38",null,"Speed limit 4",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W7]{r}"]
[41,"DW 39",null,"Speed limit 5",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W8]{r}"]
[41,"DW 40",null,"Temperature for limit range 1",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W9]{8}"]
[41,"DW 41",null,"Temperature for limit range 2",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W10]{r}"]
[41,"DW 42",null,"Temperature for limit range 3",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W11]{r}"]
[41,"DW 43",null,"Temperature for limit range 4",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W12]{r}"]
[41,"DW 44",null,"Temperature for limit range 5",null,null,"Ch1.###MNR_T_heizungsp<.m###MNR_heizsp_s_1>[W13]{r}"]
[41,"DW 010-049",null,"Heater 1","HeaterSpecial.###MNR.1","###INDEX:HeaterSpecial.###MNR.1:INDEX"]
[41,"DW 050-089",null,"Heater 2","HeaterSpecial.###MNR.2","###INDEX:HeaterSpecial.###MNR.2:INDEX"]
[41,"DW 090-129",null,"Heater 3","HeaterSpecial.###MNR.3","###INDEX:HeaterSpecial.###MNR.3:INDEX"]
[41,"DW 130-169",null,"Heater 4","HeaterSpecial.###MNR.11","###INDEX:HeaterSpecial.###MNR.11:INDEX"]
[41,"DW 170-209",null,"Heater 5","HeaterSpecial.###MNR.12","###INDEX:HeaterSpecial.###MNR.12:INDEX"]
[41,"DW 210-249",null,"Heater 6","HeaterSpecial.###MNR.13","###INDEX:HeaterSpecial.###MNR.13:INDEX"]

{"sheet":"Heater48","index":69,"n_rows":74,"n_cols":7,"rows_kept":74,"flags":["formulas_cached_only"]}
["Heater48","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 280","Heaters 1st Machine "]
[41,"DB 280-284","Heaters Machine 2-5"]
[1,"###MAIN"]
[1,"DB 280-284 Heaters"]
[41,"DW 0","Bit 0","Heaters changed",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heizaend>[B]{w}"]
[41,"DW 1",null,"Fault word",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W0]{p}"]
[41,null,1,"wire break","Heater.20","###INDEX:Heater.20:INDEX"]
[41,null,2,"short-circuit","Heater.21","###INDEX:Heater.21:INDEX"]
[41,null,3,"temperature > 215","Heater.22","###INDEX:Heater.22:INDEX"]
[41,null,4,"temperature too high","Heater.23","###INDEX:Heater.23:INDEX"]
[41,null,5,"temperture too low","Heater.24","###INDEX:Heater.24:INDEX"]
[41,"DW 2",null,"status word",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W1]{p}"]
[41,null,0,"inhibited","Heater.11","###INDEX:Heater.11:INDEX"]
[41,null,1,"active","Heater.10","###INDEX:Heater.10:INDEX"]
[41,null,2,"defective","Heater.12","###INDEX:Heater.12:INDEX"]
[41,"DW 5",null,"actual value","Heater.0","###INDEX:Heater.0:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W4]{p}"]
[41,"DW 6",null,"Y",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_l_1>[W5]{r}"]
[41,"DW 10",null,"Setpoint ","Heater.1","###INDEX:Heater.1:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W0]{r}"]
[41,"DW 11",null,"lower warning limit","Heater.2","###INDEX:Heater.2:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W1]{r}"]
[41,"DW 12",null,"upper warning limit","Heater.3","###INDEX:Heater.3:INDEX","Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W2]{r}"]
[41,"DW 13",null,"P",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W3]{r}"]
[41,"DW 14",null,"I",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W4]{r}"]
[41,"DW 15",null,"D",null,null,"Ch1.###MNR_T_heizung<.m###MNR_heiz_s_1>[W5]{r}"]
[21,"DB ###ADDR:100+1[MNR]:ADDR","Heaters ###MNR"]
[41,"DW 1-19",null,"Heater  1","Heater.###MNR.1","###INDEX:Heater.###MNR.1:INDEX"]
[41,"DW 21-39",null,"Heater  2","Heater.###MNR.2","###INDEX:Heater.###MNR.2:INDEX"]
[41,"DW 41-59",null,"Heater  3","Heater.###MNR.3","###INDEX:Heater.###MNR.3:INDEX"]
[41,"DW 61-79",null,"Heater  4","Heater.###MNR.4","###INDEX:Heater.###MNR.4:INDEX"]
[41,"DW 81-99",null,"Heater  5","Heater.###MNR.5","###INDEX:Heater.###MNR.5:INDEX"]
[41,"DW 101-119",null,"Heater  6","Heater.###MNR.6","###INDEX:Heater.###MNR.6:INDEX"]
[41,"DW 121-139",null,"Heater  7","Heater.###MNR.10","###INDEX:Heater.###MNR.10:INDEX"]
[41,"DW 141-159",null,"Heater  8","Heater.###MNR.11","###INDEX:Heater.###MNR.11:INDEX"]
[41,"DW 161-179",null,"Heater  9","Heater.###MNR.12","###INDEX:Heater.###MNR.12:INDEX"]
[41,"DW 181-199",null,"Heater  10","Heater.###MNR.13","###INDEX:Heater.###MNR.13:INDEX"]
[41,"DW 201-219",null,"Heater  11","Heater.###MNR.14","###INDEX:Heater.###MNR.14:INDEX"]
[41,"DW 221-239",null,"Heater  12","Heater.###MNR.15","###INDEX:Heater.###MNR.15:INDEX"]
[41,"DW 241-259",null,"Heater  13","Heater.###MNR.20","###INDEX:Heater.###MNR.20:INDEX"]
[41,"DW 261-279",null,"Heater  14","Heater.###MNR.21","###INDEX:Heater.###MNR.21:INDEX"]
[41,"DW 281-299",null,"Heater  15","Heater.###MNR.22","###INDEX:Heater.###MNR.22:INDEX"]
[41,"DW 301-319",null,"Heater  16","Heater.###MNR.23","###INDEX:Heater.###MNR.23:INDEX"]
[41,"DW 321-339",null,"Heater  17","Heater.###MNR.24","###INDEX:Heater.###MNR.24:INDEX"]
[41,"DW 341-359",null,"Heater  18","Heater.###MNR.25","###INDEX:Heater.###MNR.25:INDEX"]
[41,"DW 361-379",null,"Heater  19","Heater.###MNR.30","###INDEX:Heater.###MNR.30:INDEX"]
[41,"DW 381-399",null,"Heater  20","Heater.###MNR.31","###INDEX:Heater.###MNR.31:INDEX"]
[41,"DW 401-419",null,"Heater  21","Heater.###MNR.32","###INDEX:Heater.###MNR.32:INDEX"]
[41,"DW 421-439",null,"Heater  22","Heater.###MNR.33","###INDEX:Heater.###MNR.33:INDEX"]
[41,"DW 441-459",null,"Heater  23","Heater.###MNR.34","###INDEX:Heater.###MNR.34:INDEX"]
[41,"DW 461-479",null,"Heater  24","Heater.###MNR.35","###INDEX:Heater.###MNR.35:INDEX"]
[41,"DW 481-499",null,"Heater 25","Heater.###MNR.40","###INDEX:Heater.###MNR.40:INDEX"]
[41,"DW 501-519",null,"Heater 26","Heater.###MNR.41","###INDEX:Heater.###MNR.41:INDEX"]
[41,"DW 521-539",null,"Heater 27","Heater.###MNR.42","###INDEX:Heater.###MNR.42:INDEX"]
[41,"DW 541-559",null,"Heater 28","Heater.###MNR.43","###INDEX:Heater.###MNR.43:INDEX"]
[41,"DW 561-579",null,"Heater 29","Heater.###MNR.44","###INDEX:Heater.###MNR.44:INDEX"]
[41,"DW 581-599",null,"Heater 30","Heater.###MNR.45","###INDEX:Heater.###MNR.45:INDEX"]
[41,"DW 601-619",null,"Heater 31","Heater.###MNR.50","###INDEX:Heater.###MNR.50:INDEX"]
[41,"DW 621-639",null,"Heater 32","Heater.###MNR.51","###INDEX:Heater.###MNR.51:INDEX"]
[41,"DW 641-659",null,"Heater 33","Heater.###MNR.52","###INDEX:Heater.###MNR.52:INDEX"]
[41,"DW 661-679",null,"Heater 34","Heater.###MNR.53","###INDEX:Heater.###MNR.53:INDEX"]
[41,"DW 681-699",null,"Heater 35","Heater.###MNR.54","###INDEX:Heater.###MNR.54:INDEX"]
[41,"DW 701-719",null,"Heater 36","Heater.###MNR.55","###INDEX:Heater.###MNR.55:INDEX"]
[41,"DW 721-739",null,"Heater 37","Heater.###MNR.60","###INDEX:Heater.###MNR.60:INDEX"]
[41,"DW 741-759",null,"Heater 38","Heater.###MNR.61","###INDEX:Heater.###MNR.61:INDEX"]
[41,"DW 761-779",null,"Heater 39","Heater.###MNR.62","###INDEX:Heater.###MNR.62:INDEX"]
[41,"DW 781-799",null,"Heater 40","Heater.###MNR.63","###INDEX:Heater.###MNR.63:INDEX"]
[41,"DW 801-819",null,"Heater 41","Heater.###MNR.64","###INDEX:Heater.###MNR.64:INDEX"]
[41,"DW 821-839",null,"Heater 42","Heater.###MNR.65","###INDEX:Heater.###MNR.65:INDEX"]
[41,"DW 841-859",null,"Heater 43","Heater.###MNR.70","###INDEX:Heater.###MNR.70:INDEX"]
[41,"DW 861-879",null,"Heater 44","Heater.###MNR.71","###INDEX:Heater.###MNR.71:INDEX"]
[41,"DW 881-899",null,"Heater 45","Heater.###MNR.72","###INDEX:Heater.###MNR.72:INDEX"]
[41,"DW 901-919",null,"Heater 46","Heater.###MNR.73","###INDEX:Heater.###MNR.73:INDEX"]
[41,"DW 921-939",null,"Heater 47","Heater.###MNR.74","###INDEX:Heater.###MNR.74:INDEX"]
[41,"DW 941-959",null,"Heater 48","Heater.###MNR.75","###INDEX:Heater.###MNR.75:INDEX"]

{"sheet":"HeaterImpulse","index":70,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
["HeaterImpulse","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 290","Heaters Impulse 1st Machine "]
[41,"DB 291-294","Heaters Impulse Machine 2-5"]
[1,"###MAIN"]
[1,"DB 290-294 Heaters Impulse"]
[41,"DW 0","Bit 0","Heaters changed ",null,null,"Ch1.###MNR_T_heizungimp<.m###MNR_heizimpaend>[B]{w}"]
[41,"DW 11","Bit 0 -15","Good/Bad register 1-16",null,null,"Ch1.###MNR_T_heizungimp<.m###MNR_heizimp_l_1>[W0]{r}"]
[41,"DW 12","Bit 0 -11","Good/Bad register 17-28",null,null,"Ch1.###MNR_T_heizungimp<.m###MNR_heizimp_l_1>[W1]{r}"]
[41,"DW 21",null,"Setpoint temperature",null,null,"Ch1.###MNR_T_heizungimp<.m###MNR_heizimp_s_1>[W0]{r}"]
[41,"DW 22",null,"Setpoint pulses",null,null,"Ch1.###MNR_T_heizungimp<.m###MNR_heizimp_s_1>[W1]{r}"]
[41,"DW 011-030",null,"Heater 1","HeaterImpulse.###MNR.1","###INDEX:HeaterImpulse.###MNR.1:INDEX"]
[41,"DW 031-050",null,"Heater 2","HeaterImpulse.###MNR.2","###INDEX:HeaterImpulse.###MNR.2:INDEX"]
[41,"DW 051-070",null,"Heater 3","HeaterImpulse.###MNR.3","###INDEX:HeaterImpulse.###MNR.3:INDEX"]
[41,"DW 071-090",null,"Heater 4","HeaterImpulse.###MNR.11","###INDEX:HeaterImpulse.###MNR.11:INDEX"]
[41,"DW 091-110",null,"Heater 5","HeaterImpulse.###MNR.12","###INDEX:HeaterImpulse.###MNR.12:INDEX"]
[41,"DW 111-130",null,"Heater 6","HeaterImpulse.###MNR.13","###INDEX:HeaterImpulse.###MNR.13:INDEX"]

{"sheet":"Functions_Palletizer","index":71,"n_rows":257,"n_cols":7,"rows_kept":257,"flags":["formulas_cached_only"]}
["Functions_Palletizer","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 300","Palletierer 1st Machine "]
[21,"DB 300-304","Palletierer Machine  2-5"]
[21,"DB 310","Stringverarbeitung Palletierer 1st Machine "]
[21,"DB 310-314","Stringverarbeitung Palletierer Machine  2-5"]
[1,"###MAIN"]
[1,"DB 300-314 Palletierer"]
[21,"DB ###ADDR:300+1[MNR]:ADDR","Palletierer ###MNR"]
[41,"DW 0","Bit 0","Size changed, Pallet 1",null,null,"Ch1.###MNR_T_roby<.m###MNR_roby_for_aen1>[B]{w}"]
[41,null,"Bit 1","Size changed, Pallet 2",null,null,"Ch1.###MNR_T_roby<.m###MNR_roby_for_aen2>[B]{w}"]
[41,null,"Bit 2","Size changed, Pallet 3",null,null,"Ch1.###MNR_T_roby<.m###MNR_roby_for_aen3>[B]{w}"]
[41,null,"Bit 3","Palletizer changed",null,null,"Ch1.###MNR_T_roby<.m###MNR_roby__aend>[B]{w}"]
[41,"DW 1","Bit 0","Size via network","SizeSelection.1","###INDEX:SizeSelection.1:INDEX","Ch1.###MNR_T_roby<.m###MNR_roby_for_netz>[B]{r}"]
[41,null,"Bit 1","Repeat cycle, yes",null,null,"Ch1.###MNR_T_roby<.m###MNR_zyklus_ja>[B]{r}"]
[41,null,"Bit 2","Repeat cycle, no",null,null,"Ch1.###MNR_T_roby<.m###MNR_zyklus_nein>[B]{r}"]
[41,"DW 9",null,"Repeat pallet number for cycle",null,null,"Ch1.###MNR_T_roby<.m###MNR_zyklus_maschine>[W]{r}"]
[41,"DW 10-37","Speeds"]
[41,"DW 10",null,"Actual speed ","Speed_Palettizer.10","###INDEX:Speed_Palettizer.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_geschwind>[W]{p}"]
[41,"DW 11",null,"Actual acceleration ","Speed_Palettizer.11","###INDEX:Speed_Palettizer.11:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_beschleun>[W]{p}"]
[41,"DW 12",null,"Overdrive ","Speed_Palettizer.32","###INDEX:Speed_Palettizer.32:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_overdrive>[W]{p}"]
[41,"DW 20","Bit 0","Speed with case",null,null,"Ch1.###MNR_T_roby<.m###MNR_akt_ge_mit>[B]{p}"]
[41,null,"Bit 1","Acceleration with case",null,null,"Ch1.###MNR_T_roby<.m###MNR_akt_be_mit>[B]{p}"]
[41,"DW 30",null,"Speed 1","Speed_Palettizer.20","###INDEX:Speed_Palettizer.20:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W0]{r}"]
[41,"DW 31",null,"Speed 2","Speed_Palettizer.21","###INDEX:Speed_Palettizer.21:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W1]{r}"]
[41,"DW 32",null,"Speed 3","Speed_Palettizer.22","###INDEX:Speed_Palettizer.22:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W2]{r}"]
[41,"DW 33",null,"Speed 4","Speed_Palettizer.23","###INDEX:Speed_Palettizer.23:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W3]{r}"]
[41,"DW 34",null,"Acceleration 1","Speed_Palettizer.20","###INDEX:Speed_Palettizer.20:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W4]{r}"]
[41,"DW 35",null,"Acceleration 2 ","Speed_Palettizer.21","###INDEX:Speed_Palettizer.21:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W5]{r}"]
[41,"DW 36",null,"Acceleration 3 ","Speed_Palettizer.22","###INDEX:Speed_Palettizer.22:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W6]{r}"]
[41,"DW 37",null,"Acceleration 4 ","Speed_Palettizer.23","###INDEX:Speed_Palettizer.23:INDEX","Ch1.###MNR_T_roby<.m###MNR_geschwindig>[W7]{r}"]
[31,"DW 40-48","Pallets"]
[41,"DW 40",null,"No. of cases, Pallet A",null,null,"Ch1.###MNR_T_roby<.m###MNR_kartonzahl_1>[W]{p}"]
[41,"DW 41",null,"No. of cases, Pallet B",null,null,"Ch1.###MNR_T_roby<.m###MNR_kartonzahl_2>[W]{p}"]
[41,"DW 42",null,"No. of cases, Pallet C",null,null,"Ch1.###MNR_T_roby<.m###MNR_kartonzahl_3>[W]{p}"]
[41,"DW 43",null,"Status, Pallet A",null,null,"Ch1.###MNR_T_roby<.m###MNR_zustand_1>[W]{p}"]
[41,null,"Bit 0","Pallet empty"]
[41,null,"Bit 1","Pallet half full"]
[41,null,"Bit 2","Pallet full"]
[41,null,"Bit 3","No pallet "]
[41,null,"Bit 4","Reset and start"]
[41,null,"Bit 5","Interrupt safety lamp grid"]
[41,null,"Bit 8","Pallet in"]
[41,null,"Bit 9","Pallet out"]
[41,null,"Bit 10","Pallet yellow"]
[41,null,"Bit 11","Palette red"]
[41,null,"Bit 12","Pallet flashing"]
[41,"DW 44",null,"Status, Pallet B",null,null,"Ch1.###MNR_T_roby<.m###MNR_zustand_2>[W]{p}"]
[41,"DW 45",null,"Status, Pallet C",null,null,"Ch1.###MNR_T_roby<.m###MNR_zustand_3>[W]{p}"]
[41,"DW 46",null,"Pallet type A",null,null,"Ch1.###MNR_T_roby<.m###MNR_palart_1>[W]{p}"]
[41,"DW 47",null,"Pallet type B",null,null,"Ch1.###MNR_T_roby<.m###MNR_palart_2>[W]{p}"]
[41,"DW 48",null,"Pallet type C",null,null,"Ch1.###MNR_T_roby<.m###MNR_palart_3>[W]{p}"]
[31,"DW 50-56","Palletizer functions"]
[41,"DW 50","Bit 0","Presetting 0","Functions_Palletizer.10","###INDEX:Functions_Palletizer.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_funktion>[W]{r}"]
[41,null,"Bit 1","Presetting 1","Functions_Palletizer.11","###INDEX:Functions_Palletizer.10:INDEX"]
[41,null,"Bit 2","Presetting 2","Functions_Palletizer.12","###INDEX:Functions_Palletizer.10:INDEX"]
[41,null,"Bit 3","Presetting 3","Functions_Palletizer.13","###INDEX:Functions_Palletizer.10:INDEX"]
[41,"DW 51","Bit 0","Bit field 1 / 1","Functions_Palletizer.20","###INDEX:Functions_Palletizer.20:INDEX","Ch1.###MNR_T_roby<.m###MNR_funk_ini_1>[W]{r}"]
[41,null,"Bit 1","Bit field 1 / 2","Functions_Palletizer.21","###INDEX:Functions_Palletizer.21:INDEX"]
[41,null,"Bit 2","Bit field 1 / 3","Functions_Palletizer.22","###INDEX:Functions_Palletizer.22:INDEX"]
[41,null,"Bit 3","Bit field 1 / 4","Functions_Palletizer.23","###INDEX:Functions_Palletizer.23:INDEX"]
[41,"DW 52","Bit 0","Bit field 2 / 1","Functions_Palletizer.30","###INDEX:Functions_Palletizer.30:INDEX","Ch1.###MNR_T_roby<.m###MNR_funk_ini_2>[W]{r}"]
[41,null,"Bit 1","Bit field 2 / 2","Functions_Palletizer.31","###INDEX:Functions_Palletizer.31:INDEX"]
[41,null,"Bit 2","Bit field 2 / 3","Functions_Palletizer.32","###INDEX:Functions_Palletizer.32:INDEX"]
[41,null,"Bit 3","Bit field 2 / 4","Functions_Palletizer.33","###INDEX:Functions_Palletizer.33:INDEX"]
[41,null,"Bit 4","Bit field 2 / 5","Functions_Palletizer.34","###INDEX:Functions_Palletizer.34:INDEX"]
[41,null,"Bit 5","Bit field 2 / 6","Functions_Palletizer.35","###INDEX:Functions_Palletizer.35:INDEX"]
[41,null,"Bit 6","Bit field 2 / 7","Functions_Palletizer.36","###INDEX:Functions_Palletizer.36:INDEX"]
[41,null,"Bit 7","Bit field 2 / 8","Functions_Palletizer.37","###INDEX:Functions_Palletizer.37:INDEX"]
[41,"DW 53",null,"Position, Axis 1","Functions_Palletizer.40","###INDEX:Functions_Palletizer.40:INDEX","Ch1.###MNR_T_roby<.m###MNR_funk_pos_1>[W]{p}"]
[41,"DW 54",null,"Position, Axis 2","Functions_Palletizer.41","###INDEX:Functions_Palletizer.41:INDEX","Ch1.###MNR_T_roby<.m###MNR_funk_pos_2>[W]{p}"]
[41,"DW 55",null,"Position, Axis 3","Functions_Palletizer.42","###INDEX:Functions_Palletizer.42:INDEX","Ch1.###MNR_T_roby<.m###MNR_funk_pos_3>[W]{p}"]
[41,"DW 56",null,"Position, Axis 4","Functions_Palletizer.43","###INDEX:Functions_Palletizer.43:INDEX","Ch1.###MNR_T_roby<.m###MNR_funk_pos_4>[W]{p}"]
[31,"DW 60-64","Pallet positions A"]
[41,"DW 60","Bit 0","Automatic","Pallet_Positions.10","###INDEX:Pallet_Positions.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_1_pos>[W]{r}"]
[41,null,"Bit 1","Pallet in"]
[41,null,"Bit 2","Pallet out"]
[41,null,"Bit 3","Pallet up"]
[41,null,"Bit 4","Pallet down"]
[41,null,"Bit 5","Teach in on / off","Pallet_Positions.18","###INDEX:Pallet_Positions.18:INDEX"]
[41,null,"Bit 6","Program cancelled","Pallet_Positions.19","###INDEX:Pallet_Positions.19:INDEX"]
[41,"DW 61",null,"Input value","Pallet_Positions.20","###INDEX:Pallet_Positions.20:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_1_pos_e1>[W]{r}"]
[41,"DW 62",null,"Output value","Pallet_Positions.30","###INDEX:Pallet_Positions.30:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_1_pos_a1>[W]{r}"]
[41,"DW 63","Bit 0","Bit field 1 / 1","Pallet_Positions.40","###INDEX:Pallet_Positions.40:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_1_pos_i1>[W]{r}"]
[41,null,"Bit 1","Bit field 1 / 2","Pallet_Positions.41","###INDEX:Pallet_Positions.41:INDEX"]
[41,null,"Bit 2","Bit field 1 / 3","Pallet_Positions.42","###INDEX:Pallet_Positions.42:INDEX"]
[41,null,"Bit 3","Bit field 1 / 4","Pallet_Positions.43","###INDEX:Pallet_Positions.43:INDEX"]
[41,null,"Bit 4","Bit field 1 / 5","Pallet_Positions.44","###INDEX:Pallet_Positions.44:INDEX"]
[41,null,"Bit 5","Bit field 1 / 6","Pallet_Positions.45","###INDEX:Pallet_Positions.45:INDEX"]
[41,null,"Bit 6","Bit field 1 / 7","Pallet_Positions.46","###INDEX:Pallet_Positions.46:INDEX"]
[41,null,"Bit 7","Bit field 1 / 8","Pallet_Positions.47","###INDEX:Pallet_Positions.47:INDEX"]
[41,"DW 64","Bit 0","Bit field 2 / 1","Pallet_Positions.50","###INDEX:Pallet_Positions.50:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_1_pos_i2>[W]{r}"]
[41,null,"Bit 1","Bit field 2 / 2","Pallet_Positions.51","###INDEX:Pallet_Positions.51:INDEX"]
[41,null,"Bit 2","Bit field 2 / 3","Pallet_Positions.52","###INDEX:Pallet_Positions.52:INDEX"]
[41,null,"Bit 3","Bit field 2 / 4","Pallet_Positions.53","###INDEX:Pallet_Positions.53:INDEX"]
[41,null,"Bit 4","Bit field 2 / 5","Pallet_Positions.54","###INDEX:Pallet_Positions.54:INDEX"]
[41,null,"Bit 5","Bit field 2 / 6","Pallet_Positions.55","###INDEX:Pallet_Positions.55:INDEX"]
[41,null,"Bit 6","Bit field 2 / 7","Pallet_Positions.56","###INDEX:Pallet_Positions.56:INDEX"]
[41,null,"Bit 7","Bit field 2 / 8","Pallet_Positions.57","###INDEX:Pallet_Positions.57:INDEX"]
[31,"DW 70-74","Pallet positions B"]
[41,"DW 70","Bit 0","Automatic","Pallet_Positions.10","###INDEX:Pallet_Positions.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_2_pos>[W]{r}"]
[41,null,"Bit 1","Pallet in"]
[41,null,"Bit 2","Pallet out"]
[41,null,"Bit 3","Pallet up"]
[41,null,"Bit 4","Pallet down"]
[41,null,"Bit 5","Teach in on / off","Pallet_Positions.18","###INDEX:Pallet_Positions.18:INDEX"]
[41,null,"Bit 6","Program cancelled","Pallet_Positions.19","###INDEX:Pallet_Positions.19:INDEX"]
[41,"DW 71",null,"Input value","Pallet_Positions.20","###INDEX:Pallet_Positions.20:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_2_pos_e1>[W]{r}"]
[41,"DW 72",null,"Output value","Pallet_Positions.30","###INDEX:Pallet_Positions.30:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_2_pos_a1>[W]{r}"]
[41,"DW 73","Bit 0","Bit field 1 / 1","Pallet_Positions.60","###INDEX:Pallet_Positions.60:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_2_pos_i1>[W]{r}"]
[41,null,"Bit 1","Bit field 1 / 2","Pallet_Positions.61","###INDEX:Pallet_Positions.61:INDEX"]
[41,null,"Bit 2","Bit field 1 / 3","Pallet_Positions.62","###INDEX:Pallet_Positions.62:INDEX"]
[41,null,"Bit 3","Bit field 1 / 4","Pallet_Positions.63","###INDEX:Pallet_Positions.63:INDEX"]
[41,null,"Bit 4","Bit field 1 / 5","Pallet_Positions.64","###INDEX:Pallet_Positions.64:INDEX"]
[41,null,"Bit 5","Bit field 1 / 6","Pallet_Positions.65","###INDEX:Pallet_Positions.65:INDEX"]
[41,null,"Bit 6","Bit field 1 / 7","Pallet_Positions.66","###INDEX:Pallet_Positions.66:INDEX"]
[41,null,"Bit 7","Bit field 1 / 8","Pallet_Positions.67","###INDEX:Pallet_Positions.67:INDEX"]
[41,"DW 74","Bit 0","Bit field 2 / 1","Pallet_Positions.70","###INDEX:Pallet_Positions.70:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_2_pos_i2>[W]{r}"]
[41,null,"Bit 1","Bit field 2 / 2","Pallet_Positions.71","###INDEX:Pallet_Positions.71:INDEX"]
[41,null,"Bit 2","Bit field 2 / 3","Pallet_Positions.72","###INDEX:Pallet_Positions.72:INDEX"]
[41,null,"Bit 3","Bit field 2 / 4","Pallet_Positions.73","###INDEX:Pallet_Positions.73:INDEX"]
[41,null,"Bit 4","Bit field 2 / 5","Pallet_Positions.74","###INDEX:Pallet_Positions.74:INDEX"]
[41,null,"Bit 5","Bit field 2 / 6","Pallet_Positions.75","###INDEX:Pallet_Positions.75:INDEX"]
[41,null,"Bit 6","Bit field 2 / 7","Pallet_Positions.76","###INDEX:Pallet_Positions.76:INDEX"]
[41,null,"Bit 7","Bit field 2 / 8","Pallet_Positions.77","###INDEX:Pallet_Positions.77:INDEX"]
[31,"DW 80-84","Pallet positions C"]
[41,"DW 80","Bit 0","Automatic","Pallet_Positions.10","###INDEX:Pallet_Positions.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_3_pos>[W]{r}"]
[41,null,"Bit 1","Pallet in"]
[41,null,"Bit 2","Pallet out"]
[41,null,"Bit 3","Pallet up"]
[41,null,"Bit 4","Pallet down"]
[41,null,"Bit 5","Teach in on / off","Pallet_Positions.18","###INDEX:Pallet_Positions.18:INDEX"]
[41,null,"Bit 6","Program cancelled","Pallet_Positions.19","###INDEX:Pallet_Positions.19:INDEX"]
[41,"DW 81",null,"Input value","Pallet_Positions.20","###INDEX:Pallet_Positions.20:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_3_pos_e1>[W]{r}"]
[41,"DW 82",null,"Output value","Pallet_Positions.30","###INDEX:Pallet_Positions.30:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_3_pos_a1>[W]{r}"]
[41,"DW 83","Bit 0","Bit field 1 / 1","Pallet_Positions.80","###INDEX:Pallet_Positions.80:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_3_pos_i1>[W]{r}"]
[41,null,"Bit 1","Bit field 1 / 2","Pallet_Positions.81","###INDEX:Pallet_Positions.81:INDEX"]
[41,null,"Bit 2","Bit field 1 / 3","Pallet_Positions.82","###INDEX:Pallet_Positions.82:INDEX"]
[41,null,"Bit 3","Bit field 1 / 4","Pallet_Positions.83","###INDEX:Pallet_Positions.83:INDEX"]
[41,null,"Bit 4","Bit field 1 / 5","Pallet_Positions.84","###INDEX:Pallet_Positions.84:INDEX"]
[41,null,"Bit 5","Bit field 1 / 6","Pallet_Positions.85","###INDEX:Pallet_Positions.85:INDEX"]
[41,null,"Bit 6","Bit field 1 / 7","Pallet_Positions.86","###INDEX:Pallet_Positions.86:INDEX"]
[41,null,"Bit 7","Bit field 1 / 8","Pallet_Positions.87","###INDEX:Pallet_Positions.87:INDEX"]
[41,"DW 84","Bit 0","Bit field 2 / 1","Pallet_Positions.90","###INDEX:Pallet_Positions.90:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_3_pos_i2>[W]{r}"]
[41,null,"Bit 1","Bit field 2 / 2","Pallet_Positions.91","###INDEX:Pallet_Positions.91:INDEX"]
[41,null,"Bit 2","Bit field 2 / 3","Pallet_Positions.92","###INDEX:Pallet_Positions.92:INDEX"]
[41,null,"Bit 3","Bit field 2 / 4","Pallet_Positions.93","###INDEX:Pallet_Positions.93:INDEX"]
[41,null,"Bit 4","Bit field 2 / 5","Pallet_Positions.94","###INDEX:Pallet_Positions.94:INDEX"]
[41,null,"Bit 5","Bit field 2 / 6","Pallet_Positions.95","###INDEX:Pallet_Positions.95:INDEX"]
[41,null,"Bit 6","Bit field 2 / 7","Pallet_Positions.96","###INDEX:Pallet_Positions.96:INDEX"]
[41,null,"Bit 7","Bit field 2 / 8","Pallet_Positions.97","###INDEX:Pallet_Positions.97:INDEX"]
[31,"DW 90-91","Infeed A"]
[41,"DW 90","Bit 0","Automatic","Infeed_Palletizer.10","###INDEX:Infeed_Palletizer.10:INDEX","Ch1.###MNR_T_roby<.m###MNRE_pal_1_ein>[W]{r}"]
[41,null,"Bit 1","Rotating station +90°"]
[41,null,"Bit 2","Rotating station –90°"]
[41,null,"Bit 3","Rotating station up / down"]
[41,null,"Bit 4","Tipping device, forwards"]
[41,null,"Bit 5","Tipping device, backwards"]
[41,"DW 91","Bit 0","Bit field 1","Infeed_Palletizer.20","###INDEX:Infeed_Palletizer.20:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_1_ein_i1>[W]{r}"]
[41,null,"Bit 1","Bit field 2","Infeed_Palletizer.21","###INDEX:Infeed_Palletizer.21:INDEX"]
[41,null,"Bit 2","Bit field 3","Infeed_Palletizer.22","###INDEX:Infeed_Palletizer.22:INDEX"]
[41,null,"Bit 3","Bit field 4","Infeed_Palletizer.23","###INDEX:Infeed_Palletizer.23:INDEX"]
[41,null,"Bit 4","Bit field 5","Infeed_Palletizer.24","###INDEX:Infeed_Palletizer.24:INDEX"]
[41,null,"Bit 5","Bit field 6","Infeed_Palletizer.25","###INDEX:Infeed_Palletizer.25:INDEX"]
[41,null,"Bit 6","Bit field 7","Infeed_Palletizer.26","###INDEX:Infeed_Palletizer.26:INDEX"]
[41,null,"Bit 7","Bit field 8","Infeed_Palletizer.27","###INDEX:Infeed_Palletizer.27:INDEX"]
[41,null,"Bit 8","Bit field 9","Infeed_Palletizer.28","###INDEX:Infeed_Palletizer.28:INDEX"]
[41,null,"Bit 9","Bit field 10","Infeed_Palletizer.29","###INDEX:Infeed_Palletizer.29:INDEX"]
[41,null,"Bit 10","Bit field 11","Infeed_Palletizer.30","###INDEX:Infeed_Palletizer.30:INDEX"]
[41,null,"Bit 11","Bit field 12","Infeed_Palletizer.31","###INDEX:Infeed_Palletizer.31:INDEX"]
[41,null,"Bit 12","Bit field 13","Infeed_Palletizer.32","###INDEX:Infeed_Palletizer.32:INDEX"]
[41,null,"Bit 13","Bit field 14","Infeed_Palletizer.33","###INDEX:Infeed_Palletizer.33:INDEX"]
[41,null,"Bit 14","Bit field 15","Infeed_Palletizer.34","###INDEX:Infeed_Palletizer.34:INDEX"]
[41,null,"Bit 15","Bit field 16","Infeed_Palletizer.35","###INDEX:Infeed_Palletizer.35:INDEX"]
[31,"DW 93-94","Infeed B"]
[41,"DW 93","Bit 0","Automatic","Infeed_Palletizer.10","###INDEX:Infeed_Palletizer.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_2_ein>[W]{r}"]
[41,null,"Bit 1","Rotating station +90°"]
[41,null,"Bit 2","Rotating station –90°"]
[41,null,"Bit 3","Rotating station up / down"]
[41,null,"Bit 4","Tipping device, forwards"]
[41,null,"Bit 5","Tipping device, backwards"]
[41,"DW 94","Bit 0","Bit field 1","Infeed_Palletizer.40","###INDEX:Infeed_Palletizer.40:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_2_ein_i1>[W]{r}"]
[41,null,"Bit 1","Bit field 2","Infeed_Palletizer.41","###INDEX:Infeed_Palletizer.41:INDEX"]
[41,null,"Bit 2","Bit field 3","Infeed_Palletizer.42","###INDEX:Infeed_Palletizer.42:INDEX"]
[41,null,"Bit 3","Bit field 4","Infeed_Palletizer.43","###INDEX:Infeed_Palletizer.43:INDEX"]
[41,null,"Bit 4","Bit field 5","Infeed_Palletizer.44","###INDEX:Infeed_Palletizer.44:INDEX"]
[41,null,"Bit 5","Bit field 6","Infeed_Palletizer.45","###INDEX:Infeed_Palletizer.45:INDEX"]
[41,null,"Bit 6","Bit field 7","Infeed_Palletizer.46","###INDEX:Infeed_Palletizer.46:INDEX"]
[41,null,"Bit 7","Bit field 8","Infeed_Palletizer.47","###INDEX:Infeed_Palletizer.47:INDEX"]
[41,null,"Bit 8","Bit field 9","Infeed_Palletizer.48","###INDEX:Infeed_Palletizer.48:INDEX"]
[41,null,"Bit 9","Bit field 10","Infeed_Palletizer.49","###INDEX:Infeed_Palletizer.49:INDEX"]
[41,null,"Bit 10","Bit field 11","Infeed_Palletizer.50","###INDEX:Infeed_Palletizer.50:INDEX"]
[41,null,"Bit 11","Bit field 12","Infeed_Palletizer.51","###INDEX:Infeed_Palletizer.51:INDEX"]
[41,null,"Bit 12","Bit field 13","Infeed_Palletizer.52","###INDEX:Infeed_Palletizer.52:INDEX"]
[41,null,"Bit 13","Bit field 14","Infeed_Palletizer.53","###INDEX:Infeed_Palletizer.53:INDEX"]
[41,null,"Bit 14","Bit field 15","Infeed_Palletizer.54","###INDEX:Infeed_Palletizer.54:INDEX"]
[41,null,"Bit 15","Bit field 16","Infeed_Palletizer.55","###INDEX:Infeed_Palletizer.55:INDEX"]
[31,"DW 96-97","Infeed C"]
[41,"DW 96","Bit 0","Automatic","Infeed_Palletizer.10","###INDEX:Infeed_Palletizer.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_3_ein>[W]{r}"]
[41,null,"Bit 1","Rotating station +90°"]
[41,null,"Bit 2","Rotating station –90°"]
[41,null,"Bit 3","Rotating station up / down"]
[41,null,"Bit 4","Tipping device, forwards"]
[41,null,"Bit 5","Tipping device, backwards"]
[41,"DW 97","Bit 0","Bit field 1","Infeed_Palletizer.60","###INDEX:Infeed_Palletizer.60:INDEX","Ch1.###MNR_T_roby<.m###MNR_pal_3_ein_i1>[W]{r}"]
[41,null,"Bit 1","Bit field 2","Infeed_Palletizer.61","###INDEX:Infeed_Palletizer.61:INDEX"]
[41,null,"Bit 2","Bit field 3","Infeed_Palletizer.62","###INDEX:Infeed_Palletizer.62:INDEX"]
[41,null,"Bit 3","Bit field 4","Infeed_Palletizer.63","###INDEX:Infeed_Palletizer.63:INDEX"]
[41,null,"Bit 4","Bit field 5","Infeed_Palletizer.64","###INDEX:Infeed_Palletizer.64:INDEX"]
[41,null,"Bit 5","Bit field 6","Infeed_Palletizer.65","###INDEX:Infeed_Palletizer.65:INDEX"]
[41,null,"Bit 6","Bit field 7","Infeed_Palletizer.66","###INDEX:Infeed_Palletizer.66:INDEX"]
[41,null,"Bit 7","Bit field 8","Infeed_Palletizer.67","###INDEX:Infeed_Palletizer.67:INDEX"]
[41,null,"Bit 8","Bit field 9","Infeed_Palletizer.68","###INDEX:Infeed_Palletizer.68:INDEX"]
[41,null,"Bit 9","Bit field 10","Infeed_Palletizer.69","###INDEX:Infeed_Palletizer.69:INDEX"]
[41,null,"Bit 10","Bit field 11","Infeed_Palletizer.70","###INDEX:Infeed_Palletizer.70:INDEX"]
[41,null,"Bit 11","Bit field 12","Infeed_Palletizer.71","###INDEX:Infeed_Palletizer.71:INDEX"]
[41,null,"Bit 12","Bit field 13","Infeed_Palletizer.72","###INDEX:Infeed_Palletizer.72:INDEX"]
[41,null,"Bit 13","Bit field 14","Infeed_Palletizer.73","###INDEX:Infeed_Palletizer.73:INDEX"]
[41,null,"Bit 14","Bit field 15","Infeed_Palletizer.74","###INDEX:Infeed_Palletizer.74:INDEX"]
[41,null,"Bit 15","Bit field 16","Infeed_Palletizer.75","###INDEX:Infeed_Palletizer.75:INDEX"]
[31,"DW 100-130","Maintenance"]
[41,"DW 100",null,"Offset 1","Presets_Palletizer.10","###INDEX:Presets_Palletizer.10:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W0]{r}"]
[41,"DW 101",null,"Offset 2","Presets_Palletizer.11","###INDEX:Presets_Palletizer.11:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W1]{r}"]
[41,"DW 102",null,"Offset 3","Presets_Palletizer.12","###INDEX:Presets_Palletizer.12:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W2]{r}"]
[41,"DW 103",null,"Offset 4","Presets_Palletizer.13","###INDEX:Presets_Palletizer.13:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W3]{r}"]
[41,"DW 104",null,"Offset 5","Presets_Palletizer.14","###INDEX:Presets_Palletizer.14:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W4]{r}"]
[41,"DW 105",null,"Offset 6","Presets_Palletizer.15","###INDEX:Presets_Palletizer.15:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W5]{r}"]
[41,"DW 106",null,"Offset 7","Presets_Palletizer.16","###INDEX:Presets_Palletizer.16:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W6]{r}"]
[41,"DW 107",null,"Offset 8","Presets_Palletizer.17","###INDEX:Presets_Palletizer.17:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset>[W7]{r}"]
[41,"DW 110",null,"Maintenance 1","Presets_Palletizer.30","###INDEX:Presets_Palletizer.30:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W0]{r}"]
[41,"DW 111",null,"Maintenance 2","Presets_Palletizer.31","###INDEX:Presets_Palletizer.31:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W1]{r}"]
[41,"DW 112",null,"Maintenance 3","Presets_Palletizer.32","###INDEX:Presets_Palletizer.32:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W2]{r}"]
[41,"DW 113",null,"Maintenance 4","Presets_Palletizer.33","###INDEX:Presets_Palletizer.33:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W3]{r}"]
[41,"DW 114",null,"Maintenance 5","Presets_Palletizer.34","###INDEX:Presets_Palletizer.34:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W4]{r}"]
[41,"DW 115",null,"Maintenance 6","Presets_Palletizer.35","###INDEX:Presets_Palletizer.35:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W5]{r}"]
[41,"DW 116",null,"Maintenance 7","Presets_Palletizer.36","###INDEX:Presets_Palletizer.36:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W6]{r}"]
[41,"DW 117",null,"Maintenance 8","Presets_Palletizer.37","###INDEX:Presets_Palletizer.37:INDEX","Ch1.###MNR_T_roby<.m###MNR_offset_wartung_soll>[W7]{r}"]
[41,"DW 120-127",null,"Maintenance, actual values",null,null,"Ch1.###MNR_T_roby<.m###MNR_wartung_ist>[W0-7]{r}"]
[41,"DW 130","Bit 0-7","Reset maintenance 1-8",null,null,"Ch1.###MNR_T_roby<.m###MNR_wartung_reset>[W0-7]{r}"]
[41]
[41,"DW 140-152","Palletizer_TargetPos"]
[41]
[31,"DB ###ADDR:310+1[MNR]:ADDR","String processing, Palletizer ###MNR"]
[31,"DW 0-95","Infeed sizes"]
[41,"DW 0-15",null,"Current Size A (30 characters +1*line end)",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_alt_form_ein_1>[S0-15]{r}"]
[41,"DW 16-31",null,"New Size A",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_neu_form_ein_1>[S0-15]{r}"]
[41,"DW 32-47",null,"Current Size B (30 characters +1*line end)",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_alt_form_ein_2>[S0-15]{r}"]
[41,"DW 48-63",null,"New Size B",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_neu_form_ein_2>[S0-15]{r}"]
[41,"DW 64-79",null,"Current Size C (30 characters +1*line end)",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_alt_form_ein_3>[S0-15]{r}"]
[41,"DW 80-95",null,"New Size C",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_neu_form_ein_3>[S0-15]{r}"]
[31,"DW 96-110","Pallet formats"]
[41,"DW 96-110",null,"Current Size A (30 characters +1*line end)",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_alt_form_pal_1>[S0-15]{r}"]
[41,"DW 111-125",null,"New Size A",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_neu_form_pal_1>[S0-15]{r}"]
[41,"DW 126-140",null,"Current Size B (30 characters +1*line end)",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_alt_form_pal_2>[S0-15]{r}"]
[41,"DW 141-155",null,"New Size B",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_neu_form_pal_2>[S0-15]{r}"]
[41,"DW 156-170",null,"Current Size C (30 characters +1*line end)",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_alt_form_pal_3>[S0-15]{r}"]
[41,"DW 171-185",null,"New Size C",null,null,"Ch1.###MNR_T_roby_string<.m###MNR_r_neu_form_pal_3>[S0-15]{r}"]

{"sheet":"Palletizer_TargetPos","index":72,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
["Palletizer_TargetPos","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 300","Palletierer 1st Machine "]
[21,"DB 300-304","Palletierer Machine  2-5"]
[21,"DB 310","Stringverarbeitung Palletierer 1st Machine "]
[21,"DB 310-314","Stringverarbeitung Palletierer Machine  2-5"]
[1,"###MAIN"]
[1,"DB 300-314 Palletierer"]
[21,"DB ###ADDR:300+1[MNR]:ADDR","Palletierer ###MNR"]
[41,"DW 0 - 139 Functions_Palletizer"]
[41]
[31,"DW 130-152","Maintenance"]
[41,"DW 140","Bit 0","Target changed",null,null,"Ch1.###MNR_T_roby<.m###MNR_roby_ziel_aend>[B]{w}"]
[41,"DW 141",null,"Current target, Loading Position A","Palletizer_TargetPos.1","###INDEX: Palletizer_TargetPos.1:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_ziel_be_a>[W]{p}"]
[41,"DW 142",null,"New target, Loading Position A",null,null,"Ch1.###MNR_T_roby<.m###MNR_neu_ziel_be_a>[W]{r}"]
[41,"DW 143",null,"Current target, Unloading Position A","Palletizer_TargetPos.2","###INDEX: Palletizer_TargetPos.2:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_ziel_en_a>[W]{p}"]
[41,"DW 144",null,"New target, Unloading Position A",null,null,"Ch1.###MNR_T_roby<.m###MNR_neu_ziel_en_a>[W]{r}"]
[41,"DW 145",null,"Current target, Loading Position B","Palletizer_TargetPos.1","###INDEX: Palletizer_TargetPos.1:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_ziel_be_b>[W]{p}"]
[41,"DW 146",null,"New target, Loading Position B",null,null,"Ch1.###MNR_T_roby<.m###MNR_neu_ziel_be_b>[W]{r}"]
[41,"DW 147",null,"Current target, Unloading Position B","Palletizer_TargetPos.2","###INDEX: Palletizer_TargetPos.2:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_ziel_en_b>[W]{p}"]
[41,"DW 148",null,"New target, Unloading Position B",null,null,"Ch1.###MNR_T_roby<.m###MNR_neu_ziel_en_b>[W]{r}"]
[41,"DW 149",null,"Current target, Loading Position C","Palletizer_TargetPos.1","###INDEX: Palletizer_TargetPos.1:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_ziel_be_c>[W]{p}"]
[41,"DW 150",null,"New target, Loading Position C",null,null,"Ch1.###MNR_T_roby<.m###MNR_neu_ziel_be_c>[W]{r}"]
[41,"DW 151",null,"Current target, Unloading Position C","Palletizer_TargetPos.2","###INDEX: Palletizer_TargetPos.2:INDEX","Ch1.###MNR_T_roby<.m###MNR_akt_ziel_en_c>[W]{p}"]
[41,"DW 152",null,"New target, Unloading Position C",null,null,"Ch1.###MNR_T_roby<.m###MNR_neu_ziel_en_c>[W]{r}"]

{"sheet":"TaxStampMonitoring","index":73,"n_rows":28,"n_cols":7,"rows_kept":28,"flags":["formulas_cached_only"]}
["TaxStampMonitoring","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 320","Banderolenendkontrolle 1st Machine "]
[21,"DB 320-324","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 320-324 Banderolenendkontrolle"]
[21,"DB ###ADDR:320+1[MNR]:ADDR","Banderolenendkontrolle ###MNR"]
[41,"DW 0","Bit 0","Banderolenendkontrolle geändert",null,null,"Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_aender>[B]{w}"]
[41,"DW 1","Bit 0 ","Versionsinfo FB "]
[41]
[41,"DW 10","Bit 0","Daten senden","TaxStampMonitoring.10","###INDEX:TaxStampMonitoring.10:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_bit>[W]{r}"]
[41,null,"Bit 1","Daten holen","TaxStampMonitoring.11","###INDEX:TaxStampMonitoring.11:INDEX"]
[41,"DW 11","Bit 0 ","Versionsinfo FB "]
[41,"DW 20",null,"Fenster rechts","TaxStampMonitoring.20","###INDEX:TaxStampMonitoring.20:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W0]{r}"]
[41,"DW 21",null,"Fenster links","TaxStampMonitoring.21","###INDEX:TaxStampMonitoring.21:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W1]{r}"]
[41,"DW 22",null,"Fenster oben","TaxStampMonitoring.22","###INDEX:TaxStampMonitoring.22:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W2]{r}"]
[41,"DW 23",null,"Fenster unten","TaxStampMonitoring.23","###INDEX:TaxStampMonitoring.23:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W3]{r}"]
[41,"DW 24",null,"Helligkeit","TaxStampMonitoring.24","###INDEX:TaxStampMonitoring.24:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W4]{r}"]
[41,"DW 25",null,"Format","TaxStampMonitoring.25","###INDEX:TaxStampMonitoring.25:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W5]{r}"]
[41,"DW 26",null,"Teach value 1","TaxStampMonitoring.30","###INDEX:TaxStampMonitoring.30:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W6]{r}"]
[41,"DW 27",null,"Teach value 2","TaxStampMonitoring.31","###INDEX:TaxStampMonitoring.31:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll>[W7]{r}"]
[41]
[41,"DW 30",null,"Istwert 1","TaxStampMonitoring.30","###INDEX:TaxStampMonitoring.30:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist>[W0]{p}"]
[41,"DW 31",null,"Istwert 2","TaxStampMonitoring.31","###INDEX:TaxStampMonitoring.31:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist>[W1]{p}"]
[41,"DW 32",null,"Istwert 3","TaxStampMonitoring.32","###INDEX:TaxStampMonitoring.32:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist>[W2]{p}"]
[41,"DW 33",null,"Istwert 4","TaxStampMonitoring.33","###INDEX:TaxStampMonitoring.33:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist>[W3]{p}"]
[41,"DW 34",null,"Istwert 5","TaxStampMonitoring.34","###INDEX:TaxStampMonitoring.34:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist>[W4]{p}"]

{"sheet":"TaxStampMonitoring2","index":74,"n_rows":46,"n_cols":7,"rows_kept":46,"flags":["formulas_cached_only"]}
["TaxStampMonitoring2","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 320","Banderolenendkontrolle 1st Machine "]
[21,"DB 320-324","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 320-324 Banderolenendkontrolle"]
[21,"DB ###ADDR:320+1[MNR]:ADDR","Banderolenendkontrolle ###MNR"]
[41,"DW 0","Bit 0","Banderolenendkontrolle geändert",null,null,"Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_aender>[B]{w}"]
[41,"DW 1","Bit 0 ","Versionsinfo FB "]
[41]
[21,null,"Page 1"]
[41,"DW 10","Bit 0","Daten senden","TaxStampMonitoring.10","###INDEX:TaxStampMonitoring.10:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_bit1>[W]{r}"]
[41,null,"Bit 1","Daten holen","TaxStampMonitoring.11","###INDEX:TaxStampMonitoring.11:INDEX"]
[41,"DW 20",null,"Fenster rechts","TaxStampMonitoring.20","###INDEX:TaxStampMonitoring.20:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W0]{r}"]
[41,"DW 21",null,"Fenster links","TaxStampMonitoring.21","###INDEX:TaxStampMonitoring.21:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W1]{r}"]
[41,"DW 22",null,"Fenster oben","TaxStampMonitoring.22","###INDEX:TaxStampMonitoring.22:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W2]{r}"]
[41,"DW 23",null,"Fenster unten","TaxStampMonitoring.23","###INDEX:TaxStampMonitoring.23:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W3]{r}"]
[41,"DW 24",null,"Helligkeit","TaxStampMonitoring.24","###INDEX:TaxStampMonitoring.24:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W4]{r}"]
[41,"DW 25",null,"Format","TaxStampMonitoring.25","###INDEX:TaxStampMonitoring.25:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W5]{r}"]
[41,"DW 26",null,"Teach value 1","TaxStampMonitoring.30","###INDEX:TaxStampMonitoring.30:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W6]{r}"]
[41,"DW 27",null,"Teach value 2","TaxStampMonitoring.31","###INDEX:TaxStampMonitoring.31:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll1>[W7]{r}"]
[41]
[41,"DW 30",null,"Istwert 1","TaxStampMonitoring.30","###INDEX:TaxStampMonitoring.30:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist1>[W0]{p}"]
[41,"DW 31",null,"Istwert 2","TaxStampMonitoring.31","###INDEX:TaxStampMonitoring.31:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist1>[W1]{p}"]
[41,"DW 32",null,"Istwert 3","TaxStampMonitoring.32","###INDEX:TaxStampMonitoring.32:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist1>[W2]{p}"]
[41,"DW 33",null,"Istwert 4","TaxStampMonitoring.33","###INDEX:TaxStampMonitoring.33:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist1>[W3]{p}"]
[41,"DW 34",null,"Istwert 5","TaxStampMonitoring.34","###INDEX:TaxStampMonitoring.34:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist1>[W4]{p}"]
[41]
[21,null,"Page 2"]
[41,"DW 40","Bit 0","Daten senden","TaxStampMonitoring.60","###INDEX:TaxStampMonitoring.60:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_bit2>[W]{r}"]
[41,null,"Bit 1","Daten holen","TaxStampMonitoring.61","###INDEX:TaxStampMonitoring.61:INDEX"]
[41,"DW 50",null,"Fenster rechts","TaxStampMonitoring.70","###INDEX:TaxStampMonitoring.70:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W0]{r}"]
[41,"DW 51",null,"Fenster links","TaxStampMonitoring.71","###INDEX:TaxStampMonitoring.71:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W1]{r}"]
[41,"DW 52",null,"Fenster oben","TaxStampMonitoring.72","###INDEX:TaxStampMonitoring.72:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W2]{r}"]
[41,"DW 53",null,"Fenster unten","TaxStampMonitoring.73","###INDEX:TaxStampMonitoring.73:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W3]{r}"]
[41,"DW 54",null,"Helligkeit","TaxStampMonitoring.74","###INDEX:TaxStampMonitoring.74:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W4]{r}"]
[41,"DW 55",null,"Format","TaxStampMonitoring.75","###INDEX:TaxStampMonitoring.75:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W5]{r}"]
[41,"DW 56",null,"Teach value 1","TaxStampMonitoring.80","###INDEX:TaxStampMonitoring.80:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W6]{r}"]
[41,"DW 57",null,"Teach value 2","TaxStampMonitoring.81","###INDEX:TaxStampMonitoring.81:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_soll2>[W7]{r}"]
[41]
[41,"DW 60",null,"Istwert 1","TaxStampMonitoring.80","###INDEX:TaxStampMonitoring.80:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist2>[W0]{p}"]
[41,"DW 61",null,"Istwert 2","TaxStampMonitoring.81","###INDEX:TaxStampMonitoring.81:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist2>[W1]{p}"]
[41,"DW 62",null,"Istwert 3","TaxStampMonitoring.82","###INDEX:TaxStampMonitoring.82:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist2>[W2]{p}"]
[41,"DW 63",null,"Istwert 4","TaxStampMonitoring.83","###INDEX:TaxStampMonitoring.83:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist2>[W3]{p}"]
[41,"DW 64",null,"Istwert 5","TaxStampMonitoring.84","###INDEX:TaxStampMonitoring.84:INDEX","Ch1.###MNR_T_taxstampmon<.m###MNR_taxstampmon_ist2>[W4]{p}"]

{"sheet":"DCS_MainPicture","index":75,"n_rows":23,"n_cols":6,"rows_kept":23,"flags":["formulas_cached_only"]}
["DCS_MainPicture","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 330","DCS-Efficiency 1st Machine "]
[21,"DB 331-334","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 330-334 DCS-Efficiency"]
[21,"DB ###ADDR:330+1[MNR]:ADDR","DCS-Efficiency ###MNR"]
[41,"DD 10",null,"Abgelaufene Schichtzeit"]
[41,"DD 12",null,"Schichtzeit Insgesamt"]
[41]
[41,"DD 20",null,"Theoretische Gesamtproduktion derSchicht","DCS-Efficiency.10","###INDEX:TaxStampMonitoring.20:INDEX"]
[41,"DW 21",null,"Fenster links","TaxStampMonitoring.21","###INDEX:TaxStampMonitoring.21:INDEX"]
[41,"DW 22",null,"Fenster oben","TaxStampMonitoring.22","###INDEX:TaxStampMonitoring.22:INDEX"]
[41,"DW 23",null,"Fenster unten","TaxStampMonitoring.23","###INDEX:TaxStampMonitoring.23:INDEX"]
[41,"DW 24",null,"Helligkeit","TaxStampMonitoring.24","###INDEX:TaxStampMonitoring.24:INDEX"]
[41,"DW 25",null,"Format","TaxStampMonitoring.25","###INDEX:TaxStampMonitoring.25:INDEX"]
[41]
[41,"DW 30",null,"Istwert 1","TaxStampMonitoring.30","###INDEX:TaxStampMonitoring.30:INDEX"]
[41,"DW 31",null,"Istwert 2","TaxStampMonitoring.31","###INDEX:TaxStampMonitoring.31:INDEX"]
[41,"DW 32",null,"Istwert 3","TaxStampMonitoring.32","###INDEX:TaxStampMonitoring.32:INDEX"]
[41,"DW 33",null,"Istwert 4","TaxStampMonitoring.33","###INDEX:TaxStampMonitoring.33:INDEX"]
[41,"DW 34",null,"Istwert 5","TaxStampMonitoring.34","###INDEX:TaxStampMonitoring.34:INDEX"]

{"sheet":"ServicePresets","index":76,"n_rows":338,"n_cols":7,"rows_kept":338,"flags":["formulas_cached_only"]}
["ServicePresets","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 340","ServicePresets 1st Machine "]
[21,"DB 341-344","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 340-344 Voreinstellungen Service"]
[21,"DB ###ADDR:340+1[MNR]:ADDR","Voreinstellungen Service ###MNR"]
[41,"DW 0","Bit 0","Voreinstellungen Service geändert",null,null,"Ch1.###MNR_T_sp<.m###MNR_sp_aender>[B]{w}"]
[41,"DD 10 - 136","64 Eingabewerte"]
[41,"DD 10",null,"Eingabewert 1","ServicePresets.1","###INDEX:ServicePresets.###MNR.1:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW0]{r}"]
[41,"DD 12 ",null,"Eingabewert 2","ServicePresets.2","###INDEX:ServicePresets.###MNR.2:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW1]{r}"]
[41,"DD 14",null,"Eingabewert 3","ServicePresets.3","###INDEX:ServicePresets.###MNR.3:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW2]{r}"]
[41,"DD 16",null,"Eingabewert 4","ServicePresets.4","###INDEX:ServicePresets.###MNR.4:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW3]{r}"]
[41,"DD 18",null,"Eingabewert 5","ServicePresets.5","###INDEX:ServicePresets.###MNR.5:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW4]{r}"]
[41,"DD 20",null,"Eingabewert 6","ServicePresets.6","###INDEX:ServicePresets.###MNR.6:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW5]{r}"]
[41,"DD 22",null,"Eingabewert 7","ServicePresets.7","###INDEX:ServicePresets.###MNR.7:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW6]{r}"]
[41,"DD 24",null,"Eingabewert 8","ServicePresets.8","###INDEX:ServicePresets.###MNR.8:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW7]{r}"]
[41,"DD 26",null,"Eingabewert 9","ServicePresets.9","###INDEX:ServicePresets.###MNR.9:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW8]{r}"]
[41,"DD 28",null,"Eingabewert 10","ServicePresets.10","###INDEX:ServicePresets.###MNR.10:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW9]{r}"]
[41,"DD 30",null,"Eingabewert 11","ServicePresets.11","###INDEX:ServicePresets.###MNR.11:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW10]{r}"]
[41,"DD 32",null,"Eingabewert 12","ServicePresets.12","###INDEX:ServicePresets.###MNR.12:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW11]{r}"]
[41,"DD 34",null,"Eingabewert 13","ServicePresets.13","###INDEX:ServicePresets.###MNR.13:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW12]{r}"]
[41,"DD 36",null,"Eingabewert 14","ServicePresets.14","###INDEX:ServicePresets.###MNR.14:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW13]{r}"]
[41,"DD 38",null,"Eingabewert 15","ServicePresets.15","###INDEX:ServicePresets.###MNR.15:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW14]{r}"]
[41,"DD 40",null,"Eingabewert 16","ServicePresets.16","###INDEX:ServicePresets.###MNR.16:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW15]{r}"]
[41,"DD 42",null,"Eingabewert 17","ServicePresets.17","###INDEX:ServicePresets.###MNR.17:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW16]{r}"]
[41,"DD 44",null,"Eingabewert 18","ServicePresets.18","###INDEX:ServicePresets.###MNR.18:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW17]{r}"]
[41,"DD 46",null,"Eingabewert 19","ServicePresets.19","###INDEX:ServicePresets.###MNR.19:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW18]{r}"]
[41,"DD 48",null,"Eingabewert 20","ServicePresets.20","###INDEX:ServicePresets.###MNR.20:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW19]{r}"]
[41,"DD 50",null,"Eingabewert 21","ServicePresets.21","###INDEX:ServicePresets.###MNR.21:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW20]{r}"]
[41,"DD 52",null,"Eingabewert 22","ServicePresets.22","###INDEX:ServicePresets.###MNR.22:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW21]{r}"]
[41,"DD 54",null,"Eingabewert 23","ServicePresets.23","###INDEX:ServicePresets.###MNR.23:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW22]{r}"]
[41,"DD 56",null,"Eingabewert 24","ServicePresets.24","###INDEX:ServicePresets.###MNR.24:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW23]{r}"]
[41,"DD 58",null,"Eingabewert 25","ServicePresets.25","###INDEX:ServicePresets.###MNR.25:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW24]{r}"]
[41,"DD 60",null,"Eingabewert 26","ServicePresets.26","###INDEX:ServicePresets.###MNR.26:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW25]{r}"]
[41,"DD 62",null,"Eingabewert 27","ServicePresets.27","###INDEX:ServicePresets.###MNR.27:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW26]{r}"]
[41,"DD 64",null,"Eingabewert 28","ServicePresets.28","###INDEX:ServicePresets.###MNR.28:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW27]{r}"]
[41,"DD 66",null,"Eingabewert 29","ServicePresets.29","###INDEX:ServicePresets.###MNR.29:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW28]{r}"]
[41,"DD 68",null,"Eingabewert 30","ServicePresets.30","###INDEX:ServicePresets.###MNR.30:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW29]{r}"]
[41,"DD 70",null,"Eingabewert 31","ServicePresets.31","###INDEX:ServicePresets.###MNR.31:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW30]{r}"]
[41,"DD 72",null,"Eingabewert 32","ServicePresets.32","###INDEX:ServicePresets.###MNR.32:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW31]{r}"]
[41,"DD 74",null,"Eingabewert 33","ServicePresets.33","###INDEX:ServicePresets.###MNR.33:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW32]{r}"]
[41,"DD 76",null,"Eingabewert 34","ServicePresets.34","###INDEX:ServicePresets.###MNR.34:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW33]{r}"]
[41,"DD 78",null,"Eingabewert 35","ServicePresets.35","###INDEX:ServicePresets.###MNR.35:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW34]{r}"]
[41,"DD 80",null,"Eingabewert 36","ServicePresets.36","###INDEX:ServicePresets.###MNR.36:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW35]{r}"]
[41,"DD 82",null,"Eingabewert 37","ServicePresets.37","###INDEX:ServicePresets.###MNR.37:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW36]{r}"]
[41,"DD 84",null,"Eingabewert 38","ServicePresets.38","###INDEX:ServicePresets.###MNR.38:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW37]{r}"]
[41,"DD 86",null,"Eingabewert 39","ServicePresets.39","###INDEX:ServicePresets.###MNR.39:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW38]{r}"]
[41,"DD 88",null,"Eingabewert 40","ServicePresets.40","###INDEX:ServicePresets.###MNR.40:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW39]{r}"]
[41,"DD 90",null,"Eingabewert 41","ServicePresets.41","###INDEX:ServicePresets.###MNR.41:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW40]{r}"]
[41,"DD 92",null,"Eingabewert 42","ServicePresets.42","###INDEX:ServicePresets.###MNR.42:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW41]{r}"]
[41,"DD 94",null,"Eingabewert 43","ServicePresets.43","###INDEX:ServicePresets.###MNR.43:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW42]{r}"]
[41,"DD 96",null,"Eingabewert 44","ServicePresets.44","###INDEX:ServicePresets.###MNR.44:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW43]{r}"]
[41,"DD 98",null,"Eingabewert 45","ServicePresets.45","###INDEX:ServicePresets.###MNR.45:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW44]{r}"]
[41,"DD 100",null,"Eingabewert 46","ServicePresets.46","###INDEX:ServicePresets.###MNR.46:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW45]{r}"]
[41,"DD 102",null,"Eingabewert 47","ServicePresets.47","###INDEX:ServicePresets.###MNR.47:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW46]{r}"]
[41,"DD 104",null,"Eingabewert 48","ServicePresets.48","###INDEX:ServicePresets.###MNR.48:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW47]{r}"]
[41,"DD 106",null,"Eingabewert 49","ServicePresets.49","###INDEX:ServicePresets.###MNR.49:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW48]{r}"]
[41,"DD 108",null,"Eingabewert 50","ServicePresets.50","###INDEX:ServicePresets.###MNR.50:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW49]{r}"]
[41,"DD 110",null,"Eingabewert 51","ServicePresets.51","###INDEX:ServicePresets.###MNR.51:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW50]{r}"]
[41,"DD 112",null,"Eingabewert 52","ServicePresets.52","###INDEX:ServicePresets.###MNR.52:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW51]{r}"]
[41,"DD 114",null,"Eingabewert 53","ServicePresets.53","###INDEX:ServicePresets.###MNR.53:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW52]{r}"]
[41,"DD 116",null,"Eingabewert 54","ServicePresets.54","###INDEX:ServicePresets.###MNR.54:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW53]{r}"]
[41,"DD 118",null,"Eingabewert 55","ServicePresets.55","###INDEX:ServicePresets.###MNR.55:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW54]{r}"]
[41,"DD 120",null,"Eingabewert 56","ServicePresets.56","###INDEX:ServicePresets.###MNR.56:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW55]{r}"]
[41,"DD 122",null,"Eingabewert 57","ServicePresets.57","###INDEX:ServicePresets.###MNR.57:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW56]{r}"]
[41,"DD 124",null,"Eingabewert 58","ServicePresets.58","###INDEX:ServicePresets.###MNR.58:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW57]{r}"]
[41,"DD 126",null,"Eingabewert 59","ServicePresets.59","###INDEX:ServicePresets.###MNR.59:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW58]{r}"]
[41,"DD 128",null,"Eingabewert 60","ServicePresets.60","###INDEX:ServicePresets.###MNR.60:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW59]{r}"]
[41,"DD 130",null,"Eingabewert 61","ServicePresets.61","###INDEX:ServicePresets.###MNR.61:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW60]{r}"]
[41,"DD 132",null,"Eingabewert 62","ServicePresets.62","###INDEX:ServicePresets.###MNR.62:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW61]{r}"]
[41,"DD 134",null,"Eingabewert 63","ServicePresets.63","###INDEX:ServicePresets.###MNR.63:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW62]{r}"]
[41,"DD 136",null,"Eingabewert 64","ServicePresets.64","###INDEX:ServicePresets.###MNR.64:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input>[DW63]{r}"]
[41,"DD 140 - 266","64 Ausgabewerte"]
[41,"DD 140",null,"Ausgabewert 1","ServicePresets.101","###INDEX:ServicePresets.###MNR.101:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW0]{r}"]
[41,"DD 142",null,"Ausgabewert 2","ServicePresets.102","###INDEX:ServicePresets.###MNR.102:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW1]{r}"]
[41,"DD 144",null,"Ausgabewert 3","ServicePresets.103","###INDEX:ServicePresets.###MNR.103:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW2]{r}"]
[41,"DD 146",null,"Ausgabewert 4","ServicePresets.104","###INDEX:ServicePresets.###MNR.104:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW3]{r}"]
[41,"DD 148",null,"Ausgabewert 5","ServicePresets.105","###INDEX:ServicePresets.###MNR.105:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW4]{r}"]
[41,"DD 150",null,"Ausgabewert 6","ServicePresets.106","###INDEX:ServicePresets.###MNR.106:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW5]{r}"]
[41,"DD 152",null,"Ausgabewert 7","ServicePresets.107","###INDEX:ServicePresets.###MNR.107:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW6]{r}"]
[41,"DD 154",null,"Ausgabewert 8","ServicePresets.108","###INDEX:ServicePresets.###MNR.108:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW7]{r}"]
[41,"DD 156",null,"Ausgabewert 9","ServicePresets.109","###INDEX:ServicePresets.###MNR.109:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW8]{r}"]
[41,"DD 158",null,"Ausgabewert 10","ServicePresets.110","###INDEX:ServicePresets.###MNR.110:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW9]{r}"]
[41,"DD 160",null,"Ausgabewert 11","ServicePresets.111","###INDEX:ServicePresets.###MNR.111:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW10]{r}"]
[41,"DD 162",null,"Ausgabewert 12","ServicePresets.112","###INDEX:ServicePresets.###MNR.112:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW11]{r}"]
[41,"DD 164",null,"Ausgabewert 13","ServicePresets.113","###INDEX:ServicePresets.###MNR.113:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW12]{r}"]
[41,"DD 166",null,"Ausgabewert 14","ServicePresets.114","###INDEX:ServicePresets.###MNR.114:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW13]{r}"]
[41,"DD 168",null,"Ausgabewert 15","ServicePresets.115","###INDEX:ServicePresets.###MNR.115:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW14]{r}"]
[41,"DD 170",null,"Ausgabewert 16","ServicePresets.116","###INDEX:ServicePresets.###MNR.116:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW15]{r}"]
[41,"DD 172",null,"Ausgabewert 17","ServicePresets.117","###INDEX:ServicePresets.###MNR.117:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW16]{r}"]
[41,"DD 174",null,"Ausgabewert 18","ServicePresets.118","###INDEX:ServicePresets.###MNR.118:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW17]{r}"]
[41,"DD 176",null,"Ausgabewert 19","ServicePresets.119","###INDEX:ServicePresets.###MNR.119:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW18]{r}"]
[41,"DD 178",null,"Ausgabewert 20","ServicePresets.120","###INDEX:ServicePresets.###MNR.120:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW19]{r}"]
[41,"DD 180",null,"Ausgabewert 21","ServicePresets.121","###INDEX:ServicePresets.###MNR.121:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW20]{r}"]
[41,"DD 182",null,"Ausgabewert 22","ServicePresets.122","###INDEX:ServicePresets.###MNR.122:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW21]{r}"]
[41,"DD 184",null,"Ausgabewert 23","ServicePresets.123","###INDEX:ServicePresets.###MNR.123:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW22]{r}"]
[41,"DD 186",null,"Ausgabewert 24","ServicePresets.124","###INDEX:ServicePresets.###MNR.124:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW23]{r}"]
[41,"DD 188",null,"Ausgabewert 25","ServicePresets.125","###INDEX:ServicePresets.###MNR.125:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW24]{r}"]
[41,"DD 190",null,"Ausgabewert 26","ServicePresets.126","###INDEX:ServicePresets.###MNR.126:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW25]{r}"]
[41,"DD 192",null,"Ausgabewert 27","ServicePresets.127","###INDEX:ServicePresets.###MNR.127:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW26]{r}"]
[41,"DD 194",null,"Ausgabewert 28","ServicePresets.128","###INDEX:ServicePresets.###MNR.128:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW27]{r}"]
[41,"DD 196",null,"Ausgabewert 29","ServicePresets.129","###INDEX:ServicePresets.###MNR.129:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW28]{r}"]
[41,"DD 198",null,"Ausgabewert 30","ServicePresets.130","###INDEX:ServicePresets.###MNR.130:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW29]{r}"]
[41,"DD 200",null,"Ausgabewert 31","ServicePresets.131","###INDEX:ServicePresets.###MNR.131:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW30]{r}"]
[41,"DD 202",null,"Ausgabewert 32","ServicePresets.132","###INDEX:ServicePresets.###MNR.132:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW31]{r}"]
[41,"DD 204",null,"Ausgabewert 33","ServicePresets.133","###INDEX:ServicePresets.###MNR.133:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW32]{r}"]
[41,"DD 206",null,"Ausgabewert 34","ServicePresets.134","###INDEX:ServicePresets.###MNR.134:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW33]{r}"]
[41,"DD 208",null,"Ausgabewert 35","ServicePresets.135","###INDEX:ServicePresets.###MNR.135:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW34]{r}"]
[41,"DD 210",null,"Ausgabewert 36","ServicePresets.136","###INDEX:ServicePresets.###MNR.136:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW35]{r}"]
[41,"DD 212",null,"Ausgabewert 37","ServicePresets.137","###INDEX:ServicePresets.###MNR.137:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW36]{r}"]
[41,"DD 214",null,"Ausgabewert 38","ServicePresets.138","###INDEX:ServicePresets.###MNR.138:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW37]{r}"]
[41,"DD 216",null,"Ausgabewert 39","ServicePresets.139","###INDEX:ServicePresets.###MNR.139:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW38]{r}"]
[41,"DD 218",null,"Ausgabewert 40","ServicePresets.140","###INDEX:ServicePresets.###MNR.140:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW39]{r}"]
[41,"DD 220",null,"Ausgabewert 41","ServicePresets.141","###INDEX:ServicePresets.###MNR.141:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW40]{r}"]
[41,"DD 222",null,"Ausgabewert 42","ServicePresets.142","###INDEX:ServicePresets.###MNR.142:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW41]{r}"]
[41,"DD 224",null,"Ausgabewert 43","ServicePresets.143","###INDEX:ServicePresets.###MNR.143:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW42]{r}"]
[41,"DD 226",null,"Ausgabewert 44","ServicePresets.144","###INDEX:ServicePresets.###MNR.144:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW43]{r}"]
[41,"DD 228",null,"Ausgabewert 45","ServicePresets.145","###INDEX:ServicePresets.###MNR.145:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW44]{r}"]
[41,"DD 230",null,"Ausgabewert 46","ServicePresets.146","###INDEX:ServicePresets.###MNR.146:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW45]{r}"]
[41,"DD 232",null,"Ausgabewert 47","ServicePresets.147","###INDEX:ServicePresets.###MNR.147:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW46]{r}"]
[41,"DD 234",null,"Ausgabewert 48","ServicePresets.148","###INDEX:ServicePresets.###MNR.148:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW47]{r}"]
[41,"DD 236",null,"Ausgabewert 49","ServicePresets.149","###INDEX:ServicePresets.###MNR.149:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW48]{r}"]
[41,"DD 238",null,"Ausgabewert 50","ServicePresets.150","###INDEX:ServicePresets.###MNR.150:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW49]{r}"]
[41,"DD 240",null,"Ausgabewert 51","ServicePresets.151","###INDEX:ServicePresets.###MNR.151:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW50]{r}"]
[41,"DD 242",null,"Ausgabewert 52","ServicePresets.152","###INDEX:ServicePresets.###MNR.152:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW51]{r}"]
[41,"DD 244",null,"Ausgabewert 53","ServicePresets.153","###INDEX:ServicePresets.###MNR.153:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW52]{r}"]
[41,"DD 246",null,"Ausgabewert 54","ServicePresets.154","###INDEX:ServicePresets.###MNR.154:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW53]{r}"]
[41,"DD 248",null,"Ausgabewert 55","ServicePresets.155","###INDEX:ServicePresets.###MNR.155:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW54]{r}"]
[41,"DD 250",null,"Ausgabewert 56","ServicePresets.156","###INDEX:ServicePresets.###MNR.156:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW55]{r}"]
[41,"DD 252",null,"Ausgabewert 57","ServicePresets.157","###INDEX:ServicePresets.###MNR.157:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW56]{r}"]
[41,"DD 254",null,"Ausgabewert 58","ServicePresets.158","###INDEX:ServicePresets.###MNR.158:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW57]{r}"]
[41,"DD 256",null,"Ausgabewert 59","ServicePresets.159","###INDEX:ServicePresets.###MNR.159:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW58]{r}"]
[41,"DD 258",null,"Ausgabewert 60","ServicePresets.160","###INDEX:ServicePresets.###MNR.160:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW59]{r}"]
[41,"DD 260",null,"Ausgabewert 61","ServicePresets.161","###INDEX:ServicePresets.###MNR.161:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW60]{r}"]
[41,"DD 262",null,"Ausgabewert 62","ServicePresets.162","###INDEX:ServicePresets.###MNR.162:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW61]{r}"]
[41,"DD 264",null,"Ausgabewert 63","ServicePresets.163","###INDEX:ServicePresets.###MNR.163:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW62]{r}"]
[41,"DD 266",null,"Ausgabewert 64","ServicePresets.164","###INDEX:ServicePresets.###MNR.164:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output>[DW63]{r}"]
[41,"DW 270 - 271","32 Schalter"]
[41,"DW 270","Bit 0","Schalter 1","ServicePresets.201","###INDEX:ServicePresets.###MNR.201:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_schalter1>[W]{r}"]
[41,null,"Bit 1","Schalter 2","ServicePresets.202","###INDEX:ServicePresets.###MNR.202:INDEX"]
[41,null,"Bit 2","Schalter 3","ServicePresets.203","###INDEX:ServicePresets.###MNR.203:INDEX"]
[41,null,"Bit 3","Schalter 4","ServicePresets.204","###INDEX:ServicePresets.###MNR.204:INDEX"]
[41,null,"Bit 4","Schalter 5","ServicePresets.205","###INDEX:ServicePresets.###MNR.205:INDEX"]
[41,null,"Bit 5","Schalter 6","ServicePresets.206","###INDEX:ServicePresets.###MNR.206:INDEX"]
[41,null,"Bit 6","Schalter 7","ServicePresets.207","###INDEX:ServicePresets.###MNR.207:INDEX"]
[41,null,"Bit 7","Schalter 8","ServicePresets.208","###INDEX:ServicePresets.###MNR.208:INDEX"]
[41,null,"Bit 8","Schalter 9","ServicePresets.209","###INDEX:ServicePresets.###MNR.209:INDEX"]
[41,null,"Bit 9","Schalter 10","ServicePresets.210","###INDEX:ServicePresets.###MNR.210:INDEX"]
[41,null,"Bit 10","Schalter 11","ServicePresets.211","###INDEX:ServicePresets.###MNR.211:INDEX"]
[41,null,"Bit 11","Schalter 12","ServicePresets.212","###INDEX:ServicePresets.###MNR.212:INDEX"]
[41,null,"Bit 12","Schalter 13","ServicePresets.213","###INDEX:ServicePresets.###MNR.213:INDEX"]
[41,null,"Bit 13","Schalter 14","ServicePresets.214","###INDEX:ServicePresets.###MNR.214:INDEX"]
[41,null,"Bit 14","Schalter 15","ServicePresets.215","###INDEX:ServicePresets.###MNR.215:INDEX"]
[41,null,"Bit 15","Schalter 16","ServicePresets.216","###INDEX:ServicePresets.###MNR.216:INDEX"]
[41,"DW 271","Bit 0","Schalter 17","ServicePresets.217","###INDEX:ServicePresets.###MNR.217:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_schalter2>[W]{r}"]
[41,null,"Bit 1","Schalter 18","ServicePresets.218","###INDEX:ServicePresets.###MNR.218:INDEX"]
[41,null,"Bit 2","Schalter 19","ServicePresets.219","###INDEX:ServicePresets.###MNR.219:INDEX"]
[41,null,"Bit 3","Schalter 20","ServicePresets.220","###INDEX:ServicePresets.###MNR.220:INDEX"]
[41,null,"Bit 4","Schalter 21","ServicePresets.221","###INDEX:ServicePresets.###MNR.221:INDEX"]
[41,null,"Bit 5","Schalter 22","ServicePresets.222","###INDEX:ServicePresets.###MNR.222:INDEX"]
[41,null,"Bit 6","Schalter 23","ServicePresets.223","###INDEX:ServicePresets.###MNR.223:INDEX"]
[41,null,"Bit 7","Schalter 24","ServicePresets.224","###INDEX:ServicePresets.###MNR.224:INDEX"]
[41,null,"Bit 8","Schalter 25","ServicePresets.225","###INDEX:ServicePresets.###MNR.225:INDEX"]
[41,null,"Bit 9","Schalter 26","ServicePresets.226","###INDEX:ServicePresets.###MNR.226:INDEX"]
[41,null,"Bit 10","Schalter 27","ServicePresets.227","###INDEX:ServicePresets.###MNR.227:INDEX"]
[41,null,"Bit 11","Schalter 28","ServicePresets.228","###INDEX:ServicePresets.###MNR.228:INDEX"]
[41,null,"Bit 12","Schalter 29","ServicePresets.229","###INDEX:ServicePresets.###MNR.229:INDEX"]
[41,null,"Bit 13","Schalter 30","ServicePresets.230","###INDEX:ServicePresets.###MNR.230:INDEX"]
[41,null,"Bit 14","Schalter 31","ServicePresets.231","###INDEX:ServicePresets.###MNR.231:INDEX"]
[41,null,"Bit 15","Schalter 32","ServicePresets.232","###INDEX:ServicePresets.###MNR.232:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41"]
["###IF MITZUSATZSERVICEPRESETS###21","DB ###ADDR:340+1[MNR]:ADDR"]
["###IF MITZUSATZSERVICEPRESETS###41"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 310 - 436","64 Eingabewerte"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 310",null,"Eingabewert 65","ServicePresets.301","###INDEX:ServicePresets.###MNR.301:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW0]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 312 ",null,"Eingabewert 66","ServicePresets.302","###INDEX:ServicePresets.###MNR.302:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW1]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 314",null,"Eingabewert 67","ServicePresets.303","###INDEX:ServicePresets.###MNR.303:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW2]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 316",null,"Eingabewert 68","ServicePresets.304","###INDEX:ServicePresets.###MNR.304:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW3]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 318",null,"Eingabewert 69","ServicePresets.305","###INDEX:ServicePresets.###MNR.305:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW4]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 320",null,"Eingabewert 70","ServicePresets.306","###INDEX:ServicePresets.###MNR.306:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW5]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 322",null,"Eingabewert 71","ServicePresets.307","###INDEX:ServicePresets.###MNR.307:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW6]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 324",null,"Eingabewert 72","ServicePresets.308","###INDEX:ServicePresets.###MNR.308:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW7]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 326",null,"Eingabewert 73","ServicePresets.309","###INDEX:ServicePresets.###MNR.309:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW8]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 328",null,"Eingabewert 74","ServicePresets.310","###INDEX:ServicePresets.###MNR.310:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW9]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 330",null,"Eingabewert 75","ServicePresets.311","###INDEX:ServicePresets.###MNR.311:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW10]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 332",null,"Eingabewert 76","ServicePresets.312","###INDEX:ServicePresets.###MNR.312:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW11]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 334",null,"Eingabewert 77","ServicePresets.313","###INDEX:ServicePresets.###MNR.313:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW12]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 336",null,"Eingabewert 78","ServicePresets.314","###INDEX:ServicePresets.###MNR.314:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW13]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 338",null,"Eingabewert 79","ServicePresets.315","###INDEX:ServicePresets.###MNR.315:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW14]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 340",null,"Eingabewert 80","ServicePresets.316","###INDEX:ServicePresets.###MNR.316:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW15]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 342",null,"Eingabewert 81","ServicePresets.317","###INDEX:ServicePresets.###MNR.317:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW16]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 344",null,"Eingabewert 82","ServicePresets.318","###INDEX:ServicePresets.###MNR.318:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW17]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 346",null,"Eingabewert 83","ServicePresets.319","###INDEX:ServicePresets.###MNR.319:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW18]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 348",null,"Eingabewert 84","ServicePresets.320","###INDEX:ServicePresets.###MNR.320:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW19]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 350",null,"Eingabewert 85","ServicePresets.321","###INDEX:ServicePresets.###MNR.321:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW20]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 352",null,"Eingabewert 86","ServicePresets.322","###INDEX:ServicePresets.###MNR.322:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW21]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 354",null,"Eingabewert 87","ServicePresets.323","###INDEX:ServicePresets.###MNR.323:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW22]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 356",null,"Eingabewert 88","ServicePresets.324","###INDEX:ServicePresets.###MNR.324:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW23]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 358",null,"Eingabewert 89","ServicePresets.325","###INDEX:ServicePresets.###MNR.325:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW24]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 360",null,"Eingabewert 90","ServicePresets.326","###INDEX:ServicePresets.###MNR.326:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW25]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 362",null,"Eingabewert 91","ServicePresets.327","###INDEX:ServicePresets.###MNR.327:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW26]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 364",null,"Eingabewert 92","ServicePresets.328","###INDEX:ServicePresets.###MNR.328:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW27]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 366",null,"Eingabewert 93","ServicePresets.329","###INDEX:ServicePresets.###MNR.329:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_inpu2>[DW28]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 368",null,"Eingabewert 94","ServicePresets.330","###INDEX:ServicePresets.###MNR.330:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW29]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 370",null,"Eingabewert 95","ServicePresets.331","###INDEX:ServicePresets.###MNR.331:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW30]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 372",null,"Eingabewert 96","ServicePresets.332","###INDEX:ServicePresets.###MNR.332:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW31]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 374",null,"Eingabewert 97","ServicePresets.333","###INDEX:ServicePresets.###MNR.333:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW32]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 376",null,"Eingabewert 98","ServicePresets.334","###INDEX:ServicePresets.###MNR.334:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW33]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 378",null,"Eingabewert 99","ServicePresets.335","###INDEX:ServicePresets.###MNR.335:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW34]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 380",null,"Eingabewert 100","ServicePresets.336","###INDEX:ServicePresets.###MNR.336:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW35]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 382",null,"Eingabewert 101","ServicePresets.337","###INDEX:ServicePresets.###MNR.337:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW36]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 384",null,"Eingabewert 102","ServicePresets.338","###INDEX:ServicePresets.###MNR.338:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW37]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 386",null,"Eingabewert 103","ServicePresets.339","###INDEX:ServicePresets.###MNR.339:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW38]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 388",null,"Eingabewert 104","ServicePresets.340","###INDEX:ServicePresets.###MNR.340:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW39]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 390",null,"Eingabewert 105","ServicePresets.341","###INDEX:ServicePresets.###MNR.341:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW40]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 392",null,"Eingabewert 106","ServicePresets.342","###INDEX:ServicePresets.###MNR.342:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW41]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 394",null,"Eingabewert 107","ServicePresets.343","###INDEX:ServicePresets.###MNR.343:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW42]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 396",null,"Eingabewert 108","ServicePresets.344","###INDEX:ServicePresets.###MNR.344:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW43]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 398",null,"Eingabewert 109","ServicePresets.345","###INDEX:ServicePresets.###MNR.345:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW44]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 400",null,"Eingabewert 110","ServicePresets.346","###INDEX:ServicePresets.###MNR.346:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW45]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 402",null,"Eingabewert 111","ServicePresets.347","###INDEX:ServicePresets.###MNR.347:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW46]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 404",null,"Eingabewert 112","ServicePresets.348","###INDEX:ServicePresets.###MNR.348:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW47]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 406",null,"Eingabewert 113","ServicePresets.349","###INDEX:ServicePresets.###MNR.349:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW48]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 408",null,"Eingabewert 114","ServicePresets.350","###INDEX:ServicePresets.###MNR.350:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW49]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 410",null,"Eingabewert 115","ServicePresets.351","###INDEX:ServicePresets.###MNR.351:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW50]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 412",null,"Eingabewert 116","ServicePresets.352","###INDEX:ServicePresets.###MNR.352:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW51]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 414",null,"Eingabewert 117","ServicePresets.353","###INDEX:ServicePresets.###MNR.353:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW52]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 416",null,"Eingabewert 118","ServicePresets.354","###INDEX:ServicePresets.###MNR.354:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW53]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 418",null,"Eingabewert 119","ServicePresets.355","###INDEX:ServicePresets.###MNR.355:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW54]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 420",null,"Eingabewert 120","ServicePresets.356","###INDEX:ServicePresets.###MNR.356:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW55]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 422",null,"Eingabewert 121","ServicePresets.357","###INDEX:ServicePresets.###MNR.357:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW56]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 424",null,"Eingabewert 122","ServicePresets.358","###INDEX:ServicePresets.###MNR.358:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW57]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 426",null,"Eingabewert 123","ServicePresets.359","###INDEX:ServicePresets.###MNR.359:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW58]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 428",null,"Eingabewert 124","ServicePresets.360","###INDEX:ServicePresets.###MNR.360:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW59]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 430",null,"Eingabewert 125","ServicePresets.361","###INDEX:ServicePresets.###MNR.361:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW60]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 432",null,"Eingabewert 126","ServicePresets.362","###INDEX:ServicePresets.###MNR.362:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW61]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 434",null,"Eingabewert 127","ServicePresets.363","###INDEX:ServicePresets.###MNR.363:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW62]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 436",null,"Eingabewert 128","ServicePresets.364","###INDEX:ServicePresets.###MNR.364:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_input2>[DW63]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 440 - 566","64 Ausgabewerte"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 440",null,"Ausgabewert 65","ServicePresets.401","###INDEX:ServicePresets.###MNR.401:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW0]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 442",null,"Ausgabewert 66","ServicePresets.402","###INDEX:ServicePresets.###MNR.402:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW1]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 444",null,"Ausgabewert 67","ServicePresets.403","###INDEX:ServicePresets.###MNR.403:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW2]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 446",null,"Ausgabewert 68","ServicePresets.404","###INDEX:ServicePresets.###MNR.404:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW3]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 448",null,"Ausgabewert 69","ServicePresets.405","###INDEX:ServicePresets.###MNR.405:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW4]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 450",null,"Ausgabewert 70","ServicePresets.406","###INDEX:ServicePresets.###MNR.406:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW5]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 452",null,"Ausgabewert 71","ServicePresets.407","###INDEX:ServicePresets.###MNR.407:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW6]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 454",null,"Ausgabewert 72","ServicePresets.408","###INDEX:ServicePresets.###MNR.408:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW7]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 456",null,"Ausgabewert 73","ServicePresets.409","###INDEX:ServicePresets.###MNR.409:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW8]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 458",null,"Ausgabewert 74","ServicePresets.410","###INDEX:ServicePresets.###MNR.410:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW9]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 460",null,"Ausgabewert 75","ServicePresets.411","###INDEX:ServicePresets.###MNR.411:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW10]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 462",null,"Ausgabewert 76","ServicePresets.412","###INDEX:ServicePresets.###MNR.412:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW11]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 464",null,"Ausgabewert 77","ServicePresets.413","###INDEX:ServicePresets.###MNR.413:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW12]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 466",null,"Ausgabewert 78","ServicePresets.414","###INDEX:ServicePresets.###MNR.414:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW13]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 468",null,"Ausgabewert 79","ServicePresets.415","###INDEX:ServicePresets.###MNR.415:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW14]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 470",null,"Ausgabewert 80","ServicePresets.416","###INDEX:ServicePresets.###MNR.416:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW15]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 472",null,"Ausgabewert 81","ServicePresets.417","###INDEX:ServicePresets.###MNR.417:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW16]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 474",null,"Ausgabewert 82","ServicePresets.418","###INDEX:ServicePresets.###MNR.418:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW17]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 476",null,"Ausgabewert 83","ServicePresets.419","###INDEX:ServicePresets.###MNR.419:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW18]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 478",null,"Ausgabewert 84","ServicePresets.420","###INDEX:ServicePresets.###MNR.420:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW19]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 480",null,"Ausgabewert 85","ServicePresets.421","###INDEX:ServicePresets.###MNR.421:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW20]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 482",null,"Ausgabewert 86","ServicePresets.422","###INDEX:ServicePresets.###MNR.422:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW21]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 484",null,"Ausgabewert 87","ServicePresets.423","###INDEX:ServicePresets.###MNR.423:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW22]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 486",null,"Ausgabewert 88","ServicePresets.424","###INDEX:ServicePresets.###MNR.424:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW23]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 488",null,"Ausgabewert 89","ServicePresets.425","###INDEX:ServicePresets.###MNR.425:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW24]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 490",null,"Ausgabewert 90","ServicePresets.426","###INDEX:ServicePresets.###MNR.426:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW25]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 492",null,"Ausgabewert 91","ServicePresets.427","###INDEX:ServicePresets.###MNR.427:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW26]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 494",null,"Ausgabewert 92","ServicePresets.428","###INDEX:ServicePresets.###MNR.428:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW27]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 496",null,"Ausgabewert 93","ServicePresets.429","###INDEX:ServicePresets.###MNR.429:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW28]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 498",null,"Ausgabewert 94","ServicePresets.430","###INDEX:ServicePresets.###MNR.430:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW29]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 500",null,"Ausgabewert 95","ServicePresets.431","###INDEX:ServicePresets.###MNR.431:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW30]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 502",null,"Ausgabewert 96","ServicePresets.432","###INDEX:ServicePresets.###MNR.432:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW31]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 504",null,"Ausgabewert 97","ServicePresets.433","###INDEX:ServicePresets.###MNR.433:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW32]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 506",null,"Ausgabewert 98","ServicePresets.434","###INDEX:ServicePresets.###MNR.434:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW33]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 508",null,"Ausgabewert 99","ServicePresets.435","###INDEX:ServicePresets.###MNR.435:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW34]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 510",null,"Ausgabewert 100","ServicePresets.436","###INDEX:ServicePresets.###MNR.436:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW35]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 512",null,"Ausgabewert 101","ServicePresets.437","###INDEX:ServicePresets.###MNR.437:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW36]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 514",null,"Ausgabewert 102","ServicePresets.438","###INDEX:ServicePresets.###MNR.438:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW37]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 516",null,"Ausgabewert 103","ServicePresets.439","###INDEX:ServicePresets.###MNR.439:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW38]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 518",null,"Ausgabewert 104","ServicePresets.440","###INDEX:ServicePresets.###MNR.440:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW39]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 520",null,"Ausgabewert 105","ServicePresets.441","###INDEX:ServicePresets.###MNR.441:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW40]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 522",null,"Ausgabewert 106","ServicePresets.442","###INDEX:ServicePresets.###MNR.442:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW41]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 524",null,"Ausgabewert 107","ServicePresets.443","###INDEX:ServicePresets.###MNR.443:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW42]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 526",null,"Ausgabewert 108","ServicePresets.444","###INDEX:ServicePresets.###MNR.444:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW43]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 528",null,"Ausgabewert 109","ServicePresets.445","###INDEX:ServicePresets.###MNR.445:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW44]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 530",null,"Ausgabewert 110","ServicePresets.446","###INDEX:ServicePresets.###MNR.446:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW45]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 532",null,"Ausgabewert 111","ServicePresets.447","###INDEX:ServicePresets.###MNR.447:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW46]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 534",null,"Ausgabewert 112","ServicePresets.448","###INDEX:ServicePresets.###MNR.448:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW47]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 536",null,"Ausgabewert 113","ServicePresets.449","###INDEX:ServicePresets.###MNR.449:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW48]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 538",null,"Ausgabewert 114","ServicePresets.450","###INDEX:ServicePresets.###MNR.450:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW49]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 540",null,"Ausgabewert 115","ServicePresets.451","###INDEX:ServicePresets.###MNR.451:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW50]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 542",null,"Ausgabewert 116","ServicePresets.452","###INDEX:ServicePresets.###MNR.452:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW51]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 544",null,"Ausgabewert 117","ServicePresets.453","###INDEX:ServicePresets.###MNR.453:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW52]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 546",null,"Ausgabewert 118","ServicePresets.454","###INDEX:ServicePresets.###MNR.454:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW53]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 548",null,"Ausgabewert 119","ServicePresets.455","###INDEX:ServicePresets.###MNR.455:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW54]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 550",null,"Ausgabewert 120","ServicePresets.456","###INDEX:ServicePresets.###MNR.456:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW55]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 552",null,"Ausgabewert 121","ServicePresets.457","###INDEX:ServicePresets.###MNR.457:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW56]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 554",null,"Ausgabewert 122","ServicePresets.458","###INDEX:ServicePresets.###MNR.458:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW57]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 556",null,"Ausgabewert 123","ServicePresets.459","###INDEX:ServicePresets.###MNR.459:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW58]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 558",null,"Ausgabewert 124","ServicePresets.460","###INDEX:ServicePresets.###MNR.460:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW59]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 560",null,"Ausgabewert 125","ServicePresets.461","###INDEX:ServicePresets.###MNR.461:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW60]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 562",null,"Ausgabewert 126","ServicePresets.462","###INDEX:ServicePresets.###MNR.462:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW61]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 564",null,"Ausgabewert 127","ServicePresets.463","###INDEX:ServicePresets.###MNR.463:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW62]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DD 566",null,"Ausgabewert 128","ServicePresets.464","###INDEX:ServicePresets.###MNR.464:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_output2>[DW63]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41","DW 570 - 571","32 Schalter"]
["###IF MITZUSATZSERVICEPRESETS###41","DW 570","Bit 0","Schalter 33","ServicePresets.501","###INDEX:ServicePresets.###MNR.501:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_schalter21>[W]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 1","Schalter 34","ServicePresets.502","###INDEX:ServicePresets.###MNR.502:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 2","Schalter 35","ServicePresets.503","###INDEX:ServicePresets.###MNR.503:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 3","Schalter 36","ServicePresets.504","###INDEX:ServicePresets.###MNR.504:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 4","Schalter 37","ServicePresets.505","###INDEX:ServicePresets.###MNR.505:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 5","Schalter 38","ServicePresets.506","###INDEX:ServicePresets.###MNR.506:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 6","Schalter 39","ServicePresets.507","###INDEX:ServicePresets.###MNR.507:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 7","Schalter 40","ServicePresets.508","###INDEX:ServicePresets.###MNR.508:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 8","Schalter 41","ServicePresets.509","###INDEX:ServicePresets.###MNR.509:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 9","Schalter 42","ServicePresets.510","###INDEX:ServicePresets.###MNR.510:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 10","Schalter 43","ServicePresets.511","###INDEX:ServicePresets.###MNR.511:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 11","Schalter 44","ServicePresets.512","###INDEX:ServicePresets.###MNR.512:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 12","Schalter 45","ServicePresets.513","###INDEX:ServicePresets.###MNR.513:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 13","Schalter 46","ServicePresets.514","###INDEX:ServicePresets.###MNR.514:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 14","Schalter 47","ServicePresets.515","###INDEX:ServicePresets.###MNR.515:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 15","Schalter 48","ServicePresets.516","###INDEX:ServicePresets.###MNR.516:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41","DW 571","Bit 0","Schalter 49","ServicePresets.517","###INDEX:ServicePresets.###MNR.517:INDEX","Ch1.###MNR_T_sp<.m###MNR_sp_schalter22>[W]{r}"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 1","Schalter 50","ServicePresets.518","###INDEX:ServicePresets.###MNR.518:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 2","Schalter 51","ServicePresets.519","###INDEX:ServicePresets.###MNR.519:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 3","Schalter 52","ServicePresets.520","###INDEX:ServicePresets.###MNR.520:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 4","Schalter 53","ServicePresets.521","###INDEX:ServicePresets.###MNR.521:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 5","Schalter 54","ServicePresets.522","###INDEX:ServicePresets.###MNR.522:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 6","Schalter 55","ServicePresets.523","###INDEX:ServicePresets.###MNR.523:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 7","Schalter 56","ServicePresets.524","###INDEX:ServicePresets.###MNR.524:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 8","Schalter 57","ServicePresets.525","###INDEX:ServicePresets.###MNR.525:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 9","Schalter 58","ServicePresets.526","###INDEX:ServicePresets.###MNR.526:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 10","Schalter 59","ServicePresets.527","###INDEX:ServicePresets.###MNR.527:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 11","Schalter 60","ServicePresets.528","###INDEX:ServicePresets.###MNR.528:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 12","Schalter 61","ServicePresets.529","###INDEX:ServicePresets.###MNR.529:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 13","Schalter 62","ServicePresets.530","###INDEX:ServicePresets.###MNR.530:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 14","Schalter 63","ServicePresets.531","###INDEX:ServicePresets.###MNR.531:INDEX"]
["###IF MITZUSATZSERVICEPRESETS###41",null,"Bit 15","Schalter 64","ServicePresets.532","###INDEX:ServicePresets.###MNR.532:INDEX"]

{"sheet":"CamExt","index":77,"n_rows":207,"n_cols":7,"rows_kept":207,"flags":["formulas_cached_only"]}
["CamExt","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 350","Cams 1st Machine "]
[41,"DB 351-354","Cams Machine 2-5"]
[1,"###MAIN"]
[1,"DB 350-354 Cams"]
[41,"DW 0","Bit 0","Cams changed",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_aend>[B]{w}"]
[]
[]
[41,"DW 10-49",null,"Offset part 1-40",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_offset>[W0-39]{r}"]
[41,"DW 50-89",null,"Number of setpints part 1-40",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzahl>[W0-39]{r}"]
[41,"DW 90",null,"Cam position part 1",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_stell_1>[W]{r}"]
[41,"DW 91-129",null,"Cam position part 2-40",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_stell_2-40>[W]{r}"]
[41,"DW 130","Bit 0-15","Cam 1-16 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W0]{r}"]
[41,"DW 131","Bit 0-15","Cam 17-32 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W1]{r}"]
[41,"DW 132","Bit 0-15","Cam 33-48 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W2]{r}"]
[41,"DW 133","Bit 0-15","Cam 49-64 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W3]{r}"]
[41,"DW 134","Bit 0-15","Cam 65-80 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W4]{r}"]
[41,"DW 135","Bit 0-15","Cam 81-96 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W5]{r}"]
[41,"DW 136","Bit 0-15","Cam 97-112 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W6]{r}"]
[41,"DW 137","Bit 0-15","Cam 113-128 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W7]{r}"]
[41,"DW 138","Bit 0-15","Cam 129-144 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W8]{r}"]
[41,"DW 139","Bit 0-15","Cam 145-160 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W9]{r}"]
[41,"DW 140","Bit 0-15","Cam 161-176 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W10]{r}"]
[41,"DW 141","Bit 0-5","Cam 177-181 exist",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv_anzeige>[W11]{r}"]
[41]
[41,"DW 170",null,"Cam 1 Start","CamExt.###MNR.101","###INDEX:CamExt.###MNR.101:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W0]{r}"]
[41,"DW 171",null,"Cam 1 End",null,null,"Ch1.###MNR_T_kurven<.m###MNR_kurv>[W1]{r}"]
[41,"DW 172",null,"Cam 2 Start","CamExt.###MNR.102","###INDEX:CamExt.###MNR.102:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W2]{r}"]
[41,"DW 174",null,"Cam 3 Start","CamExt.###MNR.103","###INDEX:CamExt.###MNR.103:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W4]{r}"]
[41,"DW 176",null,"Cam 4 Start","CamExt.###MNR.104","###INDEX:CamExt.###MNR.104:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W6]{r}"]
[41,"DW 178",null,"Cam 5 Start","CamExt.###MNR.105","###INDEX:CamExt.###MNR.105:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W8]{r}"]
[41,"DW 180",null,"Cam 6 Start","CamExt.###MNR.106","###INDEX:CamExt.###MNR.106:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W10]{r}"]
[41,"DW 182",null,"Cam 7 Start","CamExt.###MNR.107","###INDEX:CamExt.###MNR.107:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W12]{r}"]
[41,"DW 184",null,"Cam 8 Start","CamExt.###MNR.108","###INDEX:CamExt.###MNR.108:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W14]{r}"]
[41,"DW 186",null,"Cam 9 Start","CamExt.###MNR.109","###INDEX:CamExt.###MNR.109:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W16]{r}"]
[41,"DW 188",null,"Cam 10 Start","CamExt.###MNR.110","###INDEX:CamExt.###MNR.110:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W18]{r}"]
[41,"DW 190",null,"Cam 11 Start","CamExt.###MNR.111","###INDEX:CamExt.###MNR.111:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W20]{r}"]
[41,"DW 192",null,"Cam 12 Start","CamExt.###MNR.112","###INDEX:CamExt.###MNR.112:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W22]{r}"]
[41,"DW 194",null,"Cam 13 Start","CamExt.###MNR.113","###INDEX:CamExt.###MNR.113:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W24]{r}"]
[41,"DW 196",null,"Cam 14 Start","CamExt.###MNR.114","###INDEX:CamExt.###MNR.114:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W26]{r}"]
[41,"DW 198",null,"Cam 15 Start","CamExt.###MNR.115","###INDEX:CamExt.###MNR.115:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W28]{r}"]
[41,"DW 200",null,"Cam 16 Start","CamExt.###MNR.116","###INDEX:CamExt.###MNR.116:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W30]{r}"]
[41,"DW 202",null,"Cam 17 Start","CamExt.###MNR.117","###INDEX:CamExt.###MNR.117:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W32]{r}"]
[41,"DW 204",null,"Cam 18 Start","CamExt.###MNR.118","###INDEX:CamExt.###MNR.118:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W34]{r}"]
[41,"DW 206",null,"Cam 19 Start","CamExt.###MNR.119","###INDEX:CamExt.###MNR.119:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W36]{r}"]
[41,"DW 208",null,"Cam 20 Start","CamExt.###MNR.120","###INDEX:CamExt.###MNR.120:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W38]{r}"]
[41,"DW 210",null,"Cam 21 Start","CamExt.###MNR.121","###INDEX:CamExt.###MNR.121:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W40]{r}"]
[41,"DW 212",null,"Cam 22 Start","CamExt.###MNR.122","###INDEX:CamExt.###MNR.122:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W42]{r}"]
[41,"DW 214",null,"Cam 23 Start","CamExt.###MNR.123","###INDEX:CamExt.###MNR.123:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W44]{r}"]
[41,"DW 216",null,"Cam 24 Start","CamExt.###MNR.124","###INDEX:CamExt.###MNR.124:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W46]{r}"]
[41,"DW 218",null,"Cam 25 Start","CamExt.###MNR.125","###INDEX:CamExt.###MNR.125:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W48]{r}"]
[41,"DW 220",null,"Cam 26 Start","CamExt.###MNR.126","###INDEX:CamExt.###MNR.126:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W50]{r}"]
[41,"DW 222",null,"Cam 27 Start","CamExt.###MNR.127","###INDEX:CamExt.###MNR.127:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W52]{r}"]
[41,"DW 224",null,"Cam 28 Start","CamExt.###MNR.128","###INDEX:CamExt.###MNR.128:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W54]{r}"]
[41,"DW 226",null,"Cam 29 Start","CamExt.###MNR.129","###INDEX:CamExt.###MNR.129:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W56]{r}"]
[41,"DW 228",null,"Cam 30 Start","CamExt.###MNR.130","###INDEX:CamExt.###MNR.130:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W58]{r}"]
[41,"DW 230",null,"Cam 31 Start","CamExt.###MNR.131","###INDEX:CamExt.###MNR.131:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W60]{r}"]
[41,"DW 232",null,"Cam 32 Start","CamExt.###MNR.132","###INDEX:CamExt.###MNR.132:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W62]{r}"]
[41,"DW 234",null,"Cam 33 Start","CamExt.###MNR.133","###INDEX:CamExt.###MNR.133:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W64]{r}"]
[41,"DW 236",null,"Cam 34 Start","CamExt.###MNR.134","###INDEX:CamExt.###MNR.134:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W66]{r}"]
[41,"DW 238",null,"Cam 35 Start","CamExt.###MNR.135","###INDEX:CamExt.###MNR.135:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W68]{r}"]
[41,"DW 240",null,"Cam 36 Start","CamExt.###MNR.136","###INDEX:CamExt.###MNR.136:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W70]{r}"]
[41,"DW 242",null,"Cam 37 Start","CamExt.###MNR.137","###INDEX:CamExt.###MNR.137:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W72]{r}"]
[41,"DW 244",null,"Cam 38 Start","CamExt.###MNR.138","###INDEX:CamExt.###MNR.138:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W74]{r}"]
[41,"DW 246",null,"Cam 39 Start","CamExt.###MNR.139","###INDEX:CamExt.###MNR.139:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W76]{r}"]
[41,"DW 248",null,"Cam 40 Start","CamExt.###MNR.140","###INDEX:CamExt.###MNR.140:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W78]{r}"]
[41,"DW 250",null,"Cam 41 Start","CamExt.###MNR.141","###INDEX:CamExt.###MNR.141:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W80]{r}"]
[41,"DW 252",null,"Cam 42 Start","CamExt.###MNR.142","###INDEX:CamExt.###MNR.142:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W82]{r}"]
[41,"DW 254",null,"Cam 43 Start","CamExt.###MNR.143","###INDEX:CamExt.###MNR.143:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W84]{r}"]
[41,"DW 256",null,"Cam 44 Start","CamExt.###MNR.144","###INDEX:CamExt.###MNR.144:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W86]{r}"]
[41,"DW 258",null,"Cam 45 Start","CamExt.###MNR.145","###INDEX:CamExt.###MNR.145:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W88]{r}"]
[41,"DW 260",null,"Cam 46 Start","CamExt.###MNR.146","###INDEX:CamExt.###MNR.146:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W90]{r}"]
[41,"DW 262",null,"Cam 47 Start","CamExt.###MNR.147","###INDEX:CamExt.###MNR.147:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W92]{r}"]
[41,"DW 264",null,"Cam 48 Start","CamExt.###MNR.148","###INDEX:CamExt.###MNR.148:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W94]{r}"]
[41,"DW 266",null,"Cam 49 Start","CamExt.###MNR.149","###INDEX:CamExt.###MNR.149:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W96]{r}"]
[41,"DW 268",null,"Cam 50 Start","CamExt.###MNR.150","###INDEX:CamExt.###MNR.150:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W98]{r}"]
[41,"DW 270",null,"Cam 51 Start","CamExt.###MNR.151","###INDEX:CamExt.###MNR.151:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W100]{r}"]
[41,"DW 272",null,"Cam 52 Start","CamExt.###MNR.152","###INDEX:CamExt.###MNR.152:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W102]{r}"]
[41,"DW 274",null,"Cam 53 Start","CamExt.###MNR.153","###INDEX:CamExt.###MNR.153:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W104]{r}"]
[41,"DW 276",null,"Cam 54 Start","CamExt.###MNR.154","###INDEX:CamExt.###MNR.154:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W106]{r}"]
[41,"DW 278",null,"Cam 55 Start","CamExt.###MNR.155","###INDEX:CamExt.###MNR.155:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W108]{r}"]
[41,"DW 280",null,"Cam 56 Start","CamExt.###MNR.156","###INDEX:CamExt.###MNR.156:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W110]{r}"]
[41,"DW 282",null,"Cam 57 Start","CamExt.###MNR.157","###INDEX:CamExt.###MNR.157:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W112]{r}"]
[41,"DW 284",null,"Cam 58 Start","CamExt.###MNR.158","###INDEX:CamExt.###MNR.158:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W114]{r}"]
[41,"DW 286",null,"Cam 59 Start","CamExt.###MNR.159","###INDEX:CamExt.###MNR.159:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W116]{r}"]
[41,"DW 288",null,"Cam 60 Start","CamExt.###MNR.160","###INDEX:CamExt.###MNR.160:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W118]{r}"]
[41,"DW 290",null,"Cam 61 Start","CamExt.###MNR.161","###INDEX:CamExt.###MNR.161:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W120]{r}"]
[41,"DW 292",null,"Cam 62 Start","CamExt.###MNR.162","###INDEX:CamExt.###MNR.162:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W122]{r}"]
[41,"DW 294",null,"Cam 63 Start","CamExt.###MNR.163","###INDEX:CamExt.###MNR.163:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W124]{r}"]
[41,"DW 296",null,"Cam 64 Start","CamExt.###MNR.164","###INDEX:CamExt.###MNR.164:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W126]{r}"]
[41,"DW 298",null,"Cam 65 Start","CamExt.###MNR.165","###INDEX:CamExt.###MNR.165:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W128]{r}"]
[41,"DW 300",null,"Cam 66 Start","CamExt.###MNR.166","###INDEX:CamExt.###MNR.166:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W130]{r}"]
[41,"DW 302",null,"Cam 67 Start","CamExt.###MNR.167","###INDEX:CamExt.###MNR.167:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W132]{r}"]
[41,"DW 304",null,"Cam 68 Start","CamExt.###MNR.168","###INDEX:CamExt.###MNR.168:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W134]{r}"]
[41,"DW 306",null,"Cam 69 Start","CamExt.###MNR.169","###INDEX:CamExt.###MNR.169:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W136]{r}"]
[41,"DW 308",null,"Cam 70 Start","CamExt.###MNR.170","###INDEX:CamExt.###MNR.170:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W138]{r}"]
[41,"DW 310",null,"Cam 71 Start","CamExt.###MNR.171","###INDEX:CamExt.###MNR.171:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W140]{r}"]
[41,"DW 312",null,"Cam 72 Start","CamExt.###MNR.172","###INDEX:CamExt.###MNR.172:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W142]{r}"]
[41,"DW 314",null,"Cam 73 Start","CamExt.###MNR.173","###INDEX:CamExt.###MNR.173:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W144]{r}"]
[41,"DW 316",null,"Cam 74 Start","CamExt.###MNR.174","###INDEX:CamExt.###MNR.174:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W146]{r}"]
[41,"DW 318",null,"Cam 75 Start","CamExt.###MNR.175","###INDEX:CamExt.###MNR.175:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W148]{r}"]
[41,"DW 320",null,"Cam 76 Start","CamExt.###MNR.176","###INDEX:CamExt.###MNR.176:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W150]{r}"]
[41,"DW 322",null,"Cam 77 Start","CamExt.###MNR.177","###INDEX:CamExt.###MNR.177:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W152]{r}"]
[41,"DW 324",null,"Cam 78 Start","CamExt.###MNR.178","###INDEX:CamExt.###MNR.178:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W154]{r}"]
[41,"DW 326",null,"Cam 79 Start","CamExt.###MNR.179","###INDEX:CamExt.###MNR.179:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W156]{r}"]
[41,"DW 328",null,"Cam 80 Start","CamExt.###MNR.180","###INDEX:CamExt.###MNR.180:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W158]{r}"]
[41,"DW 330",null,"Cam 81 Start","CamExt.###MNR.181","###INDEX:CamExt.###MNR.181:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W160]{r}"]
[41,"DW 332",null,"Cam 82 Start","CamExt.###MNR.182","###INDEX:CamExt.###MNR.182:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W162]{r}"]
[41,"DW 334",null,"Cam 83 Start","CamExt.###MNR.183","###INDEX:CamExt.###MNR.183:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W164]{r}"]
[41,"DW 336",null,"Cam 84 Start","CamExt.###MNR.184","###INDEX:CamExt.###MNR.184:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W166]{r}"]
[41,"DW 338",null,"Cam 85 Start","CamExt.###MNR.185","###INDEX:CamExt.###MNR.185:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W168]{r}"]
[41,"DW 340",null,"Cam 86 Start","CamExt.###MNR.186","###INDEX:CamExt.###MNR.186:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W170]{r}"]
[41,"DW 342",null,"Cam 87 Start","CamExt.###MNR.187","###INDEX:CamExt.###MNR.187:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W172]{r}"]
[41,"DW 344",null,"Cam 88 Start","CamExt.###MNR.188","###INDEX:CamExt.###MNR.188:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W174]{r}"]
[41,"DW 346",null,"Cam 89 Start","CamExt.###MNR.189","###INDEX:CamExt.###MNR.189:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W176]{r}"]
[41,"DW 348",null,"Cam 90 Start","CamExt.###MNR.190","###INDEX:CamExt.###MNR.190:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W178]{r}"]
[41,"DW 350",null,"Cam 91 Start","CamExt.###MNR.191","###INDEX:CamExt.###MNR.191:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W180]{r}"]
[41,"DW 352",null,"Cam 92 Start","CamExt.###MNR.192","###INDEX:CamExt.###MNR.192:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W182]{r}"]
[41,"DW 354",null,"Cam 93 Start","CamExt.###MNR.193","###INDEX:CamExt.###MNR.193:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W184]{r}"]
[41,"DW 356",null,"Cam 94 Start","CamExt.###MNR.194","###INDEX:CamExt.###MNR.194:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W186]{r}"]
[41,"DW 358",null,"Cam 95 Start","CamExt.###MNR.195","###INDEX:CamExt.###MNR.195:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W188]{r}"]
[41,"DW 360",null,"Cam 96 Start","CamExt.###MNR.196","###INDEX:CamExt.###MNR.196:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W190]{r}"]
[41,"DW 362",null,"Cam 97 Start","CamExt.###MNR.197","###INDEX:CamExt.###MNR.197:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W192]{r}"]
[41,"DW 364",null,"Cam 98 Start","CamExt.###MNR.198","###INDEX:CamExt.###MNR.198:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W194]{r}"]
[41,"DW 366",null,"Cam 99 Start","CamExt.###MNR.199","###INDEX:CamExt.###MNR.199:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W196]{r}"]
[41,"DW 368",null,"Cam 100 Start","CamExt.###MNR.200","###INDEX:CamExt.###MNR.200:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W198]{r}"]
[41,"DW 370",null,"Cam 101 Start","CamExt.###MNR.201","###INDEX:CamExt.###MNR.201:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W200]{r}"]
[41,"DW 372",null,"Cam 102 Start","CamExt.###MNR.202","###INDEX:CamExt.###MNR.202:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W202]{r}"]
[41,"DW 374",null,"Cam 103 Start","CamExt.###MNR.203","###INDEX:CamExt.###MNR.203:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W204]{r}"]
[41,"DW 376",null,"Cam 104 Start","CamExt.###MNR.204","###INDEX:CamExt.###MNR.204:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W206]{r}"]
[41,"DW 378",null,"Cam 105 Start","CamExt.###MNR.205","###INDEX:CamExt.###MNR.205:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W208]{r}"]
[41,"DW 380",null,"Cam 106 Start","CamExt.###MNR.206","###INDEX:CamExt.###MNR.206:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W210]{r}"]
[41,"DW 382",null,"Cam 107 Start","CamExt.###MNR.207","###INDEX:CamExt.###MNR.207:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W212]{r}"]
[41,"DW 384",null,"Cam 108 Start","CamExt.###MNR.208","###INDEX:CamExt.###MNR.208:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W214]{r}"]
[41,"DW 386",null,"Cam 109 Start","CamExt.###MNR.209","###INDEX:CamExt.###MNR.209:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W216]{r}"]
[41,"DW 388",null,"Cam 110 Start","CamExt.###MNR.210","###INDEX:CamExt.###MNR.210:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W218]{r}"]
[41,"DW 390",null,"Cam 111 Start","CamExt.###MNR.211","###INDEX:CamExt.###MNR.211:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W220]{r}"]
[41,"DW 392",null,"Cam 112 Start","CamExt.###MNR.212","###INDEX:CamExt.###MNR.212:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W222]{r}"]
[41,"DW 394",null,"Cam 113 Start","CamExt.###MNR.213","###INDEX:CamExt.###MNR.213:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W224]{r}"]
[41,"DW 396",null,"Cam 114 Start","CamExt.###MNR.214","###INDEX:CamExt.###MNR.214:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W226]{r}"]
[41,"DW 398",null,"Cam 115 Start","CamExt.###MNR.215","###INDEX:CamExt.###MNR.215:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W228]{r}"]
[41,"DW 400",null,"Cam 116 Start","CamExt.###MNR.216","###INDEX:CamExt.###MNR.216:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W230]{r}"]
[41,"DW 402",null,"Cam 117 Start","CamExt.###MNR.217","###INDEX:CamExt.###MNR.217:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W232]{r}"]
[41,"DW 404",null,"Cam 118 Start","CamExt.###MNR.218","###INDEX:CamExt.###MNR.218:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W234]{r}"]
[41,"DW 406",null,"Cam 119 Start","CamExt.###MNR.219","###INDEX:CamExt.###MNR.219:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W236]{r}"]
[41,"DW 408",null,"Cam 120 Start","CamExt.###MNR.220","###INDEX:CamExt.###MNR.220:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W238]{r}"]
[41,"DW 410",null,"Cam 121 Start","CamExt.###MNR.221","###INDEX:CamExt.###MNR.221:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W240]{r}"]
[41,"DW 412",null,"Cam 122 Start","CamExt.###MNR.222","###INDEX:CamExt.###MNR.222:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W242]{r}"]
[41,"DW 414",null,"Cam 123 Start","CamExt.###MNR.223","###INDEX:CamExt.###MNR.223:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W244]{r}"]
[41,"DW 416",null,"Cam 124 Start","CamExt.###MNR.224","###INDEX:CamExt.###MNR.224:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W246]{r}"]
[41,"DW 418",null,"Cam 125 Start","CamExt.###MNR.225","###INDEX:CamExt.###MNR.225:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W248]{r}"]
[41,"DW 420",null,"Cam 126 Start","CamExt.###MNR.226","###INDEX:CamExt.###MNR.226:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W250]{r}"]
[41,"DW 422",null,"Cam 127 Start","CamExt.###MNR.227","###INDEX:CamExt.###MNR.227:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W252]{r}"]
[41,"DW 424",null,"Cam 128 Start","CamExt.###MNR.228","###INDEX:CamExt.###MNR.228:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W254]{r}"]
[41,"DW 426",null,"Cam 129 Start","CamExt.###MNR.229","###INDEX:CamExt.###MNR.229:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W256]{r}"]
[41,"DW 428",null,"Cam 130 Start","CamExt.###MNR.230","###INDEX:CamExt.###MNR.230:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W258]{r}"]
[41,"DW 430",null,"Cam 131 Start","CamExt.###MNR.231","###INDEX:CamExt.###MNR.231:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W260]{r}"]
[41,"DW 432",null,"Cam 132 Start","CamExt.###MNR.232","###INDEX:CamExt.###MNR.232:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W262]{r}"]
[41,"DW 434",null,"Cam 133 Start","CamExt.###MNR.233","###INDEX:CamExt.###MNR.233:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W264]{r}"]
[41,"DW 436",null,"Cam 134 Start","CamExt.###MNR.234","###INDEX:CamExt.###MNR.234:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W266]{r}"]
[41,"DW 438",null,"Cam 135 Start","CamExt.###MNR.235","###INDEX:CamExt.###MNR.235:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W268]{r}"]
[41,"DW 440",null,"Cam 136 Start","CamExt.###MNR.236","###INDEX:CamExt.###MNR.236:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W270]{r}"]
[41,"DW 442",null,"Cam 137 Start","CamExt.###MNR.237","###INDEX:CamExt.###MNR.237:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W272]{r}"]
[41,"DW 444",null,"Cam 138 Start","CamExt.###MNR.238","###INDEX:CamExt.###MNR.238:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W274]{r}"]
[41,"DW 446",null,"Cam 139 Start","CamExt.###MNR.239","###INDEX:CamExt.###MNR.239:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W276]{r}"]
[41,"DW 448",null,"Cam 140 Start","CamExt.###MNR.240","###INDEX:CamExt.###MNR.240:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W278]{r}"]
[41,"DW 450",null,"Cam 141 Start","CamExt.###MNR.241","###INDEX:CamExt.###MNR.241:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W280]{r}"]
[41,"DW 452",null,"Cam 142 Start","CamExt.###MNR.242","###INDEX:CamExt.###MNR.242:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W282]{r}"]
[41,"DW 454",null,"Cam 143 Start","CamExt.###MNR.243","###INDEX:CamExt.###MNR.243:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W284]{r}"]
[41,"DW 456",null,"Cam 144 Start","CamExt.###MNR.244","###INDEX:CamExt.###MNR.244:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W286]{r}"]
[41,"DW 458",null,"Cam 145 Start","CamExt.###MNR.245","###INDEX:CamExt.###MNR.245:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W288]{r}"]
[41,"DW 460",null,"Cam 146 Start","CamExt.###MNR.246","###INDEX:CamExt.###MNR.246:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W290]{r}"]
[41,"DW 462",null,"Cam 147 Start","CamExt.###MNR.247","###INDEX:CamExt.###MNR.247:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W292]{r}"]
[41,"DW 464",null,"Cam 148 Start","CamExt.###MNR.248","###INDEX:CamExt.###MNR.248:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W294]{r}"]
[41,"DW 466",null,"Cam 149 Start","CamExt.###MNR.249","###INDEX:CamExt.###MNR.249:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W296]{r}"]
[41,"DW 468",null,"Cam 150 Start","CamExt.###MNR.250","###INDEX:CamExt.###MNR.250:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W298]{r}"]
[41,"DW 470",null,"Cam 151 Start","CamExt.###MNR.251","###INDEX:CamExt.###MNR.251:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W300]{r}"]
[41,"DW 472",null,"Cam 152 Start","CamExt.###MNR.252","###INDEX:CamExt.###MNR.252:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W302]{r}"]
[41,"DW 474",null,"Cam 153 Start","CamExt.###MNR.253","###INDEX:CamExt.###MNR.253:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W304]{r}"]
[41,"DW 476",null,"Cam 154 Start","CamExt.###MNR.254","###INDEX:CamExt.###MNR.254:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W306]{r}"]
[41,"DW 478",null,"Cam 155 Start","CamExt.###MNR.255","###INDEX:CamExt.###MNR.255:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W308]{r}"]
[41,"DW 480",null,"Cam 156 Start","CamExt.###MNR.256","###INDEX:CamExt.###MNR.256:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W310]{r}"]
[41,"DW 482",null,"Cam 157 Start","CamExt.###MNR.257","###INDEX:CamExt.###MNR.257:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W312]{r}"]
[41,"DW 484",null,"Cam 158 Start","CamExt.###MNR.258","###INDEX:CamExt.###MNR.258:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W314]{r}"]
[41,"DW 486",null,"Cam 159 Start","CamExt.###MNR.259","###INDEX:CamExt.###MNR.259:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W316]{r}"]
[41,"DW 488",null,"Cam 160 Start","CamExt.###MNR.260","###INDEX:CamExt.###MNR.260:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W318]{r}"]
[41,"DW 490",null,"Cam 161 Start","CamExt.###MNR.261","###INDEX:CamExt.###MNR.261:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W320]{r}"]
[41,"DW 492",null,"Cam 162 Start","CamExt.###MNR.262","###INDEX:CamExt.###MNR.262:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W322]{r}"]
[41,"DW 494",null,"Cam 163 Start","CamExt.###MNR.263","###INDEX:CamExt.###MNR.263:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W324]{r}"]
[41,"DW 496",null,"Cam 164 Start","CamExt.###MNR.264","###INDEX:CamExt.###MNR.264:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W326]{r}"]
[41,"DW 498",null,"Cam 165 Start","CamExt.###MNR.265","###INDEX:CamExt.###MNR.265:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W328]{r}"]
[41,"DW 500",null,"Cam 166 Start","CamExt.###MNR.266","###INDEX:CamExt.###MNR.266:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W330]{r}"]
[41,"DW 502",null,"Cam 167 Start","CamExt.###MNR.267","###INDEX:CamExt.###MNR.267:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W332]{r}"]
[41,"DW 504",null,"Cam 168 Start","CamExt.###MNR.268","###INDEX:CamExt.###MNR.268:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W334]{r}"]
[41,"DW 506",null,"Cam 169 Start","CamExt.###MNR.269","###INDEX:CamExt.###MNR.269:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W336]{r}"]
[41,"DW 508",null,"Cam 170 Start","CamExt.###MNR.270","###INDEX:CamExt.###MNR.270:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W338]{r}"]
[41,"DW 510",null,"Cam 171 Start","CamExt.###MNR.271","###INDEX:CamExt.###MNR.271:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W340]{r}"]
[41,"DW 512",null,"Cam 172 Start","CamExt.###MNR.272","###INDEX:CamExt.###MNR.272:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W342]{r}"]
[41,"DW 514",null,"Cam 173 Start","CamExt.###MNR.273","###INDEX:CamExt.###MNR.273:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W344]{r}"]
[41,"DW 516",null,"Cam 174 Start","CamExt.###MNR.274","###INDEX:CamExt.###MNR.274:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W346]{r}"]
[41,"DW 518",null,"Cam 175 Start","CamExt.###MNR.275","###INDEX:CamExt.###MNR.275:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W348]{r}"]
[41,"DW 520",null,"Cam 176 Start","CamExt.###MNR.276","###INDEX:CamExt.###MNR.276:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W350]{r}"]
[41,"DW 522",null,"Cam 177 Start","CamExt.###MNR.277","###INDEX:CamExt.###MNR.277:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W352]{r}"]
[41,"DW 524",null,"Cam 178 Start","CamExt.###MNR.278","###INDEX:CamExt.###MNR.278:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W354]{r}"]
[41,"DW 526",null,"Cam 179 Start","CamExt.###MNR.279","###INDEX:CamExt.###MNR.279:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W356]{r}"]
[41,"DW 528",null,"Cam 180 Start","CamExt.###MNR.280","###INDEX:CamExt.###MNR.280:INDEX","Ch1.###MNR_T_kurven<.m###MNR_kurv>[W358]{r}"]

{"sheet":"PLCPresetsExt","index":78,"n_rows":78,"n_cols":7,"rows_kept":78,"flags":["formulas_cached_only"]}
["PLCPresetsExt","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 360 - 364","Presets"]
[41,"DB 360 ","Presets 1st Machine "]
[41,"DW 010 –012","3*16 Bit Presets"]
[41,"DB 361-364","Presets Machine 2-5"]
[1,"###MAIN"]
[1,"DB 360-364 Presets"]
[21,"DB ###ADDR:360+1[MNR]:ADDR","Presets ###MNR"]
[41,"DW 0","Bit 0","Presets changed",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_voraender>[B]{w}"]
[41,"DW 10","Bit 0-15","Preset 1-16 exist",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_vorein_1_anzeige>[W]{r}"]
[41,"DW 11","Bit 0","Presetting   1","PLCPresetsExt.###MNR.1","###INDEX:PLCPresetsExt.###MNR.1:INDEX","Ch1.###MNR_T_voreinext<.m###MNR_vorein_1>[W]{r}"]
[41,null,"Bit 1","Presetting   2","PLCPresetsExt.###MNR.2","###INDEX:PLCPresetsExt.###MNR.2:INDEX"]
[41,null,"Bit 2","Presetting   3","PLCPresetsExt.###MNR.3","###INDEX:PLCPresetsExt.###MNR.3:INDEX"]
[41,null,"Bit 3","Presetting   4","PLCPresetsExt.###MNR.4","###INDEX:PLCPresetsExt.###MNR.4:INDEX"]
[41,null,"Bit 4","Presetting   5","PLCPresetsExt.###MNR.5","###INDEX:PLCPresetsExt.###MNR.5:INDEX"]
[41,null,"Bit 5","Presetting   6","PLCPresetsExt.###MNR.6","###INDEX:PLCPresetsExt.###MNR.6:INDEX"]
[41,null,"Bit 6","Presetting   7","PLCPresetsExt.###MNR.7","###INDEX:PLCPresetsExt.###MNR.7:INDEX"]
[41,null,"Bit 7","Presetting   8","PLCPresetsExt.###MNR.8","###INDEX:PLCPresetsExt.###MNR.8:INDEX"]
[41,null,"Bit 8","Presetting   9","PLCPresetsExt.###MNR.9","###INDEX:PLCPresetsExt.###MNR.9:INDEX"]
[41,null,"Bit 9","Presetting   10","PLCPresetsExt.###MNR.10","###INDEX:PLCPresetsExt.###MNR.10:INDEX"]
[41,null,"Bit 10","Presetting   11","PLCPresetsExt.###MNR.11","###INDEX:PLCPresetsExt.###MNR.11:INDEX"]
[41,null,"Bit 11","Presetting   12","PLCPresetsExt.###MNR.12","###INDEX:PLCPresetsExt.###MNR.12:INDEX"]
[41,null,"Bit 12","Presetting   13","PLCPresetsExt.###MNR.13","###INDEX:PLCPresetsExt.###MNR.13:INDEX"]
[41,null,"Bit 13","Presetting   14","PLCPresetsExt.###MNR.14","###INDEX:PLCPresetsExt.###MNR.14:INDEX"]
[41,null,"Bit 14","Presetting   15","PLCPresetsExt.###MNR.15","###INDEX:PLCPresetsExt.###MNR.15:INDEX"]
[41,null,"Bit 15","Presetting   16","PLCPresetsExt.###MNR.16","###INDEX:PLCPresetsExt.###MNR.16:INDEX"]
[41,"DW 12","Bit 0-15","Preset 17-32 exist",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_vorein_2_anzeige>[W]{r}"]
[41,"DW 13","Bit 0","Presetting   17","PLCPresetsExt.###MNR.17","###INDEX:PLCPresetsExt.###MNR.17:INDEX","Ch1.###MNR_T_voreinext<.m###MNR_vorein_2>[W]{r}"]
[41,null,"Bit 1","Presetting   18","PLCPresetsExt.###MNR.18","###INDEX:PLCPresetsExt.###MNR.18:INDEX"]
[41,null,"Bit 2","Presetting   19","PLCPresetsExt.###MNR.19","###INDEX:PLCPresetsExt.###MNR.19:INDEX"]
[41,null,"Bit 3","Presetting   20","PLCPresetsExt.###MNR.20","###INDEX:PLCPresetsExt.###MNR.20:INDEX"]
[41,null,"Bit 4","Presetting   21","PLCPresetsExt.###MNR.21","###INDEX:PLCPresetsExt.###MNR.21:INDEX"]
[41,null,"Bit 5","Presetting   22","PLCPresetsExt.###MNR.22","###INDEX:PLCPresetsExt.###MNR.22:INDEX"]
[41,null,"Bit 6","Presetting   23","PLCPresetsExt.###MNR.23","###INDEX:PLCPresetsExt.###MNR.23:INDEX"]
[41,null,"Bit 7","Presetting   24","PLCPresetsExt.###MNR.24","###INDEX:PLCPresetsExt.###MNR.24:INDEX"]
[41,null,"Bit 8","Presetting   25","PLCPresetsExt.###MNR.25","###INDEX:PLCPresetsExt.###MNR.25:INDEX"]
[41,null,"Bit 9","Presetting   26","PLCPresetsExt.###MNR.26","###INDEX:PLCPresetsExt.###MNR.26:INDEX"]
[41,null,"Bit 10","Presetting   27","PLCPresetsExt.###MNR.27","###INDEX:PLCPresetsExt.###MNR.27:INDEX"]
[41,null,"Bit 11","Presetting   28","PLCPresetsExt.###MNR.28","###INDEX:PLCPresetsExt.###MNR.28:INDEX"]
[41,null,"Bit 12","Presetting   29","PLCPresetsExt.###MNR.29","###INDEX:PLCPresetsExt.###MNR.29:INDEX"]
[41,null,"Bit 13","Presetting   30","PLCPresetsExt.###MNR.30","###INDEX:PLCPresetsExt.###MNR.30:INDEX"]
[41,null,"Bit 14","Presetting   31","PLCPresetsExt.###MNR.31","###INDEX:PLCPresetsExt.###MNR.31:INDEX"]
[41,null,"Bit 15","Presetting   32","PLCPresetsExt.###MNR.32","###INDEX:PLCPresetsExt.###MNR.32:INDEX"]
[41,"DW 14","Bit 0-15","Preset 33-48 exist",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_vorein_3_anzeige>[W]{r}"]
[41,"DW 15","Bit 0","Presetting   33","PLCPresetsExt.###MNR.33","###INDEX:PLCPresetsExt.###MNR.33:INDEX","Ch1.###MNR_T_voreinext<.m###MNR_vorein_3>[W]{r}"]
[41,null,"Bit 1","Presetting   34","PLCPresetsExt.###MNR.34","###INDEX:PLCPresetsExt.###MNR.34:INDEX"]
[41,null,"Bit 2","Presetting   35","PLCPresetsExt.###MNR.35","###INDEX:PLCPresetsExt.###MNR.35:INDEX"]
[41,null,"Bit 3","Presetting   36","PLCPresetsExt.###MNR.36","###INDEX:PLCPresetsExt.###MNR.36:INDEX"]
[41,null,"Bit 4","Presetting   37","PLCPresetsExt.###MNR.37","###INDEX:PLCPresetsExt.###MNR.37:INDEX"]
[41,null,"Bit 5","Presetting   38","PLCPresetsExt.###MNR.38","###INDEX:PLCPresetsExt.###MNR.38:INDEX"]
[41,null,"Bit 6","Presetting   39","PLCPresetsExt.###MNR.39","###INDEX:PLCPresetsExt.###MNR.39:INDEX"]
[41,null,"Bit 7","Presetting   40","PLCPresetsExt.###MNR.40","###INDEX:PLCPresetsExt.###MNR.40:INDEX"]
[41,null,"Bit 8","Presetting   41","PLCPresetsExt.###MNR.41","###INDEX:PLCPresetsExt.###MNR.41:INDEX"]
[41,null,"Bit 9","Presetting   42","PLCPresetsExt.###MNR.42","###INDEX:PLCPresetsExt.###MNR.42:INDEX"]
[41,null,"Bit 10","Presetting   43","PLCPresetsExt.###MNR.43","###INDEX:PLCPresetsExt.###MNR.43:INDEX"]
[41,null,"Bit 11","Presetting   44","PLCPresetsExt.###MNR.44","###INDEX:PLCPresetsExt.###MNR.44:INDEX"]
[41,null,"Bit 12","Presetting   45","PLCPresetsExt.###MNR.45","###INDEX:PLCPresetsExt.###MNR.45:INDEX"]
[41,null,"Bit 13","Presetting   46","PLCPresetsExt.###MNR.46","###INDEX:PLCPresetsExt.###MNR.46:INDEX"]
[41,null,"Bit 14","Presetting   47","PLCPresetsExt.###MNR.47","###INDEX:PLCPresetsExt.###MNR.47:INDEX"]
[41,null,"Bit 15","Presetting   48","PLCPresetsExt.###MNR.48","###INDEX:PLCPresetsExt.###MNR.48:INDEX"]
[41,"DW 16","Bit 0-15","Preset 49-64 exist",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_vorein_4_anzeige>[W]{r}"]
[41,"DW 17","Bit 0","Presetting   49","PLCPresetsExt.###MNR.49","###INDEX:PLCPresetsExt.###MNR.49:INDEX","Ch1.###MNR_T_voreinext<.m###MNR_vorein_4>[W]{r}"]
[41,null,"Bit 1","Presetting   50","PLCPresetsExt.###MNR.50","###INDEX:PLCPresetsExt.###MNR.50:INDEX"]
[41,null,"Bit 2","Presetting   51","PLCPresetsExt.###MNR.51","###INDEX:PLCPresetsExt.###MNR.51:INDEX"]
[41,null,"Bit 3","Presetting   52","PLCPresetsExt.###MNR.52","###INDEX:PLCPresetsExt.###MNR.52:INDEX"]
[41,null,"Bit 4","Presetting   53","PLCPresetsExt.###MNR.53","###INDEX:PLCPresetsExt.###MNR.53:INDEX"]
[41,null,"Bit 5","Presetting   54","PLCPresetsExt.###MNR.54","###INDEX:PLCPresetsExt.###MNR.54:INDEX"]
[41,null,"Bit 6","Presetting   55","PLCPresetsExt.###MNR.55","###INDEX:PLCPresetsExt.###MNR.55:INDEX"]
[41,null,"Bit 7","Presetting   56","PLCPresetsExt.###MNR.56","###INDEX:PLCPresetsExt.###MNR.56:INDEX"]
[41,null,"Bit 8","Presetting   57","PLCPresetsExt.###MNR.57","###INDEX:PLCPresetsExt.###MNR.57:INDEX"]
[41,null,"Bit 9","Presetting   58","PLCPresetsExt.###MNR.58","###INDEX:PLCPresetsExt.###MNR.58:INDEX"]
[41,null,"Bit 10","Presetting   59","PLCPresetsExt.###MNR.59","###INDEX:PLCPresetsExt.###MNR.59:INDEX"]
[41,null,"Bit 11","Presetting   60","PLCPresetsExt.###MNR.60","###INDEX:PLCPresetsExt.###MNR.60:INDEX"]
[41,null,"Bit 12","Presetting   61","PLCPresetsExt.###MNR.61","###INDEX:PLCPresetsExt.###MNR.61:INDEX"]
[41,null,"Bit 13","Presetting   62","PLCPresetsExt.###MNR.62","###INDEX:PLCPresetsExt.###MNR.62:INDEX"]
[41,null,"Bit 14","Presetting   63","PLCPresetsExt.###MNR.63","###INDEX:PLCPresetsExt.###MNR.63:INDEX"]
[41,null,"Bit 15","Presetting   64","PLCPresetsExt.###MNR.64","###INDEX:PLCPresetsExt.###MNR.64:INDEX"]

{"sheet":"ManualMovementExt","index":79,"n_rows":71,"n_cols":7,"rows_kept":71,"flags":["formulas_cached_only"]}
["ManualMovement","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 360 - 364","Manual movement "]
[41,"DB 360 ","Manual movement 1st Machine "]
[41,"DW 010 –012","2*12 Bit Manual movement"]
[41,"DB 361-364","Manual movement Machine  2-5"]
[1,"###MAIN"]
[1,"DB 360-364 Manual movement "]
[21,"DB ###ADDR:360+1[MNR]:ADDR","Manual movement ###MNR"]
[41,"DW 100","Bit 0","Manual movement changed",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handaender>[B]{w}"]
[41,null,"Bit 8","Manual enable","ManualMovementExt.###MNR.1","###INDEX:ManualMovementExt.###MNR.1:INDEX","Ch1.###MNR_T_voreinext<.m###MNR_handbetrieb>[B]{r}"]
[41]
[41,"DW 101",null,"Text No. Text Value 1",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handtext_1>[W]{r}"]
[41,"DW 102",null,"Text No. Unit Value 1",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handeinheit_1>[W]{r}"]
[41,"DW 103",null,"Value 1",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handwert_1>[W]{r}"]
[41,"DW 104",null,"Text No. Text Value 2",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handtext_2>[W]{r}"]
[41,"DW 105",null,"Text No. Unit Value 2",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handeinheit_2>[W]{r}"]
[41,"DW 106",null,"Value 2",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handwert_2>[W]{r}"]
[]
[]
[41,"DW 120","Bit 0","Manual movement  ","ManualMovementExt.###MNR.101","###INDEX:ManualMovementExt.###MNR.101:INDEX","Ch1.###MNR_T_vorein<.m###MNR_handver_1>[W]{r}"]
[41,null,"Bit 1","Manual movement  ","ManualMovementExt.###MNR.102","###INDEX:ManualMovementExt.###MNR.102:INDEX"]
[41,null,"Bit 2","Manual movement  ","ManualMovementExt.###MNR.103","###INDEX:ManualMovementExt.###MNR.103:INDEX"]
[41,null,"Bit 3","Manual movement  ","ManualMovementExt.###MNR.104","###INDEX:ManualMovementExt.###MNR.104:INDEX"]
[41,null,"Bit 4","Manual movement  ","ManualMovementExt.###MNR.105","###INDEX:ManualMovementExt.###MNR.105:INDEX"]
[41,null,"Bit 5","Manual movement  ","ManualMovementExt.###MNR.106","###INDEX:ManualMovementExt.###MNR.106:INDEX"]
[41,null,"Bit 6","Manual movement  ","ManualMovementExt.###MNR.107","###INDEX:ManualMovementExt.###MNR.107:INDEX"]
[41,null,"Bit 7","Manual movement  ","ManualMovementExt.###MNR.108","###INDEX:ManualMovementExt.###MNR.108:INDEX"]
[41,null,"Bit 8","Manual movement  ","ManualMovementExt.###MNR.109","###INDEX:ManualMovementExt.###MNR.109:INDEX"]
[41,null,"Bit 9","Manual movement  ","ManualMovementExt.###MNR.110","###INDEX:ManualMovementExt.###MNR.110:INDEX"]
[41,null,"Bit 10","Manual movement  ","ManualMovementExt.###MNR.111","###INDEX:ManualMovementExt.###MNR.111:INDEX"]
[41,null,"Bit 11","Manual movement  ","ManualMovementExt.###MNR.112","###INDEX:ManualMovementExt.###MNR.112:INDEX"]
[41,null,"Bit 12","Manual movement  ","ManualMovementExt.###MNR.113","###INDEX:ManualMovementExt.###MNR.113:INDEX"]
[41,null,"Bit 13","Manual movement  ","ManualMovementExt.###MNR.114","###INDEX:ManualMovementExt.###MNR.114:INDEX"]
[41,null,"Bit 14","Manual movement  ","ManualMovementExt.###MNR.115","###INDEX:ManualMovementExt.###MNR.115:INDEX"]
[41,null,"Bit 15","Manual movement  ","ManualMovementExt.###MNR.116","###INDEX:ManualMovementExt.###MNR.116:INDEX"]
[41,"DW 121","Bit 0-15","Manual movement  1-16 exist",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handver_1_anzeige>[W]{r}"]
[41,"DW 122","Bit 0","Manual movement  ","ManualMovementExt.###MNR.117","###INDEX:ManualMovementExt.###MNR.117:INDEX","Ch1.###MNR_T_vorein<.m###MNR_handver_2>[W]{r}"]
[41,null,"Bit 1","Manual movement  ","ManualMovementExt.###MNR.118","###INDEX:ManualMovementExt.###MNR.118:INDEX"]
[41,null,"Bit 2","Manual movement  ","ManualMovementExt.###MNR.119","###INDEX:ManualMovementExt.###MNR.119:INDEX"]
[41,null,"Bit 3","Manual movement  ","ManualMovementExt.###MNR.120","###INDEX:ManualMovementExt.###MNR.120:INDEX"]
[41,null,"Bit 4","Manual movement  ","ManualMovementExt.###MNR.121","###INDEX:ManualMovementExt.###MNR.121:INDEX"]
[41,null,"Bit 5","Manual movement  ","ManualMovementExt.###MNR.122","###INDEX:ManualMovementExt.###MNR.122:INDEX"]
[41,null,"Bit 6","Manual movement  ","ManualMovementExt.###MNR.123","###INDEX:ManualMovementExt.###MNR.123:INDEX"]
[41,null,"Bit 7","Manual movement  ","ManualMovementExt.###MNR.124","###INDEX:ManualMovementExt.###MNR.124:INDEX"]
[41,null,"Bit 8","Manual movement  ","ManualMovementExt.###MNR.125","###INDEX:ManualMovementExt.###MNR.125:INDEX"]
[41,null,"Bit 9","Manual movement  ","ManualMovementExt.###MNR.126","###INDEX:ManualMovementExt.###MNR.126:INDEX"]
[41,null,"Bit 10","Manual movement  ","ManualMovementExt.###MNR.127","###INDEX:ManualMovementExt.###MNR.127:INDEX"]
[41,null,"Bit 11","Manual movement  ","ManualMovementExt.###MNR.128","###INDEX:ManualMovementExt.###MNR.128:INDEX"]
[41,null,"Bit 12","Manual movement  ","ManualMovementExt.###MNR.129","###INDEX:ManualMovementExt.###MNR.129:INDEX"]
[41,null,"Bit 13","Manual movement  ","ManualMovementExt.###MNR.130","###INDEX:ManualMovementExt.###MNR.130:INDEX"]
[41,null,"Bit 14","Manual movement  ","ManualMovementExt.###MNR.131","###INDEX:ManualMovementExt.###MNR.131:INDEX"]
[41,null,"Bit 15","Manual movement  ","ManualMovementExt.###MNR.132","###INDEX:ManualMovementExt.###MNR.132:INDEX"]
[41,"DW 123","Bit 0-15","Manual movement  17-32 exist",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handver_2_anzeige>[W]{r}"]
[41,"DW 124","Bit 0","Manual movement  ","ManualMovementExt.###MNR.133","###INDEX:ManualMovementExt.###MNR.133:INDEX","Ch1.###MNR_T_vorein<.m###MNR_handver_3>[W]{r}"]
[41,null,"Bit 1","Manual movement  ","ManualMovementExt.###MNR.134","###INDEX:ManualMovementExt.###MNR.134:INDEX"]
[41,null,"Bit 2","Manual movement  ","ManualMovementExt.###MNR.135","###INDEX:ManualMovementExt.###MNR.135:INDEX"]
[41,null,"Bit 3","Manual movement  ","ManualMovementExt.###MNR.136","###INDEX:ManualMovementExt.###MNR.136:INDEX"]
[41,null,"Bit 4","Manual movement  ","ManualMovementExt.###MNR.137","###INDEX:ManualMovementExt.###MNR.137:INDEX"]
[41,null,"Bit 5","Manual movement  ","ManualMovementExt.###MNR.138","###INDEX:ManualMovementExt.###MNR.138:INDEX"]
[41,null,"Bit 6","Manual movement  ","ManualMovementExt.###MNR.139","###INDEX:ManualMovementExt.###MNR.139:INDEX"]
[41,null,"Bit 7","Manual movement  ","ManualMovementExt.###MNR.140","###INDEX:ManualMovementExt.###MNR.140:INDEX"]
[41,null,"Bit 8","Manual movement  ","ManualMovementExt.###MNR.141","###INDEX:ManualMovementExt.###MNR.141:INDEX"]
[41,null,"Bit 9","Manual movement  ","ManualMovementExt.###MNR.142","###INDEX:ManualMovementExt.###MNR.142:INDEX"]
[41,null,"Bit 10","Manual movement  ","ManualMovementExt.###MNR.143","###INDEX:ManualMovementExt.###MNR.143:INDEX"]
[41,null,"Bit 11","Manual movement  ","ManualMovementExt.###MNR.144","###INDEX:ManualMovementExt.###MNR.144:INDEX"]
[41,null,"Bit 12","Manual movement  ","ManualMovementExt.###MNR.145","###INDEX:ManualMovementExt.###MNR.145:INDEX"]
[41,null,"Bit 13","Manual movement  ","ManualMovementExt.###MNR.146","###INDEX:ManualMovementExt.###MNR.146:INDEX"]
[41,null,"Bit 14","Manual movement  ","ManualMovementExt.###MNR.147","###INDEX:ManualMovementExt.###MNR.147:INDEX"]
[41,null,"Bit 15","Manual movement  ","ManualMovementExt.###MNR.148","###INDEX:ManualMovementExt.###MNR.148:INDEX"]
[41,"DW 125","Bit 0-15","Manual movement  33-48 exist",null,null,"Ch1.###MNR_T_voreinext<.m###MNR_handver_3_anzeige>[W]{r}"]

{"sheet":"OnsertMonitoring2","index":80,"n_rows":41,"n_cols":7,"rows_kept":41,"flags":["formulas_cached_only"]}
["OnsertMonitoring2","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 370","Onsertendkontrolle 1st Machine "]
[21,"DB 370-374","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 370-374 Onsertendkontrolle"]
[21,"DB ###ADDR:370+1[MNR]:ADDR","Onsertendkontrolle ###MNR"]
[41,"DW 0","Bit 0","Onsertendkontrolle geändert",null,null,"Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon2_aender>[B]{w}"]
[41]
[41,null,"Part 1"]
[41,"DW 10","Bit 0","Daten senden","OnsertMonitoring2.10","###INDEX:OnsertMonitoring2.10:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_bit1>[W]{r}"]
[41,null,"Bit 1","Daten holen","OnsertMonitoring2.11","###INDEX:OnsertMonitoring2.11:INDEX"]
[41,"DW 20",null,"Fenster rechts","OnsertMonitoring2.20","###INDEX:OnsertMonitoring2.20:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll1>[W0]{r}"]
[41,"DW 21",null,"Fenster links","OnsertMonitoring2.21","###INDEX:OnsertMonitoring2.21:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll1>[W1]{r}"]
[41,"DW 22",null,"Fenster oben","OnsertMonitoring2.22","###INDEX:OnsertMonitoring2.22:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll1>[W2]{r}"]
[41,"DW 23",null,"Fenster unten","OnsertMonitoring2.23","###INDEX:OnsertMonitoring2.23:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll1>[W3]{r}"]
[41,"DW 24",null,"Helligkeit","OnsertMonitoring2.24","###INDEX:OnsertMonitoring2.24:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll1>[W4]{r}"]
[41,"DW 25",null,"Format","OnsertMonitoring2.25","###INDEX:OnsertMonitoring2.25:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll1>[W5]{r}"]
[41]
[41,"DW 30",null,"Istwert 1","OnsertMonitoring2.30","###INDEX:OnsertMonitoring2.30:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist1>[W0]{p}"]
[41,"DW 31",null,"Istwert 2","OnsertMonitoring2.31","###INDEX:OnsertMonitoring2.31:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist1>[W1]{p}"]
[41,"DW 32",null,"Istwert 3","OnsertMonitoring2.32","###INDEX:OnsertMonitoring2.32:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist1>[W2]{p}"]
[41,"DW 33",null,"Istwert 4","OnsertMonitoring2.33","###INDEX:OnsertMonitoring2.33:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist1>[W3]{p}"]
[41,"DW 34",null,"Istwert 5","OnsertMonitoring2.34","###INDEX:OnsertMonitoring2.34:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist1>[W4]{p}"]
[41]
[41,null,"Part 2"]
[41,"DW 40","Bit 0","Daten senden","OnsertMonitoring2.60","###INDEX:OnsertMonitoring2.60:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_bit2>[W]{r}"]
[41,null,"Bit 1","Daten holen","OnsertMonitoring2.61","###INDEX:OnsertMonitoring2.61:INDEX"]
[41,"DW 50",null,"Fenster rechts","OnsertMonitoring2.70","###INDEX:OnsertMonitoring2.70:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll2>[W0]{r}"]
[41,"DW 51",null,"Fenster links","OnsertMonitoring2.71","###INDEX:OnsertMonitoring2.71:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll2>[W1]{r}"]
[41,"DW 52",null,"Fenster oben","OnsertMonitoring2.72","###INDEX:OnsertMonitoring2.72:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll2>[W2]{r}"]
[41,"DW 53",null,"Fenster unten","OnsertMonitoring2.73","###INDEX:OnsertMonitoring2.73:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll2>[W3]{r}"]
[41,"DW 54",null,"Helligkeit","OnsertMonitoring2.74","###INDEX:OnsertMonitoring2.74:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll2>[W4]{r}"]
[41,"DW 55",null,"Format","OnsertMonitoring2.75","###INDEX:OnsertMonitoring2.75:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_soll2>[W5]{r}"]
[41]
[41,"DW 60",null,"Istwert 1","OnsertMonitoring2.80","###INDEX:OnsertMonitoring2.80:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist2>[W0]{p}"]
[41,"DW 61",null,"Istwert 2","OnsertMonitoring2.81","###INDEX:OnsertMonitoring2.81:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist2>[W1]{p}"]
[41,"DW 62",null,"Istwert 3","OnsertMonitoring2.82","###INDEX:OnsertMonitoring2.82:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist2>[W2]{p}"]
[41,"DW 63",null,"Istwert 4","OnsertMonitoring2.83","###INDEX:OnsertMonitoring2.83:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist2>[W3]{p}"]
[41,"DW 64",null,"Istwert 5","OnsertMonitoring2.84","###INDEX:OnsertMonitoring2.84:INDEX","Ch1.###MNR_T_onsertmon2<.m###MNR_onsertmon_ist2>[W4]{p}"]

{"sheet":"Register","index":81,"n_rows":68,"n_cols":7,"rows_kept":68,"flags":["formulas_cached_only"]}
["Register","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 380","Register 1st Machine "]
[21,"DB 380-384","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 380-384 Register"]
[21,"DB ###ADDR:380+1[MNR]:ADDR","Register ###MNR"]
[41,"DW 0","Bit 0","Register geändert",null,null,"Ch1.###MNR_T_register<.m###MNR_register_aender>[B]{w}"]
[41]
[41,null,"zur Steuerung"]
[41,"DW 10",null,"Registernummer",null,null,"Ch1.###MNR_T_register<.m###MNR_register_nrzs>[W]{r}"]
[41,"DW 11",null,"erste Zeile",null,null,"Ch1.###MNR_T_register<.m###MNR_register_zeile1zs>[W]{r}"]
[41]
[41,null,"von Steuerung"]
[41,"DW 20",null,"Registernummer",null,null,"Ch1.###MNR_T_register<.m###MNR_register_nrvs>[W]{r}"]
[41,"DW 21",null,"erste Zeile",null,null,"Ch1.###MNR_T_register<.m###MNR_register_zeile1vs>[W]{r}"]
[41,"DW 22",null,"Offset Register",null,null,"Ch1.###MNR_T_register<.m###MNR_register_offset>[W]{r}"]
[41,"DW 23",null,"Anzahl Register",null,null,"Ch1.###MNR_T_register<.m###MNR_register_anzahl>[W]{r}"]
[41]
[41,"DW 30","Bit 0 - 15","Maske 0-15",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W0]{r}"]
[41,"DW 31","Bit 0 - 15","Maske 16-31",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W1]{r}"]
[41,"DW 32","Bit 0 - 15","Maske 32-47",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W2]{r}"]
[41,"DW 33","Bit 0 - 15","Maske 48-63",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W3]{r}"]
[41,"DW 34","Bit 0 - 15","Maske 64-79",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W4]{r}"]
[41,"DW 35","Bit 0 - 15","Maske 80-95",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W5]{r}"]
[41,"DW 36","Bit 0 - 15","Maske 96-111",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W6]{r}"]
[41,"DW 37","Bit 0 - 15","Maske 112-127",null,null,"Ch1.###MNR_T_register<.m###MNR_register_maske>[W7]{r}"]
[41]
[41,"DW 40","Bit 0 - 15","Schritt 0 - 0-15",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W0]{r}"]
[41,"DW 41","Bit 0 - 15","Schritt 0 - 16-31",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W1]{r}"]
[41,"DW 42","Bit 0 - 15","Schritt 0 - 32-47",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W2]{r}"]
[41,"DW 43","Bit 0 - 15","Schritt 0 - 48-63",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W3]{r}"]
[41,"DW 44","Bit 0 - 15","Schritt 0 - 64-79",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W4]{r}"]
[41,"DW 45","Bit 0 - 15","Schritt 0 - 80-95",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W5]{r}"]
[41,"DW 46-50","Bit 0 - 15","Schritt 0 - 96-111",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W6]{r}"]
[41,"DW 47","Bit 0 - 15","Schritt 0 - 112-127",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W7]{r}"]
[41,"DW 48",null,"Schritt 0 - Status",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W8]{r}"]
[41,"DW 50-59",null,"Schritt 1",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W10-19]{r}"]
[41,"DW 60-60",null,"Schritt 2",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W20-29]{r}"]
[41,"DW 70-79",null,"Schritt 3",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W30-39]{r}"]
[41,"DW 80-89",null,"Schritt 4",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W40-49]{r}"]
[41,"DW 90-99",null,"Schritt 5",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W50-59]{r}"]
[41,"DW 100-109",null,"Schritt 6",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W60-69]{r}"]
[41,"DW 110-119",null,"Schritt 7",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W70-79]{r}"]
[41,"DW 120-129",null,"Schritt 8",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W80-89]{r}"]
[41,"DW 130-139",null,"Schritt 9",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W90-99]{r}"]
[41,"DW 140-149",null,"Schritt 10",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W100-109]{r}"]
[41,"DW 150-159",null,"Schritt 11",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W110-119]{r}"]
[41,"DW 160-169",null,"Schritt 12",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W120-129]{r}"]
[41,"DW 170-179",null,"Schritt 13",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W130-139]{r}"]
[41,"DW 180-189",null,"Schritt 14",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W140-149]{r}"]
[41,"DW 190-199",null,"Schritt 15",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W150-159]{r}"]
[41,"DW 200-209",null,"Schritt 16",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W160-169]{r}"]
[41,"DW 210-219",null,"Schritt 17",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W170-179]{r}"]
[41,"DW 220-229",null,"Schritt 18",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W180-189]{r}"]
[41,"DW 230-239",null,"Schritt 19",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W190-199]{r}"]
[41,"DW 240-249",null,"Schritt 20",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W200-209]{r}"]
[41,"DW 250-259",null,"Schritt 21",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W210-219]{r}"]
[41,"DW 260-269",null,"Schritt 22",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W220-229]{r}"]
[41,"DW 270-279",null,"Schritt 23",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W230-239]{r}"]
[41,"DW 280-289",null,"Schritt 24",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W240-249]{r}"]
[41,"DW 290-299",null,"Schritt 25",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W250-259]{r}"]
[41,"DW 300-309",null,"Schritt 26",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W260-269]{r}"]
[41,"DW 310-319",null,"Schritt 27",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W270-279]{r}"]
[41,"DW 320-329",null,"Schritt 28",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W280-289]{r}"]
[41,"DW 330-339",null,"Schritt 29",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W290-299]{r}"]
[41,"DW 340-349",null,"Schritt 30",null,null,"Ch1.###MNR_T_register<.m###MNR_register_schritt>[W300-309]{r}"]

{"sheet":"MaterialMechanism","index":82,"n_rows":26,"n_cols":7,"rows_kept":26,"flags":["formulas_cached_only"]}
["MaterialMechanism","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 390","Material Mechanism 1st Machine "]
[21,"DB 390-394","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 390-394 Material Mechanism"]
[21,"DB ###ADDR:390+1[MNR]:ADDR","Material Mechanism ###MNR"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_register<.m###MNR_register_aender>[B]{w}"]
[41]
[41,"DD 10",null,"Parameter 1","MaterialMechanism.###MNR.1","###INDEX:MaterialMechanism.###MNR.1:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW0]{r}"]
[41,"DD 12",null,"Parameter 2","MaterialMechanism.###MNR.2","###INDEX:MaterialMechanism.###MNR.2:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW1]{r}"]
[41,"DD 14",null,"Parameter 3","MaterialMechanism.###MNR.3","###INDEX:MaterialMechanism.###MNR.3:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW2]{r}"]
[41,"DD 16",null,"Parameter 4","MaterialMechanism.###MNR.4","###INDEX:MaterialMechanism.###MNR.4:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW3]{r}"]
[41,"DD 18",null,"Parameter 5","MaterialMechanism.###MNR.5","###INDEX:MaterialMechanism.###MNR.5:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW4]{r}"]
[41,"DD 20",null,"Parameter 6","MaterialMechanism.###MNR.6","###INDEX:MaterialMechanism.###MNR.6:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW5]{r}"]
[41,"DD 22",null,"Parameter 7","MaterialMechanism.###MNR.7","###INDEX:MaterialMechanism.###MNR.7:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW6]{r}"]
[41,"DD 24",null,"Parameter 8","MaterialMechanism.###MNR.8","###INDEX:MaterialMechanism.###MNR.8:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW7]{r}"]
[41,"DD 26",null,"Parameter 9","MaterialMechanism.###MNR.9","###INDEX:MaterialMechanism.###MNR.9:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW8]{r}"]
[41,"DD 28",null,"Parameter 10","MaterialMechanism.###MNR.10","###INDEX:MaterialMechanism.###MNR.10:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW9]{r}"]
[41,"DD 30",null,"Parameter 11","MaterialMechanism.###MNR.11","###INDEX:MaterialMechanism.###MNR.11:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW10]{r}"]
[41,"DD 32",null,"Parameter 12","MaterialMechanism.###MNR.12","###INDEX:MaterialMechanism.###MNR.12:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW11]{r}"]
[41,"DD 34",null,"Parameter 13","MaterialMechanism.###MNR.13","###INDEX:MaterialMechanism.###MNR.13:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW12]{r}"]
[41,"DD 36",null,"Parameter 14","MaterialMechanism.###MNR.14","###INDEX:MaterialMechanism.###MNR.14:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW13]{r}"]
[41,"DD 38",null,"Parameter 15","MaterialMechanism.###MNR.15","###INDEX:MaterialMechanism.###MNR.15:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW14]{r}"]
[41,"DD 40",null,"Parameter 16","MaterialMechanism.###MNR.16","###INDEX:MaterialMechanism.###MNR.16:INDEX","Ch1.###MNR_T_parameter<.m###MNR_parameter>[DW15]{r}"]

{"sheet":"IO-Link","index":83,"n_rows":54,"n_cols":4,"rows_kept":54,"flags":["formulas_cached_only"]}
["IOLink","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 400","IO-Link 1st Machine "]
[21,"DB 401-404","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 400-404 IO-Link"]
[21,"DB ###ADDR:400+1[MNR]:ADDR","IO-Link ###MNR"]
[41,"DW 0","Bit 0","Data changed"]
[41]
[41,"DW 10-99","Part 1"]
[41,"DW 100-189","Part 2"]
[41,"DW 190-279","Part 3"]
[41,"DW 280-369","Part 4"]
[41,"DW 370-459","Part 5"]
[41,"DW 460-549","Part 6"]
[41,"DW 550-629","Part 7"]
[41,"DW 640-739","Part 8"]
[41,"DW 730-819","Part 9"]
[41,"DW 820-909","Part 10"]
[]
[21,"DK12-11/10/92/1236"]
[41,"DW 0","Bit 0","Part active"]
[41,"DW 1","Bit 0","Part changed"]
[41,"DW 2-19",null,"Product Name"]
[41]
[41,"DW 20-49",null,"Values for prameter handling"]
[41,"DW 20",null,"Red Intensity M"]
[41,"DW 21",null,"Green Intensity M"]
[41,"DW 22",null,"Blue Intensity M"]
[41,"DW 23",null,"Red Intensity B"]
[41,"DW 24",null,"Green Intensity B"]
[41,"DW 25",null,"Blue Intensity B"]
[41]
[41,"DW 50-69",null,"Setpoints"]
[41,"DW 50","Bit 0","Reserve"]
[41,null,"Bit 1","Reset"]
[41,"DW 51",null,"Teach Mode"]
[41,null,1,"S"]
[41,null,2,"TB"]
[41,null,3,"TD"]
[41,null,4,"TM"]
[41]
[41,"DW 70-89",null,"Values"]
[41,"DW 70 ",null,"Status text number"]
[41,"DW 71",null,"Status number"]
[41,"DW 72",null,"Status color"]
[41,null,0,"grey"]
[41,null,1,"red"]
[41,null,2,"yellow"]
[41,null,3,"green"]
[41,"DW73","Bit 0","LED 1"]
[null,null,"Bit 1","LED 2"]
[null,null,"Bit 2","LED 3"]

{"sheet":"HotMeltTank","index":84,"n_rows":49,"n_cols":7,"rows_kept":49,"flags":["formulas_cached_only"]}
["HotMeltTank","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 410","Hotmelt Tank 1st Machine "]
[21,"DB 411-414","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 410-414 Hotmelt Tank"]
[21,"DB ###ADDR:410+1[MNR]:ADDR","Hotmelt Tank ###MNR"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_aender>[B]{w}"]
[41]
[21,null,"Page 1"]
[41,"DW 10","Bit 0","send data",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_send1>[B]{r}"]
[41]
[41,"DW 11-30",null,"SetTemp",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_settemp1>[W0-19]{r}"]
[41,"DD 31",null,"ChnEnable",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_chnenable1>[DW]{r}"]
[41,"DW 33-40",null,"Groups",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_groups1>[W0-7]{r}"]
[41,"DW 41-43",null,"GroupsPress",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_groupspress1>[W0-3]{r}"]
[41]
[41,"DW 60-99",null,"Timer",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_timer1>[W0-39]{r}"]
[41]
[41,"DW 120",null,"EcoTank",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecotank1>[W]{r}"]
[41,"DW 121",null,"EcoHose",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecohose1>[W]{r}"]
[41,"DW 122",null,"EcoHead",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecohead1>[W]{r}"]
[41,"DW 123",null,"MaxTempTank",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_maxtemptank1>[W]{r}"]
[41,"DW 124",null,"MaxTempHose",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_maxtemphose1>[W]{r}"]
[41,"DW 125",null,"MaxTempHead",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_maxtemphead1>[W]{r}"]
[41,"DW 126",null,"NoNc",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_nonc1>[W]{r}"]
[41,"DW 127",null,"FuncEnable",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_funcenable1>[W]{r}"]
[41,"DW 128",null,"EcoMode",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecomode1>[W]{r}"]
[41]
[21,null,"Page 2"]
[41,"DW 210","Bit 0","send data",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_send2>[B]{r}"]
[41]
[41,"DW 211-230",null,"SetTemp",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_settemp2>[W0-19]{r}"]
[41,"DD2 31",null,"ChnEnable",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_chnenable2>[DW]{r}"]
[41,"DW 233-240",null,"Groups",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_groups2>[W0-7]{r}"]
[41,"DW 241-243",null,"GroupsPress",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_groupspress2>[W0-3]{r}"]
[41]
[41,"DW 260-299",null,"Timer",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_timer2>[W0-39]{r}"]
[41]
[41,"DW 320",null,"EcoTank",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecotank2>[W]{r}"]
[41,"DW 321",null,"EcoHose",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecohose2>[W]{r}"]
[41,"DW 322",null,"EcoHead",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecohead2>[W]{r}"]
[41,"DW 323",null,"MaxTempTank",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_maxtemptank2>[W]{r}"]
[41,"DW 324",null,"MaxTempHose",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_maxtemphose2>[W]{r}"]
[41,"DW 325",null,"MaxTempHead",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_maxtemphead2>[W]{r}"]
[41,"DW 326",null,"NoNc",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_nonc2>[W]{r}"]
[41,"DW 327",null,"FuncEnable",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_funcenable2>[W]{r}"]
[41,"DW 328",null,"EcoMode",null,null,"Ch1.###MNR_T_hotmelt<.m###MNR_hm_ecomode2>[W]{r}"]

{"sheet":"StampInspection","index":85,"n_rows":143,"n_cols":7,"rows_kept":143,"flags":["formulas_cached_only"]}
["StampInspection","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 420","Stamp Inspection 1st Machine "]
[21,"DB 421-424","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 420-424 Stamp Inspection"]
[21,"DB ###ADDR:420+1[MNR]:ADDR","Stamp Inspection ###MNR"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_stampin<.m###MNR_si_aender>[B]{w}"]
[41]
[21,null,"Page 1"]
[41,"DW 10",null,"status communitcation"]
[41,"DW 11",null,"Schalter"]
[41,null,"Bit 0","Teachen Bahn 1"]
[41,null,"Bit 1","Teachen Bahn 2"]
[41,null,"Bit 2","Kalibrieren Bahn 1"]
[41,null,"Bit 3","Kalibrieren Bahn 2"]
[41,"DW 20-29",null,"handshake from PLC"]
[41,null,"DW 20","Auftragsnummer"]
[41,"DW 50-59",null,"handshake to PLC"]
[41,null,"DW 50","Auftragsnummer"]
[41,"DW 80-129",null,"data from PLC"]
[41,null,"DW 80","Auftragsnummer"]
[41,null,"DW 81","xOffsetPack"]
[41,null,"DW 82","yOffsetPack"]
[41,null,"DW 83","xOffsetLightsourceLeft Track 1"]
[41,null,"DW 84","yOffsetLightsourceLeft Track 1"]
[41,null,"DW 85","xOffsetLightsourceRight Track 1"]
[41,null,"DW 86","yOffsetLightsourceRight Track 1"]
[41,null,"DW 87","xOffsetLightsourceLeft Track 2"]
[41,null,"DW 88","yOffsetLightsourceLeft Track 2"]
[41,null,"DW 89","xOffsetLightsourceRight Track 2"]
[41,null,"DW 90","yOffsetLightsourceRight Track 2"]
[41,null,"DW 91","LightsourcesWidth"]
[41,null,"DW 92","LightsourcesHeight"]
[41,null,"DW 93","lightsource0_Pulse Track 1"]
[41,null,"DW 94","lightsource0_Power Track 1"]
[41,null,"DW 95","lightsource1_Pulse Track 1"]
[41,null,"DW 96","lightsource1_Power Track 1"]
[41,null,"DW 97","lightsource2_Pulse Track 1"]
[41,null,"DW 98","lightsource2_Power Track 1"]
[41,null,"DW 99","lightsource3_Pulse Track 1"]
[41,null,"DW 100","lightsource3_Power Track 1"]
[41,null,"DW 101","lightsource0_Pulse Track 2"]
[41,null,"DW 102","lightsource0_Power Track 2"]
[41,null,"DW 103","lightsource1_Pulse Track 2"]
[41,null,"DW 104","lightsource1_Power Track 2"]
[41,null,"DW 105","lightsource2_Pulse Track 2"]
[41,null,"DW 106","lightsource2_Power Track 2"]
[41,null,"DW 107","lightsource3_Pulse Track 2"]
[41,null,"DW 108","lightsource3_Power Track 2"]
[41]
[41,null,"DW 110","Schalter"]
[41,null,"Bit 0","Toleranz Banderolenlage / ein"]
[41,null,"Bit 1","Umgelegte Ecken / ein"]
[41,null,"Bit 2","Defekt / ein"]
[41,null,"Bit 3","Verdrehung / ein"]
[41]
[41,null,"DW 111","xPosition track 1"]
[41,null,"DW 112","yPosition track 1"]
[41,null,"DW 113","xPosition track 2"]
[41,null,"DW 114","yPosition track 2"]
[41,null,"DW 115","Width"]
[41,null,"DW 116","Height"]
[41,null,"DW 117","Rotation"]
[41,null,"DW 118","HoloMaskX"]
[41,null,"DW 119","HoloMaskY"]
[41,null,"DW 120","HoloMaskWidth"]
[41,null,"DW 121","HoloMaskHeight"]
[41,null,"DW 122","Toleranz Banderolenlage +X"]
[41,null,"DW 123","Toleranz Banderolenlage -X"]
[41,null,"DW 124","Toleranz Banderolenlage +Y"]
[41,null,"DW 125","Toleranz Banderolenlage -Y"]
[41,null,"DW 126","Umgelegte Ecke"]
[41,null,"DW 127","Defekt"]
[41,null,"DW 128","Anzahl Trainingspakete"]
[41]
[41,"DW 150-199",null,"data to PLC"]
[41,null,"DW 150","Auftragsnummer"]
[41,null,"DW 151","xOffsetPack"]
[41,null,"DW 152","yOffsetPack"]
[41,null,"DW 153","xOffsetLightsourceLeft Track 1"]
[41,null,"DW 154","yOffsetLightsourceLeft Track 1"]
[41,null,"DW 155","xOffsetLightsourceRight Track 1"]
[41,null,"DW 156","yOffsetLightsourceRight Track 1"]
[41,null,"DW 157","xOffsetLightsourceLeft Track 2"]
[41,null,"DW 158","yOffsetLightsourceLeft Track 2"]
[41,null,"DW 159","xOffsetLightsourceRight Track 2"]
[41,null,"DW 160","yOffsetLightsourceRight Track 2"]
[41,null,"DW 161","LightsourcesWidth"]
[41,null,"DW 162","LightsourcesHeight"]
[41,null,"DW 163","lightsource0_Pulse Track 1"]
[41,null,"DW 164","lightsource0_Power Track 1"]
[41,null,"DW 165","lightsource1_Pulse Track 1"]
[41,null,"DW 166","lightsource1_Power Track 1"]
[41,null,"DW 167","lightsource2_Pulse Track 1"]
[41,null,"DW 168","lightsource2_Power Track 1"]
[41,null,"DW 169","lightsource3_Pulse Track 1"]
[41,null,"DW 170","lightsource3_Power Track 1"]
[41,null,"DW 171","lightsource0_Pulse Track 2"]
[41,null,"DW 172","lightsource0_Power Track 2"]
[41,null,"DW 173","lightsource1_Pulse Track 2"]
[41,null,"DW 174","lightsource1_Power Track 2"]
[41,null,"DW 175","lightsource2_Pulse Track 2"]
[41,null,"DW 176","lightsource2_Power Track 2"]
[41,null,"DW 177","lightsource3_Pulse Track 2"]
[41,null,"DW 178","lightsource3_Power Track 2"]
[41]
[41,null,"DW 180","Schalter"]
[41,null,"Bit 0","Toleranz Banderolenlage / ein"]
[41,null,"Bit 1","Umgelegte Ecken / ein"]
[41,null,"Bit 2","Defekt / ein"]
[41,null,"Bit 3","Verdrehung / ein"]
[41]
[41,null,"DW 181","xPosition track 1"]
[41,null,"DW 182","yPosition track 1"]
[41,null,"DW 183","xPosition track 2"]
[41,null,"DW 184","yPosition track 2"]
[41,null,"DW 185","Width"]
[41,null,"DW 186","Height"]
[41,null,"DW 187","Rotation"]
[41,null,"DW 188","HoloMaskX"]
[41,null,"DW 189","HoloMaskY"]
[41,null,"DW 190","HoloMaskWidth"]
[41,null,"DW 191","HoloMaskHeight"]
[41,null,"DW 192","Toleranz Banderolenlage +X"]
[41,null,"DW 193","Toleranz Banderolenlage -X"]
[41,null,"DW 194","Toleranz Banderolenlage +Y"]
[41,null,"DW 195","Toleranz Banderolenlage -Y"]
[41,null,"DW 196","Umgelegte Ecke"]
[41,null,"DW 197","Defekt"]
[41,null,"DW 198","Anzahl Trainingspakete"]
[41]
[21,null,"Page 2"]
[41,"DW 220",null,"status communitcation"]
[41,"DW 221",null,"Schalter"]
[41]
[41,"DW 230-239",null,"handshake from PLC"]
[41,"DW 260-269",null,"handshake to PLC"]
[41,"DW 290-339",null,"data from PLC"]
[41,"DW 360-409",null,"data to PLC"]
[41]
[41]

{"sheet":"StampInspectionBoxer","index":86,"n_rows":55,"n_cols":7,"rows_kept":55,"flags":["formulas_cached_only"]}
["StampInspectionBoxer","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 425","Stamp Inspection Boxer 1st Machine "]
[21,"DB 426-429","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 425-429 Stamp Inspection Boxer"]
[21,"DB ###ADDR:425+1[MNR]:ADDR","Stamp Inspection Boxer ###MNR"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_bstampin<.m###MNR_bsi_aender>[B]{w}"]
[41]
[41,"DW 10",null,"status communitcation"]
[41,"DW 11",null,"Schalter"]
[41,null,"Bit 0","Teachen"]
[41,null,"Bit 1","Kalibrieren"]
[41,"DW 20-29",null,"handshake from PLC"]
[41,null,"DW 20","Auftragsnummer"]
[41,"DW 50-59",null,"handshake to PLC"]
[41,null,"DW 50","Auftragsnummer"]
[41,"DW 80-129",null,"data from PLC"]
[41,null,"DW 80","Auftragsnummer"]
[41,null,"DW 81","xOffsetPack"]
[41,null,"DW 82","yOffsetPack"]
[41,null,"DW 83","Taschenbreite"]
[41,null,"DW 84","Taschenhöhe"]
[41]
[41,null,"DW 110","Schalter"]
[41,null,"Bit 0","Toleranz Banderolenlage / ein"]
[41,null,"Bit 1","Verdrehung / ein"]
[41]
[41,null,"DW 111","Toleranz Banderolenlage +X"]
[41,null,"DW 112","Toleranz Banderolenlage -X"]
[41,null,"DW 113","Toleranz Banderolenlage +Y"]
[41,null,"DW 114","Toleranz Banderolenlage -Y"]
[41,null,"DW 115","Width"]
[41,null,"DW 116","Rotation"]
[41,null,"DW 117","Belichtungszeit"]
[41]
[41,"DW 150-199",null,"data to PLC"]
[41,null,"DW 150","Auftragsnummer"]
[41,null,"DW 151","xOffsetPack"]
[41,null,"DW 152","yOffsetPack"]
[41,null,"DW 153","Taschenbreite"]
[41,null,"DW 154","Taschenhöhe"]
[41]
[41,null,"DW 180","Schalter"]
[41,null,"Bit 0","Toleranz Banderolenlage / ein"]
[41,null,"Bit 1","Verdrehung / ein"]
[41]
[41,null,"DW 181","Toleranz Banderolenlage +X"]
[41,null,"DW 182","Toleranz Banderolenlage -X"]
[41,null,"DW 183","Toleranz Banderolenlage +Y"]
[41,null,"DW 184","Toleranz Banderolenlage -Y"]
[41,null,"DW 185","Width"]
[41,null,"DW 186","Rotation"]
[41]

{"sheet":"TopFold","index":87,"n_rows":75,"n_cols":7,"rows_kept":75,"flags":["formulas_cached_only"]}
["TopFold","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 430","Top Fold 1st Machine "]
[21,"DB 431-434","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 430-434 Top Fold"]
[21,"DB ###ADDR:430+1[MNR]:ADDR","Top Fold ###MNR"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_topfold<.m###MNR_tf_aender>[B]{w}"]
[41]
[41,"DW 10",null,"status communitcation"]
[41]
[41,"DD 20-99",null,"data from PLC"]
[41,null,"DD 20","Auftragsnummer"]
[41]
[41,null,null,"Folie"]
[41,null,"DD 22","Level"]
[41,null,"DD 24","Area"]
[41]
[41,null,null,"Folienfaltung"]
[41,null,"DD 30","Level"]
[41,null,"DD 32","Area"]
[41]
[41,null,null,"Folienkante"]
[41,null,"DD 38","Level"]
[41,null,"DD 40","Area"]
[41]
[41,null,null,"Kragen"]
[41,null,"DD 46","Anwesenheit"]
[41,null,"DD 48","Schwellwert min"]
[41,null,"DD 50","Schwellwert max"]
[41,null,"DD 52","Verschmutzung Area"]
[41,null,"DD 54","Toleranz min"]
[41,null,"DD 56","Toleranz max"]
[41]
[41,null,null,"Staublasche"]
[41,null,"DD 62","Abstand min"]
[41,null,"DD 64","Abstand max"]
[41]
[41,null,null,"Coupon"]
[41,null,"DD 70","Intensität min"]
[41,null,"DD 72","Intensität max"]
[41]
[41]
[41,"DD 140-239",null,"data to PLC"]
[41,null,"DD 140","Auftragsnummer"]
[41]
[41,null,null,"Folie"]
[41,null,"DD 142","Level"]
[41,null,"DD 144","Area"]
[41]
[41,null,null,"Folienfaltung"]
[41,null,"DD 150","Level"]
[41,null,"DD 152","Area"]
[41]
[41,null,null,"Folienkante"]
[41,null,"DD 158","Level"]
[41,null,"DD 160","Area"]
[41]
[41,null,null,"Kragen"]
[41,null,"DD 166","Anwesenheit"]
[41,null,"DD 168","Schwellwert min"]
[41,null,"DD 170","Schwellwert max"]
[41,null,"DD 172","Verschmutzung Area"]
[41,null,"DD 174","Toleranz min"]
[41,null,"DD 176","Toleranz max"]
[41]
[41,null,null,"Staublasche"]
[41,null,"DD 182","Abstand min"]
[41,null,"DD 184","Abstand max"]
[41]
[41,null,null,"Coupon"]
[41,null,"DD 190","Intensität min"]
[41,null,"DD 192","Intensität max"]
[41]

{"sheet":"FPI","index":88,"n_rows":24,"n_cols":7,"rows_kept":24,"flags":["formulas_cached_only"]}
["FPI","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 435","Stamp Inspection Boxer 1st Machine "]
[21,"DB 435-439","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 435-439 FPI"]
[21,"DB ###ADDR:435+1[MNR]:ADDR","FPI ###MNR"]
[41,"DW 0-49",null,"Visu"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_bstampin<.m###MNR_bsi_aender>[B]{w}"]
[41,"DW 1","Bit 0","Daten übertragen",null,null,"Ch1.###MNR_T_bstampin<.m###MNR_bsi_aender>[B]{w}"]
[41]
[41,"DW 10","Bit 0","Freigabe Easyteach"]
[41]
[41,"DW 50-59",null,"Communication"]
[41,null,"DW 50","status communitcation"]
[41]
[41,"DW 60-279",null,"Data from PLC"]
[41,null,"DD 60","Auftragsnummer"]
[41,null,"DW 120","Anzahl Trainingspakete"]
[41]
[41,"DW 280-499",null,"Data to PLC"]
[41,null,"DD 280","Auftragsnummer"]
[41,null,"DW 340","Anzahl Trainingspakete"]

{"sheet":"Frequenzumrichter","index":89,"n_rows":24,"n_cols":7,"rows_kept":24,"flags":["formulas_cached_only"]}
["Frequenzumrichter","MASCHINENABHAENGIG"]
[1,"###OVERVIEW",null,null,"Reserviert für HOL"]
[21,"DB 440","Stamp Inspection Boxer 1st Machine "]
[21,"DB 441-444","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 440-444 FPI"]
[21,"DB ###ADDR:440+1[MNR]:ADDR","FPI ###MNR"]
[41,"DW 0-49",null,"Visu"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_bstampin<.m###MNR_bsi_aender>[B]{w}"]
[41,"DW 1","Bit 0","Daten übertragen",null,null,"Ch1.###MNR_T_bstampin<.m###MNR_bsi_aender>[B]{w}"]
[41]
[41,"DW 10","Bit 0","Freigabe Easyteach"]
[41]
[41,"DW 50-59",null,"Communication"]
[41,null,"DW 50","status communitcation"]
[41]
[41,"DW 60-279",null,"Data from PLC"]
[41,null,"DD 60","Auftragsnummer"]
[41,null,"DW 120","Anzahl Trainingspakete"]
[41]
[41,"DW 280-499",null,"Data to PLC"]
[41,null,"DD 280","Auftragsnummer"]
[41,null,"DW 340","Anzahl Trainingspakete"]

{"sheet":"ClosureStampInspection","index":90,"n_rows":23,"n_cols":7,"rows_kept":23,"flags":["formulas_cached_only"]}
["ClosureStampInspection","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 445","Closure Stamp Inspection 1st Machine "]
[21,"DB 446-449","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 445-449 Closure Stamp Inspection"]
[21,"DB ###ADDR:445+1[MNR]:ADDR","Closure Stamp Inspection ###MNR"]
[41,"DW 0","Bit 0","geändert",null,null,"Ch1.###MNR_T_csi<.m###MNR__csi_aender>[B]{w}"]
[41,null,"Bit 1","geändert für Kamera",null,null,"Ch1.###MNR_T_csi<.m###MNR_csi_aenderka>[B]{w}"]
[41]
[41,"DW 10",null,"status communitcation"]
[41]
[41,"DD 20-99",null,"data from PLC"]
[41,null,"DD 20","Auftragsnummer"]
[41,null,"DD 34","Forcen der Ausgänge"]
[41,null,"DD 38","Area"]
[41]
[41]
[41,"DD 140-239",null,"data to PLC"]
[41,null,"DD 140","Auftragsnummer"]
[41,null,"DD 154","Forcen der Ausgänge"]
[41,null,"DD 158","Area"]

{"sheet":"LED_Diag","index":91,"n_rows":43,"n_cols":7,"rows_kept":43,"flags":["formulas_cached_only"]}
["LED_Diag","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 450","LooseEndDetector"]
[41,"DB 451-454","Loose End Detector Machine  2-5"]
[1,"###MAIN"]
[1,"DB450-454 Loose End Detector Diagnostic Taschen / Schächte"]
[21,"DB ###ADDR:450+1[MNR]:ADDR","Loose End Detector Diagnostic ###MNR"]
[41]
[21,"DW 10-130","Schächte Tabak"]
[41,"DW 10","Bit 0","Reset",null,null,"Ch1.T_led_diag<.led_d_st_reset>[B]{w}"]
[41,null,"Bit 1","Daten erzeugen",null,null,"Ch1.T_led_diag<.led_d_st_refresh>[B]{w}"]
[41,"DW 15",null,"Größe des Ringpuffers (optional)",null,null,"Ch1.T_led_diag<.led_d_st_ring>[W]{w}"]
[41,"DD 20",null,"Anzahl der Messungen (gut und schlecht)",null,null,"Ch1.T_led_diag<.led_d_st_anz_mess>[DW]{p}"]
[41,"DW 23",null,"Referenzposition",null,null,"Ch1.T_led_diag<.led_d_st_referenz>[W]{p}"]
[41,"DW 25",null,"Anzahl der fehlerhaften Messungen",null,null,"Ch1.T_led_diag<.led_d_st_anz_fehler>[DW]{p}"]
[41,"DW 30-130",null,"Tabakfehler Schacht 1-x",null,null,"Ch1.T_led_diag<.led_d_st_fehler>[W0-100]{p}"]
[41]
[21,"DW 140-260","Schächte Filter"]
[41,"DW 140","Bit 0","Reset",null,null,"Ch1.T_led_diag<.led_d_sf_reset>[B]{w}"]
[41,null,"Bit 1","Daten erzeugen",null,null,"Ch1.T_led_diag<.led_d_sf_refresh>[B]{w}"]
[41,"DW 145",null,"Größe des Ringpuffers (optional)",null,null,"Ch1.T_led_diag<.led_d_sf_ring>[W]{w}"]
[41,"DD 150",null,"Anzahl der Messungen (gut und schlecht)",null,null,"Ch1.T_led_diag<.led_d_sf_anz_mess>[DW]{p}"]
[41,"DW 153",null,"Referenzposition",null,null,"Ch1.T_led_diag<.led_d_sf_referenz>[W]{p}"]
[41,"DW 155",null,"Anzahl der fehlerhaften Messungen",null,null,"Ch1.T_led_diag<.led_d_sf_anz_fehler>[DW]{p}"]
[41,"DW 160-260",null,"Filterfehler Schacht 1-x",null,null,"Ch1.T_led_diag<.led_d_sf_fehler>[W0-100]{p}"]
[41]
[21,"DW 270-390","Taschen Tabak"]
[41,"DW 270","Bit 0","Reset",null,null,"Ch1.T_led_diag<.led_d_tt_reset>[B]{w}"]
[41,null,"Bit 1","Daten erzeugen",null,null,"Ch1.T_led_diag<.led_d_tt_refresh>[B]{w}"]
[41,"DW 275",null,"Größe des Ringpuffers (optional)",null,null,"Ch1.T_led_diag<.led_d_tt_ring>[W]{w}"]
[41,"DD 280",null,"Anzahl der Messungen (gut und schlecht)",null,null,"Ch1.T_led_diag<.led_d_tt_anz_mess>[DW]{p}"]
[41,"DW 283",null,"Referenzposition Revolver",null,null,"Ch1.T_led_diag<.led_d_tt_referenz>[W]{p}"]
[41,"DW 285",null,"Anzahl der fehlerhaften Messungen",null,null,"Ch1.T_led_diag<.led_d_tt_anz_fehler>[DW]{p}"]
[41,"DW 290-390",null,"Tabakfehler Tasche 1-x",null,null,"Ch1.T_led_diag<.led_d_tt_fehler>[W0-100]{p}"]
[41]
[21,"DW 400-510","Taschen Filter"]
[41,"DW 400","Bit 0","Reset",null,null,"Ch1.T_led_diag<.led_d_tf_reset>[B]{w}"]
[41,null,"Bit 1","Daten erzeugen",null,null,"Ch1.T_led_diag<.led_d_tf_refresh>[B]{w}"]
[41,"DW 405",null,"Größe des Ringpuffers (optional)",null,null,"Ch1.T_led_diag<.led_d_tf_ring>[W]{w}"]
[41,"DD 410",null,"Anzahl der Messungen (gut und schlecht)",null,null,"Ch1.T_led_diag<.led_d_tf_anz_mess>[DW]{p}"]
[41,"DW 413",null,"Referenzposition Revolver",null,null,"Ch1.T_led_diag<.led_d_tf_referenz>[W]{p}"]
[41,"DW 415",null,"Anzahl der fehlerhaften Messungen",null,null,"Ch1.T_led_diag<.led_d_tf_anz_fehler>[DW]{p}"]
[41,"DW 420-520",null,"Filterfehler Tasche 1-x",null,null,"Ch1.T_led_diag<.led_d_tf_fehler>[W0-100]{p}"]

{"sheet":"LED_Diag_Sensitiv","index":92,"n_rows":27,"n_cols":7,"rows_kept":27,"flags":["formulas_cached_only"]}
["LED_Diag_Sesitiv","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DBLEDADS 450","LooseEndDetector Sensitivity"]
[41,"DBLEDADS 451-454","Loose End Detector Machine  2-5"]
[1,"###MAIN"]
[1,"DBLEDADS 450-454 Loose End Detector Sensitivity"]
[21,"DBLEDADS ###ADDR:450+1[MNR]:ADDR","Loose End Detector Sesitivity ###MNR"]
[41]
[41,"DW 9",null,"Lebenszeichen",null,null,"Ch2.T_led_sens<.led_s_leben>[W]{p}"]
[41]
[21,"DW 10-130","LED Tabak"]
[41,"DW 10","Bit 0","Reset",null,null,"Ch2.T_led_sens<.led_s_t_reset>[B]{w}"]
[41,null,"Bit 1","Daten erzeugen",null,null,"Ch2.T_led_sens<.led_s_t_refresh>[B]{w}"]
[41,"DW 15",null,"Größe des Ringpuffers (optional)",null,null,"Ch2.T_led_sens<.led_s_t_ring>[W]{w}"]
[41,"DD 20",null,"Anzahl der Messungen (gut und schlecht)",null,null,"Ch2.T_led_sens<.led_s_t_anz_mess>[DW]{p}"]
[41,"DW 22",null,"Referenzposition",null,null,"Ch2.T_led_sens<.led_s_t_referenz>[W]{p}"]
[41,"DW 25",null,"Anzahl der Messungen",null,null,"Ch2.T_led_sens<.led_s_t_anz_fehler>[DW]{p}"]
[41,"DW 30-130",null,"Werte 0-100%",null,null,"Ch2.T_led_sens<.led_s_t_fehler>[W0-100]{p}"]
[41]
[21,"DW 140-260","LED Filter"]
[41,"DW 140","Bit 0","Reset",null,null,"Ch2.T_led_sens<.led_s_f_reset>[B]{w}"]
[41,null,"Bit 1","Daten erzeugen",null,null,"Ch2.T_led_sens<.led_s_f_refresh>[B]{w}"]
[41,"DW 145",null,"Größe des Ringpuffers (optional)",null,null,"Ch2.T_led_sens<.led_s_f_ring>[W]{w}"]
[41,"DD 150",null,"Anzahl der Messungen (gut und schlecht)",null,null,"Ch2.T_led_sens<.led_s_f_anz_mess>[DW]{p}"]
[41,"DW 152",null,"Referenzposition",null,null,"Ch2.T_led_sens<.led_s_f_referenz>[W]{p}"]
[41,"DW 155",null,"Anzahl der Messungen",null,null,"Ch2.T_led_sens<.led_s_f_anz_fehler>[DW]{p}"]
[41,"DW 160-260",null,"Werte 0-100%",null,null,"Ch2.T_led_sens<.led_s_f_fehler>[W0-100]{p}"]

{"sheet":"X520_MainPicture","index":93,"n_rows":23,"n_cols":7,"rows_kept":23,"flags":["formulas_cached_only"]}
["X520_MainPicture","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 500","Actual values Conveyor"]
[41,"DB 501-504","Actual values Machine  2-5"]
[1,"###MAIN"]
[null,"X520_MainPicture1_1"]
[1,"DB 500-504 Actual values Conveyor"]
[21,"DB ###ADDR:500+1[MNR]:ADDR","Actual values Conveyor ###MNR"]
[41,"DW 10","Bit 1","Status EOL 1 Warning",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_eol_zu>[W0]{p}"]
[41,null,"Bit 2","Status EOL 1 Fault"]
[41,"DW 11 - 14",null,"Status EOL 2-5",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_eol_zu>[W1-4]{p}"]
[41,"DW 20 - 28",null,"Status MPU 1- 9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_mpu_zu>[W0-8]{p}"]
[41,"DW 30 - 38",null,"Status, Guide 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_wei_zu>[W0-8]{p}"]
[41,"DW 40 - 48",null,"Status, Belt 1 Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_ba1_zu>[W0-8]{p}"]
[41,"DW 50 - 58",null,"Status, Belt 2 Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_ba2_zu>[W0-8]{p}"]
[41,"DW 60 - 68",null,"Status, Belt 3 Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_ba3_zu>[W0-8]{p}"]
[41,"DW 70 - 78",null,"Status, Belt 4 Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_ba4_zu>[W0-8]{p}"]
[41,"DW 80 - 88",null,"Status, Belt  5 Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_ba5_zu>[W0-8]{p}"]
[41,"DW 91 - 98",null,"Position (Belt 1-5) Guide 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_wei>[W0-8]{p}"]
[41]
[41,"DW 100 - 139","ConveyorSensor"]
[41,"DW 120-128",null,"Status, MPU feeder",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_mpuz_zu>[W0-8]{p}"]
[41,"DW 130-134",null,"Status, EOL feeder",null,null,"Ch1.###MNR_T_mp<.m###MNR_mp_eolz_zu>[W0-4]{p}"]

{"sheet":"ConveyorSensor","index":94,"n_rows":27,"n_cols":7,"rows_kept":27,"flags":["formulas_cached_only"]}
["XConveyorSensor","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 500","Actual values Conveyor"]
[41,"DB 501-504","Actual values Machine  2-5"]
[1,"###MAIN"]
[null,"X520_MainPicture1_1"]
[1,"DB 500-504 Actual values Conveyor"]
[21,"DB ###ADDR:500+1[MNR]:ADDR","Actual values Conveyor ###MNR"]
[41,"DW 10 - 99","520_MainPicture"]
[41]
[41,"DW 100","Bit 0","Sensor 1 MPU 1",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_sen_mpu>[W0]{p}"]
[41,null,"Bit 1","Sensor 2 MPU 1"]
[41,"DW 101-108",null,"Sensors MPU 2-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_sen_mpu>[W1-8]{p}"]
[41,"DW 110","Bit 0-8","Belt 1, run monitoring, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_spe_ba1>[W]{p}"]
[41,null,"Bit 9","Belt EOL, run monitoring "]
[41,"DW 111",null,"Belt 2, run monitoring, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_spe_ba2>[W]{p}"]
[41,"DW 112",null,"Belt 3, run monitoring, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_spe_ba3>[W]{p}"]
[41,"DW 113",null,"Belt 4, run monitoring, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_spe_ba4>[W]{p}"]
[41,"DW 114",null,"Belt 5, run monitoring, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_spe_ba5>[W]{p}"]
[41]
[41,"DW 115","Bit 0-8 ","Belt 1, Sensor 1-9 ",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_sen_ba1>[W]{p}"]
[41,null,"Bit 9","Belt 1, EOL sensor"]
[41,"DW 116",null,"Belt 2, sensor, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_sen_ba2>[W]{p}"]
[41,"DW 117",null,"Belt 3, sensor, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_sen_ba3>[W]{p}"]
[41,"DW 118",null,"Belt 4, sensor, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_sen_ba4>[W]{p}"]
[41,"DW 119",null,"Belt 5, sensor, Part 1-9",null,null,"Ch1.###MNR_T_mp<.m###MNR_con_sen_ba5>[W]{p}"]
[41,"DW 120 - 134","520_MainPicture"]

{"sheet":"PortalPallet","index":95,"n_rows":288,"n_cols":7,"rows_kept":288,"flags":["formulas_cached_only"]}
["PortalPallet","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 500","Pallet parameters 1st Machine"]
[41,"DB 500-504","Pallet parameters,Machine  2-5"]
[1,"###MAIN"]
[1,"DB 500-504 Parameter Paletten"]
[2,"DB ###ADDR:500+1[MNR]:ADDR","Pallet parameters ###MNR"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR_T_portpalp<.m###MNR_pp_aend>[B]{w}"]
[31,"DW10 – DW39",null,"Pallet station 1"]
[41,"DW 10",null,"Setpoint 1","PortalPallet.###MNR.Pallet1.10","###INDEX:PortalPallet.###MNR.Pallet1.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W0]{r}"]
[41,"DW 11",null,"Setpoint 2","PortalPallet.###MNR.Pallet1.11","###INDEX:PortalPallet.###MNR.Pallet1.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W1]{r}"]
[41,"DW 12",null,"Setpoint 3","PortalPallet.###MNR.Pallet1.12","###INDEX:PortalPallet.###MNR.Pallet1.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W2]{r}"]
[41,"DW 13",null,"Setpoint 4","PortalPallet.###MNR.Pallet1.13","###INDEX:PortalPallet.###MNR.Pallet1.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W3]{r}"]
[41,"DW 14",null,"Setpoint 5","PortalPallet.###MNR.Pallet1.14","###INDEX:PortalPallet.###MNR.Pallet1.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W4]{r}"]
[41,"DW 15",null,"Setpoint 6","PortalPallet.###MNR.Pallet1.15","###INDEX:PortalPallet.###MNR.Pallet1.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W5]{r}"]
[41,"DW 16",null,"Setpoint 7","PortalPallet.###MNR.Pallet1.16","###INDEX:PortalPallet.###MNR.Pallet1.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W6]{r}"]
[41,"DW 17",null,"Setpoint 8","PortalPallet.###MNR.Pallet1.17","###INDEX:PortalPallet.###MNR.Pallet1.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W7]{r}"]
[41,"DW 18",null,"Setpoint 9","PortalPallet.###MNR.Pallet1.18","###INDEX:PortalPallet.###MNR.Pallet1.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W8]{r}"]
[41,"DW 19",null,"Setpoint 10","PortalPallet.###MNR.Pallet1.19","###INDEX:PortalPallet.###MNR.Pallet1.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W9]{r}"]
[41,"DW 20",null,"Setpoint 11","PortalPallet.###MNR.Pallet1.20","###INDEX:PortalPallet.###MNR.Pallet1.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W10]{r}"]
[41,"DW 21",null,"Setpoint 12","PortalPallet.###MNR.Pallet1.21","###INDEX:PortalPallet.###MNR.Pallet1.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W11]{r}"]
[41,"DW 22",null,"Setpoint 13","PortalPallet.###MNR.Pallet1.22","###INDEX:PortalPallet.###MNR.Pallet1.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W12]{r}"]
[41,"DW 23",null,"Setpoint 14","PortalPallet.###MNR.Pallet1.23","###INDEX:PortalPallet.###MNR.Pallet1.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll1>[W13]{r}"]
[41,"DW 30",null,"Actual value 1","PortalPallet.###MNR.Pallet1.30","###INDEX:PortalPallet.###MNR.Pallet1.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist1>[W0]{p}"]
[41,"DW 31",null,"Actual value 2","PortalPallet.###MNR.Pallet1.31","###INDEX:PortalPallet.###MNR.Pallet1.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist1>[W1]{p}"]
[41,"DW 32",null,"Actual value 3","PortalPallet.###MNR.Pallet1.32","###INDEX:PortalPallet.###MNR.Pallet1.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist1>[W2]{p}"]
[41,"DW 33",null,"Actual value 4","PortalPallet.###MNR.Pallet1.33","###INDEX:PortalPallet.###MNR.Pallet1.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist1>[W3]{p}"]
[41,"DW 34",null,"Actual value 5","PortalPallet.###MNR.Pallet1.34","###INDEX:PortalPallet.###MNR.Pallet1.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist1>[W4]{p}"]
[41,"DW 38","Bit 0","Status bit","PortalPallet.###MNR.Pallet1.40","###INDEX:PortalPallet.###MNR.Pallet1.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit1>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet1.41","###INDEX:PortalPallet.###MNR.Pallet1.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet1.42","###INDEX:PortalPallet.###MNR.Pallet1.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet1.43","###INDEX:PortalPallet.###MNR.Pallet1.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet1.44","###INDEX:PortalPallet.###MNR.Pallet1.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet1.45","###INDEX:PortalPallet.###MNR.Pallet1.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet1.46","###INDEX:PortalPallet.###MNR.Pallet1.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet1.47","###INDEX:PortalPallet.###MNR.Pallet1.47:INDEX"]
[31,"DW40 – DW69",null,"Pallet station 2"]
[41,"DW 40",null,"Setpoint 1","PortalPallet.###MNR.Pallet2.10","###INDEX:PortalPallet.###MNR.Pallet2.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W0]{r}"]
[41,"DW 41",null,"Setpoint 2","PortalPallet.###MNR.Pallet2.11","###INDEX:PortalPallet.###MNR.Pallet2.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W1]{r}"]
[41,"DW 42",null,"Setpoint 3","PortalPallet.###MNR.Pallet2.12","###INDEX:PortalPallet.###MNR.Pallet2.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W2]{r}"]
[41,"DW 43",null,"Setpoint 4","PortalPallet.###MNR.Pallet2.13","###INDEX:PortalPallet.###MNR.Pallet2.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W3]{r}"]
[41,"DW 44",null,"Setpoint 5","PortalPallet.###MNR.Pallet2.14","###INDEX:PortalPallet.###MNR.Pallet2.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W4]{r}"]
[41,"DW 45",null,"Setpoint 6","PortalPallet.###MNR.Pallet2.15","###INDEX:PortalPallet.###MNR.Pallet2.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W5]{r}"]
[41,"DW 46",null,"Setpoint 7","PortalPallet.###MNR.Pallet2.16","###INDEX:PortalPallet.###MNR.Pallet2.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W6]{r}"]
[41,"DW 47",null,"Setpoint 8","PortalPallet.###MNR.Pallet2.17","###INDEX:PortalPallet.###MNR.Pallet2.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W7]{r}"]
[41,"DW 48",null,"Setpoint 9","PortalPallet.###MNR.Pallet2.18","###INDEX:PortalPallet.###MNR.Pallet2.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W8]{r}"]
[41,"DW 49",null,"Setpoint 10","PortalPallet.###MNR.Pallet2.19","###INDEX:PortalPallet.###MNR.Pallet2.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W9]{r}"]
[41,"DW 50",null,"Setpoint 11","PortalPallet.###MNR.Pallet2.20","###INDEX:PortalPallet.###MNR.Pallet2.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W10]{r}"]
[41,"DW 51",null,"Setpoint 12","PortalPallet.###MNR.Pallet2.21","###INDEX:PortalPallet.###MNR.Pallet2.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W11]{r}"]
[41,"DW 52",null,"Setpoint 13","PortalPallet.###MNR.Pallet2.22","###INDEX:PortalPallet.###MNR.Pallet2.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W12]{r}"]
[41,"DW 53",null,"Setpoint 14","PortalPallet.###MNR.Pallet2.23","###INDEX:PortalPallet.###MNR.Pallet2.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll2>[W13]{r}"]
[41,"DW 60",null,"Actual value 1","PortalPallet.###MNR.Pallet2.30","###INDEX:PortalPallet.###MNR.Pallet2.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist2>[W0]{p}"]
[41,"DW 61",null,"Actual value 2","PortalPallet.###MNR.Pallet2.31","###INDEX:PortalPallet.###MNR.Pallet2.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist2>[W1]{p}"]
[41,"DW 62",null,"Actual value 3","PortalPallet.###MNR.Pallet2.32","###INDEX:PortalPallet.###MNR.Pallet2.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist2>[W2]{p}"]
[41,"DW 63",null,"Actual value 4","PortalPallet.###MNR.Pallet2.33","###INDEX:PortalPallet.###MNR.Pallet2.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist2>[W3]{p}"]
[41,"DW 64",null,"Actual value 5","PortalPallet.###MNR.Pallet2.34","###INDEX:PortalPallet.###MNR.Pallet2.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist2>[W4]{p}"]
[41,"DW 68","Bit 0","Status bit","PortalPallet.###MNR.Pallet2.40","###INDEX:PortalPallet.###MNR.Pallet2.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit2>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet2.41","###INDEX:PortalPallet.###MNR.Pallet2.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet2.42","###INDEX:PortalPallet.###MNR.Pallet2.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet2.43","###INDEX:PortalPallet.###MNR.Pallet2.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet2.44","###INDEX:PortalPallet.###MNR.Pallet2.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet2.45","###INDEX:PortalPallet.###MNR.Pallet2.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet2.46","###INDEX:PortalPallet.###MNR.Pallet2.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet2.47","###INDEX:PortalPallet.###MNR.Pallet2.47:INDEX"]
[31,"DW70 – DW99","Pallet station 3"]
[41,"DW 70",null,"Setpoint 1","PortalPallet.###MNR.Pallet3.10","###INDEX:PortalPallet.###MNR.Pallet3.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W0]{r}"]
[41,"DW 71",null,"Setpoint 2","PortalPallet.###MNR.Pallet3.11","###INDEX:PortalPallet.###MNR.Pallet3.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W1]{r}"]
[41,"DW 72",null,"Setpoint 3","PortalPallet.###MNR.Pallet3.12","###INDEX:PortalPallet.###MNR.Pallet3.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W2]{r}"]
[41,"DW 73",null,"Setpoint 4","PortalPallet.###MNR.Pallet3.13","###INDEX:PortalPallet.###MNR.Pallet3.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W3]{r}"]
[41,"DW 74",null,"Setpoint 5","PortalPallet.###MNR.Pallet3.14","###INDEX:PortalPallet.###MNR.Pallet3.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W4]{r}"]
[41,"DW 75",null,"Setpoint 6","PortalPallet.###MNR.Pallet3.15","###INDEX:PortalPallet.###MNR.Pallet3.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W5]{r}"]
[41,"DW 76",null,"Setpoint 7","PortalPallet.###MNR.Pallet3.16","###INDEX:PortalPallet.###MNR.Pallet3.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W6]{r}"]
[41,"DW 77",null,"Setpoint 8","PortalPallet.###MNR.Pallet3.17","###INDEX:PortalPallet.###MNR.Pallet3.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W7]{r}"]
[41,"DW 78",null,"Setpoint 9","PortalPallet.###MNR.Pallet3.18","###INDEX:PortalPallet.###MNR.Pallet3.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W8]{r}"]
[41,"DW 79",null,"Setpoint 10","PortalPallet.###MNR.Pallet3.19","###INDEX:PortalPallet.###MNR.Pallet3.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W9]{r}"]
[41,"DW 80",null,"Setpoint 11","PortalPallet.###MNR.Pallet3.20","###INDEX:PortalPallet.###MNR.Pallet3.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W10]{r}"]
[41,"DW 81",null,"Setpoint 12","PortalPallet.###MNR.Pallet3.21","###INDEX:PortalPallet.###MNR.Pallet3.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W11]{r}"]
[41,"DW 82",null,"Setpoint 13","PortalPallet.###MNR.Pallet3.22","###INDEX:PortalPallet.###MNR.Pallet3.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W12]{r}"]
[41,"DW 83",null,"Setpoint 14","PortalPallet.###MNR.Pallet3.23","###INDEX:PortalPallet.###MNR.Pallet3.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll3>[W13]{r}"]
[41,"DW 90",null,"Actual value 1","PortalPallet.###MNR.Pallet3.30","###INDEX:PortalPallet.###MNR.Pallet3.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist3>[W0]{p}"]
[41,"DW 91",null,"Actual value 2","PortalPallet.###MNR.Pallet3.31","###INDEX:PortalPallet.###MNR.Pallet3.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist3>[W1]{p}"]
[41,"DW 92",null,"Actual value 3","PortalPallet.###MNR.Pallet3.32","###INDEX:PortalPallet.###MNR.Pallet3.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist3>[W2]{p}"]
[41,"DW 93",null,"Actual value 4","PortalPallet.###MNR.Pallet3.33","###INDEX:PortalPallet.###MNR.Pallet3.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist3>[W3]{p}"]
[41,"DW 94",null,"Actual value 5","PortalPallet.###MNR.Pallet3.34","###INDEX:PortalPallet.###MNR.Pallet3.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist3>[W4]{p}"]
[41,"DW 98","Bit 0","Status bit","PortalPallet.###MNR.Pallet3.40","###INDEX:PortalPallet.###MNR.Pallet3.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit3>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet3.41","###INDEX:PortalPallet.###MNR.Pallet3.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet3.42","###INDEX:PortalPallet.###MNR.Pallet3.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet3.43","###INDEX:PortalPallet.###MNR.Pallet3.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet3.44","###INDEX:PortalPallet.###MNR.Pallet3.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet3.45","###INDEX:PortalPallet.###MNR.Pallet3.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet3.46","###INDEX:PortalPallet.###MNR.Pallet3.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet3.47","###INDEX:PortalPallet.###MNR.Pallet3.47:INDEX"]
[31,"DW100 – DW129","Pallet station 4"]
[41,"DW 100",null,"Setpoint 1","PortalPallet.###MNR.Pallet4.10","###INDEX:PortalPallet.###MNR.Pallet4.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W0]{r}"]
[41,"DW 101",null,"Setpoint 2","PortalPallet.###MNR.Pallet4.11","###INDEX:PortalPallet.###MNR.Pallet4.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W1]{r}"]
[41,"DW 102",null,"Setpoint 3","PortalPallet.###MNR.Pallet4.12","###INDEX:PortalPallet.###MNR.Pallet4.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W2]{r}"]
[41,"DW 103",null,"Setpoint 4","PortalPallet.###MNR.Pallet4.13","###INDEX:PortalPallet.###MNR.Pallet4.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W3]{r}"]
[41,"DW 104",null,"Setpoint 5","PortalPallet.###MNR.Pallet4.14","###INDEX:PortalPallet.###MNR.Pallet4.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W4]{r}"]
[41,"DW 105",null,"Setpoint 6","PortalPallet.###MNR.Pallet4.15","###INDEX:PortalPallet.###MNR.Pallet4.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W5]{r}"]
[41,"DW 106",null,"Setpoint 7","PortalPallet.###MNR.Pallet4.16","###INDEX:PortalPallet.###MNR.Pallet4.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W6]{r}"]
[41,"DW 107",null,"Setpoint 8","PortalPallet.###MNR.Pallet4.17","###INDEX:PortalPallet.###MNR.Pallet4.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W7]{r}"]
[41,"DW 108",null,"Setpoint 9","PortalPallet.###MNR.Pallet4.18","###INDEX:PortalPallet.###MNR.Pallet4.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W8]{r}"]
[41,"DW 109",null,"Setpoint 10","PortalPallet.###MNR.Pallet4.19","###INDEX:PortalPallet.###MNR.Pallet4.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W9]{r}"]
[41,"DW 110",null,"Setpoint 11","PortalPallet.###MNR.Pallet4.20","###INDEX:PortalPallet.###MNR.Pallet4.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W10]{r}"]
[41,"DW 111",null,"Setpoint 12","PortalPallet.###MNR.Pallet4.21","###INDEX:PortalPallet.###MNR.Pallet4.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W11]{r}"]
[41,"DW 112",null,"Setpoint 13","PortalPallet.###MNR.Pallet4.22","###INDEX:PortalPallet.###MNR.Pallet4.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W12]{r}"]
[41,"DW 113",null,"Setpoint 14","PortalPallet.###MNR.Pallet4.23","###INDEX:PortalPallet.###MNR.Pallet4.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll4>[W13]{r}"]
[41,"DW 120",null,"Actual value 1","PortalPallet.###MNR.Pallet4.30","###INDEX:PortalPallet.###MNR.Pallet4.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist4>[W0]{p}"]
[41,"DW 121",null,"Actual value 2","PortalPallet.###MNR.Pallet4.31","###INDEX:PortalPallet.###MNR.Pallet4.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist4>[W1]{p}"]
[41,"DW 122",null,"Actual value 3","PortalPallet.###MNR.Pallet4.32","###INDEX:PortalPallet.###MNR.Pallet4.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist4>[W2]{p}"]
[41,"DW 123",null,"Actual value 4","PortalPallet.###MNR.Pallet4.33","###INDEX:PortalPallet.###MNR.Pallet4.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist4>[W3]{p}"]
[41,"DW 124",null,"Actual value 5","PortalPallet.###MNR.Pallet4.34","###INDEX:PortalPallet.###MNR.Pallet4.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist4>[W4]{p}"]
[41,"DW 128","Bit 0","Status bit","PortalPallet.###MNR.Pallet4.40","###INDEX:PortalPallet.###MNR.Pallet4.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit4>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet4.41","###INDEX:PortalPallet.###MNR.Pallet4.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet4.42","###INDEX:PortalPallet.###MNR.Pallet4.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet4.43","###INDEX:PortalPallet.###MNR.Pallet4.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet4.44","###INDEX:PortalPallet.###MNR.Pallet4.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet4.45","###INDEX:PortalPallet.###MNR.Pallet4.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet4.46","###INDEX:PortalPallet.###MNR.Pallet4.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet4.47","###INDEX:PortalPallet.###MNR.Pallet4.47:INDEX"]
[31,"DW130 – DW159","Pallet station 5"]
[41,"DW 130",null,"Setpoint 1","PortalPallet.###MNR.Pallet5.10","###INDEX:PortalPallet.###MNR.Pallet5.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W0]{r}"]
[41,"DW 131",null,"Setpoint 2","PortalPallet.###MNR.Pallet5.11","###INDEX:PortalPallet.###MNR.Pallet5.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W1]{r}"]
[41,"DW 132",null,"Setpoint 3","PortalPallet.###MNR.Pallet5.12","###INDEX:PortalPallet.###MNR.Pallet5.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W2]{r}"]
[41,"DW 133",null,"Setpoint 4","PortalPallet.###MNR.Pallet5.13","###INDEX:PortalPallet.###MNR.Pallet5.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W3]{r}"]
[41,"DW 134",null,"Setpoint 5","PortalPallet.###MNR.Pallet5.14","###INDEX:PortalPallet.###MNR.Pallet5.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W4]{r}"]
[41,"DW 135",null,"Setpoint 6","PortalPallet.###MNR.Pallet5.15","###INDEX:PortalPallet.###MNR.Pallet5.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W5]{r}"]
[41,"DW 136",null,"Setpoint 7","PortalPallet.###MNR.Pallet5.16","###INDEX:PortalPallet.###MNR.Pallet5.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W6]{r}"]
[41,"DW 137",null,"Setpoint 8","PortalPallet.###MNR.Pallet5.17","###INDEX:PortalPallet.###MNR.Pallet5.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W7]{r}"]
[41,"DW 138",null,"Setpoint 9","PortalPallet.###MNR.Pallet5.18","###INDEX:PortalPallet.###MNR.Pallet5.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W8]{r}"]
[41,"DW 139",null,"Setpoint 10","PortalPallet.###MNR.Pallet5.19","###INDEX:PortalPallet.###MNR.Pallet5.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W9]{r}"]
[41,"DW 140",null,"Setpoint 11","PortalPallet.###MNR.Pallet5.20","###INDEX:PortalPallet.###MNR.Pallet5.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W10]{r}"]
[41,"DW 141",null,"Setpoint 12","PortalPallet.###MNR.Pallet5.21","###INDEX:PortalPallet.###MNR.Pallet5.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W11]{r}"]
[41,"DW 142",null,"Setpoint 13","PortalPallet.###MNR.Pallet5.22","###INDEX:PortalPallet.###MNR.Pallet5.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W12]{r}"]
[41,"DW 143",null,"Setpoint 14","PortalPallet.###MNR.Pallet5.23","###INDEX:PortalPallet.###MNR.Pallet5.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll5>[W13]{r}"]
[41,"DW 150",null,"Actual value 1","PortalPallet.###MNR.Pallet5.30","###INDEX:PortalPallet.###MNR.Pallet5.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist5>[W0]{p}"]
[41,"DW 151",null,"Actual value 2","PortalPallet.###MNR.Pallet5.31","###INDEX:PortalPallet.###MNR.Pallet5.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist5>[W1]{p}"]
[41,"DW 152",null,"Actual value 3","PortalPallet.###MNR.Pallet5.32","###INDEX:PortalPallet.###MNR.Pallet5.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist5>[W2]{p}"]
[41,"DW 153",null,"Actual value 4","PortalPallet.###MNR.Pallet5.33","###INDEX:PortalPallet.###MNR.Pallet5.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist5>[W3]{p}"]
[41,"DW 154",null,"Actual value 5","PortalPallet.###MNR.Pallet5.34","###INDEX:PortalPallet.###MNR.Pallet5.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist5>[W4]{p}"]
[41,"DW 158","Bit 0","Status bit","PortalPallet.###MNR.Pallet5.40","###INDEX:PortalPallet.###MNR.Pallet5.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit5>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet5.41","###INDEX:PortalPallet.###MNR.Pallet5.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet5.42","###INDEX:PortalPallet.###MNR.Pallet5.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet5.43","###INDEX:PortalPallet.###MNR.Pallet5.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet5.44","###INDEX:PortalPallet.###MNR.Pallet5.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet5.45","###INDEX:PortalPallet.###MNR.Pallet5.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet5.46","###INDEX:PortalPallet.###MNR.Pallet5.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet5.47","###INDEX:PortalPallet.###MNR.Pallet5.47:INDEX"]
[31,"DW160 – DW189","Pallet station 6"]
[41,"DW 160",null,"Setpoint 1","PortalPallet.###MNR.Pallet6.10","###INDEX:PortalPallet.###MNR.Pallet6.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W0]{r}"]
[41,"DW 161",null,"Setpoint 2","PortalPallet.###MNR.Pallet6.11","###INDEX:PortalPallet.###MNR.Pallet6.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W1]{r}"]
[41,"DW 162",null,"Setpoint 3","PortalPallet.###MNR.Pallet6.12","###INDEX:PortalPallet.###MNR.Pallet6.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W2]{r}"]
[41,"DW 163",null,"Setpoint 4","PortalPallet.###MNR.Pallet6.13","###INDEX:PortalPallet.###MNR.Pallet6.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W3]{r}"]
[41,"DW 164",null,"Setpoint 5","PortalPallet.###MNR.Pallet6.14","###INDEX:PortalPallet.###MNR.Pallet6.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W4]{r}"]
[41,"DW 165",null,"Setpoint 6","PortalPallet.###MNR.Pallet6.15","###INDEX:PortalPallet.###MNR.Pallet6.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W5]{r}"]
[41,"DW 166",null,"Setpoint 7","PortalPallet.###MNR.Pallet6.16","###INDEX:PortalPallet.###MNR.Pallet6.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W6]{r}"]
[41,"DW 167",null,"Setpoint 8","PortalPallet.###MNR.Pallet6.17","###INDEX:PortalPallet.###MNR.Pallet6.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W7]{r}"]
[41,"DW 168",null,"Setpoint 9","PortalPallet.###MNR.Pallet6.18","###INDEX:PortalPallet.###MNR.Pallet6.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W8]{r}"]
[41,"DW 169",null,"Setpoint 10","PortalPallet.###MNR.Pallet6.19","###INDEX:PortalPallet.###MNR.Pallet6.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W9]{r}"]
[41,"DW 170",null,"Setpoint 11","PortalPallet.###MNR.Pallet6.20","###INDEX:PortalPallet.###MNR.Pallet6.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W10]{r}"]
[41,"DW 171",null,"Setpoint 12","PortalPallet.###MNR.Pallet6.21","###INDEX:PortalPallet.###MNR.Pallet6.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W11]{r}"]
[41,"DW 172",null,"Setpoint 13","PortalPallet.###MNR.Pallet6.22","###INDEX:PortalPallet.###MNR.Pallet6.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W12]{r}"]
[41,"DW 173",null,"Setpoint 14","PortalPallet.###MNR.Pallet6.23","###INDEX:PortalPallet.###MNR.Pallet6.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll6>[W13]{r}"]
[41,"DW 180",null,"Actual value 1","PortalPallet.###MNR.Pallet6.30","###INDEX:PortalPallet.###MNR.Pallet6.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist6>[W0]{p}"]
[41,"DW 181",null,"Actual value 2","PortalPallet.###MNR.Pallet6.31","###INDEX:PortalPallet.###MNR.Pallet6.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist6>[W1]{p}"]
[41,"DW 182",null,"Actual value 3","PortalPallet.###MNR.Pallet6.32","###INDEX:PortalPallet.###MNR.Pallet6.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist6>[W2]{p}"]
[41,"DW 183",null,"Actual value 4","PortalPallet.###MNR.Pallet6.33","###INDEX:PortalPallet.###MNR.Pallet6.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist6>[W3]{p}"]
[41,"DW 184",null,"Actual value 5","PortalPallet.###MNR.Pallet6.34","###INDEX:PortalPallet.###MNR.Pallet6.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist6>[W4]{p}"]
[41,"DW 188","Bit 0","Status bit","PortalPallet.###MNR.Pallet6.40","###INDEX:PortalPallet.###MNR.Pallet6.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit6>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet6.41","###INDEX:PortalPallet.###MNR.Pallet6.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet6.42","###INDEX:PortalPallet.###MNR.Pallet6.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet6.43","###INDEX:PortalPallet.###MNR.Pallet6.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet6.44","###INDEX:PortalPallet.###MNR.Pallet6.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet6.45","###INDEX:PortalPallet.###MNR.Pallet6.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet6.46","###INDEX:PortalPallet.###MNR.Pallet6.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet6.47","###INDEX:PortalPallet.###MNR.Pallet6.47:INDEX"]
[31,"DW190 – DW219","Pallet station 7"]
[41,"DW 190",null,"Setpoint 1","PortalPallet.###MNR.Pallet7.10","###INDEX:PortalPallet.###MNR.Pallet7.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W0]{r}"]
[41,"DW 191",null,"Setpoint 2","PortalPallet.###MNR.Pallet7.11","###INDEX:PortalPallet.###MNR.Pallet7.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W1]{r}"]
[41,"DW 192",null,"Setpoint 3","PortalPallet.###MNR.Pallet7.12","###INDEX:PortalPallet.###MNR.Pallet7.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W2]{r}"]
[41,"DW 193",null,"Setpoint 4","PortalPallet.###MNR.Pallet7.13","###INDEX:PortalPallet.###MNR.Pallet7.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W3]{r}"]
[41,"DW 194",null,"Setpoint 5","PortalPallet.###MNR.Pallet7.14","###INDEX:PortalPallet.###MNR.Pallet7.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W4]{r}"]
[41,"DW 195",null,"Setpoint 6","PortalPallet.###MNR.Pallet7.15","###INDEX:PortalPallet.###MNR.Pallet7.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W5]{r}"]
[41,"DW 196",null,"Setpoint 7","PortalPallet.###MNR.Pallet7.16","###INDEX:PortalPallet.###MNR.Pallet7.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W6]{r}"]
[41,"DW 197",null,"Setpoint 8","PortalPallet.###MNR.Pallet7.17","###INDEX:PortalPallet.###MNR.Pallet7.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W7]{r}"]
[41,"DW 198",null,"Setpoint 9","PortalPallet.###MNR.Pallet7.18","###INDEX:PortalPallet.###MNR.Pallet7.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W8]{r}"]
[41,"DW 199",null,"Setpoint 10","PortalPallet.###MNR.Pallet7.19","###INDEX:PortalPallet.###MNR.Pallet7.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W9]{r}"]
[41,"DW 200",null,"Setpoint 11","PortalPallet.###MNR.Pallet7.20","###INDEX:PortalPallet.###MNR.Pallet7.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W10]{r}"]
[41,"DW 201",null,"Setpoint 12","PortalPallet.###MNR.Pallet7.21","###INDEX:PortalPallet.###MNR.Pallet7.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W11]{r}"]
[41,"DW 202",null,"Setpoint 13","PortalPallet.###MNR.Pallet7.22","###INDEX:PortalPallet.###MNR.Pallet7.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W12]{r}"]
[41,"DW 203",null,"Setpoint 14","PortalPallet.###MNR.Pallet7.23","###INDEX:PortalPallet.###MNR.Pallet7.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll7>[W13]{r}"]
[41,"DW 210",null,"Actual value 1","PortalPallet.###MNR.Pallet7.30","###INDEX:PortalPallet.###MNR.Pallet7.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist7>[W0]{p}"]
[41,"DW 211",null,"Actual value 2","PortalPallet.###MNR.Pallet7.31","###INDEX:PortalPallet.###MNR.Pallet7.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist7>[W1]{p}"]
[41,"DW 212",null,"Actual value 3","PortalPallet.###MNR.Pallet7.32","###INDEX:PortalPallet.###MNR.Pallet7.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist7>[W2]{p}"]
[41,"DW 213",null,"Actual value 4","PortalPallet.###MNR.Pallet7.33","###INDEX:PortalPallet.###MNR.Pallet7.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist7>[W3]{p}"]
[41,"DW 214",null,"Actual value 5","PortalPallet.###MNR.Pallet7.34","###INDEX:PortalPallet.###MNR.Pallet7.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist7>[W4]{p}"]
[41,"DW 218","Bit 0","Status bit","PortalPallet.###MNR.Pallet7.40","###INDEX:PortalPallet.###MNR.Pallet7.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit7>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet7.41","###INDEX:PortalPallet.###MNR.Pallet7.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet7.42","###INDEX:PortalPallet.###MNR.Pallet7.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet7.43","###INDEX:PortalPallet.###MNR.Pallet7.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet7.44","###INDEX:PortalPallet.###MNR.Pallet7.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet7.45","###INDEX:PortalPallet.###MNR.Pallet7.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet7.46","###INDEX:PortalPallet.###MNR.Pallet7.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet7.47","###INDEX:PortalPallet.###MNR.Pallet7.47:INDEX"]
[31,"DW220 – DW249","Pallet station 8"]
[41,"DW 220",null,"Setpoint 1","PortalPallet.###MNR.Pallet8.10","###INDEX:PortalPallet.###MNR.Pallet8.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W0]{r}"]
[41,"DW 221",null,"Setpoint 2","PortalPallet.###MNR.Pallet8.11","###INDEX:PortalPallet.###MNR.Pallet8.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W1]{r}"]
[41,"DW 222",null,"Setpoint 3","PortalPallet.###MNR.Pallet8.12","###INDEX:PortalPallet.###MNR.Pallet8.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W2]{r}"]
[41,"DW 223",null,"Setpoint 4","PortalPallet.###MNR.Pallet8.13","###INDEX:PortalPallet.###MNR.Pallet8.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W3]{r}"]
[41,"DW 224",null,"Setpoint 5","PortalPallet.###MNR.Pallet8.14","###INDEX:PortalPallet.###MNR.Pallet8.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W4]{r}"]
[41,"DW 225",null,"Setpoint 6","PortalPallet.###MNR.Pallet8.15","###INDEX:PortalPallet.###MNR.Pallet8.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W5]{r}"]
[41,"DW 226",null,"Setpoint 7","PortalPallet.###MNR.Pallet8.16","###INDEX:PortalPallet.###MNR.Pallet8.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W6]{r}"]
[41,"DW 227",null,"Setpoint 8","PortalPallet.###MNR.Pallet8.17","###INDEX:PortalPallet.###MNR.Pallet8.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W7]{r}"]
[41,"DW 228",null,"Setpoint 9","PortalPallet.###MNR.Pallet8.18","###INDEX:PortalPallet.###MNR.Pallet8.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W8]{r}"]
[41,"DW 229",null,"Setpoint 10","PortalPallet.###MNR.Pallet8.19","###INDEX:PortalPallet.###MNR.Pallet8.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W9]{r}"]
[41,"DW 230",null,"Setpoint 11","PortalPallet.###MNR.Pallet8.20","###INDEX:PortalPallet.###MNR.Pallet8.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W10]{r}"]
[41,"DW 231",null,"Setpoint 12","PortalPallet.###MNR.Pallet8.21","###INDEX:PortalPallet.###MNR.Pallet8.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W11]{r}"]
[41,"DW 232",null,"Setpoint 13","PortalPallet.###MNR.Pallet8.22","###INDEX:PortalPallet.###MNR.Pallet8.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W12]{r}"]
[41,"DW 233",null,"Setpoint 14","PortalPallet.###MNR.Pallet8.23","###INDEX:PortalPallet.###MNR.Pallet8.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll8>[W13]{r}"]
[41,"DW 240",null,"Actual value 1","PortalPallet.###MNR.Pallet8.30","###INDEX:PortalPallet.###MNR.Pallet8.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist8>[W0]{p}"]
[41,"DW 241",null,"Actual value 2","PortalPallet.###MNR.Pallet8.31","###INDEX:PortalPallet.###MNR.Pallet8.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist8>[W1]{p}"]
[41,"DW 242",null,"Actual value 3","PortalPallet.###MNR.Pallet8.32","###INDEX:PortalPallet.###MNR.Pallet8.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist8>[W2]{p}"]
[41,"DW 243",null,"Actual value 4","PortalPallet.###MNR.Pallet8.33","###INDEX:PortalPallet.###MNR.Pallet8.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist8>[W3]{p}"]
[41,"DW 244",null,"Actual value 5","PortalPallet.###MNR.Pallet8.34","###INDEX:PortalPallet.###MNR.Pallet8.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist8>[W4]{p}"]
[41,"DW 248","Bit 0","Status bit","PortalPallet.###MNR.Pallet8.40","###INDEX:PortalPallet.###MNR.Pallet8.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit8>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet8.41","###INDEX:PortalPallet.###MNR.Pallet8.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet8.42","###INDEX:PortalPallet.###MNR.Pallet8.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet8.43","###INDEX:PortalPallet.###MNR.Pallet8.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet8.44","###INDEX:PortalPallet.###MNR.Pallet8.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet8.45","###INDEX:PortalPallet.###MNR.Pallet8.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet8.46","###INDEX:PortalPallet.###MNR.Pallet8.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet8.47","###INDEX:PortalPallet.###MNR.Pallet8.47:INDEX"]
[31,"DW250 – DW279","Pallet station 9"]
[41,"DW 250",null,"Setpoint 1","PortalPallet.###MNR.Pallet9.10","###INDEX:PortalPallet.###MNR.Pallet9.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W0]{r}"]
[41,"DW 251",null,"Setpoint 2","PortalPallet.###MNR.Pallet9.11","###INDEX:PortalPallet.###MNR.Pallet9.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W1]{r}"]
[41,"DW 252",null,"Setpoint 3","PortalPallet.###MNR.Pallet9.12","###INDEX:PortalPallet.###MNR.Pallet9.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W2]{r}"]
[41,"DW 253",null,"Setpoint 4","PortalPallet.###MNR.Pallet9.13","###INDEX:PortalPallet.###MNR.Pallet9.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W3]{r}"]
[41,"DW 254",null,"Setpoint 5","PortalPallet.###MNR.Pallet9.14","###INDEX:PortalPallet.###MNR.Pallet9.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W4]{r}"]
[41,"DW 255",null,"Setpoint 6","PortalPallet.###MNR.Pallet9.15","###INDEX:PortalPallet.###MNR.Pallet9.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W5]{r}"]
[41,"DW 256",null,"Setpoint 7","PortalPallet.###MNR.Pallet9.16","###INDEX:PortalPallet.###MNR.Pallet9.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W6]{r}"]
[41,"DW 257",null,"Setpoint 8","PortalPallet.###MNR.Pallet9.17","###INDEX:PortalPallet.###MNR.Pallet9.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W7]{r}"]
[41,"DW 258",null,"Setpoint 9","PortalPallet.###MNR.Pallet9.18","###INDEX:PortalPallet.###MNR.Pallet9.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W8]{r}"]
[41,"DW 259",null,"Setpoint 10","PortalPallet.###MNR.Pallet9.19","###INDEX:PortalPallet.###MNR.Pallet9.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W9]{r}"]
[41,"DW 260",null,"Setpoint 11","PortalPallet.###MNR.Pallet9.20","###INDEX:PortalPallet.###MNR.Pallet9.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W10]{r}"]
[41,"DW 261",null,"Setpoint 12","PortalPallet.###MNR.Pallet9.21","###INDEX:PortalPallet.###MNR.Pallet9.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W11]{r}"]
[41,"DW 262",null,"Setpoint 13","PortalPallet.###MNR.Pallet9.22","###INDEX:PortalPallet.###MNR.Pallet9.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W12]{r}"]
[41,"DW 263",null,"Setpoint 14","PortalPallet.###MNR.Pallet9.23","###INDEX:PortalPallet.###MNR.Pallet9.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll9>[W13]{r}"]
[41,"DW 270",null,"Actual value 1","PortalPallet.###MNR.Pallet9.30","###INDEX:PortalPallet.###MNR.Pallet9.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist9>[W0]{p}"]
[41,"DW 271",null,"Actual value 2","PortalPallet.###MNR.Pallet9.31","###INDEX:PortalPallet.###MNR.Pallet9.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist9>[W1]{p}"]
[41,"DW 272",null,"Actual value 3","PortalPallet.###MNR.Pallet9.32","###INDEX:PortalPallet.###MNR.Pallet9.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist9>[W2]{p}"]
[41,"DW 273",null,"Actual value 4","PortalPallet.###MNR.Pallet9.33","###INDEX:PortalPallet.###MNR.Pallet9.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist9>[W3]{p}"]
[41,"DW 274",null,"Actual value 5","PortalPallet.###MNR.Pallet9.34","###INDEX:PortalPallet.###MNR.Pallet9.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist9>[W4]{p}"]
[41,"DW 278","Bit 0","Status bit","PortalPallet.###MNR.Pallet9.40","###INDEX:PortalPallet.###MNR.Pallet9.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit9>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet9.41","###INDEX:PortalPallet.###MNR.Pallet9.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet9.42","###INDEX:PortalPallet.###MNR.Pallet9.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet9.43","###INDEX:PortalPallet.###MNR.Pallet9.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet9.44","###INDEX:PortalPallet.###MNR.Pallet9.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet9.45","###INDEX:PortalPallet.###MNR.Pallet9.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet9.46","###INDEX:PortalPallet.###MNR.Pallet9.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet9.47","###INDEX:PortalPallet.###MNR.Pallet9.47:INDEX"]
[31,"DW280 – DW309","Pallet station 10"]
[41,"DW 280",null,"Setpoint 1","PortalPallet.###MNR.Pallet10.10","###INDEX:PortalPallet.###MNR.Pallet10.10:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W0]{r}"]
[41,"DW 281",null,"Setpoint 2","PortalPallet.###MNR.Pallet10.11","###INDEX:PortalPallet.###MNR.Pallet10.11:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W1]{r}"]
[41,"DW 282",null,"Setpoint 3","PortalPallet.###MNR.Pallet10.12","###INDEX:PortalPallet.###MNR.Pallet10.12:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W2]{r}"]
[41,"DW 283",null,"Setpoint 4","PortalPallet.###MNR.Pallet10.13","###INDEX:PortalPallet.###MNR.Pallet10.13:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W3]{r}"]
[41,"DW 284",null,"Setpoint 5","PortalPallet.###MNR.Pallet10.14","###INDEX:PortalPallet.###MNR.Pallet10.14:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W4]{r}"]
[41,"DW 285",null,"Setpoint 6","PortalPallet.###MNR.Pallet10.15","###INDEX:PortalPallet.###MNR.Pallet10.15:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W5]{r}"]
[41,"DW 286",null,"Setpoint 7","PortalPallet.###MNR.Pallet10.16","###INDEX:PortalPallet.###MNR.Pallet10.16:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W6]{r}"]
[41,"DW 287",null,"Setpoint 8","PortalPallet.###MNR.Pallet10.17","###INDEX:PortalPallet.###MNR.Pallet10.17:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W7]{r}"]
[41,"DW 288",null,"Setpoint 9","PortalPallet.###MNR.Pallet10.18","###INDEX:PortalPallet.###MNR.Pallet10.18:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W8]{r}"]
[41,"DW 289",null,"Setpoint 10","PortalPallet.###MNR.Pallet10.19","###INDEX:PortalPallet.###MNR.Pallet10.19:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W9]{r}"]
[41,"DW 290",null,"Setpoint 11","PortalPallet.###MNR.Pallet10.20","###INDEX:PortalPallet.###MNR.Pallet10.20:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W10]{r}"]
[41,"DW 291",null,"Setpoint 12","PortalPallet.###MNR.Pallet10.21","###INDEX:PortalPallet.###MNR.Pallet10.21:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W11]{r}"]
[41,"DW 292",null,"Setpoint 13","PortalPallet.###MNR.Pallet10.22","###INDEX:PortalPallet.###MNR.Pallet10.22:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W12]{r}"]
[41,"DW 293",null,"Setpoint 14","PortalPallet.###MNR.Pallet10.23","###INDEX:PortalPallet.###MNR.Pallet10.23:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_soll10>[W13]{r}"]
[41,"DW 300",null,"Actual value 1","PortalPallet.###MNR.Pallet10.30","###INDEX:PortalPallet.###MNR.Pallet10.30:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist10>[W0]{p}"]
[41,"DW 301",null,"Actual value 2","PortalPallet.###MNR.Pallet10.31","###INDEX:PortalPallet.###MNR.Pallet10.31:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist10>[W1]{p}"]
[41,"DW 302",null,"Actual value 3","PortalPallet.###MNR.Pallet10.32","###INDEX:PortalPallet.###MNR.Pallet10.32:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist10>[W2]{p}"]
[41,"DW 303",null,"Actual value 4","PortalPallet.###MNR.Pallet10.33","###INDEX:PortalPallet.###MNR.Pallet10.33:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist10>[W3]{p}"]
[41,"DW 304",null,"Actual value 5","PortalPallet.###MNR.Pallet10.34","###INDEX:PortalPallet.###MNR.Pallet10.34:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_ist10>[W4]{p}"]
[41,"DW 308","Bit 0","Status bit","PortalPallet.###MNR.Pallet10.40","###INDEX:PortalPallet.###MNR.Pallet10.40:INDEX","Ch1.###MNR_T_portpalp<.m###MNR_pp_bit10>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalPallet.###MNR.Pallet10.41","###INDEX:PortalPallet.###MNR.Pallet10.41:INDEX"]
[41,null,"Bit 2","Status bit","PortalPallet.###MNR.Pallet10.42","###INDEX:PortalPallet.###MNR.Pallet10.42:INDEX"]
[41,null,"Bit 3","Status bit","PortalPallet.###MNR.Pallet10.43","###INDEX:PortalPallet.###MNR.Pallet10.43:INDEX"]
[41,null,"Bit 4","Status bit","PortalPallet.###MNR.Pallet10.44","###INDEX:PortalPallet.###MNR.Pallet10.44:INDEX"]
[41,null,"Bit 5","Status bit","PortalPallet.###MNR.Pallet10.45","###INDEX:PortalPallet.###MNR.Pallet10.45:INDEX"]
[41,null,"Bit 6","Status bit","PortalPallet.###MNR.Pallet10.46","###INDEX:PortalPallet.###MNR.Pallet10.46:INDEX"]
[41,null,"Bit 7","Status bit","PortalPallet.###MNR.Pallet10.47","###INDEX:PortalPallet.###MNR.Pallet10.47:INDEX"]

{"sheet":"ABSPalletSettings","index":96,"n_rows":33,"n_cols":7,"rows_kept":33,"flags":["formulas_cached_only"]}
["ABSPalletSettings"]
[1,"###OVERVIEW"]
[21,"DB 500","Pallet Settings"]
[41,"DB 500-504","Pallet Settings Machine  2-5"]
[1,"###MAIN"]
[1,"DB 500-504 Pallet Settings"]
[41,"DW 0","Bit 0","Parameters changed"]
[31,"DD10 – DD29",null,"Settings",null,null,"Ch1.###MNR_T_abs_set<.m###MNR_abs_set_aender>[B]{w}"]
[41,"DD10",null,"Anzahl Lagen","ABSPalletSettings.10","###INDEX:ABSPalletSettings.10:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW0]{r}"]
[41,"DD12",null,"Reihen pro Lage","ABSPalletSettings.11","###INDEX:ABSPalletSettings.11:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW1]{r}"]
[41,"DD14",null,"Stapel pro Lage","ABSPalletSettings.12","###INDEX:ABSPalletSettings.12:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW2]{r}"]
[41,"DD16",null,"Höhe der Palette","ABSPalletSettings.13","###INDEX:ABSPalletSettings.13:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW3]{r}"]
[41,"DD18",null,"Breite der Palette ","ABSPalletSettings.14","###INDEX:ABSPalletSettings.14:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW4]{r}"]
[41,"DD20",null,"Länge der Palette","ABSPalletSettings.15","###INDEX:ABSPalletSettings.15:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW5]{r}"]
[41,"DD22",null,"Stapelhöhe","ABSPalletSettings.16","###INDEX:ABSPalletSettings.16:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW6]{r}"]
[41,"DD24",null,"Stapelbreite","ABSPalletSettings.17","###INDEX:ABSPalletSettings.17:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW7]{r}"]
[41,"DD26",null,"Stapellänge","ABSPalletSettings.18","###INDEX:ABSPalletSettings.18:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW8]{r}"]
[41,"DD28",null,"Drehung des Stapels","ABSPalletSettings.19","###INDEX:ABSPalletSettings.19:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_set>[DW9]{r}"]
[41]
[41,"DW 30",null,"Achsen verfahren",null,null,"Ch1.###MNR_T_abs_set<.m###MNR_abs_achse>[W]{r}"]
[41,null,"Bit 0","X-Achse","ABSMovement.10","###INDEX:ABSMovement.10:INDEX"]
[41,null,"Bit 1","Y-Achse","ABSMovement.11","###INDEX:ABSMovement.11:INDEX"]
[41,null,"Bit 2","Z-Achse","ABSMovement.12","###INDEX:ABSMovement.12:INDEX"]
[41,null,"Bit 3","W-Achse","ABSMovement.13","###INDEX:ABSMovement.13:INDEX"]
[41,null,"Bit 4",null,"ABSMovement.14","###INDEX:ABSMovement.14:INDEX"]
[41,null,"Bit 5","5. Achse","ABSMovement.15","###INDEX:ABSMovement.15:INDEX"]
[41,"DD 32",null,"X-Achse Istwert",null,null,"Ch1.###MNR_T_abs_set<.m###MNR_abs_ist>[DW0]{r}"]
[41,"DD 34",null,"Y-Achse Istwert",null,null,"Ch1.###MNR_T_abs_set<.m###MNR_abs_ist>[DW1]{r}"]
[41,"DD 36",null,"Z-Achse Istwert",null,null,"Ch1.###MNR_T_abs_set<.m###MNR_abs_ist>[DW2]{r}"]
[41,"DD 38",null,"W-Achse Istwert",null,null,"Ch1.###MNR_T_abs_set<.m###MNR_abs_ist>[DW3]{r}"]
[41,"DW 40",null,"Anpassung Auto","ABSMovement.30","###INDEX:ABSMovement.30:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_achse_dreh>[W0]{r}"]
[41,"DW 41",null,"Anpassung Tippen","ABSMovement.31","###INDEX:ABSMovement.31:INDEX","Ch1.###MNR_T_abs_set<.m###MNR_abs_achse_dreh>[W1]{r}"]
[41,"DD 50",null,"5.Achse Istwert",null,null,"Ch1.###MNR_T_abs_set<.m###MNR_abs_ist5>[DW]{r}"]

{"sheet":"LooseEndCalibrate","index":97,"n_rows":113,"n_cols":7,"rows_kept":113,"flags":["formulas_cached_only"]}
["LooseEndCalibrate"]
[1,"###OVERVIEW"]
[21,"DB 500","Loose End BO"]
[41,"DB 501-504","Loose End BO Machine  2-5"]
[1,"###MAIN"]
[1,"DB 500-504 Loose End BO"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_geaen>[B]{w}"]
[41]
[41,"DW 10-13",null,"reserve 1-4",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve1>[W0-3]{r}"]
[41,"DW 14-29",null,"layer",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_layer>[W0-15]{r}"]
[41,"DW 30",null,"test_head",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_test_head>[W]{r}"]
[41,"DW 31",null,"reserve41",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve41>[W]{r}"]
[41,"DW 32",null,"reserve5",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve5>[W]{r}"]
[41,"DW 33",null,"send_receive_error",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_send_receive_error>[W]{r}"]
[41,"DW 34",null,"reserve6",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve6>[W]{r}"]
[41,"DW 35",null,"reservey",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reservey>[W]{r}"]
[41,"DW 36",null,"limit_faulty_cigarette_3",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_faulty_cigarette_3>[W]{r}"]
[41,"DW 37",null,"limit_faulty_cigarette_1",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_faulty_cigarette_1>[W]{r}"]
[41,"DW 38",null,"limit_faulty_cigarette_4",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_faulty_cigarette_4>[W]{r}"]
[41,"DW 39",null,"limit_faulty_cigarette_2",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_faulty_cigarette_2>[W]{r}"]
[41,"DW 40",null,"limit_missing_ciga_3",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_missing_ciga_3>[W]{r}"]
[41,"DW 41",null,"limit_missing_ciga_1",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_missing_ciga_1>[W]{r}"]
[41,"DW 42",null,"limit_missing_ciga_4",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_missing_ciga_4>[W]{r}"]
[41,"DW 43",null,"limit_missing_ciga_2",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_missing_ciga_2>[W]{r}"]
[41,"DW 44",null,"checksum_paramter",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_checksum_paramter>[W]{r}"]
[41,"DW 45",null,"old_checksum_paramter",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_checksum_paramter>[W]{r}"]
[41,"DW 46",null,"new_checksum_paramter",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_new_checksum_paramter>[W]{r}"]
[41,"DW 47",null,"adj_error_layer",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_adj_error_layer>[W]{r}"]
[41,"DW 48",null,"adj_error_sensor",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_adj_error_sensor>[W]{r}"]
[41,"DW 49",null,"adj_error_number",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_adj_error_number>[W]{r}"]
[41,"DW 50",null,"adj_error_head",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_adj_error_head>[W]{r}"]
[41,"DW 51-54",null,"reserve_8-11",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve8>[W0-3]{r}"]
[41,"DW 55-310",null,"data",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_data>[W0-255]{r}"]
[41,"DW 311",null,"reference_value_head_3",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reference_value_head_3>[W]{r}"]
[41,"DW 312",null,"reference_value_head_1",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reference_value_head_1>[W]{r}"]
[41,"DW 313",null,"reference_value_head_4",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reference_value_head_4>[W]{r}"]
[41,"DW 314",null,"reference_value_head_2",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reference_value_head_2>[W]{r}"]
[41,"DW 315",null,"calcul_ref_value_head_3",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_calcul_ref_value_head_3>[W]{r}"]
[41,"DW 316",null,"calcul_ref_value_head_1",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_calcul_ref_value_head_1>[W]{r}"]
[41,"DW 317",null,"calcul_ref_value_head_4",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_calcul_ref_value_head_4>[W]{r}"]
[41,"DW 318",null,"calcul_ref_value_head_2",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_calcul_ref_value_head_2>[W]{r}"]
[41,"DW 319",null,"version_first",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_version_first>[W]{r}"]
[41,"DW 320",null,"version_second",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_version_second>[W]{r}"]
[41,"DW 321",null,"date_day",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_date_day>[W]{r}"]
[41,"DW 322",null,"date_month",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_date_month>[W]{r}"]
[41,"DW 323",null,"date_year",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_date_year>[W]{r}"]
[41,"DW 324",null,"amount_of_test_heads",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_amount_of_test_heads>[W]{r}"]
[41,"DW 325-327",null,"reserve12-13",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve12>[W0-2]{r}"]
[41,"DW 328",null,"reserve_single_test",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve_single_test>[W]{r}"]
[41,"DW 329",null,"cig_single_test_head",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_cig_single_test_head>[W]{r}"]
[41,"DW 330",null,"cig_single_test_layer",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_cig_single_test_layer>[W]{r}"]
[41,"DW 331",null,"cig_single_test_sensor",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_cig_single_test_sensor>[W]{r}"]
[41,"DW 332",null,"cig_single_test_bias",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_cig_single_test_bias>[W]{r}"]
[41,"DW 333",null,"cig_single_test_puls",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_cig_single_test_puls>[W]{r}"]
[41,"DW 334",null,"cig_single_test_on_off",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_cig_single_test_on_off>[W]{r}"]
[41,"DW 335",null,"reserve14",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve14>[W]{r}"]
[41,"DW 336",null,"error_bits_head_3_4",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_error_bits_head_3_4>[W]{r}"]
[41,"DW 337",null,"error_bits_head_1_2",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_error_bits_head_1_2>[W]{r}"]
[41,"DW 338",null,"automatic_trigger",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_automatic_trigger>[W]{r}"]
[41,"DW 339",null,"dummy",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_dummy>[W]{r}"]
[41,"DW 340",null,"checksume",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_checksume>[W]{r}"]
[41,"DW 341",null,"reserve19",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve19>[W]{r}"]
[41,"DW 342",null,"ind_ejection_statistics",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_ind_ejection_statistics>[W]{r}"]
[41,"DW 343",null,"indication_param_head_3",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_indication_param_head_3>[W]{r}"]
[41,"DW 344",null,"indication_param_head_1",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_indication_param_head_1>[W]{r}"]
[41,"DW 345",null,"indication_state_adj",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_indication_state_adj>[W]{r}"]
[41,"DW 346",null,"checksum_cig_codes",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_checksum_cig_codes>[W]{r}"]
[41,"DW 347",null,"old_checksum_cig_codes",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_checksum_cig_codes>[W]{r}"]
[41,"DW 348",null,"indication_param_head_4",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_indication_param_head_4>[W]{r}"]
[41,"DW 349",null,"indication_param_head_2",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_indication_param_head_2>[W]{r}"]
[41,"DW 350",null,"reserve17",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve17>[W]{r}"]
[41,"DW 351",null,"adjustment_start_stop",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_adjustment_start_stop>[W]{r}"]
[41,"DW 352",null,"adjustment",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_adjustment>[W]{r}"]
[41,"DW 353",null,"limit_system_fault",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_limit_system_fault>[W]{r}"]
[41,"DW 354-362",null,"reserve20-28",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve20>[W0-8]{r}"]
[41,"DW 363-490",null,"actual_adj_refl_values",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_actual_adj_refl_values>[W0-127]{r}"]
[41,"DW 491-506",null,"reserve30-45",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_reserve30>[W0-15]{r}"]
[41,"DW 507",null,"visu_byte_01",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_byte_01>[W]{r}"]
[41,"DW 508",null,"visu_byte_02",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_byte_02>[W]{r}"]
[41,"DW 509",null,"visu_byte_03",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_byte_03>[W]{r}"]
[41,"DW 510",null,"visu_byte_04",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_byte_04>[W]{r}"]
[41,"DW 511",null,"visu_byte_05",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_byte_05>[W]{r}"]
[41,"DW 512",null,"visu_byte_06",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_byte_06>[W]{r}"]
[41,"DW 513-521",null,"visu_reserve_byte_01-09",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_reserve_byte>[W0-8]{r}"]
[41,"DW 522",null,"visu_bit_info_01",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_bit_info_01>[W]{r}"]
[41,"DW 523",null,"visu_bit_info_17",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_bit_info_17>[W]{r}"]
[41,"DW 524",null,"visu_bit_info_33",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_bit_info_33>[W]{r}"]
[41,"DW 525",null,"visu_bit_info_49",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_visu_bit_info_49>[W]{r}"]
[41,"DW 526",null,"instruction 01 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_01_l>[W]{r}"]
[41,"DW 527",null,"instruction 01 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_01_h>[W]{r}"]
[41,"DW 528",null,"instruction 02 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_02_l>[W]{r}"]
[41,"DW 529",null,"instruction 02 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_02_h>[W]{r}"]
[41,"DW 530",null,"instruction 03 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_03_l>[W]{r}"]
[41,"DW 531",null,"instruction 03 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_03_h>[W]{r}"]
[41,"DW 532",null,"instruction 04 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_04_l>[W]{r}"]
[41,"DW 533",null,"instruction 04 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_04_h>[W]{r}"]
[41,"DW 534",null,"instruction 05 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_05_l>[W]{r}"]
[41,"DW 535",null,"instruction 05 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_05_h>[W]{r}"]
[41,"DW 536",null,"instruction 06 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_06_l>[W]{r}"]
[41,"DW 537",null,"instruction 06 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_instruction_06_h>[W]{r}"]
[41,"DW 538",null,"old instruction 01 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_01_l>[W]{r}"]
[41,"DW 539",null,"old instruction 01 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_01_h>[W]{r}"]
[41,"DW 540",null,"old instruction 02 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_02_l>[W]{r}"]
[41,"DW 541",null,"old instruction 02 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_02_h>[W]{r}"]
[41,"DW 542",null,"old instruction 03 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_03_l>[W]{r}"]
[41,"DW 543",null,"old instruction 03 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_03_h>[W]{r}"]
[41,"DW 544",null,"old instruction 04 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_04_l>[W]{r}"]
[41,"DW 545",null,"old instruction 04 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_04_h>[W]{r}"]
[41,"DW 546",null,"old instruction 05 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_05_l>[W]{r}"]
[41,"DW 547",null,"old instruction 05 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_05_h>[W]{r}"]
[41,"DW 548",null,"old instruction 06 lo",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_06_l>[W]{r}"]
[41,"DW 549",null,"old instruction 06 hi",null,null,"Ch1.###MNR_T_lebo<.m###MNR_lebo_old_instruction_06_h>[W]{r}"]
[41,"DW550-599",null,"Reserve"]

{"sheet":"WeigherFormat","index":98,"n_rows":34,"n_cols":7,"rows_kept":34,"flags":["formulas_cached_only"]}
["WeigherFormat"]
[1,"###OVERVIEW"]
[21,"DB 500","Checkweigher, size selection"]
[41,"DB 500-504","Checkweigher, size selection Machine  2-5"]
[1,"###MAIN"]
[1,"DB 500-504 Waage Formatanwahl"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.T_waageformat<.mwaageformat_aender>[B]{w}"]
[41,"DW 9",null,"Size number",null,null,"Ch1.T_waageformat<.mwaageformatnr>[W]{r}"]
[31,"DW10 – DW19",null,"Size data 1"]
[41,"DW 10",null,"Nominal weight","WeigherFormat.11","###INDEX:WeigherFormat.11:INDEX","Ch1.T_waageformat<.mwaageformat>[W0]{r}"]
[41,"DW 11",null,"Set weight, overload","WeigherFormat.12","###INDEX:WeigherFormat.12:INDEX","Ch1.T_waageformat<.mwaageformat>[W1]{r}"]
[41,"DW 12",null,"Deactivation, top-up","WeigherFormat.13","###INDEX:WeigherFormat.13:INDEX","Ch1.T_waageformat<.mwaageformat>[W2]{r}"]
[41,"DW 13",null,"Overload end weight","WeigherFormat.14","###INDEX:WeigherFormat.14:INDEX","Ch1.T_waageformat<.mwaageformat>[W3]{r}"]
[41,"DW 14",null,"Tobacco block","WeigherFormat.15","###INDEX:WeigherFormat.15:INDEX","Ch1.T_waageformat<.mwaageformat>[W4]{r}"]
[41,"DW 15",null,"Underload, tobacco block","WeigherFormat.16","###INDEX:WeigherFormat.16:INDEX","Ch1.T_waageformat<.mwaageformat>[W5]{r}"]
[41,"DW 16",null,"Nominal weight correction","WeigherFormat.17","###INDEX:WeigherFormat.17:INDEX","Ch1.T_waageformat<.mwaageformat>[W6]{r}"]
[41,"DW 17",null,"Startvalue compression motor","WeigherFormat.18","###INDEX:WeigherFormat.18:INDEX","Ch1.T_waageformat<.mwaageformat>[W7]{r}"]
[41,"DW 18",null,"Speed carding drum","WeigherFormat.19","###INDEX:WeigherFormat.19:INDEX","Ch1.T_waageformat<.mwaageformat>[W8]{r}"]
[41,"DW 19",null,"Reserve","WeigherFormat.20","###INDEX:WeigherFormat.20:INDEX","Ch1.T_waageformat<.mwaageformat>[W9]{r}"]
[41,"DW 20-29",null,"Fomatdaten 2",null,null,"Ch1.T_waageformat<.mwaageformat>[W10-19]{r}"]
[41,"DW 30-39",null,"Fomatdaten 3",null,null,"Ch1.T_waageformat<.mwaageformat>[W20-29]{r}"]
[41,"DW 40-49",null,"Fomatdaten 4",null,null,"Ch1.T_waageformat<.mwaageformat>[W30-39]{r}"]
[41,"DW 50-59",null,"Fomatdaten 5",null,null,"Ch1.T_waageformat<.mwaageformat>[W40-49]{r}"]
[41,"DW 60-69",null,"Fomatdaten 6",null,null,"Ch1.T_waageformat<.mwaageformat>[W50-59]{r}"]
[41,"DW 70-79",null,"Fomatdaten 7",null,null,"Ch1.T_waageformat<.mwaageformat>[W60-69]{r}"]
[41,"DW 80-89",null,"Fomatdaten 8",null,null,"Ch1.T_waageformat<.mwaageformat>[W70-79]{r}"]
[41,"DW 90-99",null,"Fomatdaten 9",null,null,"Ch1.T_waageformat<.mwaageformat>[W80-89]{r}"]
[41,"DW 100-109",null,"Fomatdaten 10",null,null,"Ch1.T_waageformat<.mwaageformat>[W90-99]{r}"]
[41,"DW 110-119",null,"Fomatdaten 11",null,null,"Ch1.T_waageformat<.mwaageformat>[W100-109]{r}"]
[41,"DW 120-129",null,"Fomatdaten 12",null,null,"Ch1.T_waageformat<.mwaageformat>[W110-119]{r}"]
[41,"DW 130-139",null,"Fomatdaten 13",null,null,"Ch1.T_waageformat<.mwaageformat>[W110-119]{r}"]
[41,"DW 140-149",null,"Fomatdaten 14",null,null,"Ch1.T_waageformat<.mwaageformat>[W120-129]{r}"]
[41,"DW 150-159",null,"Fomatdaten 15",null,null,"Ch1.T_waageformat<.mwaageformat>[W130-139]{r}"]
[41,"DW 160-169",null,"Fomatdaten 16",null,null,"Ch1.T_waageformat<.mwaageformat>[W140-149]{r}"]

{"sheet":"251_13_MainPicture","index":99,"n_rows":44,"n_cols":6,"rows_kept":44,"flags":["formulas_cached_only"]}
["251_13_MainPicture","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 501","Checkweigher, right"]
[41,"DB 501","Checkweigher, Machine 2"]
[21,"DB 503","Checkweigher, left"]
[41,"DB 504","Checkweigher, Machine 2"]
[1,"###MAIN"]
[1,"DB 501-504 Waage"]
[2,"DB ###ADDR:501+1[MNR]:ADDR","Checkweigher, right ###MNR"]
[41,"DW 0","Bit 0","Parameters changed"]
[41,"DW 9","Bit 14","Reset checkweigher"]
[31,"DW10 – DW19",null,"Weigher classes"]
[41,"DW 10",null,"Setpoint class","WeightClass.###MNR.12","###INDEX:WeightClass.###MNR.12:INDEX"]
[41,"DW 11",null,"Setpoint class","WeightClass.###MNR.13","###INDEX:WeightClass.###MNR.13:INDEX"]
[41,"DW 12",null,"Setpoint class","WeightClass.###MNR.14","###INDEX:WeightClass.###MNR.14:INDEX"]
[41,"DW 13",null,"Setpoint class","WeightClass.###MNR.15","###INDEX:WeightClass.###MNR.15:INDEX"]
[41,"DW 14",null,"Setpoint class","WeightClass.###MNR.16","###INDEX:WeightClass.###MNR.16:INDEX"]
[41,"DW 15",null,"Setpoint class","WeightClass.###MNR.17","###INDEX:WeightClass.###MNR.17:INDEX"]
[31,"DW20 – DW62",null,"Weighing cell"]
[41,"DW 20",null,"Fault output"]
[41,"DW 50","Bit 0","Switch, weighing cell","WeigherCell.###MNR.11","###INDEX:WeigherCell.###MNR.11:INDEX"]
[41,null,"Bit 1","Switch, weighing cell","WeigherCell.###MNR.12","###INDEX:WeigherCell.###MNR.12:INDEX"]
[41,null,"Bit 4","Switch, weighing cell","WeigherCell.###MNR.15","###INDEX:WeigherCell.###MNR.15:INDEX"]
[41,null,"Bit 5","Switch, weighing cell","WeigherCell.###MNR.16","###INDEX:WeigherCell.###MNR.16:INDEX"]
[41,"DW 51",null,"Setpoint, weighing cell","WeigherCell.###MNR.21","###INDEX:WeigherCell.###MNR.21:INDEX"]
[41,"DW 55",null,"Setpoint, weighing cell","WeigherCell.###MNR.25","###INDEX:WeigherCell.###MNR.25:INDEX"]
[41,"DW 57",null,"Setpoint, weighing cell","WeigherCell.###MNR.27","###INDEX:WeigherCell.###MNR.27:INDEX"]
[41,"DW 60",null,"Actual value"]
[31,"DW111 – DW119",null,"Short time measured values"]
[41,"DW 111",null,"Average weight","WeigherMessurementl.###MNR.10","###INDEX:WeigherMessurement.###MNR.10:INDEX"]
[41,"DW 112",null,"Standard deviation","WeigherMessurementl.###MNR.11","###INDEX:WeigherMessurement.###MNR.11:INDEX"]
[41,"DW 115",null,"No. of weighings","WeigherMessurementl.###MNR.12","###INDEX:WeigherMessurement.###MNR.12:INDEX"]
[31,"DW120 – DW121",null,"Long-term analysis"]
[41,"DW 120",null,"Average weight"]
[41,"DW 121",null,"Sigma"]
[31,"DW122 – DW129",null,"Long-term analysis DD"]
[41,"DD 122",null,"Total of weights"]
[41,"DD 124",null,"Weight ok"]
[41,"DD 126",null,"Weight, upper limit"]
[41,"DD 128",null,"Weight, lower limit"]
[31,"DW151 – DW160",null,"Actual value"]
[41,"DW 151-160",null,"Shift register weight"]
[41]
[2,"DB ###ADDR:503+1[MNR]:ADDR","Checkweigher, left ###MNR"]

{"sheet":"251_13_24_MainPicture","index":100,"n_rows":44,"n_cols":6,"rows_kept":44,"flags":["formulas_cached_only"]}
["251_13_24_MainPicture","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 501","Checkweigher, right"]
[41,"DB 501","Checkweigher, Machine 2"]
[21,"DB 503","Checkweigher, left"]
[41,"DB 504","Checkweigher, Machine 2"]
[1,"###MAIN"]
[1,"DB 501-504 Waage"]
[2,"DB ###ADDR:501+1[MNR]:ADDR","Checkweigher, right ###MNR"]
[41,"DW 0","Bit 0","Parameters changed"]
[41,"DW 9","Bit 14","Reset checkweigher"]
[31,"DW10 – DW19",null,"Weight classes"]
[41,"DW 10",null,"Setpoint class","WeightClass.###MNR.12","###INDEX:WeightClass.###MNR.12:INDEX"]
[41,"DW 11",null,"Setpoint class","WeightClass.###MNR.13","###INDEX:WeightClass.###MNR.13:INDEX"]
[41,"DW 12",null,"Setpoint class","WeightClass.###MNR.14","###INDEX:WeightClass.###MNR.14:INDEX"]
[41,"DW 13",null,"Setpoint class","WeightClass.###MNR.15","###INDEX:WeightClass.###MNR.15:INDEX"]
[41,"DW 14",null,"Setpoint class","WeightClass.###MNR.16","###INDEX:WeightClass.###MNR.16:INDEX"]
[41,"DW 15",null,"Setpoint class","WeightClass.###MNR.17","###INDEX:WeightClass.###MNR.17:INDEX"]
[31,"DW20 – DW62",null,"Weighing cell"]
[41,"DW 20",null,"Fault output"]
[41,"DW 50","Bit 0","Switch, weighing cell","WeigherCell.###MNR.11","###INDEX:WeigherCell.###MNR.11:INDEX"]
[41,null,"Bit 1","Switch, weighing cell","WeigherCell.###MNR.12","###INDEX:WeigherCell.###MNR.12:INDEX"]
[41,null,"Bit 4","Switch, weighing cell","WeigherCell.###MNR.15","###INDEX:WeigherCell.###MNR.15:INDEX"]
[41,null,"Bit 5","Switch, weighing cell","WeigherCell.###MNR.16","###INDEX:WeigherCell.###MNR.16:INDEX"]
[41,"DW 51",null,"Setpoint, weighing cell","WeigherCell.###MNR.21","###INDEX:WeigherCell.###MNR.21:INDEX"]
[41,"DW 55",null,"Setpoint, weighing cell","WeigherCell.###MNR.25","###INDEX:WeigherCell.###MNR.25:INDEX"]
[41,"DW 57",null,"Setpoint, weighing cell","WeigherCell.###MNR.27","###INDEX:WeigherCell.###MNR.27:INDEX"]
[41,"DW 60",null,"Actual value"]
[31,"DW111 – DW119",null,"Short time measured values"]
[41,"DW 111",null,"Average weight","WeigherMessurementl.###MNR.10","###INDEX:WeigherMessurement.###MNR.10:INDEX"]
[41,"DW 112",null,"Standard deviation","WeigherMessurementl.###MNR.11","###INDEX:WeigherMessurement.###MNR.11:INDEX"]
[41,"DW 115",null,"No. of weighings","WeigherMessurementl.###MNR.12","###INDEX:WeigherMessurement.###MNR.12:INDEX"]
[31,"DW120 – DW121",null,"Long-term analysis"]
[41,"DW 120",null,"Average weight"]
[41,"DW 121",null,"Sigma"]
[31,"DW122 – DW129",null,"Long-term analysis DD"]
[41,"DD 122",null,"Total of weights"]
[41,"DD 124",null,"Weight ok"]
[41,"DD 126",null,"Weight, upper limit"]
[41,"DD 128",null,"Weight, lower limit"]
[31,"DW151 – DW160",null,"Actual value"]
[41,"DW 151-160",null,"Shift register weight"]
[41]
[2,"DB ###ADDR:503+1[MNR]:ADDR","Checkweigher, left ###MNR"]

{"sheet":"WeigherTobaccoBlock","index":101,"n_rows":23,"n_cols":7,"rows_kept":23,"flags":["formulas_cached_only"]}
["WeigherTobaccoBlock","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 505","Checkweigher, tobacco block"]
[41,"DB 506-509","Checkweigher, Machine 2"]
[1,"###MAIN"]
[1,"DB 505-509 Checkweigher, tobacco block"]
[2,"DB ###ADDR:505+1[MNR]:ADDR","Checkweigher, right ###MNR"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_aender>[B]{w}"]
[41,"DW 9","Bit 12","Reset set pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_ist_n1>[B]{r}"]
[41,null,"Bit 13","Reset actual pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_ist_n2>[B]{r}"]
[41,null,"Bit 14","Reset weights",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_ist_n3>[B]{r}"]
[41,"DW 111",null,"Average weight, set pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W0]{r}"]
[41,"DW 112",null,"Standard deviation, set pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W1]{r}"]
[41,"DW 115",null,"No. of weighings, set pulses ",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W4]{r}"]
[41,"DW 121",null,"Average weight, set pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W10]{r}"]
[41,"DW 122",null,"Standard deviation, set pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W11]{r}"]
[41,"DW 125",null,"No. of weighings, set pulses ",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W14]{r}"]
[41,"DW 131",null,"Average weight, weights",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W20]{r}"]
[41,"DW 132",null,"Standard deviation, weights",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W21]{r}"]
[41,"DW 135",null,"No. of weighings, weights",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_mess>[W24]{r}"]
[41,"DW 151-160",null,"Actual values, set pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_ist>[W0-9]{p}"]
[41,"DW 161-170",null,"Actual values, actual pulses",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_ist>[W10-19]{p}"]
[41,"DW 171-180",null,"Actual values, weights",null,null,"Ch1.###MNR_T_waage_m<.m###MNR_waage_ist>[W20-29]{p}"]

{"sheet":"ConveyorTimer","index":102,"n_rows":42,"n_cols":7,"rows_kept":42,"flags":["formulas_cached_only"]}
["ConveyorTimer","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 505","Setpoints Conveyor 1st Machine"]
[41,"DB 506-509","Setpoints Conveyor Machine  2-5"]
[1,"###MAIN"]
[1,"DB 505-509 Setpoints Conveyor"]
[21,"DB ###ADDR:505+1[MNR]:ADDR","Setpoints Conveyor ###MNR"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_aend>[B]{w}"]
[3,"DW 10-129","Times"]
[41,"DW 10-18",null,"Times Sensor 1 for MPU 1 – 9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W0-8]{r}"]
[41,"DW 20-28",null,"Times Sensor 2 for MPU 1 – 9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W10-18]{r}"]
[41,"DW 30-38",null,"Times Sensor 1-9 Belt 1",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W20-28]{r}"]
[41,"DW 39",null,"Times Sensor EOL Belt 1",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W29]{r}"]
[41,"DW 40-48",null,"Times Sensor 1-9 Belt 2",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W30-38]{r}"]
[41,"DW 49",null,"Times Sensor EOL Belt 2",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W39]{r}"]
[41,"DW 50-58",null,"Times Sensor 1-9 Belt 3",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W40-48]{r}"]
[41,"DW 59",null,"Times Sensor EOL Belt 3",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W49]{r}"]
[41,"DW 60-68",null,"Times Sensor 1-9 Belt 4",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W50-58]{r}"]
[41,"DW 69",null,"Times Sensor EOL Belt 4",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W59]{r}"]
[41,"DW 70-78",null,"Times Sensor 1-9 Belt 5",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W60-68]{r}"]
[41,"DW 79",null,"Times Sensor EOL Belt 5",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W69]{r}"]
[41,"DW 80-88",null,"Times run monitoring Belt 1 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W70-78]{r}"]
[41,"DW 89",null,"Times run monitoring EOL Belt 1",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W79]{r}"]
[41,"DW 90-98",null,"Times run monitoring Belt 2 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W80-88]{r}"]
[41,"DW 99",null,"Times run monitoring EOL Belt 2",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W89]{r}"]
[41,"DW 100-108",null,"Times run monitoring Belt 3 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W90-98]{r}"]
[41,"DW 109",null,"Times run monitoring EOL Belt 3",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W99]{r}"]
[41,"DW 110-118",null,"Times run monitoring Belt 4 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W100-108]{r}"]
[41,"DW 119",null,"Times run monitoring EOL Belt 4",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W109]{r}"]
[41,"DW 120-128",null,"Times run monitoring Belt 5 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W110-118]{r}"]
[41,"DW 129",null,"Times run monitoring EOL Belt 5",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W119]{r}"]
[3,"DW 130-179","Frequencies"]
[41,"DW 130",null,"Frequency EOL Belt 1",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W120]{r}"]
[41,"DW 131-139",null,"Frequencies Belt 1 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W121-129]{r}"]
[41,"DW 140",null,"Frequency EOL Part 2",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W130]{r}"]
[41,"DW 141-149",null,"Frequencies Belt 2 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W131-139]{r}"]
[41,"DW 150",null,"Frequency EOL Belt 3",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W140]{r}"]
[41,"DW 151-159",null,"Frequencies Belt 3 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W141-149]{r}"]
[41,"DW 160",null,"Frequency EOL Belt 4",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W150]{r}"]
[41,"DW 161-169",null,"Frequencies Belt 4 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W151-159]{r}"]
[41,"DW 170",null,"Frequency EOL Belt 5",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W150]{r}"]
[41,"DW 171-179",null,"Frequencies Belt 5 Part 1-9",null,null,"Ch1.###MNRT_T_mps<.m###MNR_con_soll_ze>[W161-169]{r}"]

{"sheet":"WeigherHistogram","index":103,"n_rows":93,"n_cols":6,"rows_kept":93,"flags":["formulas_cached_only"]}
["WeigherHistogram","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 510","Checkweigher histogram overview"]
[21,"DB 511","Checkweigher histogram, single, right"]
[41,"DB 512","Checkweigher histogram, single, right, Machine 2"]
[21,"DB 513","Checkweigher histogram, single, left"]
[41,"DB 514","Checkweigher histogram, single, left, Machine 2"]
[21,"DB 515","Checkweigher histogram, group"]
[41,"DB 516","Checkweigher histogram, group Machine 2"]
[1,"###MAIN"]
[1,"DB 510-516 Checkweigher histogram"]
[2,"DB 510","Checkweigher histogram overview"]
[41,"DW 1","Bit 0","Reset weight"]
[41,"DW 10",null,"Scale X, start"]
[41,"DW 11",null,"Scale X, end"]
[41,"DW 12",null,"Scale X, Limit 1"]
[41,"DW 13",null,"Scale X, Limit 2"]
[41,"DD 14",null,"Scale Y, value"]
[41,"DD 20",null,"Total, measured values"]
[41,"DW 27",null,"Sigma"]
[41,"DW 29",null,"Average value"]
[41,"DW 30-129",null,"Actual value 1- 100"]
[2,"DB ###ADDR:511+1[MNR]:ADDR","Checkweigher histogram, single, right###MNR"]
[2,"DB ###ADDR:513+1[MNR]:ADDR","Checkweigher histogram, single, left ###MNR"]
[2,"DB ###ADDR:515+1[MNR]:ADDR","Checkweigher histogram, group ###MNR"]
{"$rows_empty":17}
[31,"DW151 – DW160",null,"Actual value"]
[41,"DW 151-160",null,"Shift register weight"]
[41]
[2,"DB ###ADDR:503+1[MNR]:ADDR","Checkweigher left ###MNo"]
{"$rows_empty":11}
[2,"DB ###ADDR:501+1[MNR]:ADDR","Checkweigher right ###MNo"]
[41,"DW 0","Bit 0","Parameters changed"]
[41,"DW 9","Bit 14","Reset checkweigher"]
[31,"DW10 – DW19",null,"Weight classes"]
[41,"DW 10",null,"Setpoint class","WeightClass.###MNR.12","###INDEX:WeightClass.###MNR.12:INDEX"]
[41,"DW 11",null,"Setpoint class","WeightClass.###MNR.13","###INDEX:WeightClass.###MNR.13:INDEX"]
[41,"DW 12",null,"Setpoint class","WeightClass.###MNR.14","###INDEX:WeightClass.###MNR.14:INDEX"]
[41,"DW 13",null,"Setpoint class","WeightClass.###MNR.15","###INDEX:WeightClass.###MNR.15:INDEX"]
[41,"DW 14",null,"Setpoint class","WeightClass.###MNR.16","###INDEX:WeightClass.###MNR.16:INDEX"]
[41,"DW 15",null,"Setpoint class","WeightClass.###MNR.17","###INDEX:WeightClass.###MNR.17:INDEX"]
[31,"DW20 – DW62",null,"Weighing cell"]
[41,"DW 20",null,"Fault output"]
[41,"DW 50","Bit 0","Switch, weighing cell","WeigherCell.###MNR.11","###INDEX:WeigherCell.###MNR.11:INDEX"]
[41,null,"Bit 1","Switch, weighing cell","WeigherCell.###MNR.12","###INDEX:WeigherCell.###MNR.12:INDEX"]
[41,null,"Bit 4","Switch, weighing cell","WeigherCell.###MNR.15","###INDEX:WeigherCell.###MNR.15:INDEX"]
[41,null,"Bit 5","Switch, weighing cell","WeigherCell.###MNR.16","###INDEX:WeigherCell.###MNR.16:INDEX"]
[41,"DW 51",null,"Switch, weighing cell","WeigherCell.###MNR.21","###INDEX:WeigherCell.###MNR.21:INDEX"]
[41,"DW 55",null,"Switch, weighing cell","WeigherCell.###MNR.25","###INDEX:WeigherCell.###MNR.25:INDEX"]
[41,"DW 57",null,"Switch, weighing cell","WeigherCell.###MNR.27","###INDEX:WeigherCell.###MNR.27:INDEX"]
[41,"DW 60",null,"Actual value"]
[31,"DW111 – DW119",null,"Short time measured values"]
[41,"DW 111",null,"Average weight","WeigherMessurementl.###MNR.10","###INDEX:WeigherMessurement.###MNR.10:INDEX"]
[41,"DW 112",null,"Standard deviation","WeigherMessurementl.###MNR.11","###INDEX:WeigherMessurement.###MNR.11:INDEX"]
[41,"DW 115",null,"No. of weighings","WeigherMessurementl.###MNR.12","###INDEX:WeigherMessurement.###MNR.12:INDEX"]
[31,"DW120 – DW121",null,"Long-term analysis"]
[41,"DW 120",null,"Average weight"]
[41,"DW 121",null,"Sigma"]
[31,"DW122 – DW129",null,"Long-term analysis DD"]
[41,"DD 122",null,"Total weight"]
[41,"DD 124",null,"Weight ok"]
[41,"DD 126",null,"Weight, upper limit"]
[41,"DD 128",null,"Weight, lower limit"]
[31,"DW151 – DW160",null,"Actual value"]
[41,"DW 151-160",null,"Weight, shift register "]
[41]
[2,"DB ###ADDR:503+1[MNR]:ADDR","Checkweigher, left ###MNo"]

{"sheet":"PortalParameter","index":104,"n_rows":309,"n_cols":7,"rows_kept":309,"flags":["formulas_cached_only"]}
["PortalParameter","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 510","Portal parameters, 1st Machine"]
[null,"DB 511-514","Portal parameters, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 510-514 Portal parameters"]
[21,"DB ###ADDR:510+1[MNR]:ADDR","Portal parameters ###MNR"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR_T_portpara<.m###MNR_ppa_aend>[B]{w}"]
[31,"DW10 – DW49","Portal 1"]
[41,"DW 10",null,"Setpoint 1","PortalParameter.###MNR.Part1.10","###INDEX:PortalParameter.###MNR.Part1.10:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W0]{r}"]
[41,"DW 11",null,"Setpoint 2","PortalParameter.###MNR.Part1.11","###INDEX:PortalParameter.###MNR.Part1.11:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W1]{r}"]
[41,"DW 12",null,"Setpoint 3","PortalParameter.###MNR.Part1.12","###INDEX:PortalParameter.###MNR.Part1.12:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W2]{r}"]
[41,"DW 13",null,"Setpoint 4","PortalParameter.###MNR.Part1.13","###INDEX:PortalParameter.###MNR.Part1.13:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W3]{r}"]
[41,"DW 14",null,"Setpoint 5","PortalParameter.###MNR.Part1.14","###INDEX:PortalParameter.###MNR.Part1.14:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W4]{r}"]
[41,"DW 15",null,"Setpoint 6","PortalParameter.###MNR.Part1.15","###INDEX:PortalParameter.###MNR.Part1.15:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W5]{r}"]
[41,"DW 16",null,"Setpoint 7","PortalParameter.###MNR.Part1.16","###INDEX:PortalParameter.###MNR.Part1.16:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W6]{r}"]
[41,"DW 17",null,"Setpoint 8","PortalParameter.###MNR.Part1.17","###INDEX:PortalParameter.###MNR.Part1.17:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W7]{r}"]
[41,"DW 18",null,"Setpoint 9","PortalParameter.###MNR.Part1.18","###INDEX:PortalParameter.###MNR.Part1.18:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W8]{r}"]
[41,"DW 19",null,"Setpoint 10","PortalParameter.###MNR.Part1.19","###INDEX:PortalParameter.###MNR.Part1.19:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W9]{r}"]
[41,"DW 20",null,"Setpoint 11","PortalParameter.###MNR.Part1.20","###INDEX:PortalParameter.###MNR.Part1.20:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W10]{r}"]
[41,"DW 21",null,"Setpoint 12","PortalParameter.###MNR.Part1.21","###INDEX:PortalParameter.###MNR.Part1.21:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W11]{r}"]
[41,"DW 22",null,"Setpoint 13","PortalParameter.###MNR.Part1.22","###INDEX:PortalParameter.###MNR.Part1.22:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W12]{r}"]
[41,"DW 23",null,"Setpoint 14","PortalParameter.###MNR.Part1.23","###INDEX:PortalParameter.###MNR.Part1.23:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll1>[W13]{r}"]
[41,"DW 30",null,"Actual value 1","PortalParameter.###MNR.Part1.30","###INDEX:PortalParameter.###MNR.Part1.30:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W0]{p}"]
[41,"DW 31",null,"Actual value 2","PortalParameter.###MNR.Part1.31","###INDEX:PortalParameter.###MNR.Part1.31:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W1]{p}"]
[41,"DW 32",null,"Actual value 3","PortalParameter.###MNR.Part1.32","###INDEX:PortalParameter.###MNR.Part1.32:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W2]{p}"]
[41,"DW 33",null,"Actual value 4","PortalParameter.###MNR.Part1.33","###INDEX:PortalParameter.###MNR.Part1.33:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W3]{p}"]
[41,"DW 34",null,"Actual value 5","PortalParameter.###MNR.Part1.34","###INDEX:PortalParameter.###MNR.Part1.34:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W4]{p}"]
[41,"DW 35",null,"Actual value 6","PortalParameter.###MNR.Part1.35","###INDEX:PortalParameter.###MNR.Part1.35:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W5]{p}"]
[41,"DW 36",null,"Actual value 7","PortalParameter.###MNR.Part1.36","###INDEX:PortalParameter.###MNR.Part1.36:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W6]{p}"]
[41,"DW 37",null,"Actual value 8","PortalParameter.###MNR.Part1.37","###INDEX:PortalParameter.###MNR.Part1.37:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W7]{p}"]
[41,"DW 38",null,"Actual value 9","PortalParameter.###MNR.Part1.38","###INDEX:PortalParameter.###MNR.Part1.38:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W8]{p}"]
[41,"DW 39",null,"Actual value 10","PortalParameter.###MNR.Part1.39","###INDEX:PortalParameter.###MNR.Part1.39:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W9]{p}"]
[41,"DW 40",null,"Actual value 11","PortalParameter.###MNR.Part1.40","###INDEX:PortalParameter.###MNR.Part1.40:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W10]{p}"]
[41,"DW 41",null,"Actual value 12","PortalParameter.###MNR.Part1.41","###INDEX:PortalParameter.###MNR.Part1.41:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W11]{p}"]
[41,"DW 42",null,"Actual value 13","PortalParameter.###MNR.Part1.42","###INDEX:PortalParameter.###MNR.Part1.42:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W12]{p}"]
[41,"DW 43",null,"Actual value 14","PortalParameter.###MNR.Part1.43","###INDEX:PortalParameter.###MNR.Part1.43:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist1>[W13]{p}"]
[41,"DW 48","Bit 0","Status bit","PortalParameter.###MNR.Part1.50","###INDEX:PortalParameter.###MNR.Part1.50:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_bit1>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalParameter.###MNR.Part1.51","###INDEX:PortalParameter.###MNR.Part1.51:INDEX"]
[41,null,"Bit 2","Status bit","PortalParameter.###MNR.Part1.52","###INDEX:PortalParameter.###MNR.Part1.52:INDEX"]
[41,null,"Bit 3","Status bit","PortalParameter.###MNR.Part1.53","###INDEX:PortalParameter.###MNR.Part1.53:INDEX"]
[41,null,"Bit 4","Status bit","PortalParameter.###MNR.Part1.54","###INDEX:PortalParameter.###MNR.Part1.54:INDEX"]
[41,null,"Bit 5","Status bit","PortalParameter.###MNR.Part1.55","###INDEX:PortalParameter.###MNR.Part1.55:INDEX"]
[41,null,"Bit 6","Status bit","PortalParameter.###MNR.Part1.56","###INDEX:PortalParameter.###MNR.Part1.56:INDEX"]
[41,null,"Bit 7","Status bit","PortalParameter.###MNR.Part1.57","###INDEX:PortalParameter.###MNR.Part1.57:INDEX"]
[41,null,"Bit 8","Status bit","PortalParameter.###MNR.Part1.58","###INDEX:PortalParameter.###MNR.Part1.58:INDEX"]
[41,null,"Bit 9","Status bit","PortalParameter.###MNR.Part1.59","###INDEX:PortalParameter.###MNR.Part1.59:INDEX"]
[41,null,"Bit 10","Status bit","PortalParameter.###MNR.Part1.60","###INDEX:PortalParameter.###MNR.Part1.60:INDEX"]
[41,null,"Bit 11","Status bit","PortalParameter.###MNR.Part1.61","###INDEX:PortalParameter.###MNR.Part1.61:INDEX"]
[41,null,"Bit 12","Status bit","PortalParameter.###MNR.Part1.62","###INDEX:PortalParameter.###MNR.Part1.62:INDEX"]
[41,null,"Bit 13","Status bit","PortalParameter.###MNR.Part1.63","###INDEX:PortalParameter.###MNR.Part1.63:INDEX"]
[31,"DW50 – DW89","Portal 2"]
[41,"DW 50",null,"Setpoint 1","PortalParameter.###MNR.Part2.10","###INDEX:PortalParameter.###MNR.Part2.10:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W0]{r}"]
[41,"DW 51",null,"Setpoint 2","PortalParameter.###MNR.Part2.11","###INDEX:PortalParameter.###MNR.Part2.11:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W1]{r}"]
[41,"DW 52",null,"Setpoint 3","PortalParameter.###MNR.Part2.12","###INDEX:PortalParameter.###MNR.Part2.12:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W2]{r}"]
[41,"DW 53",null,"Setpoint 4","PortalParameter.###MNR.Part2.13","###INDEX:PortalParameter.###MNR.Part2.13:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W3]{r}"]
[41,"DW 54",null,"Setpoint 5","PortalParameter.###MNR.Part2.14","###INDEX:PortalParameter.###MNR.Part2.14:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W4]{r}"]
[41,"DW 55",null,"Setpoint 6","PortalParameter.###MNR.Part2.15","###INDEX:PortalParameter.###MNR.Part2.15:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W5]{r}"]
[41,"DW 56",null,"Setpoint 7","PortalParameter.###MNR.Part2.16","###INDEX:PortalParameter.###MNR.Part2.16:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W6]{r}"]
[41,"DW 57",null,"Setpoint 8","PortalParameter.###MNR.Part2.17","###INDEX:PortalParameter.###MNR.Part2.17:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W7]{r}"]
[41,"DW 58",null,"Setpoint 9","PortalParameter.###MNR.Part2.18","###INDEX:PortalParameter.###MNR.Part2.18:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W8]{r}"]
[41,"DW 59",null,"Setpoint 10","PortalParameter.###MNR.Part2.19","###INDEX:PortalParameter.###MNR.Part2.19:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W9]{r}"]
[41,"DW 60",null,"Setpoint 11","PortalParameter.###MNR.Part2.20","###INDEX:PortalParameter.###MNR.Part2.20:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W10]{r}"]
[41,"DW 61",null,"Setpoint 12","PortalParameter.###MNR.Part2.21","###INDEX:PortalParameter.###MNR.Part2.21:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W11]{r}"]
[41,"DW 62",null,"Setpoint 13","PortalParameter.###MNR.Part2.22","###INDEX:PortalParameter.###MNR.Part2.22:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W12]{r}"]
[41,"DW 63",null,"Setpoint 14","PortalParameter.###MNR.Part2.23","###INDEX:PortalParameter.###MNR.Part2.23:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll2>[W13]{r}"]
[41,"DW 70",null,"Actual value 1","PortalParameter.###MNR.Part2.30","###INDEX:PortalParameter.###MNR.Part2.30:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W0]{p}"]
[41,"DW 71",null,"Actual value 2","PortalParameter.###MNR.Part2.31","###INDEX:PortalParameter.###MNR.Part2.31:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W1]{p}"]
[41,"DW 72",null,"Actual value 3","PortalParameter.###MNR.Part2.32","###INDEX:PortalParameter.###MNR.Part2.32:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W2]{p}"]
[41,"DW 73",null,"Actual value 4","PortalParameter.###MNR.Part2.33","###INDEX:PortalParameter.###MNR.Part2.33:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W3]{p}"]
[41,"DW 74",null,"Actual value 5","PortalParameter.###MNR.Part2.34","###INDEX:PortalParameter.###MNR.Part2.34:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W4]{p}"]
[41,"DW 75",null,"Actual value 6","PortalParameter.###MNR.Part2.35","###INDEX:PortalParameter.###MNR.Part2.35:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W5]{p}"]
[41,"DW 76",null,"Actual value 7","PortalParameter.###MNR.Part2.36","###INDEX:PortalParameter.###MNR.Part2.36:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W6]{p}"]
[41,"DW 77",null,"Actual value 8","PortalParameter.###MNR.Part2.37","###INDEX:PortalParameter.###MNR.Part2.37:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W7]{p}"]
[41,"DW 78",null,"Actual value 9","PortalParameter.###MNR.Part2.38","###INDEX:PortalParameter.###MNR.Part2.38:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W8]{p}"]
[41,"DW 79",null,"Actual value 10","PortalParameter.###MNR.Part2.39","###INDEX:PortalParameter.###MNR.Part2.39:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W9]{p}"]
[41,"DW 80",null,"Actual value 11","PortalParameter.###MNR.Part2.40","###INDEX:PortalParameter.###MNR.Part2.40:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W10]{p}"]
[41,"DW 81",null,"Actual value 12","PortalParameter.###MNR.Part2.41","###INDEX:PortalParameter.###MNR.Part2.41:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W11]{p}"]
[41,"DW 82",null,"Actual value 13","PortalParameter.###MNR.Part2.42","###INDEX:PortalParameter.###MNR.Part2.42:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W12]{p}"]
[41,"DW 83",null,"Actual value 14","PortalParameter.###MNR.Part2.43","###INDEX:PortalParameter.###MNR.Part2.43:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist2>[W13]{p}"]
[41,"DW 88","Bit 0","Status bit","PortalParameter.###MNR.Part2.50","###INDEX:PortalParameter.###MNR.Part2.50:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_bit2>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalParameter.###MNR.Part2.51","###INDEX:PortalParameter.###MNR.Part2.51:INDEX"]
[41,null,"Bit 2","Status bit","PortalParameter.###MNR.Part2.52","###INDEX:PortalParameter.###MNR.Part2.52:INDEX"]
[41,null,"Bit 3","Status bit","PortalParameter.###MNR.Part2.53","###INDEX:PortalParameter.###MNR.Part2.53:INDEX"]
[41,null,"Bit 4","Status bit","PortalParameter.###MNR.Part2.54","###INDEX:PortalParameter.###MNR.Part2.54:INDEX"]
[41,null,"Bit 5","Status bit","PortalParameter.###MNR.Part2.55","###INDEX:PortalParameter.###MNR.Part2.55:INDEX"]
[41,null,"Bit 6","Status bit","PortalParameter.###MNR.Part2.56","###INDEX:PortalParameter.###MNR.Part2.56:INDEX"]
[41,null,"Bit 7","Status bit","PortalParameter.###MNR.Part2.57","###INDEX:PortalParameter.###MNR.Part2.57:INDEX"]
[41,null,"Bit 8","Status bit","PortalParameter.###MNR.Part2.58","###INDEX:PortalParameter.###MNR.Part2.58:INDEX"]
[41,null,"Bit 9","Status bit","PortalParameter.###MNR.Part2.59","###INDEX:PortalParameter.###MNR.Part2.59:INDEX"]
[41,null,"Bit 10","Status bit","PortalParameter.###MNR.Part2.60","###INDEX:PortalParameter.###MNR.Part2.60:INDEX"]
[41,null,"Bit 11","Status bit","PortalParameter.###MNR.Part2.61","###INDEX:PortalParameter.###MNR.Part2.61:INDEX"]
[41,null,"Bit 12","Status bit","PortalParameter.###MNR.Part2.62","###INDEX:PortalParameter.###MNR.Part2.62:INDEX"]
[41,null,"Bit 13","Status bit","PortalParameter.###MNR.Part2.63","###INDEX:PortalParameter.###MNR.Part2.63:INDEX"]
[31,"DW90 – DW129","Portal 3"]
[41,"DW 90",null,"Setpoint 1","PortalParameter.###MNR.Part3.10","###INDEX:PortalParameter.###MNR.Part3.10:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W0]{r}"]
[41,"DW 91",null,"Setpoint 2","PortalParameter.###MNR.Part3.11","###INDEX:PortalParameter.###MNR.Part3.11:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W1]{r}"]
[41,"DW 92",null,"Setpoint 3","PortalParameter.###MNR.Part3.12","###INDEX:PortalParameter.###MNR.Part3.12:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W2]{r}"]
[41,"DW 93",null,"Setpoint 4","PortalParameter.###MNR.Part3.13","###INDEX:PortalParameter.###MNR.Part3.13:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W3]{r}"]
[41,"DW 94",null,"Setpoint 5","PortalParameter.###MNR.Part3.14","###INDEX:PortalParameter.###MNR.Part3.14:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W4]{r}"]
[41,"DW 95",null,"Setpoint 6","PortalParameter.###MNR.Part3.15","###INDEX:PortalParameter.###MNR.Part3.15:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W5]{r}"]
[41,"DW 96",null,"Setpoint 7","PortalParameter.###MNR.Part3.16","###INDEX:PortalParameter.###MNR.Part3.16:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W6]{r}"]
[41,"DW 97",null,"Setpoint 8","PortalParameter.###MNR.Part3.17","###INDEX:PortalParameter.###MNR.Part3.17:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W7]{r}"]
[41,"DW 98",null,"Setpoint 9","PortalParameter.###MNR.Part3.18","###INDEX:PortalParameter.###MNR.Part3.18:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W8]{r}"]
[41,"DW 99",null,"Setpoint 10","PortalParameter.###MNR.Part3.19","###INDEX:PortalParameter.###MNR.Part3.19:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W9]{r}"]
[41,"DW 100",null,"Setpoint 11","PortalParameter.###MNR.Part3.20","###INDEX:PortalParameter.###MNR.Part3.20:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W10]{r}"]
[41,"DW 101",null,"Setpoint 12","PortalParameter.###MNR.Part3.21","###INDEX:PortalParameter.###MNR.Part3.21:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W11]{r}"]
[41,"DW 102",null,"Setpoint 13","PortalParameter.###MNR.Part3.22","###INDEX:PortalParameter.###MNR.Part3.22:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W12]{r}"]
[41,"DW 103",null,"Setpoint 14","PortalParameter.###MNR.Part3.23","###INDEX:PortalParameter.###MNR.Part3.23:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll3>[W13]{r}"]
[41,"DW 110",null,"Actual value 1","PortalParameter.###MNR.Part3.30","###INDEX:PortalParameter.###MNR.Part3.30:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W0]{p}"]
[41,"DW 111",null,"Actual value 2","PortalParameter.###MNR.Part3.31","###INDEX:PortalParameter.###MNR.Part3.31:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W1]{p}"]
[41,"DW 112",null,"Actual value 3","PortalParameter.###MNR.Part3.32","###INDEX:PortalParameter.###MNR.Part3.32:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W2]{p}"]
[41,"DW 113",null,"Actual value 4","PortalParameter.###MNR.Part3.33","###INDEX:PortalParameter.###MNR.Part3.33:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W3]{p}"]
[41,"DW 114",null,"Actual value 5","PortalParameter.###MNR.Part3.34","###INDEX:PortalParameter.###MNR.Part3.34:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W4]{p}"]
[41,"DW 115",null,"Actual value 6","PortalParameter.###MNR.Part3.35","###INDEX:PortalParameter.###MNR.Part3.35:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W5]{p}"]
[41,"DW 116",null,"Actual value 7","PortalParameter.###MNR.Part3.36","###INDEX:PortalParameter.###MNR.Part3.36:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W6]{p}"]
[41,"DW 117",null,"Actual value 8","PortalParameter.###MNR.Part3.37","###INDEX:PortalParameter.###MNR.Part3.37:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W7]{p}"]
[41,"DW 118",null,"Actual value 9","PortalParameter.###MNR.Part3.38","###INDEX:PortalParameter.###MNR.Part3.38:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W8]{p}"]
[41,"DW 119",null,"Actual value 10","PortalParameter.###MNR.Part3.39","###INDEX:PortalParameter.###MNR.Part3.39:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W9]{p}"]
[41,"DW 120",null,"Actual value 11","PortalParameter.###MNR.Part3.40","###INDEX:PortalParameter.###MNR.Part3.40:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W10]{p}"]
[41,"DW 121",null,"Actual value 12","PortalParameter.###MNR.Part3.41","###INDEX:PortalParameter.###MNR.Part3.41:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W11]{p}"]
[41,"DW 122",null,"Actual value 13","PortalParameter.###MNR.Part3.42","###INDEX:PortalParameter.###MNR.Part3.42:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W12]{p}"]
[41,"DW 123",null,"Actual value 14","PortalParameter.###MNR.Part3.43","###INDEX:PortalParameter.###MNR.Part3.43:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist3>[W13]{p}"]
[41,"DW 128","Bit 0","Status bit","PortalParameter.###MNR.Part3.50","###INDEX:PortalParameter.###MNR.Part3.50:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_bit3>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalParameter.###MNR.Part3.51","###INDEX:PortalParameter.###MNR.Part3.51:INDEX"]
[41,null,"Bit 2","Status bit","PortalParameter.###MNR.Part3.52","###INDEX:PortalParameter.###MNR.Part3.52:INDEX"]
[41,null,"Bit 3","Status bit","PortalParameter.###MNR.Part3.53","###INDEX:PortalParameter.###MNR.Part3.53:INDEX"]
[41,null,"Bit 4","Status bit","PortalParameter.###MNR.Part3.54","###INDEX:PortalParameter.###MNR.Part3.54:INDEX"]
[41,null,"Bit 5","Status bit","PortalParameter.###MNR.Part3.55","###INDEX:PortalParameter.###MNR.Part3.55:INDEX"]
[41,null,"Bit 6","Status bit","PortalParameter.###MNR.Part3.56","###INDEX:PortalParameter.###MNR.Part3.56:INDEX"]
[41,null,"Bit 7","Status bit","PortalParameter.###MNR.Part3.57","###INDEX:PortalParameter.###MNR.Part3.57:INDEX"]
[41,null,"Bit 8","Status bit","PortalParameter.###MNR.Part3.58","###INDEX:PortalParameter.###MNR.Part3.58:INDEX"]
[41,null,"Bit 9","Status bit","PortalParameter.###MNR.Part3.59","###INDEX:PortalParameter.###MNR.Part3.59:INDEX"]
[41,null,"Bit 10","Status bit","PortalParameter.###MNR.Part3.60","###INDEX:PortalParameter.###MNR.Part3.60:INDEX"]
[41,null,"Bit 11","Status bit","PortalParameter.###MNR.Part3.61","###INDEX:PortalParameter.###MNR.Part3.61:INDEX"]
[41,null,"Bit 12","Status bit","PortalParameter.###MNR.Part3.62","###INDEX:PortalParameter.###MNR.Part3.62:INDEX"]
[41,null,"Bit 13","Status bit","PortalParameter.###MNR.Part3.63","###INDEX:PortalParameter.###MNR.Part3.63:INDEX"]
[31,"DW130 – DW169","Portal 4"]
[41,"DW 130",null,"Setpoint 1","PortalParameter.###MNR.Part4.10","###INDEX:PortalParameter.###MNR.Part4.10:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W0]{r}"]
[41,"DW 131",null,"Setpoint 2","PortalParameter.###MNR.Part4.11","###INDEX:PortalParameter.###MNR.Part4.11:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W1]{r}"]
[41,"DW 132",null,"Setpoint 3","PortalParameter.###MNR.Part4.12","###INDEX:PortalParameter.###MNR.Part4.12:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W2]{r}"]
[41,"DW 133",null,"Setpoint 4","PortalParameter.###MNR.Part4.13","###INDEX:PortalParameter.###MNR.Part4.13:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W3]{r}"]
[41,"DW 134",null,"Setpoint 5","PortalParameter.###MNR.Part4.14","###INDEX:PortalParameter.###MNR.Part4.14:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W4]{r}"]
[41,"DW 135",null,"Setpoint 6","PortalParameter.###MNR.Part4.15","###INDEX:PortalParameter.###MNR.Part4.15:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W5]{r}"]
[41,"DW 136",null,"Setpoint 7","PortalParameter.###MNR.Part4.16","###INDEX:PortalParameter.###MNR.Part4.16:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W6]{r}"]
[41,"DW 137",null,"Setpoint 8","PortalParameter.###MNR.Part4.17","###INDEX:PortalParameter.###MNR.Part4.17:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W7]{r}"]
[41,"DW 138",null,"Setpoint 9","PortalParameter.###MNR.Part4.18","###INDEX:PortalParameter.###MNR.Part4.18:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W8]{r}"]
[41,"DW 139",null,"Setpoint 10","PortalParameter.###MNR.Part4.19","###INDEX:PortalParameter.###MNR.Part4.19:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W9]{r}"]
[41,"DW 130",null,"Setpoint 11","PortalParameter.###MNR.Part4.20","###INDEX:PortalParameter.###MNR.Part4.20:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W10]{r}"]
[41,"DW 131",null,"Setpoint 12","PortalParameter.###MNR.Part4.21","###INDEX:PortalParameter.###MNR.Part4.21:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W11]{r}"]
[41,"DW 132",null,"Setpoint 13","PortalParameter.###MNR.Part4.22","###INDEX:PortalParameter.###MNR.Part4.22:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W12]{r}"]
[41,"DW 133",null,"Setpoint 14","PortalParameter.###MNR.Part4.23","###INDEX:PortalParameter.###MNR.Part4.23:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll4>[W13]{r}"]
[41,"DW 140",null,"Actual value 1","PortalParameter.###MNR.Part4.30","###INDEX:PortalParameter.###MNR.Part4.30:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W0]{p}"]
[41,"DW 141",null,"Actual value 2","PortalParameter.###MNR.Part4.31","###INDEX:PortalParameter.###MNR.Part4.31:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W1]{p}"]
[41,"DW 142",null,"Actual value 3","PortalParameter.###MNR.Part4.32","###INDEX:PortalParameter.###MNR.Part4.32:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W2]{p}"]
[41,"DW 143",null,"Actual value 4","PortalParameter.###MNR.Part4.33","###INDEX:PortalParameter.###MNR.Part4.33:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W3]{p}"]
[41,"DW 144",null,"Actual value 5","PortalParameter.###MNR.Part4.34","###INDEX:PortalParameter.###MNR.Part4.34:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W4]{p}"]
[41,"DW 145",null,"Actual value 6","PortalParameter.###MNR.Part4.35","###INDEX:PortalParameter.###MNR.Part4.35:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W5]{p}"]
[41,"DW 146",null,"Actual value 7","PortalParameter.###MNR.Part4.36","###INDEX:PortalParameter.###MNR.Part4.36:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W6]{p}"]
[41,"DW 147",null,"Actual value 8","PortalParameter.###MNR.Part4.37","###INDEX:PortalParameter.###MNR.Part4.37:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W7]{p}"]
[41,"DW 148",null,"Actual value 9","PortalParameter.###MNR.Part4.38","###INDEX:PortalParameter.###MNR.Part4.38:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W8]{p}"]
[41,"DW 149",null,"Actual value 10","PortalParameter.###MNR.Part4.39","###INDEX:PortalParameter.###MNR.Part4.39:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W9]{p}"]
[41,"DW 150",null,"Actual value 11","PortalParameter.###MNR.Part4.40","###INDEX:PortalParameter.###MNR.Part4.40:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W10]{p}"]
[41,"DW 151",null,"Actual value 12","PortalParameter.###MNR.Part4.41","###INDEX:PortalParameter.###MNR.Part4.41:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W11]{p}"]
[41,"DW 152",null,"Actual value 13","PortalParameter.###MNR.Part4.42","###INDEX:PortalParameter.###MNR.Part4.42:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W12]{p}"]
[41,"DW 153",null,"Actual value 14","PortalParameter.###MNR.Part4.43","###INDEX:PortalParameter.###MNR.Part4.43:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist4>[W13]{p}"]
[41,"DW 158","Bit 0","Status bit","PortalParameter.###MNR.Part4.50","###INDEX:PortalParameter.###MNR.Part4.50:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_bit4>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalParameter.###MNR.Part4.51","###INDEX:PortalParameter.###MNR.Part4.51:INDEX"]
[41,null,"Bit 2","Status bit","PortalParameter.###MNR.Part4.52","###INDEX:PortalParameter.###MNR.Part4.52:INDEX"]
[41,null,"Bit 3","Status bit","PortalParameter.###MNR.Part4.53","###INDEX:PortalParameter.###MNR.Part4.53:INDEX"]
[41,null,"Bit 4","Status bit","PortalParameter.###MNR.Part4.54","###INDEX:PortalParameter.###MNR.Part4.54:INDEX"]
[41,null,"Bit 5","Status bit","PortalParameter.###MNR.Part4.55","###INDEX:PortalParameter.###MNR.Part4.55:INDEX"]
[41,null,"Bit 6","Status bit","PortalParameter.###MNR.Part4.56","###INDEX:PortalParameter.###MNR.Part4.56:INDEX"]
[41,null,"Bit 7","Status bit","PortalParameter.###MNR.Part4.57","###INDEX:PortalParameter.###MNR.Part4.57:INDEX"]
[41,null,"Bit 8","Status bit","PortalParameter.###MNR.Part4.58","###INDEX:PortalParameter.###MNR.Part4.58:INDEX"]
[41,null,"Bit 9","Status bit","PortalParameter.###MNR.Part4.59","###INDEX:PortalParameter.###MNR.Part4.59:INDEX"]
[41,null,"Bit 10","Status bit","PortalParameter.###MNR.Part4.60","###INDEX:PortalParameter.###MNR.Part4.60:INDEX"]
[41,null,"Bit 11","Status bit","PortalParameter.###MNR.Part4.61","###INDEX:PortalParameter.###MNR.Part4.61:INDEX"]
[41,null,"Bit 12","Status bit","PortalParameter.###MNR.Part4.62","###INDEX:PortalParameter.###MNR.Part4.62:INDEX"]
[41,null,"Bit 13","Status bit","PortalParameter.###MNR.Part4.63","###INDEX:PortalParameter.###MNR.Part4.63:INDEX"]
[31,"DW170 – DW209","Portal 5"]
[41,"DW 170",null,"Setpoint 1","PortalParameter.###MNR.Part5.10","###INDEX:PortalParameter.###MNR.Part5.10:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W0]{r}"]
[41,"DW 171",null,"Setpoint 2","PortalParameter.###MNR.Part5.11","###INDEX:PortalParameter.###MNR.Part5.11:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W1]{r}"]
[41,"DW 172",null,"Setpoint 3","PortalParameter.###MNR.Part5.12","###INDEX:PortalParameter.###MNR.Part5.12:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W2]{r}"]
[41,"DW 173",null,"Setpoint 4","PortalParameter.###MNR.Part5.13","###INDEX:PortalParameter.###MNR.Part5.13:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W3]{r}"]
[41,"DW 174",null,"Setpoint 5","PortalParameter.###MNR.Part5.14","###INDEX:PortalParameter.###MNR.Part5.14:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W4]{r}"]
[41,"DW 175",null,"Setpoint 6","PortalParameter.###MNR.Part5.15","###INDEX:PortalParameter.###MNR.Part5.15:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W5]{r}"]
[41,"DW 176",null,"Setpoint 7","PortalParameter.###MNR.Part5.16","###INDEX:PortalParameter.###MNR.Part5.16:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W6]{r}"]
[41,"DW 177",null,"Setpoint 8","PortalParameter.###MNR.Part5.17","###INDEX:PortalParameter.###MNR.Part5.17:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W7]{r}"]
[41,"DW 178",null,"Setpoint 9","PortalParameter.###MNR.Part5.18","###INDEX:PortalParameter.###MNR.Part5.18:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W8]{r}"]
[41,"DW 179",null,"Setpoint 10","PortalParameter.###MNR.Part5.19","###INDEX:PortalParameter.###MNR.Part5.19:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W9]{r}"]
[41,"DW 180",null,"Setpoint 11","PortalParameter.###MNR.Part5.20","###INDEX:PortalParameter.###MNR.Part5.20:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W10]{r}"]
[41,"DW 181",null,"Setpoint 12","PortalParameter.###MNR.Part5.21","###INDEX:PortalParameter.###MNR.Part5.21:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W11]{r}"]
[41,"DW 182",null,"Setpoint 13","PortalParameter.###MNR.Part5.22","###INDEX:PortalParameter.###MNR.Part5.22:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W12]{r}"]
[41,"DW 183",null,"Setpoint 14","PortalParameter.###MNR.Part5.23","###INDEX:PortalParameter.###MNR.Part5.23:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll5>[W13]{r}"]
[41,"DW 190",null,"Actual value 1","PortalParameter.###MNR.Part5.30","###INDEX:PortalParameter.###MNR.Part5.30:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W0]{p}"]
[41,"DW 191",null,"Actual value 2","PortalParameter.###MNR.Part5.31","###INDEX:PortalParameter.###MNR.Part5.31:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W1]{p}"]
[41,"DW 192",null,"Actual value 3","PortalParameter.###MNR.Part5.32","###INDEX:PortalParameter.###MNR.Part5.32:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W2]{p}"]
[41,"DW 193",null,"Actual value 4","PortalParameter.###MNR.Part5.33","###INDEX:PortalParameter.###MNR.Part5.33:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W3]{p}"]
[41,"DW 194",null,"Actual value 5","PortalParameter.###MNR.Part5.34","###INDEX:PortalParameter.###MNR.Part5.34:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W4]{p}"]
[41,"DW 195",null,"Actual value 6","PortalParameter.###MNR.Part5.35","###INDEX:PortalParameter.###MNR.Part5.35:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W5]{p}"]
[41,"DW 196",null,"Actual value 7","PortalParameter.###MNR.Part5.36","###INDEX:PortalParameter.###MNR.Part5.36:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W6]{p}"]
[41,"DW 197",null,"Actual value 8","PortalParameter.###MNR.Part5.37","###INDEX:PortalParameter.###MNR.Part5.37:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W7]{p}"]
[41,"DW 198",null,"Actual value 9","PortalParameter.###MNR.Part5.38","###INDEX:PortalParameter.###MNR.Part5.38:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W8]{p}"]
[41,"DW 199",null,"Actual value 10","PortalParameter.###MNR.Part5.39","###INDEX:PortalParameter.###MNR.Part5.39:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W9]{p}"]
[41,"DW 200",null,"Actual value 11","PortalParameter.###MNR.Part5.40","###INDEX:PortalParameter.###MNR.Part5.40:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W10]{p}"]
[41,"DW 201",null,"Actual value 12","PortalParameter.###MNR.Part5.41","###INDEX:PortalParameter.###MNR.Part5.41:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W11]{p}"]
[41,"DW 202",null,"Actual value 13","PortalParameter.###MNR.Part5.42","###INDEX:PortalParameter.###MNR.Part5.42:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W12]{p}"]
[41,"DW 203",null,"Actual value 14","PortalParameter.###MNR.Part5.43","###INDEX:PortalParameter.###MNR.Part5.43:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist5>[W13]{p}"]
[41,"DW 208","Bit 0","Status bit","PortalParameter.###MNR.Part5.50","###INDEX:PortalParameter.###MNR.Part5.50:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_bit5>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalParameter.###MNR.Part5.51","###INDEX:PortalParameter.###MNR.Part5.51:INDEX"]
[41,null,"Bit 2","Status bit","PortalParameter.###MNR.Part5.52","###INDEX:PortalParameter.###MNR.Part5.52:INDEX"]
[41,null,"Bit 3","Status bit","PortalParameter.###MNR.Part5.53","###INDEX:PortalParameter.###MNR.Part5.53:INDEX"]
[41,null,"Bit 4","Status bit","PortalParameter.###MNR.Part5.54","###INDEX:PortalParameter.###MNR.Part5.54:INDEX"]
[41,null,"Bit 5","Status bit","PortalParameter.###MNR.Part5.55","###INDEX:PortalParameter.###MNR.Part5.55:INDEX"]
[41,null,"Bit 6","Status bit","PortalParameter.###MNR.Part5.56","###INDEX:PortalParameter.###MNR.Part5.56:INDEX"]
[41,null,"Bit 7","Status bit","PortalParameter.###MNR.Part5.57","###INDEX:PortalParameter.###MNR.Part5.57:INDEX"]
[41,null,"Bit 8","Status bit","PortalParameter.###MNR.Part5.58","###INDEX:PortalParameter.###MNR.Part5.58:INDEX"]
[41,null,"Bit 9","Status bit","PortalParameter.###MNR.Part5.59","###INDEX:PortalParameter.###MNR.Part5.59:INDEX"]
[41,null,"Bit 10","Status bit","PortalParameter.###MNR.Part5.60","###INDEX:PortalParameter.###MNR.Part5.60:INDEX"]
[41,null,"Bit 11","Status bit","PortalParameter.###MNR.Part5.61","###INDEX:PortalParameter.###MNR.Part5.61:INDEX"]
[41,null,"Bit 12","Status bit","PortalParameter.###MNR.Part5.62","###INDEX:PortalParameter.###MNR.Part5.62:INDEX"]
[41,null,"Bit 13","Status bit","PortalParameter.###MNR.Part5.63","###INDEX:PortalParameter.###MNR.Part5.63:INDEX"]
[31,"DW210 – DW249","Portal 6"]
[41,"DW 210",null,"Setpoint 1","PortalParameter.###MNR.Part6.10","###INDEX:PortalParameter.###MNR.Part6.10:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W0]{r}"]
[41,"DW 211",null,"Setpoint 2","PortalParameter.###MNR.Part6.11","###INDEX:PortalParameter.###MNR.Part6.11:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W1]{r}"]
[41,"DW 212",null,"Setpoint 3","PortalParameter.###MNR.Part6.12","###INDEX:PortalParameter.###MNR.Part6.12:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W2]{r}"]
[41,"DW 213",null,"Setpoint 4","PortalParameter.###MNR.Part6.13","###INDEX:PortalParameter.###MNR.Part6.13:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W3]{r}"]
[41,"DW 214",null,"Setpoint 5","PortalParameter.###MNR.Part6.14","###INDEX:PortalParameter.###MNR.Part6.14:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W4]{r}"]
[41,"DW 215",null,"Setpoint 6","PortalParameter.###MNR.Part6.15","###INDEX:PortalParameter.###MNR.Part6.15:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W5]{r}"]
[41,"DW 216",null,"Setpoint 7","PortalParameter.###MNR.Part6.16","###INDEX:PortalParameter.###MNR.Part6.16:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W6]{r}"]
[41,"DW 217",null,"Setpoint 8","PortalParameter.###MNR.Part6.17","###INDEX:PortalParameter.###MNR.Part6.17:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W7]{r}"]
[41,"DW 218",null,"Setpoint 9","PortalParameter.###MNR.Part6.18","###INDEX:PortalParameter.###MNR.Part6.18:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W8]{r}"]
[41,"DW 219",null,"Setpoint 10","PortalParameter.###MNR.Part6.19","###INDEX:PortalParameter.###MNR.Part6.19:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W9]{r}"]
[41,"DW 220",null,"Setpoint 11","PortalParameter.###MNR.Part6.20","###INDEX:PortalParameter.###MNR.Part6.20:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W10]{r}"]
[41,"DW 221",null,"Setpoint 12","PortalParameter.###MNR.Part6.21","###INDEX:PortalParameter.###MNR.Part6.21:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W11]{r}"]
[41,"DW 222",null,"Setpoint 13","PortalParameter.###MNR.Part6.22","###INDEX:PortalParameter.###MNR.Part6.22:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W12]{r}"]
[41,"DW 223",null,"Setpoint 14","PortalParameter.###MNR.Part6.23","###INDEX:PortalParameter.###MNR.Part6.23:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll6>[W13]{r}"]
[41,"DW 230",null,"Actual value 1","PortalParameter.###MNR.Part6.30","###INDEX:PortalParameter.###MNR.Part6.30:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W0]{p}"]
[41,"DW 231",null,"Actual value 2","PortalParameter.###MNR.Part6.31","###INDEX:PortalParameter.###MNR.Part6.31:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W1]{p}"]
[41,"DW 232",null,"Actual value 3","PortalParameter.###MNR.Part6.32","###INDEX:PortalParameter.###MNR.Part6.32:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W2]{p}"]
[41,"DW 233",null,"Actual value 4","PortalParameter.###MNR.Part6.33","###INDEX:PortalParameter.###MNR.Part6.33:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W3]{p}"]
[41,"DW 234",null,"Actual value 5","PortalParameter.###MNR.Part6.34","###INDEX:PortalParameter.###MNR.Part6.34:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W4]{p}"]
[41,"DW 235",null,"Actual value 6","PortalParameter.###MNR.Part6.35","###INDEX:PortalParameter.###MNR.Part6.35:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W5]{p}"]
[41,"DW 236",null,"Actual value 7","PortalParameter.###MNR.Part6.36","###INDEX:PortalParameter.###MNR.Part6.36:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W6]{p}"]
[41,"DW 237",null,"Actual value 8","PortalParameter.###MNR.Part6.37","###INDEX:PortalParameter.###MNR.Part6.37:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W7]{p}"]
[41,"DW 238",null,"Actual value 9","PortalParameter.###MNR.Part6.38","###INDEX:PortalParameter.###MNR.Part6.38:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W8]{p}"]
[41,"DW 239",null,"Actual value 10","PortalParameter.###MNR.Part6.39","###INDEX:PortalParameter.###MNR.Part6.39:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W9]{p}"]
[41,"DW 240",null,"Actual value 11","PortalParameter.###MNR.Part6.40","###INDEX:PortalParameter.###MNR.Part6.40:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W10]{p}"]
[41,"DW 241",null,"Actual value 12","PortalParameter.###MNR.Part6.41","###INDEX:PortalParameter.###MNR.Part6.41:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W11]{p}"]
[41,"DW 242",null,"Actual value 13","PortalParameter.###MNR.Part6.42","###INDEX:PortalParameter.###MNR.Part6.42:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W12]{p}"]
[41,"DW 243",null,"Actual value 14","PortalParameter.###MNR.Part6.43","###INDEX:PortalParameter.###MNR.Part6.43:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist6>[W13]{p}"]
[41,"DW 248","Bit 0","Status bit","PortalParameter.###MNR.Part6.50","###INDEX:PortalParameter.###MNR.Part6.50:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_bit6>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalParameter.###MNR.Part6.51","###INDEX:PortalParameter.###MNR.Part6.51:INDEX"]
[41,null,"Bit 2","Status bit","PortalParameter.###MNR.Part6.52","###INDEX:PortalParameter.###MNR.Part6.52:INDEX"]
[41,null,"Bit 3","Status bit","PortalParameter.###MNR.Part6.53","###INDEX:PortalParameter.###MNR.Part6.53:INDEX"]
[41,null,"Bit 4","Status bit","PortalParameter.###MNR.Part6.54","###INDEX:PortalParameter.###MNR.Part6.54:INDEX"]
[41,null,"Bit 5","Status bit","PortalParameter.###MNR.Part6.55","###INDEX:PortalParameter.###MNR.Part6.55:INDEX"]
[41,null,"Bit 6","Status bit","PortalParameter.###MNR.Part6.56","###INDEX:PortalParameter.###MNR.Part6.56:INDEX"]
[41,null,"Bit 7","Status bit","PortalParameter.###MNR.Part6.57","###INDEX:PortalParameter.###MNR.Part6.57:INDEX"]
[41,null,"Bit 8","Status bit","PortalParameter.###MNR.Part6.58","###INDEX:PortalParameter.###MNR.Part6.58:INDEX"]
[41,null,"Bit 9","Status bit","PortalParameter.###MNR.Part6.59","###INDEX:PortalParameter.###MNR.Part6.59:INDEX"]
[41,null,"Bit 10","Status bit","PortalParameter.###MNR.Part6.60","###INDEX:PortalParameter.###MNR.Part6.60:INDEX"]
[41,null,"Bit 11","Status bit","PortalParameter.###MNR.Part6.61","###INDEX:PortalParameter.###MNR.Part6.61:INDEX"]
[41,null,"Bit 12","Status bit","PortalParameter.###MNR.Part6.62","###INDEX:PortalParameter.###MNR.Part6.62:INDEX"]
[41,null,"Bit 13","Status bit","PortalParameter.###MNR.Part6.63","###INDEX:PortalParameter.###MNR.Part6.63:INDEX"]
[31,"DW250 – DW289","Portal 7"]
[41,"DW 250",null,"Setpoint 1","PortalParameter.###MNR.Part7.10","###INDEX:PortalParameter.###MNR.Part7.10:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W0]{r}"]
[41,"DW 251",null,"Setpoint 2","PortalParameter.###MNR.Part7.11","###INDEX:PortalParameter.###MNR.Part7.11:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W1]{r}"]
[41,"DW 252",null,"Setpoint 3","PortalParameter.###MNR.Part7.12","###INDEX:PortalParameter.###MNR.Part7.12:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W2]{r}"]
[41,"DW 253",null,"Setpoint 4","PortalParameter.###MNR.Part7.13","###INDEX:PortalParameter.###MNR.Part7.13:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W3]{r}"]
[41,"DW 254",null,"Setpoint 5","PortalParameter.###MNR.Part7.14","###INDEX:PortalParameter.###MNR.Part7.14:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W4]{r}"]
[41,"DW 255",null,"Setpoint 6","PortalParameter.###MNR.Part7.15","###INDEX:PortalParameter.###MNR.Part7.15:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W5]{r}"]
[41,"DW 256",null,"Setpoint 7","PortalParameter.###MNR.Part7.16","###INDEX:PortalParameter.###MNR.Part7.16:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W6]{r}"]
[41,"DW 257",null,"Setpoint 8","PortalParameter.###MNR.Part7.17","###INDEX:PortalParameter.###MNR.Part7.17:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W7]{r}"]
[41,"DW 258",null,"Setpoint 9","PortalParameter.###MNR.Part7.18","###INDEX:PortalParameter.###MNR.Part7.18:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W8]{r}"]
[41,"DW 259",null,"Setpoint 10","PortalParameter.###MNR.Part7.19","###INDEX:PortalParameter.###MNR.Part7.19:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W9]{r}"]
[41,"DW 260",null,"Setpoint 11","PortalParameter.###MNR.Part7.20","###INDEX:PortalParameter.###MNR.Part7.20:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W10]{r}"]
[41,"DW 261",null,"Setpoint 12","PortalParameter.###MNR.Part7.21","###INDEX:PortalParameter.###MNR.Part7.21:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W11]{r}"]
[41,"DW 262",null,"Setpoint 13","PortalParameter.###MNR.Part7.22","###INDEX:PortalParameter.###MNR.Part7.22:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W12]{r}"]
[41,"DW 263",null,"Setpoint 14","PortalParameter.###MNR.Part7.23","###INDEX:PortalParameter.###MNR.Part7.23:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_soll7>[W13]{r}"]
[41,"DW 270",null,"Actual value 1","PortalParameter.###MNR.Part7.30","###INDEX:PortalParameter.###MNR.Part7.30:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W0]{p}"]
[41,"DW 271",null,"Actual value 2","PortalParameter.###MNR.Part7.31","###INDEX:PortalParameter.###MNR.Part7.31:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W1]{p}"]
[41,"DW 272",null,"Actual value 3","PortalParameter.###MNR.Part7.32","###INDEX:PortalParameter.###MNR.Part7.32:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W2]{p}"]
[41,"DW 273",null,"Actual value 4","PortalParameter.###MNR.Part7.33","###INDEX:PortalParameter.###MNR.Part7.33:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W3]{p}"]
[41,"DW 274",null,"Actual value 5","PortalParameter.###MNR.Part7.34","###INDEX:PortalParameter.###MNR.Part7.34:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W4]{p}"]
[41,"DW 275",null,"Actual value 6","PortalParameter.###MNR.Part7.35","###INDEX:PortalParameter.###MNR.Part7.35:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W5]{p}"]
[41,"DW 276",null,"Actual value 7","PortalParameter.###MNR.Part7.36","###INDEX:PortalParameter.###MNR.Part7.36:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W6]{p}"]
[41,"DW 277",null,"Actual value 8","PortalParameter.###MNR.Part7.37","###INDEX:PortalParameter.###MNR.Part7.37:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W7]{p}"]
[41,"DW 278",null,"Actual value 9","PortalParameter.###MNR.Part7.38","###INDEX:PortalParameter.###MNR.Part7.38:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W8]{p}"]
[41,"DW 279",null,"Actual value 10","PortalParameter.###MNR.Part7.39","###INDEX:PortalParameter.###MNR.Part7.39:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W9]{p}"]
[41,"DW 280",null,"Actual value 11","PortalParameter.###MNR.Part7.40","###INDEX:PortalParameter.###MNR.Part7.40:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W10]{p}"]
[41,"DW 281",null,"Actual value 12","PortalParameter.###MNR.Part7.41","###INDEX:PortalParameter.###MNR.Part7.41:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W11]{p}"]
[41,"DW 282",null,"Actual value 13","PortalParameter.###MNR.Part7.42","###INDEX:PortalParameter.###MNR.Part7.42:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W12]{p}"]
[41,"DW 283",null,"Actual value 14","PortalParameter.###MNR.Part7.43","###INDEX:PortalParameter.###MNR.Part7.43:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_ist7>[W13]{p}"]
[41,"DW 288","Bit 0","Status bit","PortalParameter.###MNR.Part7.50","###INDEX:PortalParameter.###MNR.Part7.50:INDEX","Ch1.###MNR_T_portpara<.m###MNR_ppa_bit7>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalParameter.###MNR.Part7.51","###INDEX:PortalParameter.###MNR.Part7.51:INDEX"]
[41,null,"Bit 2","Status bit","PortalParameter.###MNR.Part7.52","###INDEX:PortalParameter.###MNR.Part7.52:INDEX"]
[41,null,"Bit 3","Status bit","PortalParameter.###MNR.Part7.53","###INDEX:PortalParameter.###MNR.Part7.53:INDEX"]
[41,null,"Bit 4","Status bit","PortalParameter.###MNR.Part7.54","###INDEX:PortalParameter.###MNR.Part7.54:INDEX"]
[41,null,"Bit 5","Status bit","PortalParameter.###MNR.Part7.55","###INDEX:PortalParameter.###MNR.Part7.55:INDEX"]
[41,null,"Bit 6","Status bit","PortalParameter.###MNR.Part7.56","###INDEX:PortalParameter.###MNR.Part7.56:INDEX"]
[41,null,"Bit 7","Status bit","PortalParameter.###MNR.Part7.57","###INDEX:PortalParameter.###MNR.Part7.57:INDEX"]
[41,null,"Bit 8","Status bit","PortalParameter.###MNR.Part7.58","###INDEX:PortalParameter.###MNR.Part7.58:INDEX"]
[41,null,"Bit 9","Status bit","PortalParameter.###MNR.Part7.59","###INDEX:PortalParameter.###MNR.Part7.59:INDEX"]
[41,null,"Bit 10","Status bit","PortalParameter.###MNR.Part7.60","###INDEX:PortalParameter.###MNR.Part7.60:INDEX"]
[41,null,"Bit 11","Status bit","PortalParameter.###MNR.Part7.61","###INDEX:PortalParameter.###MNR.Part7.61:INDEX"]
[41,null,"Bit 12","Status bit","PortalParameter.###MNR.Part7.62","###INDEX:PortalParameter.###MNR.Part7.62:INDEX"]
[41,null,"Bit 13","Status bit","PortalParameter.###MNR.Part7.63","###INDEX:PortalParameter.###MNR.Part7.63:INDEX"]

{"sheet":"BobDepalSettings","index":105,"n_rows":55,"n_cols":7,"rows_kept":55,"flags":["formulas_cached_only"]}
["BobDepalSettings"]
[1,"###OVERVIEW"]
[21,"DB 510","Bobbin Depalettizer Settings"]
[41,"DB 510-514","Pallet Settings Machine  2-5"]
[1,"###MAIN"]
[1,"DB 510-514 Bobbin Depalettizer Settings"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR__T_bobdepalset<.m###MNR_abs_set_aender>[B]{w}"]
[31,"DD10 – DD29",null,"Settings place 1"]
[41,"DD10",null,"Anzahl Lagen","BobDepalSettings.10","###INDEX:BobDeplaSettings.10:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW0]{r}"]
[41,"DD12",null,"Reihen pro Lage","BobDepalSettings.11","###INDEX:BobDeplaSettings.11:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW1]{r}"]
[41,"DD14",null,"Stapel pro Lage","BobDepalSettings.12","###INDEX:BobDeplaSettings.12:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW2]{r}"]
[41,"DD16",null,"Höhe der Palette","BobDepalSettings.13","###INDEX:BobDeplaSettings.13:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW3]{r}"]
[41,"DD18",null,"Breite der Palette ","BobDepalSettings.14","###INDEX:BobDeplaSettings.14:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW4]{r}"]
[41,"DD20",null,"Länge der Palette","BobDepalSettings.15","###INDEX:BobDeplaSettings.15:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW5]{r}"]
[41,"DD22",null,"Stapelhöhe","BobDepalSettings.16","###INDEX:BobDeplaSettings.16:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW6]{r}"]
[41,"DD24",null,"Stapelbreite","BobDepalSettings.17","###INDEX:BobDeplaSettings.17:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW7]{r}"]
[41,"DD26",null,"Stapellänge","BobDepalSettings.18","###INDEX:BobDeplaSettings.18:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW8]{r}"]
[41,"DD28",null,"Drehung des Stapels","BobDepalSettings.19","###INDEX:BobDeplaSettings.19:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset1>[DW9]{r}"]
[41]
[31,"DD50 – DD69",null,"Settings place 2"]
[41,"DD50",null,"Anzahl Lagen","BobDepalSettings.10","###INDEX:BobDeplaSettings.10:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW0]{r}"]
[41,"DD52",null,"Reihen pro Lage","BobDepalSettings.11","###INDEX:BobDeplaSettings.11:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW1]{r}"]
[41,"DD54",null,"Stapel pro Lage","BobDepalSettings.12","###INDEX:BobDeplaSettings.12:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW2]{r}"]
[41,"DD56",null,"Höhe der Palette","BobDepalSettings.13","###INDEX:BobDeplaSettings.13:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW3]{r}"]
[41,"DD58",null,"Breite der Palette ","BobDepalSettings.14","###INDEX:BobDeplaSettings.14:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW4]{r}"]
[41,"DD60",null,"Länge der Palette","BobDepalSettings.15","###INDEX:BobDeplaSettings.15:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW5]{r}"]
[41,"DD62",null,"Stapelhöhe","BobDepalSettings.16","###INDEX:BobDeplaSettings.16:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW6]{r}"]
[41,"DD64",null,"Stapelbreite","BobDepalSettings.17","###INDEX:BobDeplaSettings.17:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW7]{r}"]
[41,"DD66",null,"Stapellänge","BobDepalSettings.18","###INDEX:BobDeplaSettings.18:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW8]{r}"]
[41,"DD68",null,"Drehung des Stapels","BobDepalSettings.19","###INDEX:BobDeplaSettings.19:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset2>[DW9]{r}"]
[41]
[31,"DD90 – DD109",null,"Settings place 3"]
[41,"DD90",null,"Anzahl Lagen","BobDepalSettings.10","###INDEX:BobDeplaSettings.10:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW0]{r}"]
[41,"DD92",null,"Reihen pro Lage","BobDepalSettings.11","###INDEX:BobDeplaSettings.11:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW1]{r}"]
[41,"DD94",null,"Stapel pro Lage","BobDepalSettings.12","###INDEX:BobDeplaSettings.12:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW2]{r}"]
[41,"DD96",null,"Höhe der Palette","BobDepalSettings.13","###INDEX:BobDeplaSettings.13:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW3]{r}"]
[41,"DD98",null,"Breite der Palette ","BobDepalSettings.14","###INDEX:BobDeplaSettings.14:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW4]{r}"]
[41,"DD100",null,"Länge der Palette","BobDepalSettings.15","###INDEX:BobDeplaSettings.15:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW5]{r}"]
[41,"DD102",null,"Stapelhöhe","BobDepalSettings.16","###INDEX:BobDeplaSettings.16:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW6]{r}"]
[41,"DD104",null,"Stapelbreite","BobDepalSettings.17","###INDEX:BobDeplaSettings.17:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW7]{r}"]
[41,"DD106",null,"Stapellänge","BobDepalSettings.18","###INDEX:BobDeplaSettings.18:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW8]{r}"]
[41,"DD108",null,"Drehung des Stapels","BobDepalSettings.19","###INDEX:BobDeplaSettings.19:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset3>[DW9]{r}"]
[41]
[31,"DD130 – DD149",null,"Settings place 4"]
[41,"DD130",null,"Anzahl Lagen","BobDepalSettings.10","###INDEX:BobDeplaSettings.10:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW0]{r}"]
[41,"DD132",null,"Reihen pro Lage","BobDepalSettings.11","###INDEX:BobDeplaSettings.11:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW1]{r}"]
[41,"DD134",null,"Stapel pro Lage","BobDepalSettings.12","###INDEX:BobDeplaSettings.12:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW2]{r}"]
[41,"DD136",null,"Höhe der Palette","BobDepalSettings.13","###INDEX:BobDeplaSettings.13:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW3]{r}"]
[41,"DD138",null,"Breite der Palette ","BobDepalSettings.14","###INDEX:BobDeplaSettings.14:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW4]{r}"]
[41,"DD140",null,"Länge der Palette","BobDepalSettings.15","###INDEX:BobDeplaSettings.15:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW5]{r}"]
[41,"DD142",null,"Stapelhöhe","BobDepalSettings.16","###INDEX:BobDeplaSettings.16:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW6]{r}"]
[41,"DD144",null,"Stapelbreite","BobDepalSettings.17","###INDEX:BobDeplaSettings.17:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW7]{r}"]
[41,"DD146",null,"Stapellänge","BobDepalSettings.18","###INDEX:BobDeplaSettings.18:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW8]{r}"]
[41,"DD148",null,"Drehung des Stapels","BobDepalSettings.19","###INDEX:BobDeplaSettings.19:INDEX","Ch1.###MNR_T_bobdepalset<.m###MNR_bobdepalset4>[DW9]{r}"]
[41]

{"sheet":"X545_MainPicture","index":106,"n_rows":28,"n_cols":7,"rows_kept":28,"flags":["formulas_cached_only"]}
["X545_MainPicture","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 520","Main picture parameters, 1st Machine"]
[41,"DB 521-524","Main picture parameters, Machine  2-5"]
[1,"###MAIN"]
[1,"DB 520-524 Main picture parameters"]
[21,"DB ###ADDR:520+1[MNR]:ADDR","Main picture parameters ###MNR"]
[41,"DW 10",null,"Status, Pallet 1",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa1>[W]{p}"]
[41,null,"Bit 0","Pallet empty"]
[41,null,"Bit 1","Pallet half full"]
[41,null,"Bit 2","Pallet full"]
[41,null,"Bit 3","No pallet"]
[41,null,"Bit 4","Reset and start"]
[41,null,"Bit 5","Door open / closed"]
[41,null,"Bit 8","Pallet in"]
[41,null,"Bit 9","Pallet out"]
[41,null,"Bit 10","Pallet, yellow"]
[41,null,"Bit 11","Pallet, red"]
[41,null,"Bit 12","Pallet, flashing"]
[41,"DW 11",null,"Status, Pallet 2",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa2>[W]{p}"]
[41,"DW 12",null,"Status, Pallet 3",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa3>[W]{p}"]
[41,"DW 13",null,"Status, Pallet 4",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa4>[W]{p}"]
[41,"DW 14",null,"Status, Pallet 5",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa5>[W]{p}"]
[41,"DW 15",null,"Status, Pallet 6",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa6>[W]{p}"]
[41,"DW 16",null,"Status, Pallet 7",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa7>[W]{p}"]
[41,"DW 17",null,"Status, Pallet 8",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa8>[W]{p}"]
[41,"DW 18",null,"Status, Pallet 9",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa9>[W]{p}"]
[41,"DW 19",null,"Status, Pallet 10",null,null,"Ch1.###MNR_T_port<.m###MNR_po_zupa10>[W]{p}"]

{"sheet":"X794_MainPicture","index":107,"n_rows":36,"n_cols":7,"rows_kept":36,"flags":["formulas_cached_only"]}
["X794_MainPicture","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 520","Main picture parameters, 1st Machine"]
[41,"DB 521-524","Main picture parameters 2-5"]
[1,"###MAIN"]
[1,"DB 520-524 Main picture parameters"]
[21,"DB ###ADDR:520+1[MNR]:ADDR","Main picture parameters ###MNR"]
[41,"DW 10",null,"Status, suspended track",null,null,"Ch1.###MNR_T_ehb<.m###MNR_ehb_zust>[W]{p}"]
[41,null,"Bit 0","Empty"]
[41,null,"Bit 1","Loaded"]
[41,null,"Bit 2","Up"]
[41,null,"Bit 3","Down"]
[41,null,"Bit 4","Already in place"]
[41,null,"Bit 5","Forwards"]
[41,null,"Bit 6","Backwards"]
[41,null,"Bit 9"]
[41,null,"Bit 10","Pallet, yellow"]
[41,null,"Bit 11","Pallet, red"]
[41,null,"Bit 12","Pallet, flashing"]
[41,"DW 11",null,"Target ",null,null,"Ch1.###MNR_T_ehb<.m###MNR_ehb_ziel>[W]{p}"]
[41,null,null,"1: Cigarette paper, Line 1"]
[41,null,null,"2: Filter paper, Line 1"]
[41,null,null,"3: Inner frame, Line 1"]
[41,null,null,"4: Inner liner, Line 1"]
[41,null,null,"5: Foil 1"]
[41,null,null,"6-10: 1-5 for Line 2"]
[41,null,null,"11: Removal point 1"]
[41,null,null,"12: Removal point 2"]
[41,null,null,"13: Emergency tray"]
[41,"DW 12",null,"Loaded with",null,null,"Ch1.###MNR_T_ehb<.m###MNR_ehb_mat>[W]{p}"]
[41,null,null,"0: Nothing"]
[41,null,null,"1: Cigarette paper"]
[41,null,null,"2: Filter paper"]
[41,null,null,"3: Inner frame"]
[41,null,null,"4: Inner liner"]
[41,null,null,"5: Foil"]

{"sheet":"X930_ScanCode","index":108,"n_rows":34,"n_cols":7,"rows_kept":34,"flags":["formulas_cached_only"]}
["X930_ScanCode","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 520","Scancode parameter"]
[41,"DB 521-524","Scancode parameter 2-5"]
[21,"DB 525","Scancode codes"]
[41,"DB 526-529","Scancode codes 2-5"]
[1,"###MAIN"]
[1,"DB 520-524 Scancode parameters"]
[21,"DB ###ADDR:520+1[MNR]:ADDR","Scancode parameters ###MNR"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR_T_930sc<.m###MNR_930sc_aender>[B]{w}"]
[41,"DW 10","Bit 0","Teachen erlaubt",null,null,"Ch1.###MNR_T_930sc<.m###MNR_930sc_erlaubt>[B]{r}"]
[41]
[41,"DW 20","Bit 0","Scanner Vorwahl Hand",null,null,"Ch1.###MNR_T_930sc<.m###MNR_930sc_vwhand>[B]{r}"]
[41,null,"Bit 1","Scanner Vorwahl Maschine",null,null,"Ch1.###MNR_T_930sc<.m###MNR_930sc_vwmasch>[B]{r}"]
[41,null,"Bit 8","Teachen Start",null,null,"Ch1.###MNR_T_930sc<.m###MNR_930sc_vwstart>[B]{r}"]
[41,null,"Bit 9","Teachen verwerfen",null,null,"Ch1.###MNR_T_930sc<.m###MNR_930sc_vwverw>[B]{r}"]
[41,null,"Bit 10","Teachen Übernehmen",null,null,"Ch1.###MNR_T_930sc<.m###MNR_930sc_vwueber>[B]{r}"]
[41]
[1,"DB 525-529 Scancode codes"]
[21,"DB ###ADDR:525+1[MNR]:ADDR","Scancode codes ###MNR"]
[41,"DW 0-19",null,"aktueller Code",null,null,"Ch1.###MNR_T_930scstr<.m###MNR_930sc_codeneu>[S0-19]{r}"]
[41,"DW 41-60",null,"neuer Code",null,null,"Ch1.###MNR_T_930scstr<.m###MNR_930sc_codeakt>[S0-19]{r}"]
[41,"DW 123-142",null,"Code Links 0",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes1>[S0-19]{r}"]
[41,"DW 164-183",null,"Code Links -1",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes2>[S0-19]{r}"]
[41,"DW 205-224",null,"Code Links -2",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes3>[S0-19]{r}"]
[41,"DW 246-265",null,"Code Links -3",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes4>[S0-19]{r}"]
[41,"DW 287-306",null,"Code Links -4",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes5>[S0-19]{r}"]
[41,"DW 328-347",null,"Code Links -5",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes6>[S0-19]{r}"]
[41,"DW 410-429",null,"Code Rechts 0",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes7>[S0-19]{r}"]
[41,"DW 451-470",null,"Code Rechts -1",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes8>[S0-19]{r}"]
[41,"DW 492-511",null,"Code Rechts -2",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes9>[S0-19]{r}"]
[41,"DW 533-554",null,"Code Rechts -3",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes10>[S0-19]{r}"]
[41,"DW 574-593",null,"Code Rechts -4",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes11>[S0-19]{r}"]
[41,"DW 615-634",null,"Code Rechts -5",null,null,"Ch1.###MNR_T_930scstr<.m###MNRE_930sc_codes12>[S0-19]{r}"]

{"sheet":"ServiceIntervalDisplay","index":109,"n_rows":7,"n_cols":3,"rows_kept":7,"flags":["formulas_cached_only"]}
["ServiceIntervalDisplay","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 530","Service Interval Display 1st Machine"]
[41,"DB 530-534","Service Interval Display,Machine  2-5"]
[1,"###MAIN"]
[1,"DB 530-534 Service Interval Display"]
[2,"DB ###ADDR:500+1[MNR]:ADDR","Service Interval Display ###MNR"]

{"sheet":"PortalAGV","index":110,"n_rows":258,"n_cols":7,"rows_kept":258,"flags":["formulas_cached_only"]}
["PortalAGV","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 530","AGV parameters 1st Machine"]
[41,"DB 530-534","AGV parameters,Machine  2-5"]
[1,"###MAIN"]
[1,"DB 530-534 Parameter AGV"]
[2,"DB ###ADDR:500+1[MNR]:ADDR","Pallet parameters ###MNR"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR_T_portagv<.m###MNR_pagv_aend>[B]{w}"]
[31,"DW10 – DW39",null,"Pallet station 1"]
[41,"DW 10","Bit 0","Switch 1","PortalAGV.###MNR.Pallet1.10","###INDEX:PortalAGV.###MNR.Pallet1.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch1>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet1.11","###INDEX:PortalAGV.###MNR.Pallet1.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet1.12","###INDEX:PortalAGV.###MNR.Pallet1.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet1.13","###INDEX:PortalAGV.###MNR.Pallet1.11:INDEX"]
[41,"DW 11","Bit 0","Status bit","PortalAGV.###MNR.Pallet1.20","###INDEX:PortalAGV.###MNR.Pallet1.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit1>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet1.21","###INDEX:PortalAGV.###MNR.Pallet1.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet1.22","###INDEX:PortalAGV.###MNR.Pallet1.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet1.23","###INDEX:PortalAGV.###MNR.Pallet1.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet1.24","###INDEX:PortalAGV.###MNR.Pallet1.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet1.25","###INDEX:PortalAGV.###MNR.Pallet1.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet1.26","###INDEX:PortalAGV.###MNR.Pallet1.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet1.27","###INDEX:PortalAGV.###MNR.Pallet1.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet1.28","###INDEX:PortalAGV.###MNR.Pallet1.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet1.29","###INDEX:PortalAGV.###MNR.Pallet1.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet1.30","###INDEX:PortalAGV.###MNR.Pallet1.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet1.31","###INDEX:PortalAGV.###MNR.Pallet1.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet1.32","###INDEX:PortalAGV.###MNR.Pallet1.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet1.33","###INDEX:PortalAGV.###MNR.Pallet1.33:INDEX"]
[41,"DW 20",null,"Setpoint 1","PortalAGV.###MNR.Pallet1.40","###INDEX:PortalAGV.###MNR.Pallet1.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll1>[W0]{r}"]
[41,"DW 21",null,"Setpoint 2","PortalAGV.###MNR.Pallet1.41","###INDEX:PortalAGV.###MNR.Pallet1.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll1>[W1]{r}"]
[41,"DW 22",null,"Setpoint 3","PortalAGV.###MNR.Pallet1.42","###INDEX:PortalAGV.###MNR.Pallet1.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll1>[W2]{r}"]
[41,"DW 30",null,"Actual value 1","PortalAGV.###MNR.Pallet1.50","###INDEX:PortalAGV.###MNR.Pallet1.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist1>[W0]{p}"]
[41,"DW 31",null,"Actual value 2","PortalAGV.###MNR.Pallet1.51","###INDEX:PortalAGV.###MNR.Pallet1.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist1>[W1]{p}"]
[41,"DW 32",null,"Actual value 3","PortalAGV.###MNR.Pallet1.52","###INDEX:PortalAGV.###MNR.Pallet1.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist1>[W2]{p}"]
[31,"DW40 – DW69",null,"Pallet station 2"]
[41,"DW 40","Bit 0","Switch 1","PortalAGV.###MNR.Pallet2.10","###INDEX:PortalAGV.###MNR.Pallet2.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch2>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet2.11","###INDEX:PortalAGV.###MNR.Pallet2.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet2.12","###INDEX:PortalAGV.###MNR.Pallet2.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet2.13","###INDEX:PortalAGV.###MNR.Pallet2.11:INDEX"]
[41,"DW 41","Bit 0","Status bit","PortalAGV.###MNR.Pallet2.20","###INDEX:PortalAGV.###MNR.Pallet2.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit2>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet2.21","###INDEX:PortalAGV.###MNR.Pallet2.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet2.22","###INDEX:PortalAGV.###MNR.Pallet2.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet2.23","###INDEX:PortalAGV.###MNR.Pallet2.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet2.24","###INDEX:PortalAGV.###MNR.Pallet2.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet2.25","###INDEX:PortalAGV.###MNR.Pallet2.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet2.26","###INDEX:PortalAGV.###MNR.Pallet2.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet2.27","###INDEX:PortalAGV.###MNR.Pallet2.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet2.28","###INDEX:PortalAGV.###MNR.Pallet2.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet2.29","###INDEX:PortalAGV.###MNR.Pallet2.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet2.30","###INDEX:PortalAGV.###MNR.Pallet2.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet2.31","###INDEX:PortalAGV.###MNR.Pallet2.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet2.32","###INDEX:PortalAGV.###MNR.Pallet2.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet2.33","###INDEX:PortalAGV.###MNR.Pallet2.33:INDEX"]
[41,"DW 50",null,"Setpoint 1","PortalAGV.###MNR.Pallet2.40","###INDEX:PortalAGV.###MNR.Pallet2.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll2>[W0]{r}"]
[41,"DW 51",null,"Setpoint 2","PortalAGV.###MNR.Pallet2.41","###INDEX:PortalAGV.###MNR.Pallet2.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll2>[W1]{r}"]
[41,"DW 52",null,"Setpoint 3","PortalAGV.###MNR.Pallet2.42","###INDEX:PortalAGV.###MNR.Pallet2.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll2>[W2]{r}"]
[41,"DW 60",null,"Actual value 1","PortalAGV.###MNR.Pallet2.50","###INDEX:PortalAGV.###MNR.Pallet2.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist2>[W0]{p}"]
[41,"DW 61",null,"Actual value 2","PortalAGV.###MNR.Pallet2.51","###INDEX:PortalAGV.###MNR.Pallet2.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist2>[W1]{p}"]
[41,"DW 62",null,"Actual value 3","PortalAGV.###MNR.Pallet2.52","###INDEX:PortalAGV.###MNR.Pallet2.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist2>[W2]{p}"]
[31,"DW70 – DW99","Pallet station 3"]
[41,"DW 70","Bit 0","Switch 1","PortalAGV.###MNR.Pallet3.10","###INDEX:PortalAGV.###MNR.Pallet3.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch3>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet3.11","###INDEX:PortalAGV.###MNR.Pallet3.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet3.12","###INDEX:PortalAGV.###MNR.Pallet3.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet3.13","###INDEX:PortalAGV.###MNR.Pallet3.11:INDEX"]
[41,"DW 71","Bit 0","Status bit","PortalAGV.###MNR.Pallet3.20","###INDEX:PortalAGV.###MNR.Pallet3.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit3>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet3.21","###INDEX:PortalAGV.###MNR.Pallet3.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet3.22","###INDEX:PortalAGV.###MNR.Pallet3.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet3.23","###INDEX:PortalAGV.###MNR.Pallet3.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet3.24","###INDEX:PortalAGV.###MNR.Pallet3.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet3.25","###INDEX:PortalAGV.###MNR.Pallet3.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet3.26","###INDEX:PortalAGV.###MNR.Pallet3.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet3.27","###INDEX:PortalAGV.###MNR.Pallet3.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet3.28","###INDEX:PortalAGV.###MNR.Pallet3.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet3.29","###INDEX:PortalAGV.###MNR.Pallet3.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet3.30","###INDEX:PortalAGV.###MNR.Pallet3.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet3.31","###INDEX:PortalAGV.###MNR.Pallet3.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet3.32","###INDEX:PortalAGV.###MNR.Pallet3.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet3.33","###INDEX:PortalAGV.###MNR.Pallet3.33:INDEX"]
[41,"DW 80",null,"Setpoint 1","PortalAGV.###MNR.Pallet3.40","###INDEX:PortalAGV.###MNR.Pallet3.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll3>[W0]{r}"]
[41,"DW 81",null,"Setpoint 2","PortalAGV.###MNR.Pallet3.41","###INDEX:PortalAGV.###MNR.Pallet3.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll3>[W1]{r}"]
[41,"DW 82",null,"Setpoint 3","PortalAGV.###MNR.Pallet3.42","###INDEX:PortalAGV.###MNR.Pallet3.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll3>[W2]{r}"]
[41,"DW 90",null,"Actual value 1","PortalAGV.###MNR.Pallet3.50","###INDEX:PortalAGV.###MNR.Pallet3.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist3>[W0]{p}"]
[41,"DW 91",null,"Actual value 2","PortalAGV.###MNR.Pallet3.51","###INDEX:PortalAGV.###MNR.Pallet3.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist3>[W1]{p}"]
[41,"DW 92",null,"Actual value 3","PortalAGV.###MNR.Pallet3.52","###INDEX:PortalAGV.###MNR.Pallet3.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist3>[W2]{p}"]
[31,"DW100 – DW129","Pallet station 4"]
[41,"DW 100","Bit 0","Switch 1","PortalAGV.###MNR.Pallet4.10","###INDEX:PortalAGV.###MNR.Pallet4.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch4>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet4.11","###INDEX:PortalAGV.###MNR.Pallet4.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet4.12","###INDEX:PortalAGV.###MNR.Pallet4.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet4.13","###INDEX:PortalAGV.###MNR.Pallet4.11:INDEX"]
[41,"DW 101","Bit 0","Status bit","PortalAGV.###MNR.Pallet4.20","###INDEX:PortalAGV.###MNR.Pallet4.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit4>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet4.21","###INDEX:PortalAGV.###MNR.Pallet4.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet4.22","###INDEX:PortalAGV.###MNR.Pallet4.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet4.23","###INDEX:PortalAGV.###MNR.Pallet4.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet4.24","###INDEX:PortalAGV.###MNR.Pallet4.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet4.25","###INDEX:PortalAGV.###MNR.Pallet4.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet4.26","###INDEX:PortalAGV.###MNR.Pallet4.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet4.27","###INDEX:PortalAGV.###MNR.Pallet4.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet4.28","###INDEX:PortalAGV.###MNR.Pallet4.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet4.29","###INDEX:PortalAGV.###MNR.Pallet4.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet4.30","###INDEX:PortalAGV.###MNR.Pallet4.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet4.31","###INDEX:PortalAGV.###MNR.Pallet4.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet4.32","###INDEX:PortalAGV.###MNR.Pallet4.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet4.33","###INDEX:PortalAGV.###MNR.Pallet4.33:INDEX"]
[41,"DW 110",null,"Setpoint 1","PortalAGV.###MNR.Pallet4.40","###INDEX:PortalAGV.###MNR.Pallet4.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll4>[W0]{r}"]
[41,"DW 111",null,"Setpoint 2","PortalAGV.###MNR.Pallet4.41","###INDEX:PortalAGV.###MNR.Pallet4.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll4>[W1]{r}"]
[41,"DW 112",null,"Setpoint 3","PortalAGV.###MNR.Pallet4.42","###INDEX:PortalAGV.###MNR.Pallet4.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll4>[W2]{r}"]
[41,"DW 120",null,"Actual value 1","PortalAGV.###MNR.Pallet4.50","###INDEX:PortalAGV.###MNR.Pallet4.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist4>[W0]{p}"]
[41,"DW 121",null,"Actual value 2","PortalAGV.###MNR.Pallet4.51","###INDEX:PortalAGV.###MNR.Pallet4.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist4>[W1]{p}"]
[41,"DW 122",null,"Actual value 3","PortalAGV.###MNR.Pallet4.52","###INDEX:PortalAGV.###MNR.Pallet4.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist4>[W2]{p}"]
[31,"DW130 – DW159","Pallet station 5"]
[41,"DW 130","Bit 0","Switch 1","PortalAGV.###MNR.Pallet5.10","###INDEX:PortalAGV.###MNR.Pallet5.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch5>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet5.11","###INDEX:PortalAGV.###MNR.Pallet5.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet5.12","###INDEX:PortalAGV.###MNR.Pallet5.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet5.13","###INDEX:PortalAGV.###MNR.Pallet5.11:INDEX"]
[41,"DW 131","Bit 0","Status bit","PortalAGV.###MNR.Pallet5.20","###INDEX:PortalAGV.###MNR.Pallet5.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit5>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet5.21","###INDEX:PortalAGV.###MNR.Pallet5.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet5.22","###INDEX:PortalAGV.###MNR.Pallet5.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet5.23","###INDEX:PortalAGV.###MNR.Pallet5.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet5.24","###INDEX:PortalAGV.###MNR.Pallet5.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet5.25","###INDEX:PortalAGV.###MNR.Pallet5.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet5.26","###INDEX:PortalAGV.###MNR.Pallet5.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet5.27","###INDEX:PortalAGV.###MNR.Pallet5.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet5.28","###INDEX:PortalAGV.###MNR.Pallet5.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet5.29","###INDEX:PortalAGV.###MNR.Pallet5.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet5.30","###INDEX:PortalAGV.###MNR.Pallet5.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet5.31","###INDEX:PortalAGV.###MNR.Pallet5.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet5.32","###INDEX:PortalAGV.###MNR.Pallet5.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet5.33","###INDEX:PortalAGV.###MNR.Pallet5.33:INDEX"]
[41,"DW 140",null,"Setpoint 1","PortalAGV.###MNR.Pallet5.40","###INDEX:PortalAGV.###MNR.Pallet5.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll5>[W0]{r}"]
[41,"DW 141",null,"Setpoint 2","PortalAGV.###MNR.Pallet5.41","###INDEX:PortalAGV.###MNR.Pallet5.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll5>[W1]{r}"]
[41,"DW 142",null,"Setpoint 3","PortalAGV.###MNR.Pallet5.42","###INDEX:PortalAGV.###MNR.Pallet5.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll5>[W2]{r}"]
[41,"DW 150",null,"Actual value 1","PortalAGV.###MNR.Pallet5.50","###INDEX:PortalAGV.###MNR.Pallet5.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist5>[W0]{p}"]
[41,"DW 151",null,"Actual value 2","PortalAGV.###MNR.Pallet5.51","###INDEX:PortalAGV.###MNR.Pallet5.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist5>[W1]{p}"]
[41,"DW 152",null,"Actual value 3","PortalAGV.###MNR.Pallet5.52","###INDEX:PortalAGV.###MNR.Pallet5.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist5>[W2]{p}"]
[31,"DW160 – DW189","Pallet station 6"]
[41,"DW 160","Bit 0","Switch 1","PortalAGV.###MNR.Pallet6.10","###INDEX:PortalAGV.###MNR.Pallet6.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch6>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet6.11","###INDEX:PortalAGV.###MNR.Pallet6.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet6.12","###INDEX:PortalAGV.###MNR.Pallet6.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet6.13","###INDEX:PortalAGV.###MNR.Pallet6.11:INDEX"]
[41,"DW 161","Bit 0","Status bit","PortalAGV.###MNR.Pallet6.20","###INDEX:PortalAGV.###MNR.Pallet6.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit6>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet6.21","###INDEX:PortalAGV.###MNR.Pallet6.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet6.22","###INDEX:PortalAGV.###MNR.Pallet6.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet6.23","###INDEX:PortalAGV.###MNR.Pallet6.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet6.24","###INDEX:PortalAGV.###MNR.Pallet6.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet6.25","###INDEX:PortalAGV.###MNR.Pallet6.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet6.26","###INDEX:PortalAGV.###MNR.Pallet6.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet6.27","###INDEX:PortalAGV.###MNR.Pallet6.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet6.28","###INDEX:PortalAGV.###MNR.Pallet6.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet6.29","###INDEX:PortalAGV.###MNR.Pallet6.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet6.30","###INDEX:PortalAGV.###MNR.Pallet6.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet6.31","###INDEX:PortalAGV.###MNR.Pallet6.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet6.32","###INDEX:PortalAGV.###MNR.Pallet6.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet6.33","###INDEX:PortalAGV.###MNR.Pallet6.33:INDEX"]
[41,"DW 170",null,"Setpoint 1","PortalAGV.###MNR.Pallet6.40","###INDEX:PortalAGV.###MNR.Pallet6.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll6>[W0]{r}"]
[41,"DW 171",null,"Setpoint 2","PortalAGV.###MNR.Pallet6.41","###INDEX:PortalAGV.###MNR.Pallet6.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll6>[W1]{r}"]
[41,"DW 172",null,"Setpoint 3","PortalAGV.###MNR.Pallet6.42","###INDEX:PortalAGV.###MNR.Pallet6.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll6>[W2]{r}"]
[41,"DW 180",null,"Actual value 1","PortalAGV.###MNR.Pallet6.50","###INDEX:PortalAGV.###MNR.Pallet6.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist6>[W0]{p}"]
[41,"DW 181",null,"Actual value 2","PortalAGV.###MNR.Pallet6.51","###INDEX:PortalAGV.###MNR.Pallet6.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist6>[W1]{p}"]
[41,"DW 182",null,"Actual value 3","PortalAGV.###MNR.Pallet6.52","###INDEX:PortalAGV.###MNR.Pallet6.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist6>[W2]{p}"]
[31,"DW190 – DW219","Pallet station 7"]
[41,"DW 190","Bit 0","Switch 1","PortalAGV.###MNR.Pallet7.10","###INDEX:PortalAGV.###MNR.Pallet7.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch7>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet7.11","###INDEX:PortalAGV.###MNR.Pallet7.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet7.12","###INDEX:PortalAGV.###MNR.Pallet7.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet7.13","###INDEX:PortalAGV.###MNR.Pallet7.11:INDEX"]
[41,"DW 191","Bit 0","Status bit","PortalAGV.###MNR.Pallet7.20","###INDEX:PortalAGV.###MNR.Pallet7.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit7>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet7.21","###INDEX:PortalAGV.###MNR.Pallet7.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet7.22","###INDEX:PortalAGV.###MNR.Pallet7.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet7.23","###INDEX:PortalAGV.###MNR.Pallet7.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet7.24","###INDEX:PortalAGV.###MNR.Pallet7.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet7.25","###INDEX:PortalAGV.###MNR.Pallet7.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet7.26","###INDEX:PortalAGV.###MNR.Pallet7.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet7.27","###INDEX:PortalAGV.###MNR.Pallet7.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet7.28","###INDEX:PortalAGV.###MNR.Pallet7.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet7.29","###INDEX:PortalAGV.###MNR.Pallet7.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet7.30","###INDEX:PortalAGV.###MNR.Pallet7.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet7.31","###INDEX:PortalAGV.###MNR.Pallet7.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet7.32","###INDEX:PortalAGV.###MNR.Pallet7.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet7.33","###INDEX:PortalAGV.###MNR.Pallet7.33:INDEX"]
[41,"DW 200",null,"Setpoint 1","PortalAGV.###MNR.Pallet7.40","###INDEX:PortalAGV.###MNR.Pallet7.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll7>[W0]{r}"]
[41,"DW 201",null,"Setpoint 2","PortalAGV.###MNR.Pallet7.41","###INDEX:PortalAGV.###MNR.Pallet7.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll7>[W1]{r}"]
[41,"DW 202",null,"Setpoint 3","PortalAGV.###MNR.Pallet7.42","###INDEX:PortalAGV.###MNR.Pallet7.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll7>[W2]{r}"]
[41,"DW 210",null,"Actual value 1","PortalAGV.###MNR.Pallet7.50","###INDEX:PortalAGV.###MNR.Pallet7.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist7>[W0]{p}"]
[41,"DW 211",null,"Actual value 2","PortalAGV.###MNR.Pallet7.51","###INDEX:PortalAGV.###MNR.Pallet7.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist7>[W1]{p}"]
[41,"DW 212",null,"Actual value 3","PortalAGV.###MNR.Pallet7.52","###INDEX:PortalAGV.###MNR.Pallet7.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist7>[W2]{p}"]
[31,"DW220 – DW249","Pallet station 8"]
[41,"DW 220","Bit 0","Switch 1","PortalAGV.###MNR.Pallet8.10","###INDEX:PortalAGV.###MNR.Pallet8.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch8>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet8.11","###INDEX:PortalAGV.###MNR.Pallet8.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet8.12","###INDEX:PortalAGV.###MNR.Pallet8.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet8.13","###INDEX:PortalAGV.###MNR.Pallet8.11:INDEX"]
[41,"DW 221","Bit 0","Status bit","PortalAGV.###MNR.Pallet8.20","###INDEX:PortalAGV.###MNR.Pallet8.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit8>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet8.21","###INDEX:PortalAGV.###MNR.Pallet8.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet8.22","###INDEX:PortalAGV.###MNR.Pallet8.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet8.23","###INDEX:PortalAGV.###MNR.Pallet8.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet8.24","###INDEX:PortalAGV.###MNR.Pallet8.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet8.25","###INDEX:PortalAGV.###MNR.Pallet8.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet8.26","###INDEX:PortalAGV.###MNR.Pallet8.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet8.27","###INDEX:PortalAGV.###MNR.Pallet8.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet8.28","###INDEX:PortalAGV.###MNR.Pallet8.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet8.29","###INDEX:PortalAGV.###MNR.Pallet8.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet8.30","###INDEX:PortalAGV.###MNR.Pallet8.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet8.31","###INDEX:PortalAGV.###MNR.Pallet8.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet8.32","###INDEX:PortalAGV.###MNR.Pallet8.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet8.33","###INDEX:PortalAGV.###MNR.Pallet8.33:INDEX"]
[41,"DW 230",null,"Setpoint 1","PortalAGV.###MNR.Pallet8.40","###INDEX:PortalAGV.###MNR.Pallet8.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll8>[W0]{r}"]
[41,"DW 231",null,"Setpoint 2","PortalAGV.###MNR.Pallet8.41","###INDEX:PortalAGV.###MNR.Pallet8.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll8>[W1]{r}"]
[41,"DW 232",null,"Setpoint 3","PortalAGV.###MNR.Pallet8.42","###INDEX:PortalAGV.###MNR.Pallet8.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll8>[W2]{r}"]
[41,"DW 240",null,"Actual value 1","PortalAGV.###MNR.Pallet8.50","###INDEX:PortalAGV.###MNR.Pallet8.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist8>[W0]{p}"]
[41,"DW 241",null,"Actual value 2","PortalAGV.###MNR.Pallet8.51","###INDEX:PortalAGV.###MNR.Pallet8.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist8>[W1]{p}"]
[41,"DW 242",null,"Actual value 3","PortalAGV.###MNR.Pallet8.52","###INDEX:PortalAGV.###MNR.Pallet8.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist8>[W2]{p}"]
[31,"DW250 – DW279","Pallet station 9"]
[41,"DW 250","Bit 0","Switch 1","PortalAGV.###MNR.Pallet9.10","###INDEX:PortalAGV.###MNR.Pallet9.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch9>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet9.11","###INDEX:PortalAGV.###MNR.Pallet9.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet9.12","###INDEX:PortalAGV.###MNR.Pallet9.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet9.13","###INDEX:PortalAGV.###MNR.Pallet9.11:INDEX"]
[41,"DW 251","Bit 0","Status bit","PortalAGV.###MNR.Pallet9.20","###INDEX:PortalAGV.###MNR.Pallet9.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit9>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet9.21","###INDEX:PortalAGV.###MNR.Pallet9.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet9.22","###INDEX:PortalAGV.###MNR.Pallet9.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet9.23","###INDEX:PortalAGV.###MNR.Pallet9.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet9.24","###INDEX:PortalAGV.###MNR.Pallet9.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet9.25","###INDEX:PortalAGV.###MNR.Pallet9.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet9.26","###INDEX:PortalAGV.###MNR.Pallet9.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet9.27","###INDEX:PortalAGV.###MNR.Pallet9.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet9.28","###INDEX:PortalAGV.###MNR.Pallet9.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet9.29","###INDEX:PortalAGV.###MNR.Pallet9.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet9.30","###INDEX:PortalAGV.###MNR.Pallet9.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet9.31","###INDEX:PortalAGV.###MNR.Pallet9.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet9.32","###INDEX:PortalAGV.###MNR.Pallet9.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet9.33","###INDEX:PortalAGV.###MNR.Pallet9.33:INDEX"]
[41,"DW 260",null,"Setpoint 1","PortalAGV.###MNR.Pallet9.40","###INDEX:PortalAGV.###MNR.Pallet9.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll9>[W0]{r}"]
[41,"DW 261",null,"Setpoint 2","PortalAGV.###MNR.Pallet9.41","###INDEX:PortalAGV.###MNR.Pallet9.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll9>[W1]{r}"]
[41,"DW 262",null,"Setpoint 3","PortalAGV.###MNR.Pallet9.42","###INDEX:PortalAGV.###MNR.Pallet9.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll9>[W2]{r}"]
[41,"DW 270",null,"Actual value 1","PortalAGV.###MNR.Pallet9.50","###INDEX:PortalAGV.###MNR.Pallet9.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist9>[W0]{p}"]
[41,"DW 271",null,"Actual value 2","PortalAGV.###MNR.Pallet9.51","###INDEX:PortalAGV.###MNR.Pallet9.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist9>[W1]{p}"]
[41,"DW 272",null,"Actual value 3","PortalAGV.###MNR.Pallet9.52","###INDEX:PortalAGV.###MNR.Pallet9.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist9>[W2]{p}"]
[31,"DW280 – DW309","Pallet station 10"]
[41,"DW 280","Bit 0","Switch 1","PortalAGV.###MNR.Pallet10.10","###INDEX:PortalAGV.###MNR.Pallet10.10:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_sch10>[W]{r}"]
[41,null,"Bit 1","Switch 2","PortalAGV.###MNR.Pallet10.11","###INDEX:PortalAGV.###MNR.Pallet10.11:INDEX"]
[41,null,"Bit 2","Switch 3","PortalAGV.###MNR.Pallet10.12","###INDEX:PortalAGV.###MNR.Pallet10.11:INDEX"]
[41,null,"Bit 3","Switch 4","PortalAGV.###MNR.Pallet10.13","###INDEX:PortalAGV.###MNR.Pallet10.11:INDEX"]
[41,"DW 281","Bit 0","Status bit","PortalAGV.###MNR.Pallet10.20","###INDEX:PortalAGV.###MNR.Pallet10.20:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_bit10>[W]{p}"]
[41,null,"Bit 1","Status bit","PortalAGV.###MNR.Pallet10.21","###INDEX:PortalAGV.###MNR.Pallet10.21:INDEX"]
[41,null,"Bit 2","Status bit","PortalAGV.###MNR.Pallet10.22","###INDEX:PortalAGV.###MNR.Pallet10.22:INDEX"]
[41,null,"Bit 3","Status bit","PortalAGV.###MNR.Pallet10.23","###INDEX:PortalAGV.###MNR.Pallet10.23:INDEX"]
[41,null,"Bit 4","Status bit","PortalAGV.###MNR.Pallet10.24","###INDEX:PortalAGV.###MNR.Pallet10.24:INDEX"]
[41,null,"Bit 5","Status bit","PortalAGV.###MNR.Pallet10.25","###INDEX:PortalAGV.###MNR.Pallet10.25:INDEX"]
[41,null,"Bit 6","Status bit","PortalAGV.###MNR.Pallet10.26","###INDEX:PortalAGV.###MNR.Pallet10.26:INDEX"]
[41,null,"Bit 7","Status bit","PortalAGV.###MNR.Pallet10.27","###INDEX:PortalAGV.###MNR.Pallet10.27:INDEX"]
[41,null,"Bit 8","Status bit","PortalAGV.###MNR.Pallet10.28","###INDEX:PortalAGV.###MNR.Pallet10.28:INDEX"]
[41,null,"Bit 9","Status bit","PortalAGV.###MNR.Pallet10.29","###INDEX:PortalAGV.###MNR.Pallet10.29:INDEX"]
[41,null,"Bit 10","Status bit","PortalAGV.###MNR.Pallet10.30","###INDEX:PortalAGV.###MNR.Pallet10.30:INDEX"]
[41,null,"Bit 11","Status bit","PortalAGV.###MNR.Pallet10.31","###INDEX:PortalAGV.###MNR.Pallet10.31:INDEX"]
[41,null,"Bit 12","Status bit","PortalAGV.###MNR.Pallet10.32","###INDEX:PortalAGV.###MNR.Pallet10.32:INDEX"]
[41,null,"Bit 13","Status bit","PortalAGV.###MNR.Pallet10.33","###INDEX:PortalAGV.###MNR.Pallet10.33:INDEX"]
[41,"DW 290",null,"Setpoint 1","PortalAGV.###MNR.Pallet10.40","###INDEX:PortalAGV.###MNR.Pallet10.40:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll10>[W0]{r}"]
[41,"DW 291",null,"Setpoint 2","PortalAGV.###MNR.Pallet10.41","###INDEX:PortalAGV.###MNR.Pallet10.41:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll10>[W1]{r}"]
[41,"DW 292",null,"Setpoint 3","PortalAGV.###MNR.Pallet10.42","###INDEX:PortalAGV.###MNR.Pallet10.42:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_soll10>[W2]{r}"]
[41,"DW 300",null,"Actual value 1","PortalAGV.###MNR.Pallet10.50","###INDEX:PortalAGV.###MNR.Pallet10.50:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist10>[W0]{p}"]
[41,"DW 301",null,"Actual value 2","PortalAGV.###MNR.Pallet10.51","###INDEX:PortalAGV.###MNR.Pallet10.51:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist10>[W1]{p}"]
[41,"DW 302",null,"Actual value 3","PortalAGV.###MNR.Pallet10.52","###INDEX:PortalAGV.###MNR.Pallet10.52:INDEX","Ch1.###MNR_T_portagv<.m###MNR_pagv_ist10>[W2]{p}"]

{"sheet":"ServoRes","index":111,"n_rows":10,"n_cols":3,"rows_kept":10,"flags":["formulas_cached_only"]}
["ServoExt","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 130 ","Servo 1, 1st Machine "]
[21,"DB 131-139","Servo 2-10 1st Machine "]
[41,"DB 140-179","Servo Machine 2-5"]
[21,"DB 540","Servo 11, 1st Machine "]
[21,"DB 541-579","Servo 12-50 1st Machine "]
[41,"DB 580-739","Servo Machine 2-5"]
[1,"###MAIN"]
[1,"DB 130-179 / 540-739 Servos"]

{"sheet":"BucketChain","index":112,"n_rows":20,"n_cols":7,"rows_kept":20,"flags":["formulas_cached_only"]}
["XBucketChain","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 740","Parameter Becherkette"]
[41,"DB 741-744","Parameter Becherkette 2-5"]
[1,"###MAIN"]
[1,"DB 740-744 Parameter Becherkette"]
[21,"DB ###ADDR:530+1[MNR]:ADDR","Parameter Becherkette ###MNR"]
[41,"DW 0","Bit 0","Parameters changed",null,null,"Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_aender>[B]{w}"]
[41]
[41,"DW 10",null,"Value 1","BucketChain.10","###INDEX:BucketChain.10:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_aist[W0]{r}"]
[41,"DW 20",null,"Value 1 left","BucketChain.20","###INDEX:BucketChain.20:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_list[W0]{r}"]
[41,"DW 21",null,"Value 2 left","BucketChain.21","###INDEX:BucketChain.21:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_list[W1]{r}"]
[41,"DW 30",null,"Value 1 right","BucketChain.20","###INDEX:BucketChain.20:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_rist[W0]{r}"]
[41,"DW 31",null,"Value 2 right","BucketChain.21","###INDEX:BucketChain.21:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_rist[W1]{r}"]
[41]
[41,"DW 40",null,"Parameter 1","BucketChain.40","###INDEX:BucketChain.40:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_asoll[W0]{r}"]
[41,"DW 41",null,"Parameter 2","BucketChain.41","###INDEX:BucketChain.41:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_asoll[W1]{r}"]
[41,"DW 42",null,"Parameter 3","BucketChain.42","###INDEX:BucketChain.42:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_asoll[W2]{r}"]
[41,"DW 50",null,"Parameter 1 left","BucketChain.50","###INDEX:BucketChain.50:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_lsoll[W0]{r}"]
[41,"DW 60",null,"Parameter 1 right","BucketChain.50","###INDEX:BucketChain.50:INDEX","Ch1.###MNR_T_bucketchain<.m###MNR_bucketchain_rsoll[W0]{r}"]

{"sheet":"DCS_Trend","index":113,"n_rows":34,"n_cols":7,"rows_kept":34,"flags":["formulas_cached_only"]}
["DCS_Trend","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 900","DCS trends 1st Machine, from control"]
[41,"DB 905","Trends Machine  2-5"]
[21,"DB 950","DCS trends 1st Machine, to control"]
[41,"DB 955","Trends Machine  2-5"]
[1,"###MAIN"]
[1,"DB 900-920 / 950-970 DCS Trends"]
[21,"DB ###ADDR:900+5[MNR]:ADDR","DCS trends ###MNR from control"]
[41,"DW 0 - 99",null,"Trend 1 data from control (shift register)",null,null,"Ch1.###MNR_T_zyk_trendr<.m###MNR_tr1_data>[W0-99]{r}"]
[41,"DW 100 - 199",null,"Trend 2 data from control (shift register)",null,null,"Ch1.###MNR_T_zyk_trendr<.m###MNR_tr2_data>[W0-99]{r}"]
[41,"DW 200 - 299",null,"Trend 3 data from control (shift register)",null,null,"Ch1.###MNR_T_zyk_trendr<.m###MNR_tr3_data>[W0-99]{r}"]
[41,"DW 300 - 399",null,"Trend 4 data from control (shift register)",null,null,"Ch1.###MNR_T_zyk_trendr<.m###MNR_tr4_data>[W0-99]{r}"]
[41,"DW 400 - 499",null,"Trend 5 data from control (shift register)",null,null,"Ch1.###MNR_T_zyk_trendr<.m###MNR_tr5_data>[W0-99]{r}"]
[21,"DB ###ADDR:950+5[MNR]:ADDR","DCS trends ###MNR to control"]
[41,"DW 0","Bit 14","Request new data record trend 1",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr1_new_record>[B]{r}"]
[41,null,"Bit 15","Reset trend 1",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr1_reset>[B]{r}"]
[41,"DW 1",null,"Pointer read position trend 1",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr1_lese_idx>[W]{r}"]
[41]
[41,"DW 5","Bit 14","Request new data record trend 2",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr2_new_record>[B]{r}"]
[41,null,"Bit 15","Reset trend 2",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr2_reset>[B]{r}"]
[41,"DW 6",null,"Pointer read position trend 2",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr2_lese_idx>[W]{r}"]
[41]
[41,"DW 10","Bit 14","Request new data record trend 3",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr3_new_record>[B]{r}"]
[41,null,"Bit 15","Reset trend 3",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr3_reset>[B]{r}"]
[41,"DW 11",null,"Pointer read position trend 3",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr3_lese_idx>[W]{r}"]
[41]
[41,"DW 15","Bit 14","Request new data record trend 4",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr4_new_record>[B]{r}"]
[41,null,"Bit 15","Reset trend 4",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr4_reset>[B]{r}"]
[41,"DW 16",null,"Pointer read position trend 4",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr4_lese_idx>[W]{r}"]
[41]
[41,"DW 20","Bit 14","Request new data record trend 5",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr5_new_record>[B]{r}"]
[41,null,"Bit 15","Reset trend 5",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr5_reset>[B]{r}"]
[41,"DW 21",null,"Pointer read position trend 5",null,null,"Ch1.###MNR_T_zyk_trendw<.m###MNR_tr5_lese_idx>[W]{r}"]

{"sheet":"leer (3)","index":114,"n_rows":4,"n_cols":2,"rows_kept":4,"hidden":true,"flags":["formulas_cached_only"]}
["NAME"]
[1,"###OVERVIEW"]
[]
[1,"###MAIN"]

{"sheet":"MaterialChange","index":115,"n_rows":54,"n_cols":4,"rows_kept":54,"flags":["formulas_cached_only"]}
["MaterialChange","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 901","Write brand change"]
[21,"DB 902","Write brand codes"]
[41,"DB 906-922","Brand codes, Machine 2-5"]
[21,"DB 951","Read brand change"]
[21,"DB 952","Read brand codes"]
[41,"DB 956-972","Brand change, Machine 2-5"]
[21,"DB 980","Brand change / Scan codes"]
[1,"###MAIN"]
[1,"DB 901-980 Brand change"]
[21,"DB ###ADDR:901+5[MNR]:ADDR","Write brand change ###MNR"]
[41,"DW 10",null,"Bitmap to Visu"]
[41,null,"Bit 0","Move Scancode old/new allowed"]
[41,"DW 81",null,"Material number, last read MC"]
[41,"DW 82-121",null,"Material 1, scanned"]
[41,"DW 122-161",null,"Material 2, scanned"]
[41,"DW 162-201",null,"Material 3, scanned"]
[21,"DB ###ADDR:902+5[MNR]:ADDR","Write brand codes ###MNR"]
[41,"DW 2",null,"DB identification"]
[41,"DW 3",null,"Material no."]
[41,"DW 4",null,"Fault no."]
[41,"DW 5",null,"Apperate Versinon"]
[41,"DW 6",null,"Order no."]
[41,"DW 7",null,"Recipe ID"]
[41,"DW 10-49",null,"Material code"]
[21,"DB ###ADDR:951+5[MNR]:ADDR","Read brand change ###MNR"]
[41,"DW 21-60",null,"Material 1, Code 1, c"]
[41,"DW 61-100",null,"Material 1, Code 2, c"]
[41,"DW 101-140",null,"Material 1, Code 3, c"]
[41,"DW 141-180",null,"Material 2, Code 1, c"]
[41,"DW 181-220",null,"Material 2, Code 2, c"]
[41,"DW 221-260",null,"Material 2, Code 3, c"]
[41,"DW 1221-1260",null,"Material 1, Code 1, n"]
[41,"DW 1261-1300",null,"Material 1, Code 2, n"]
[41,"DW 1301-1340",null,"Material 1, Code 3, n"]
[41,"DW 1341-1380",null,"Material 2, Code 1, n"]
[41,"DW 1381-1420",null,"Material 2, Code 2, n"]
[41,"DW 1421-1460",null,"Material 2, Code 3, n"]
[21,"DB ###ADDR:952+5[MNR]:ADDR","Read brand code ###MNR"]
[41,"DW 2",null,"DB identification"]
[41,"DW 3",null,"Material no."]
[41,"DW 4",null,"Fault no."]
[41,"DW 5",null,"Apperate Versinon"]
[41,"DW 6",null,"Order no."]
[41,"DW 7",null,"Recipe ID"]
[21,"DB 980","Brand change / Scan codes"]
[41,"DW 11",null,"Bits from control"]
[41,"DW 12",null,"Material no."]
[41,"DW 15",null,"Bits to control"]
[41,"DW 21-60",null,"Scan code 1"]
[41,"DW 61-100",null,"Scan code 2"]
[41,"DW 101-140",null,"Scan code 3"]
[41]

{"sheet":"RecipeManagement","index":116,"n_rows":33,"n_cols":4,"rows_kept":33,"flags":["formulas_cached_only"]}
["RecipeManagement","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 931","Recipe management"]
[41,"DB 931-935","Rezept Management Machine 2-5"]
[1,"###MAIN"]
[1,"DB 931-935 Recipe management"]
[21,"DB ###ADDR:931+1[MNR]:ADDR","Recipe management ###MNR"]
[41,"DW 10",null,"Recipe number"]
[41,"DW 12",null,"Task coding "]
[41,null,null,"16: Save"]
[41,null,null,"17: Load"]
[41,null,null,"19: Delete"]
[41,null,null,">100: Fault = Number -100"]
[41,"DW 13","Bit 0","Material(1) oder Rezeptverwaltung (0)"]
[41]
[41,"DW 40",null,"Apparatenummer"]
[41,"DW 41",null,"Auftrag"]
[41,"DW 42",null,"Status"]
[41,"DW 43",null,"ButtontextNr. OK"]
[41,"DW 44",null,"ButtontextNr. Wiederholen"]
[41]
[41,"DW 50",null,"From Control"]
[41,null,"Bit 0","Normal"]
[41,null,"Bit 1","Warning"]
[41,null,"Bit 2","Fault"]
[41,null,"Bit 3","mit Bestätigung"]
[41,null,"Bit 4","Techniker anfaordern"]
[41,null,"Bit 5","Wiederholen ?"]
[41,null,"Bit 6","Rezept / Parameter aktiv"]
[41,null,"Bit 7","Freigabe Rezeptverwaltung (Drehzahl)"]
[41,"DW 60",null,"To Control"]
[41,null,"Bit 3","mit Bestätigung"]
[41,null,"Bit 5","Wiederholen"]

{"sheet":"MaterialChangeStep","index":117,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
["MaterialChangeStep"]
[1,"###OVERVIEW"]
[21,"DB 940","Weiterschaltbedingungen"]
[]
[1,"###MAIN"]
[1,"DB 940 Weiterschaltbedingungen Materialwechsel"]
[21,"DB 940","Weiterschaltbedingungen"]
[41,"DW 10-19",null,"Text Weiterschaltbedingung 1-10",null,null,"Ch1.T_mw_weiterschalt<.mw_weiter_text>[W0-9]{r}"]
[41,"DW 20",null,"Status Weiterschaltbedingung 1",null,null,"Ch1.T_mw_weiterschalt<.mw_weiter_status>[W0]{r}"]
[41,null,"Bit 0","Bedingung erfüllt"]
[41,null,"Bit 1","Bedingung nicht erfüllt"]
[41,null,"Bit 2","Bedingung wurde manuell bestätigt"]
[41,null,"Bit 3","Freigabe manuelle Bestätigung"]
[41,null,"Bit 4","Zähler anzeigen"]
[41,"DW 21-29",null,"Status Weiterschaltbedingung 2-10",null,null,"Ch1.T_mw_weiterschalt<.mw_weiter_status>[W1-9]{r}"]
[41]
[41,"DW 50",null,"Weiterschaltbedingung 1 von Visu",null,null,"Ch1.T_mw_weiterschalt<.mw_weiter_visu>[W0]{r}"]
[41,null,"Bit 0","manuelle Bestätigung "]
[41,"DW 51-59",null,"Weiterschaltbedingung 2-10 von Visu",null,null,"Ch1.T_mw_weiterschalt<.mw_weiter_visu>[W1-9]{r}"]
[41]
[41,"DW 60",null,"Weiterschaltbedingung 1 von Visu",null,null,"Ch1.T_mw_weiterschalt<.mw_weiter_visu_2>[W]{r}"]
[41,null,"Bit 0","Schritt abbrechen"]
[41,null,"Bit 1","Schritt Wiederholen"]
[41]
[41,"DW 70-79",null,"Counter 1-10",null,null,"Ch1.T_mw_weiterschalt<.mw_weiter_zaehler>[W0-9]{r}"]

{"sheet":"StepSequence","index":118,"n_rows":39,"n_cols":7,"rows_kept":39,"flags":["formulas_cached_only"]}
["StepSequence"]
[1,"###OVERVIEW"]
[21,"DB 945","Weiterschaltbedingungen"]
[]
[1,"###MAIN"]
[1,"DB 945 Weiterschaltbedingungen"]
[21,"DB 945 Weiterschaltbedingungen","Weiterschaltbedingungen"]
[41,"DW 20",null,"Current machine  (1-5)",null,null,"Ch1.T_weiterschalt<.ws_aktmaschine>[W]{r}"]
[41,"DW 21",null,"Step chain number (1000...5999)",null,null,"Ch1.T_weiterschalt<.ws_schritt_am>[W]{r}"]
[41,"DW 22",null,"Manual intervention",null,null,"Ch1.T_weiterschalt<.ws_handein>[W]{r}"]
[41,"DW 22","Bit 0","Hand"]
[41,null,"Bit 1","Service hand"]
[41,null,"Bit 2","Reset"]
[41,null,"Bit 3","Start"]
[41,null,"Bit 4","Sichtkontrolle"]
[41,null,"Bit 8","With confirmation"]
[41,"DW 24","Bit 0","Hand Bestätigung zur SPS",null,null,"Ch1.T_weiterschalt<.ws_von_visu>[W]{r}"]
[41,"DW 25","Bit 0","Funktionsnummer",null,null,"Ch1.T_weiterschalt<.ws_funktion>[W]{r}"]
[41]
[41,"DW 30-39",null,"Text Weiterschaltbedingung 1-10",null,null,"Ch1.T_weiterschalt<.ws_weiter_text>[W0-9]{r}"]
[41,"DW 40",null,"Status Weiterschaltbedingung 1",null,null,"Ch1.T_weiterschalt<.ws_weiter_status>[W0]{r}"]
[41,null,"Bit 0","Bedingung erfüllt"]
[41,null,"Bit 1","Bedingung nicht erfüllt"]
[41,null,"Bit 2","Bedingung wurde manuell bestätigt"]
[41,null,"Bit 3","Freigabe manuelle Bestätigung"]
[41,null,"Bit 4","Zähler anzeigen"]
[41,"DW 41-49",null,"Status Weiterschaltbedingung 2-10",null,null,"Ch1.T_weiterschalt<.ws_weiter_status>[W1-9]{r}"]
[41]
[41,"DW 50",null,"Weiterschaltbedingung 1 von Visu",null,null,"Ch1.T_weiterschalt<.ws_weiter_visu>[W0]{r}"]
[41,null,"Bit 0","manuelle Bestätigung "]
[41,"DW 51-59",null,"Weiterschaltbedingung 2-10 von Visu",null,null,"Ch1T_weiterschalt<.ws_weiter_visu>[W1-9]{r}"]
[41]
[41,"DW 60",null,"Weiterschaltbedingung 1 von Visu",null,null,"Ch1.T_weiterschalt<.ws_weiter_visu_2>[W]{r}"]
[41,null,"Bit 0","Schritt abbrechen"]
[41,null,"Bit 1","Schritt Wiederholen"]
[41,"DW 63",null,"Reserve SPS"]
[41,"DW 62",null,"Reserve SPS"]
[41]
[41,"DW 70-79",null,"Counter 1-10",null,null,"Ch1.T_weiterschalt<.ws_weiter_zaehler>[W0-9]{r}"]

{"sheet":"Sonder RJR 531","index":119,"n_rows":7,"n_cols":3,"rows_kept":7,"flags":["formulas_cached_only"]}
["DCS_MainPicture"]
[1,"###OVERVIEW"]
[21,"DB 975","Datenaustausch Hostrechner"]
[1,"###MAIN"]
[1,"DB 975 Datenaustausch Hostrechner"]
[21,"DB 975","Datenaustausch Hostrechner"]
[41,"DW 0 - DW 512"]

{"sheet":"Sonder RJR","index":120,"n_rows":15,"n_cols":4,"rows_kept":15,"flags":["formulas_cached_only"]}
["DCS_MainPicture"]
[1,"###OVERVIEW"]
[21,"DB 986","Barcode Scanner RJR"]
[1,"###MAIN"]
[1,"DB 986 Barcode Scanner RJR"]
[21,"DB 986","Barcode Scanner RJR"]
[41,"DW 0","Bit 0","Wird vom BDE bei einem Markenwechsel gesetzt"]
[41,"DD 1",null,"actual Value 1"]
[41,"DD 3-31",null,"actual Value 2-16"]
[41,"DD 33",null,"last value 1"]
[41,"DD 35-63",null,"last value 2-16"]
[41,"DW70-109",null,"Text 1"]
[41,"DW 110-149",null,"Text 2"]
[41,"DW 150-709",null,"Text 3-16"]
[41]

{"sheet":"Sonder Countdown","index":121,"n_rows":8,"n_cols":4,"rows_kept":8,"flags":["formulas_cached_only"]}
["DCS_MainPicture"]
[1,"###OVERVIEW"]
[21,"DB 980","Countdown bis Schichtwechsel"]
[1,"###MAIN"]
[1,"DB 980 Countdown bis Schichtwechsel"]
[21,"DB 987","Countdown bis Schichtwechsel"]
[41]
[41,"DW 10",null,"Countdown bias zur nächsten aktiven Schicht"]

{"sheet":"ReserviertFürSPS","index":122,"n_rows":5,"n_cols":3,"rows_kept":5,"flags":["formulas_cached_only"]}
["ReserviertFürSPS"]
[1,"###OVERVIEW"]
[21,"DB 990-999","Reserviert für SPS-Remanente Daten"]
[1,"###MAIN"]
[1,"DB 990-999 Reserviert für SPS-Remanente Daten"]

{"sheet":"Printer001","index":123,"n_rows":144,"n_cols":7,"rows_kept":144,"flags":["formulas_cached_only"]}
["Printer001","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 1000","Printer001 1st Machine "]
[21,"DB 1001-1004","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 1000-1004 Printer 001"]
[21,"DB ###ADDR:1000+1[MNR]:ADDR","Printer 001 ###MNR"]
[41,"DW 0","Bit 0","Printer 001 changed",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_printer_aend>[B]{w}"]
[41,"DW 10-49",null,"LAYOUT_REGEL1",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL1>[S0-79]{w}"]
[41,"DW 50-89",null,"LAYOUT_REGEL2",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL2>[S0-79]{w}"]
[41,"DW 90-129",null,"LAYOUT_REGEL3",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL3>[S0-79]{w}"]
[41,"DW 130-169",null,"LAYOUT_REGEL4",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL4>[S0-79]{w}"]
[41,"DW 170-209",null,"LAYOUT_REGEL5",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL5>[S0-79]{w}"]
[41,"DW 210-249",null,"LAYOUT_REGEL6",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL6>[S0-79]{w}"]
[41,"DW 250-289",null,"LAYOUT_REGEL7",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL7>[S0-79]{w}"]
[41,"DW 290-329",null,"LAYOUT_REGEL8",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL8>[S0-79]{w}"]
[41,"DW 330-369",null,"LAYOUT_REGEL9",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL9>[S0-79]{w}"]
[41,"DW 370-409",null,"LAYOUT_REGEL10",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL10>[S0-79]{w}"]
[41,"DW 410-449",null,"LAYOUT_REGEL11",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL11>[S0-79]{w}"]
[41,"DW 450-489",null,"LAYOUT_REGEL12",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL12>[S0-79]{w}"]
[41,"DW 490-529",null,"LAYOUT_REGEL13",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL13>[S0-79]{w}"]
[41,"DW 530-569",null,"LAYOUT_REGEL14",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL14>[S0-79]{w}"]
[41,"DW 570-609",null,"LAYOUT_REGEL15",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL15>[S0-79]{w}"]
[41,"DW 610-649",null,"LAYOUT_REGEL16",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL16>[S0-79]{w}"]
[41,"DW 650-689",null,"LAYOUT_REGEL17",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL17>[S0-79]{w}"]
[41,"DW 690-729",null,"LAYOUT_REGEL18",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL18>[S0-79]{w}"]
[41,"DW 730-769",null,"LAYOUT_REGEL19",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL19>[S0-79]{w}"]
[41,"DW 770-809",null,"LAYOUT_REGEL20",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL20>[S0-79]{w}"]
[41,"DW 810-849",null,"LAYOUT_REGEL21",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL21>[S0-79]{w}"]
[41,"DW 850-889",null,"LAYOUT_REGEL22",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL22>[S0-79]{w}"]
[41,"DW 890-929",null,"LAYOUT_REGEL23",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL23>[S0-79]{w}"]
[41,"DW 930-969",null,"LAYOUT_REGEL24",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL24>[S0-79]{w}"]
[41,"DW 970-1009",null,"LAYOUT_REGEL25",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL25>[S0-79]{w}"]
[41,"DW 1010-1049",null,"LAYOUT_REGEL26",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL26>[S0-79]{w}"]
[41,"DW 1050-1089",null,"LAYOUT_REGEL27",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL27>[S0-79]{w}"]
[41,"DW 1090-1129",null,"LAYOUT_REGEL28",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL28>[S0-79]{w}"]
[41,"DW 1130-1169",null,"LAYOUT_REGEL29",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL29>[S0-79]{w}"]
[41,"DW 1170-1209",null,"LAYOUT_REGEL30",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL30>[S0-79]{w}"]
[41,"DW 1210-1249",null,"LAYOUT_REGEL31",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL31>[S0-79]{w}"]
[41,"DW 1250-1289",null,"LAYOUT_REGEL32",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL32>[S0-79]{w}"]
[41,"DW 1290-1329",null,"LAYOUT_REGEL33",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL33>[S0-79]{w}"]
[41,"DW 1330-1369",null,"LAYOUT_REGEL34",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL34>[S0-79]{w}"]
[41,"DW 1370-1409",null,"LAYOUT_REGEL35",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL35>[S0-79]{w}"]
[41,"DW 1410-1449",null,"LAYOUT_REGEL36",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL36>[S0-79]{w}"]
[41,"DW 1450-1489",null,"LAYOUT_REGEL37",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL37>[S0-79]{w}"]
[41,"DW 1490-1529",null,"LAYOUT_REGEL38",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL38>[S0-79]{w}"]
[41,"DW 1530-1569",null,"LAYOUT_REGEL39",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL39>[S0-79]{w}"]
[41,"DW 1570-1609",null,"LAYOUT_REGEL40",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL40>[S0-79]{w}"]
[41,"DW 1610-1649",null,"LAYOUT_REGEL41",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL41>[S0-79]{w}"]
[41,"DW 1650-1689",null,"LAYOUT_REGEL42",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL42>[S0-79]{w}"]
[41,"DW 1690-1729",null,"LAYOUT_REGEL43",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL43>[S0-79]{w}"]
[41,"DW 1730-1769",null,"LAYOUT_REGEL44",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL44>[S0-79]{w}"]
[41,"DW 1770-1809",null,"LAYOUT_REGEL45",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL45>[S0-79]{w}"]
[41,"DW 1810-1849",null,"LAYOUT_REGEL46",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL46>[S0-79]{w}"]
[41,"DW 1850-1889",null,"LAYOUT_REGEL47",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL47>[S0-79]{w}"]
[41,"DW 1890-1929",null,"LAYOUT_REGEL48",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL48>[S0-79]{w}"]
[41,"DW 1930-1969",null,"LAYOUT_REGEL49",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL49>[S0-79]{w}"]
[41,"DW 1970-2009",null,"LAYOUT_REGEL50",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL50>[S0-79]{w}"]
[41,"DW 2010-2049",null,"LAYOUT_REGEL51",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL51>[S0-79]{w}"]
[41,"DW 2050-2089",null,"LAYOUT_REGEL52",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL52>[S0-79]{w}"]
[41,"DW 2090-2129",null,"LAYOUT_REGEL53",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL53>[S0-79]{w}"]
[41,"DW 2130-2169",null,"LAYOUT_REGEL54",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL54>[S0-79]{w}"]
[41,"DW 2170-2209",null,"LAYOUT_REGEL55",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL55>[S0-79]{w}"]
[41,"DW 2210-2249",null,"LAYOUT_REGEL56",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL56>[S0-79]{w}"]
[41,"DW 2250-2289",null,"LAYOUT_REGEL57",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL57>[S0-79]{w}"]
[41,"DW 2290-2329",null,"LAYOUT_REGEL58",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL58>[S0-79]{w}"]
[41,"DW 2330-2369",null,"LAYOUT_REGEL59",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL59>[S0-79]{w}"]
[41,"DW 2370-2409",null,"LAYOUT_REGEL60",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL60>[S0-79]{w}"]
[41,"DW 2410-2449",null,"LAYOUT_REGEL61",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL61>[S0-79]{w}"]
[41,"DW 2450-2489",null,"LAYOUT_REGEL62",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL62>[S0-79]{w}"]
[41,"DW 2490-2529",null,"LAYOUT_REGEL63",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL63>[S0-79]{w}"]
[41,"DW 2530-2569",null,"LAYOUT_REGEL64",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL64>[S0-79]{w}"]
[41,"DW 2570-2609",null,"LAYOUT_REGEL65",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL65>[S0-79]{w}"]
[41,"DW 2610-2649",null,"LAYOUT_REGEL66",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL66>[S0-79]{w}"]
[41,"DW 2650-2689",null,"LAYOUT_REGEL67",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL67>[S0-79]{w}"]
[41,"DW 2690-2729",null,"LAYOUT_REGEL68",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL68>[S0-79]{w}"]
[41,"DW 2730-2769",null,"LAYOUT_REGEL69",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL69>[S0-79]{w}"]
[41,"DW 2770-2809",null,"LAYOUT_REGEL70",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL70>[S0-79]{w}"]
[41,"DW 2810-2849",null,"LAYOUT_REGEL71",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL71>[S0-79]{w}"]
[41,"DW 2850-2889",null,"LAYOUT_REGEL72",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL72>[S0-79]{w}"]
[41,"DW 2890-2929",null,"LAYOUT_REGEL73",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL73>[S0-79]{w}"]
[41,"DW 2930-2969",null,"LAYOUT_REGEL74",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL74>[S0-79]{w}"]
[41,"DW 2970-3009",null,"LAYOUT_REGEL75",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL75>[S0-79]{w}"]
[41,"DW 3010-3049",null,"LAYOUT_REGEL76",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL76>[S0-79]{w}"]
[41,"DW 3050-3089",null,"LAYOUT_REGEL77",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL77>[S0-79]{w}"]
[41,"DW 3090-3129",null,"LAYOUT_REGEL78",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL78>[S0-79]{w}"]
[41,"DW 3130-3169",null,"LAYOUT_REGEL79",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL79>[S0-79]{w}"]
[41,"DW 3170-3209",null,"LAYOUT_REGEL80",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL80>[S0-79]{w}"]
[41,"DW 3210-3249",null,"LAYOUT_REGEL81",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL81>[S0-79]{w}"]
[41,"DW 3250-3289",null,"LAYOUT_REGEL82",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL82>[S0-79]{w}"]
[41,"DW 3290-3329",null,"LAYOUT_REGEL83",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL83>[S0-79]{w}"]
[41,"DW 3330-3369",null,"LAYOUT_REGEL84",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL84>[S0-79]{w}"]
[41,"DW 3370-3409",null,"LAYOUT_REGEL85",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL85>[S0-79]{w}"]
[41,"DW 3410-2449",null,"LAYOUT_REGEL86",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL86>[S0-79]{w}"]
[41,"DW 3450-2489",null,"LAYOUT_REGEL87",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL87>[S0-79]{w}"]
[41,"DW 3490-3529",null,"LAYOUT_REGEL88",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL88>[S0-79]{w}"]
[41,"DW 3530-3569",null,"LAYOUT_REGEL89",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL89>[S0-79]{w}"]
[41,"DW 3570-3609",null,"LAYOUT_REGEL90",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL90>[S0-79]{w}"]
[41,"DW 3610-3649",null,"LAYOUT_REGEL91",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL91>[S0-79]{w}"]
[41,"DW 3650-3689",null,"LAYOUT_REGEL92",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL92>[S0-79]{w}"]
[41,"DW 3690-3729",null,"LAYOUT_REGEL93",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL93>[S0-79]{w}"]
[41,"DW 3730-3769",null,"LAYOUT_REGEL94",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL94>[S0-79]{w}"]
[41,"DW 3770-3809",null,"LAYOUT_REGEL95",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL95>[S0-79]{w}"]
[41,"DW 3810-3849",null,"LAYOUT_REGEL96",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL96>[S0-79]{w}"]
[41,"DW 3850-3889",null,"LAYOUT_REGEL97",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL97>[S0-79]{w}"]
[41,"DW 3890-3929",null,"LAYOUT_REGEL98",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL98>[S0-79]{w}"]
[41,"DW 3930-3969",null,"LAYOUT_REGEL99",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_LAYOUT_REGEL99>[S0-79]{w}"]
[41,"DW 4000-4000",null,"P_BRCVA","Printer001.###MNR.101","###INDEX:Printer001.###MNR.101:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_BRCVA>[S0-1]{w}"]
[41,"DW 4002-4002",null,"P_CASE","Printer001.###MNR.102","###INDEX:Printer001.###MNR.102:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CASE>[S0-1]{w}"]
[41,"DW 4004-4014",null,"P_CU001","Printer001.###MNR.201","###INDEX:Printer001.###MNR.201:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU001>[S0-19]{w}"]
[41,"DW 4015-4025",null,"P_CU002","Printer001.###MNR.202","###INDEX:Printer001.###MNR.202:INDEX","Ch1.###MNR_T_printer001<.m###MNR_P_CU002>[S0-19]{w}"]
[41,"DW 4026-4036",null,"P_CU003","Printer001.###MNR.203","###INDEX:Printer001.###MNR.203:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU003>[S0-19]{w}"]
[41,"DW 4037-4047",null,"P_CU004","Printer001.###MNR.204","###INDEX:Printer001.###MNR.204:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU004>[S0-19]{w}"]
[41,"DW 4048-4058",null,"P_CU005","Printer001.###MNR.205","###INDEX:Printer001.###MNR.205:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU005>[S0-19]{w}"]
[41,"DW 4059-4069",null,"P_CU006","Printer001.###MNR.206","###INDEX:Printer001.###MNR.206:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU006>[S0-19]{w}"]
[41,"DW 4070-4080",null,"P_CU007","Printer001.###MNR.207","###INDEX:Printer001.###MNR.207:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU007>[S0-19]{w}"]
[41,"DW 4081-4091",null,"P_CU008","Printer001.###MNR.208","###INDEX:Printer001.###MNR.208:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU008>[S0-19]{w}"]
[41,"DW 4092-4102",null,"P_CU009","Printer001.###MNR.209","###INDEX:Printer001.###MNR.209:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU009>[S0-19]{w}"]
[41,"DW 4103-4113",null,"P_CU010","Printer001.###MNR.210","###INDEX:Printer001.###MNR.210:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU010>[S0-19]{w}"]
[41,"DW 4114-4124",null,"P_CU011","Printer001.###MNR.211","###INDEX:Printer001.###MNR.211:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU011>[S0-19]{w}"]
[41,"DW 4125-4135",null,"P_CU012","Printer001.###MNR.212","###INDEX:Printer001.###MNR.212:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU012>[S0-19]{w}"]
[41,"DW 4136-4146",null,"P_CU013","Printer001.###MNR.213","###INDEX:Printer001.###MNR.213:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU013>[S0-19]{w}"]
[41,"DW 4147-4157",null,"P_CU014","Printer001.###MNR.214","###INDEX:Printer001.###MNR.214:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU014>[S0-19]{w}"]
[41,"DW 4158-4168",null,"P_CU015","Printer001.###MNR.215","###INDEX:Printer001.###MNR.215:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU015>[S0-19]{w}"]
[41,"DW 4169-4179",null,"P_CU016","Printer001.###MNR.216","###INDEX:Printer001.###MNR.216:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU016>[S0-19]{w}"]
[41,"DW 4180-4190",null,"P_CU017","Printer001.###MNR.217","###INDEX:Printer001.###MNR.217:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU017>[S0-19]{w}"]
[41,"DW 4191-4201",null,"P_CU018","Printer001.###MNR.218","###INDEX:Printer001.###MNR.218:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU018>[S0-19]{w}"]
[41,"DW 4202-4212",null,"P_CU019","Printer001.###MNR.219","###INDEX:Printer001.###MNR.219:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU019>[S0-19]{w}"]
[41,"DW 4213-4223",null,"P_CU020","Printer001.###MNR.220","###INDEX:Printer001.###MNR.220:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU020>[S0-19]{w}"]
[41,"DW 4224-4234",null,"P_CU021","Printer001.###MNR.221","###INDEX:Printer001.###MNR.221:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_CU021>[S0-19]{w}"]
[41,"DW 4400-4406",null,"P_EAN12","Printer001.###MNR.121","###INDEX:Printer001.###MNR.121:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_EAN12>[S0-11]{w}"]
[41,"DW 4407-4413",null,"P_EAN13","Printer001.###MNR.122","###INDEX:Printer001.###MNR.122:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_EAN13>[S0-12]{w}"]
[41,"DW 4414-4416",null,"P_MARKE","Printer001.###MNR.103","###INDEX:Printer001.###MNR.103:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_MARKE>[S0-3]{w}"]
[41,"DW 4417-4427",null,"P_PRODATXT","Printer001.###MNR.104","###INDEX:Printer001.###MNR.104:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_PRODATXT>[S0-19]{w}"]
[41,"DW 4428-4428",null,"P_PRODV","Printer001.###MNR.105","###INDEX:Printer001.###MNR.105:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_PRODV>[S0-1]{w}"]
[41,"DW 4430-4440",null,"P_PRONO","Printer001.###MNR.106","###INDEX:Printer001.###MNR.106:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_PRONO>[S0-19]{w}"]
[41,"DW 4441-4441",null,"P_PROTY","Printer001.###MNR.107","###INDEX:Printer001.###MNR.107:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_PROTY>[S0-1]{w}"]
[41,"DW 4443-4453",null,"P_PSDES","Printer001.###MNR.108","###INDEX:Printer001.###MNR.108:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_PSDES>[S0-19]{w}"]
[41]
[41,"DW 4800","Bit 0","P_EnableDataflow",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_EnableDataflow>[B]{w}"]
[41,"DW 4800","Bit 1","P_Dataflow",null,null,"Ch1.###MNR_T_printer001<.m###MNR_p001_Dataflow>[B]{w}"]
[41]
[41,"DW 4810-4816",null,"ScanCodeFromPLC","Printer001.###MNR.151","###INDEX:Printer001.###MNR.151:INDEX","Ch1.###MNR_T_printer001<.m###MNR_p001_ScanCodeFromPLC>[S0-12]{w}"]

{"sheet":"Printer002","index":124,"n_rows":144,"n_cols":7,"rows_kept":144,"flags":["formulas_cached_only"]}
["Printer002","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 1005","Printer002 1st Machine "]
[21,"DB 1006-1009","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 1005-1009 Printer 002"]
[21,"DB ###ADDR:1005+1[MNR]:ADDR","Printer 002 ###MNR"]
[41,"DW 0","Bit 0","Printer 002 changed",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_printer_aend>[B]{w}"]
[41,"DW 10-49",null,"LAYOUT_REGEL1",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL1>[S0-79]{w}"]
[41,"DW 50-89",null,"LAYOUT_REGEL2",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL2>[S0-79]{w}"]
[41,"DW 90-129",null,"LAYOUT_REGEL3",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL3>[S0-79]{w}"]
[41,"DW 130-169",null,"LAYOUT_REGEL4",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL4>[S0-79]{w}"]
[41,"DW 170-209",null,"LAYOUT_REGEL5",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL5>[S0-79]{w}"]
[41,"DW 210-249",null,"LAYOUT_REGEL6",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL6>[S0-79]{w}"]
[41,"DW 250-289",null,"LAYOUT_REGEL7",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL7>[S0-79]{w}"]
[41,"DW 290-329",null,"LAYOUT_REGEL8",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL8>[S0-79]{w}"]
[41,"DW 330-369",null,"LAYOUT_REGEL9",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL9>[S0-79]{w}"]
[41,"DW 370-409",null,"LAYOUT_REGEL10",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL10>[S0-79]{w}"]
[41,"DW 410-449",null,"LAYOUT_REGEL11",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL11>[S0-79]{w}"]
[41,"DW 450-489",null,"LAYOUT_REGEL12",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL12>[S0-79]{w}"]
[41,"DW 490-529",null,"LAYOUT_REGEL13",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL13>[S0-79]{w}"]
[41,"DW 530-569",null,"LAYOUT_REGEL14",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL14>[S0-79]{w}"]
[41,"DW 570-609",null,"LAYOUT_REGEL15",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL15>[S0-79]{w}"]
[41,"DW 610-649",null,"LAYOUT_REGEL16",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL16>[S0-79]{w}"]
[41,"DW 650-689",null,"LAYOUT_REGEL17",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL17>[S0-79]{w}"]
[41,"DW 690-729",null,"LAYOUT_REGEL18",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL18>[S0-79]{w}"]
[41,"DW 730-769",null,"LAYOUT_REGEL19",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL19>[S0-79]{w}"]
[41,"DW 770-809",null,"LAYOUT_REGEL20",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL20>[S0-79]{w}"]
[41,"DW 810-849",null,"LAYOUT_REGEL21",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL21>[S0-79]{w}"]
[41,"DW 850-889",null,"LAYOUT_REGEL22",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL22>[S0-79]{w}"]
[41,"DW 890-929",null,"LAYOUT_REGEL23",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL23>[S0-79]{w}"]
[41,"DW 930-969",null,"LAYOUT_REGEL24",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL24>[S0-79]{w}"]
[41,"DW 970-1009",null,"LAYOUT_REGEL25",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL25>[S0-79]{w}"]
[41,"DW 1010-1049",null,"LAYOUT_REGEL26",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL26>[S0-79]{w}"]
[41,"DW 1050-1089",null,"LAYOUT_REGEL27",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL27>[S0-79]{w}"]
[41,"DW 1090-1129",null,"LAYOUT_REGEL28",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL28>[S0-79]{w}"]
[41,"DW 1130-1169",null,"LAYOUT_REGEL29",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL29>[S0-79]{w}"]
[41,"DW 1170-1209",null,"LAYOUT_REGEL30",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL30>[S0-79]{w}"]
[41,"DW 1210-1249",null,"LAYOUT_REGEL31",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL31>[S0-79]{w}"]
[41,"DW 1250-1289",null,"LAYOUT_REGEL32",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL32>[S0-79]{w}"]
[41,"DW 1290-1329",null,"LAYOUT_REGEL33",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL33>[S0-79]{w}"]
[41,"DW 1330-1369",null,"LAYOUT_REGEL34",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL34>[S0-79]{w}"]
[41,"DW 1370-1409",null,"LAYOUT_REGEL35",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL35>[S0-79]{w}"]
[41,"DW 1410-1449",null,"LAYOUT_REGEL36",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL36>[S0-79]{w}"]
[41,"DW 1450-1489",null,"LAYOUT_REGEL37",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL37>[S0-79]{w}"]
[41,"DW 1490-1529",null,"LAYOUT_REGEL38",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL38>[S0-79]{w}"]
[41,"DW 1530-1569",null,"LAYOUT_REGEL39",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL39>[S0-79]{w}"]
[41,"DW 1570-1609",null,"LAYOUT_REGEL40",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL40>[S0-79]{w}"]
[41,"DW 1610-1649",null,"LAYOUT_REGEL41",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL41>[S0-79]{w}"]
[41,"DW 1650-1689",null,"LAYOUT_REGEL42",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL42>[S0-79]{w}"]
[41,"DW 1690-1729",null,"LAYOUT_REGEL43",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL43>[S0-79]{w}"]
[41,"DW 1730-1769",null,"LAYOUT_REGEL44",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL44>[S0-79]{w}"]
[41,"DW 1770-1809",null,"LAYOUT_REGEL45",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL45>[S0-79]{w}"]
[41,"DW 1810-1849",null,"LAYOUT_REGEL46",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL46>[S0-79]{w}"]
[41,"DW 1850-1889",null,"LAYOUT_REGEL47",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL47>[S0-79]{w}"]
[41,"DW 1890-1929",null,"LAYOUT_REGEL48",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL48>[S0-79]{w}"]
[41,"DW 1930-1969",null,"LAYOUT_REGEL49",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL49>[S0-79]{w}"]
[41,"DW 1970-2009",null,"LAYOUT_REGEL50",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL50>[S0-79]{w}"]
[41,"DW 2010-2049",null,"LAYOUT_REGEL51",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL51>[S0-79]{w}"]
[41,"DW 2050-2089",null,"LAYOUT_REGEL52",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL52>[S0-79]{w}"]
[41,"DW 2090-2129",null,"LAYOUT_REGEL53",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL53>[S0-79]{w}"]
[41,"DW 2130-2169",null,"LAYOUT_REGEL54",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL54>[S0-79]{w}"]
[41,"DW 2170-2209",null,"LAYOUT_REGEL55",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL55>[S0-79]{w}"]
[41,"DW 2210-2249",null,"LAYOUT_REGEL56",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL56>[S0-79]{w}"]
[41,"DW 2250-2289",null,"LAYOUT_REGEL57",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL57>[S0-79]{w}"]
[41,"DW 2290-2329",null,"LAYOUT_REGEL58",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL58>[S0-79]{w}"]
[41,"DW 2330-2369",null,"LAYOUT_REGEL59",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL59>[S0-79]{w}"]
[41,"DW 2370-2409",null,"LAYOUT_REGEL60",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL60>[S0-79]{w}"]
[41,"DW 2410-2449",null,"LAYOUT_REGEL61",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL61>[S0-79]{w}"]
[41,"DW 2450-2489",null,"LAYOUT_REGEL62",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL62>[S0-79]{w}"]
[41,"DW 2490-2529",null,"LAYOUT_REGEL63",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL63>[S0-79]{w}"]
[41,"DW 2530-2569",null,"LAYOUT_REGEL64",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL64>[S0-79]{w}"]
[41,"DW 2570-2609",null,"LAYOUT_REGEL65",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL65>[S0-79]{w}"]
[41,"DW 2610-2649",null,"LAYOUT_REGEL66",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL66>[S0-79]{w}"]
[41,"DW 2650-2689",null,"LAYOUT_REGEL67",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL67>[S0-79]{w}"]
[41,"DW 2690-2729",null,"LAYOUT_REGEL68",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL68>[S0-79]{w}"]
[41,"DW 2730-2769",null,"LAYOUT_REGEL69",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL69>[S0-79]{w}"]
[41,"DW 2770-2809",null,"LAYOUT_REGEL70",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL70>[S0-79]{w}"]
[41,"DW 2810-2849",null,"LAYOUT_REGEL71",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL71>[S0-79]{w}"]
[41,"DW 2850-2889",null,"LAYOUT_REGEL72",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL72>[S0-79]{w}"]
[41,"DW 2890-2929",null,"LAYOUT_REGEL73",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL73>[S0-79]{w}"]
[41,"DW 2930-2969",null,"LAYOUT_REGEL74",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL74>[S0-79]{w}"]
[41,"DW 2970-3009",null,"LAYOUT_REGEL75",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL75>[S0-79]{w}"]
[41,"DW 3010-3049",null,"LAYOUT_REGEL76",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL76>[S0-79]{w}"]
[41,"DW 3050-3089",null,"LAYOUT_REGEL77",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL77>[S0-79]{w}"]
[41,"DW 3090-3129",null,"LAYOUT_REGEL78",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL78>[S0-79]{w}"]
[41,"DW 3130-3169",null,"LAYOUT_REGEL79",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL79>[S0-79]{w}"]
[41,"DW 3170-3209",null,"LAYOUT_REGEL80",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL80>[S0-79]{w}"]
[41,"DW 3210-3249",null,"LAYOUT_REGEL81",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL81>[S0-79]{w}"]
[41,"DW 3250-3289",null,"LAYOUT_REGEL82",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL82>[S0-79]{w}"]
[41,"DW 3290-3329",null,"LAYOUT_REGEL83",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL83>[S0-79]{w}"]
[41,"DW 3330-3369",null,"LAYOUT_REGEL84",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL84>[S0-79]{w}"]
[41,"DW 3370-3409",null,"LAYOUT_REGEL85",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL85>[S0-79]{w}"]
[41,"DW 3410-2449",null,"LAYOUT_REGEL86",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL86>[S0-79]{w}"]
[41,"DW 3450-2489",null,"LAYOUT_REGEL87",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL87>[S0-79]{w}"]
[41,"DW 3490-3529",null,"LAYOUT_REGEL88",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL88>[S0-79]{w}"]
[41,"DW 3530-3569",null,"LAYOUT_REGEL89",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL89>[S0-79]{w}"]
[41,"DW 3570-3609",null,"LAYOUT_REGEL90",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL90>[S0-79]{w}"]
[41,"DW 3610-3649",null,"LAYOUT_REGEL91",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL91>[S0-79]{w}"]
[41,"DW 3650-3689",null,"LAYOUT_REGEL92",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL92>[S0-79]{w}"]
[41,"DW 3690-3729",null,"LAYOUT_REGEL93",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL93>[S0-79]{w}"]
[41,"DW 3730-3769",null,"LAYOUT_REGEL94",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL94>[S0-79]{w}"]
[41,"DW 3770-3809",null,"LAYOUT_REGEL95",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL95>[S0-79]{w}"]
[41,"DW 3810-3849",null,"LAYOUT_REGEL96",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL96>[S0-79]{w}"]
[41,"DW 3850-3889",null,"LAYOUT_REGEL97",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL97>[S0-79]{w}"]
[41,"DW 3890-3929",null,"LAYOUT_REGEL98",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL98>[S0-79]{w}"]
[41,"DW 3930-3969",null,"LAYOUT_REGEL99",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_LAYOUT_REGEL99>[S0-79]{w}"]
[41,"DW 4000-4000",null,"P_BRCVA","Printer002.###MNR.101","###INDEX:Printer002.###MNR.101:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_BRCVA>[S0-1]{w}"]
[41,"DW 4002-4002",null,"P_CASE","Printer002.###MNR.102","###INDEX:Printer002.###MNR.102:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CASE>[S0-1]{w}"]
[41,"DW 4004-4014",null,"P_CU001","Printer002.###MNR.201","###INDEX:Printer002.###MNR.201:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU002>[S0-19]{w}"]
[41,"DW 4015-4025",null,"P_CU002","Printer002.###MNR.202","###INDEX:Printer002.###MNR.202:INDEX","Ch1.###MNR_T_printer002<.m###MNR_P_CU002>[S0-19]{w}"]
[41,"DW 4026-4036",null,"P_CU003","Printer002.###MNR.203","###INDEX:Printer002.###MNR.203:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU003>[S0-19]{w}"]
[41,"DW 4037-4047",null,"P_CU004","Printer002.###MNR.204","###INDEX:Printer002.###MNR.204:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU004>[S0-19]{w}"]
[41,"DW 4048-4058",null,"P_CU005","Printer002.###MNR.205","###INDEX:Printer002.###MNR.205:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU005>[S0-19]{w}"]
[41,"DW 4059-4069",null,"P_CU006","Printer002.###MNR.206","###INDEX:Printer002.###MNR.206:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU006>[S0-19]{w}"]
[41,"DW 4070-4080",null,"P_CU007","Printer002.###MNR.207","###INDEX:Printer002.###MNR.207:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU007>[S0-19]{w}"]
[41,"DW 4081-4091",null,"P_CU008","Printer002.###MNR.208","###INDEX:Printer002.###MNR.208:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU008>[S0-19]{w}"]
[41,"DW 4092-4102",null,"P_CU009","Printer002.###MNR.209","###INDEX:Printer002.###MNR.209:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU009>[S0-19]{w}"]
[41,"DW 4103-4113",null,"P_CU010","Printer002.###MNR.210","###INDEX:Printer002.###MNR.210:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU010>[S0-19]{w}"]
[41,"DW 4114-4124",null,"P_CU011","Printer002.###MNR.211","###INDEX:Printer002.###MNR.211:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU011>[S0-19]{w}"]
[41,"DW 4125-4135",null,"P_CU012","Printer002.###MNR.212","###INDEX:Printer002.###MNR.212:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU012>[S0-19]{w}"]
[41,"DW 4136-4146",null,"P_CU013","Printer002.###MNR.213","###INDEX:Printer002.###MNR.213:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU013>[S0-19]{w}"]
[41,"DW 4147-4157",null,"P_CU014","Printer002.###MNR.214","###INDEX:Printer002.###MNR.214:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU014>[S0-19]{w}"]
[41,"DW 4158-4168",null,"P_CU015","Printer002.###MNR.215","###INDEX:Printer002.###MNR.215:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU015>[S0-19]{w}"]
[41,"DW 4169-4179",null,"P_CU016","Printer002.###MNR.216","###INDEX:Printer002.###MNR.216:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU016>[S0-19]{w}"]
[41,"DW 4180-4190",null,"P_CU017","Printer002.###MNR.217","###INDEX:Printer002.###MNR.217:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU017>[S0-19]{w}"]
[41,"DW 4191-4201",null,"P_CU018","Printer002.###MNR.218","###INDEX:Printer002.###MNR.218:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU018>[S0-19]{w}"]
[41,"DW 4202-4212",null,"P_CU019","Printer002.###MNR.219","###INDEX:Printer002.###MNR.219:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU019>[S0-19]{w}"]
[41,"DW 4213-4223",null,"P_CU020","Printer002.###MNR.220","###INDEX:Printer002.###MNR.220:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU020>[S0-19]{w}"]
[41,"DW 4224-4234",null,"P_CU021","Printer002.###MNR.221","###INDEX:Printer002.###MNR.221:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_CU021>[S0-19]{w}"]
[41,"DW 4400-4406",null,"P_EAN12","Printer002.###MNR.121","###INDEX:Printer002.###MNR.121:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_EAN12>[S0-11]{w}"]
[41,"DW 4407-4413",null,"P_EAN13","Printer002.###MNR.122","###INDEX:Printer002.###MNR.122:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_EAN13>[S0-12]{w}"]
[41,"DW 4414-4416",null,"P_MARKE","Printer002.###MNR.103","###INDEX:Printer002.###MNR.103:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_MARKE>[S0-3]{w}"]
[41,"DW 4417-4427",null,"P_PRODATXT","Printer002.###MNR.104","###INDEX:Printer002.###MNR.104:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_PRODATXT>[S0-19]{w}"]
[41,"DW 4428-4428",null,"P_PRODV","Printer002.###MNR.105","###INDEX:Printer002.###MNR.105:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_PRODV>[S0-1]{w}"]
[41,"DW 4430-4440",null,"P_PRONO","Printer002.###MNR.106","###INDEX:Printer002.###MNR.106:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_PRONO>[S0-19]{w}"]
[41,"DW 4441-4441",null,"P_PROTY","Printer002.###MNR.107","###INDEX:Printer002.###MNR.107:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_PROTY>[S0-1]{w}"]
[41,"DW 4443-4453",null,"P_PSDES","Printer002.###MNR.108","###INDEX:Printer002.###MNR.108:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_PSDES>[S0-19]{w}"]
[41]
[41,"DW 4800","Bit 0","P_EnableDataflow",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_EnableDataflow>[B]{w}"]
[41,"DW 4800","Bit 1","P_Dataflow",null,null,"Ch1.###MNR_T_printer002<.m###MNR_p002_Dataflow>[B]{w}"]
[41]
[41,"DW 4810-4816",null,"ScanCodeFromPLC","Printer002.###MNR.151","###INDEX:Printer002.###MNR.151:INDEX","Ch1.###MNR_T_printer002<.m###MNR_p002_ScanCodeFromPLC>[S0-12]{w}"]

{"sheet":"Printer003","index":125,"n_rows":24,"n_cols":7,"rows_kept":24,"flags":["formulas_cached_only"]}
["Printer003","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 1010","Printer003 1st Machine "]
[21,"DB 1010-1014","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 1010-1014 Printer 003"]
[21,"DB ###ADDR:1010+1[MNR]:ADDR","Printer 003 ###MNR"]
[41,"DW 0","Bit 0","Printer 003 changed",null,null,"Ch1.###MNR_T_printer003<.m###MNR_p003_printer_aend>[B]{w}"]
[41]
[41]
[21,null,null,"from HMI"]
[41,"DW 10","Bit 0","EAN Bypass",null,null,"Ch1.###MNR_T_printer003<.m###MNR_p003_EAN_Bypass_from_HMI>[B]{r}"]
[41,"DW 20-26",null,"EAN Code","Printer003.###MNR.11","###INDEX:Printer003.###MNR.11:INDEX","Ch1.###MNR_T_printer003<.m###MNR_p003_EAN_from_HMI>[S0-12]{r}"]
[41]
[21,null,null,"from PLC"]
[41,"DW 100",null,"Life counter",null,null,"Ch1.###MNR_T_printer003<.m###MNR_p003_LifeCounter_from_PLC>[W]{r}"]
[41,"DW 110-116",null,"EAN Code","Printer003.###MNR.11","###INDEX:Printer003.###MNR.11:INDEX","Ch1.###MNR_T_printer003<.m###MNR_p003_EAN_from_PLC>[S0-12]{r}"]
[41,"DW 117-123",null,"ScanCode","Printer003.###MNR.151","###INDEX:Printer003.###MNR.151:INDEX","Ch1.###MNR_T_printer003<.m###MNR_p003_ScanCode_from_PLC>[S0-12]{w}"]
[41]
[21,null,null,"from Host"]
[41,"DW 200",null,"Life counter",null,null,"Ch1.###MNR_T_printer003<.m###MNR_p003_LifeCounter_from_Host>[W]{w}"]
[41,"DW 210-216",null,"EAN Code","Printer003.###MNR.11","###INDEX:Printer003.###MNR.11:INDEX","Ch1.###MNR_T_printer003<.m###MNR_p003_EAN_from_Host>[S0-12]{r}"]
[41]

{"sheet":"Printer004","index":126,"n_rows":24,"n_cols":7,"rows_kept":24,"flags":["formulas_cached_only"]}
["Printer004","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[21,"DB 1015","printer004 1st Machine "]
[21,"DB 1015-1019","Machine  2-5"]
[]
[1,"###MAIN"]
[1,"DB 1015-1019 Printer 004"]
[21,"DB ###ADDR:1015+1[MNR]:ADDR","Printer 004 ###MNR"]
[41,"DW 0","Bit 0","Printer 004 changed",null,null,"Ch1.###MNR_T_printer004<.m###MNR_p004_printer_aend>[B]{w}"]
[41]
[41]
[21,null,null,"from HMI"]
[41,"DW 10","Bit 0","EAN Bypass",null,null,"Ch1.###MNR_T_printer004<.m###MNR_p004_EAN_Bypass_from_HMI>[B]{r}"]
[41,"DW 20-26",null,"EAN Code","printer004.###MNR.11","###INDEX:printer004.###MNR.11:INDEX","Ch1.###MNR_T_printer004<.m###MNR_p004_EAN_from_HMI>[S0-12]{r}"]
[41]
[21,null,null,"from PLC"]
[41,"DW 100",null,"Life counter",null,null,"Ch1.###MNR_T_printer004<.m###MNR_p004_LifeCounter_from_PLC>[W]{r}"]
[41,"DW 110-116",null,"EAN Code","printer004.###MNR.11","###INDEX:printer004.###MNR.11:INDEX","Ch1.###MNR_T_printer004<.m###MNR_p004_EAN_from_PLC>[S0-12]{r}"]
[41,"DW 117-123",null,"ScanCode","printer004.###MNR.151","###INDEX:printer004.###MNR.151:INDEX","Ch1.###MNR_T_printer004<.m###MNR_p004_ScanCode_from_PLC>[S0-12]{w}"]
[41]
[21,null,null,"from Host"]
[41,"DW 200",null,"Life counter",null,null,"Ch1.###MNR_T_printer004<.m###MNR_p004_LifeCounter_from_Host>[W]{w}"]
[41,"DW 210-216",null,"EAN Code","printer004.###MNR.11","###INDEX:printer004.###MNR.11:INDEX","Ch1.###MNR_T_printer004<.m###MNR_p004_EAN_from_Host>[S0-12]{r}"]
[41]

{"sheet":"Beispiel","index":127,"n_rows":36,"n_cols":2,"rows_kept":36,"flags":["formulas_cached_only"]}
["Beispiel","MASCHINENABHAENGIG"]
[1,"###OVERVIEW"]
[]
[1,"###MAIN"]
{"$rows_empty":25}
[1,"Hauptüberschrift Alles in einem Rahmen"]
[2,"Überschrift"]
[21,"Überschrift in Tabelle"]
[3,"Zwischenüberschrift"]
[31,"Überschrift in Tabelle"]
[4,"Eintrag"]
[41,"Eintrag in Tabelle"]